1 Choose menu option => 
11 Choose menu option (%d) => 
111      (%s) : 
11101 Graphics Device Selection
11102 Starting Segment = 0x%x
11103 %2d) %s
11104 PgDn for Next Page
11105 PgDn for Next Page, PgUp for Previous Page
11106 PgUp for Previous Page
11107 Enter device selection (%d) => 
11111 Graphics Device Mode Selection
11112 %2d) %d x %d, mono
11113 %2d) %d x %d, mono, %s
11114 %2d) %d x %d, %d colors
11115 %2d) %d x %d, %d colors, %s
11116 Enter mode selection (%d) => 
11117 %s
11121 Graphics Display Monitors
11122 %2d) %s
11123 %6.3f x %6.3f
11124 Enter monitor selection (%d) => 
11131 %2d) Enter screen dimensions
11132 The current screen dimensions are:
11133   horizontal size = %.3f in.
11134   vertical size   = %.3f in.
11135 Enter horizontal size of graphics display       (%.3f in.) => 
11136 Enter vertical size of graphics display         (%.3f in.) => 
11140 Enter the x size for the CADKEY graphics cursor   (%f in.) => 
11141 Enter the y size for the CADKEY graphics cursor   (%f in.) => 
11142 Enter the size for the CADKEY graphics marker     (%f in.) =>
11143 Enter the maximum number of horizontal and 
11144   vertical grid points                            (%d) =>
11145 Enter the maximum number of entities to display
11146   while dynamically rotating part                 (%d) =>
11147 Enter a value (1.0 to 5.0) for curve display, 
11148   where 5.0 is the smoothest. For faster drawing 
11149   and selection, use a coarser display.           (%.3f) => 
11150 Enter the minimum increment for sketching         (%f in.) =>
11151 'n' for Next Page
11152 'n' for Next Page, 'p' for Previous Page
11153 'p' for Previous Page
1121 The range for the current color graphics palette is 0-%d.
11201 Set Menu Options Window Colors
112011 Enter the border color             (%d) => 
112012 Enter the background color         (%d) => 
112013 Enter the text/draw color          (%d) => 
112014 Enter the border style:
112015   0 = none, 1 = single, 2 = double (%d) => 
11202 Set System Mode Indicator Colors
11203 Set Break Window Colors
11204 Set Status Window Colors
11205 Set History Line Colors
11206 Set Prompt Line Colors
11207 Set Cursor Tracking Window Colors
11208 Set Pop Up Menus Colors
11209 Set Viewport Area Colors
112091 Enter the border color for primary graphics viewport  (%d) => 
112092 Enter the border color for other graphics viewports   (%d) => 
112093 Enter the background color for all graphics viewports (%d) => 
112094 Enter the border style for all graphics viewports:
112095   0 = none, 1 = single, 2 = double                    (%d) => 
11210 Set Cursor and Marker Colors
112101 Enter the color for the CADKEY graphics cursor (%d) => 
112102 Enter the color for rubber banding             (%d) => 
112103 Enter the color for the CADKEY prompt marker   (%d) =>
1131 Set Viewport Options
1132 Enter maximum allowable number of viewports      (%d) =>
1133 Enter the spacing between viewports when using 
1134   automatic viewport placement options           (%f in.) =>
1135 Should display view axes appear in each viewport
1136   upon initial entry                                  (%c) ? 
1137 Choose display option for construction view axes
1138   upon initial entry                             (%d) =>
1141 Please enter the name of the graphics CDE to use (%s) => 
12000 CADKEY Input Device Selection
12001 CADL Input Device Selection
12002 none (keyboard cursor keys only)
12003 none (use CADKEY input device)
12100 Do you wish to redefine the tablet/mouse working area (%c) ? 
12101 Enter x dimension of tablet/mouse active area (%f in.) => 
12102 Enter y dimension of tablet/mouse active area (%f in.) => 
12103 Enter x min for cursor control area (%f in.) => 
12104 Enter y min for cursor control area (%f in.) => 
12105 Enter x max for cursor control area (%f in.) => 
12106 Enter y max for cursor control area (%f in.) => 
12107 Enter x min for function selection area (%f in.) => 
12108 Enter y min for function selection area (%f in.) => 
12109 Enter x max for function selection area (%f in.) => 
12110 Enter y max for function selection area (%f in.) => 
12111 Enter number of columns in the function area (%d) => 
12112 Enter number of rows in the function area    (%d) => 
12200 Do you wish to assign the cursor puck buttons (%c) ? 
12201 To assign functions to input device buttons:
12202   1) Use your input device to "point" to the desired function item.
12203   2) Press the input device button to which you wish to assign this
12204      function. (Some input devices also support combinations of buttons
12205      pressed simultaneously as additional "buttons".)
12206   3) Repeat step 2 for all buttons and button combinations to be assigned.
12207   4) Select "-VERIFY-" to check the value of a previously assigned button.
12208   5) Press RETURN when done.
12209 NOTE: If you do not have cursor control in this function, ensure proper
12210       connection of the input device and that you have chosen the correct
12211       input device configuration options.
12212                 BUTTON RETURN CODE: %2d        FUNCTION SELECTED: %8s
12213      VERIFY =>  BUTTON RETURN CODE: %2d        ASSIGNED FUNCTION: %8s
12214      Can't assign button: too many buttons
12215 Specify the device to which the input device is attached;
12216 If the driver for your mouse is loaded, please run CONFIG
12217 again and select Microsoft Mouse.  
12218 Now you must enter which device your mouse is attached 
12219 to.  Most users will enter COM1 or COM2 at this point.
13000 CADKEY Plotter Selection
13001 XXnone
13100 Choose plot paper size (%d) => 
13101 Enter plot paper X size in inches (%f) => 
13102 Enter plot paper Y size in inches (%f) => 
13200 The following clip limits correspond to the soft clip limits
13210 for the selected plotter. These will determine the plotting
13220 area used by the plotter. Refer to your plotter manual for 
13230 clip limits used by your plotter.
13240 Enter X min clip limit in millimeters (%f) =>
13250 Enter Y min clip limit in millimeters (%f) =>
13260 Enter X max clip limit in millimeters (%f) =>
13270 Enter Y max clip limit in millimeters (%f) =>
13300 CADKEY attempts to center plots on the paper, but some plotters
13301 automatically add a small offset. If you wish to compensate for
13302 this offset or if you do not wish to have a centered plot, use
13303 non-zero values for X and Y offsets. Note that offsets are
13304 expressed in terms of the units being plotted (in/mm) and are 
13305 independent of plotting scale.
13306 Enter X offset for plot (%f) => 
13307 Enter Y offset for plot (%f) => 
13400 Enter plotter pen width in mm (%f) => 
13500 Refer to your plotter manual for pen velocities supported by your
13501 plotter. Enter a value between 1 and the maximum speed supported.
13502 Enter value in cm/sec (%d) => 
13600 Do you wish to change the assignment of plot pens to CADKEY colors (%c) ? 
13601 Plotter pen numbers 1-16 are available for CADKEY color #%d.
13602 Enter value (%d) => 
13610 Enter a factor (greater than 1.0) for curve tolerance. A higher
13615 factor will generate smoother curves but will take longer to plot.
13620 This value corresponds to the number of lines that a curve will be
13625 broken up into regardless of its size.
13630 Enter curve tolerance factor (%f) => 
13650 Choose pen sorting option (%d) => 
13700 Plotter codes may be sent to a serial port (-n), parallel port (+n)
13701 or a file.  If a serial port is specified explicitly (eg. COM1 instead
13702 of -1) then you must configure the port for the correct communication's
13703 parameters using the DOS MODE command.
13704 NOTE: If the plotter is on a network the port should be specified
13705 explicitly (eg. COM1).
13706 Enter the name of the output port or file (%s) : 
13707 Choose baud rate (%d) => 
13710 Plotter output may be sent to a file or device by specifying the
13711 file or device name or may be sent to a spooler or filter program
13712 by preceding the spooler or filter name with '|'.
14000 CADKEY Printer Selection
14001 XXnone
14100 Choose printing resolution (%d) => 
14101 Choose printing mode: 0. Black and white, 1. color (%d) => 
14200 Do you wish to reassign the printer paper limits (%c) ? 
14201 Enter X min for paper (%f in.) => 
14202 Enter Y min for paper (%f in.) => 
14203 Enter X max for paper (%f in.) => 
14204 Enter Y max for paper (%f in.) => 
14303 Enter value (%d) => 
14400 Printer codes may be sent to a serial port (-n), parallel port (+n)
14401 or a file. If a serial port is specified explicitly (eg. COM1 instead
14402 of -1) then you must configure the port for the correct communication's
14403 parameters using the DOS MODE command.
14404 NOTE: If the printer is on a network the port should be specified
14405 explicitly (eg. COM1).
14406 Enter the name of the output port or file (%s) : 
14407 Choose baud rate (%d) => 
14410 Printer output may be sent to a file or device by specifying the
14411 file or device name or may be sent to a spooler or filter program
14412 by preceding the spooler or filter name with '|'.
151012 CADKEY uses temporary storage when it runs out of memory for the
151013 data base.  Temporary storage for your data base may reside in one 
151014 or more areas.  To store data base files on disk, a full path name 
151015 must be specified.  CADKEY allows up to two database storage areas.
151018 To specify more than one storage area separate with a semi-colon. 
1510121 CADKEY uses temporary storage when it runs out of memory for the
1510131 data base.  Temporary storage for your data base may reside in one 
1510141 or more areas.  To store data base files on disk, a full path name 
1510151 must be specified.  To specify more than one storage area separate 
1510161 with a semi-colon. CADKEY allows up to two database storage areas.
151019 For example:
151020   d:\tmp;c:\cadkey\db
151022     -- "d:\tmp" is the primary data base storage area.
151023     -- "c:\cadkey\db" is the secondary data base storage area.
1510201   /bin;/cadkey/db
1510221     -- "/bin" is the primary data base storage area.
1510231     -- "/cadkey/db" is the secondary data base storage area.
151025   /tmp;/usr/tmp;.
151027     -- "/tmp" is the primary data base storage area.
151028     -- "/usr/tmp" is the secondary data base storage area.
151029     -- "." is the tertiary data base storage area.
1510251   \tmp;.
1510271     -- "\tmp" is the primary data base storage area.
1510281     -- "." is the secondary data base storage area.
151030 Enter storage path(s) for data base files:
151040 Enter path for other system scratch files: 
151050 The CADKEY database will page to disk when there is no more memory
151051 available. The amount of memory that the database will use before it
151052 starts to page can be set here. Setting the value too low may degrade
151053 performance. Setting the value too high may cause the database to use
151054 all available memory and therefore cripple some CADKEY functions that
151055 require temporary memory. Setting a value of 0 will cause CADKEY to
151056 calculate an optimal setting for this value.
151057 Enter the number of K to use for database storage (%ld) => 
15108 System memory must be allocated for on-line printing and executing  
15109 complex functions from within CADKEY. At least 25K must be allocated
15110 for this purpose. By specifying a larger amount of memory, performance
15111 may be increased. The amount of memory available depends on your 
15112 CADKEY version, hardware configuration, and other software being run. 
15113 Enter K value between 25 and ? (%d) => 
15114 Choose UNITS mode for CADKEY (%d) => 
15115 The decimal precision for CADL output of REAL data may be controlled 
15116 by specifying the number of places to the RIGHT of the decimal point.
15117 Enter a value between 4 and 10 (%d) => 
15118 Enter the maximum number of CADL program statement labels supported. 
15119 Enter a value between 0 and 1000 (%d) => 
15120 Enter the maximum number of register variables supported at one time.
15121 Enter a value between 0 and 1000 (%d) => 
15122 Specify the maximum font size which may be accepted by the system.
15123 Enter K value greater than or equal to 8 (%d) => 
15124 Specify the CHAINING TOLERANCE, or the allowable distance between the
15125 endpoints of entities when performing CHAIN SELECTION.
15126 Enter value, in system units between .00001 and .02 (%f) => 
15127 Choose highlighting option (%d) =>  
15128 Choose part file auto-saving option (%d) => 
15129 Enter the time interval in minutes between auto-saves, the interval
15130 must be greater than 4 minutes or less than 1 hour (%d) =>
15131 Enter the auto-save part file name (%s) : 
15132 Will you be running other DOS Extender programs
15133 from within CADKEY or from the DOS shell (Y/N) (%c) ? 
15134 Memory will have to be released by CADKEY to allow the other DOS
15135 Extender program to execute properly. It is recommended that at
15136 least 2048K be released for running other DOS Extender programs. 
15137 Enter the number of Kbytes to release (%ld) => 
15200        CADKEY part files can now be locked by individual users.
15210     This eliminates the possiblity of users overwriting each others 
15220     modifications to the same part file.  
15230        When a part file is loaded it will be automatically locked.  
15240     The user who originally loaded the part file is the only user who
15250     can save modifications to this file under its current name.  
15260     Other users can load the part file but will be unable to save
15270     any modifications to the part file until the part file is unlocked.  
15280        Part files are automatically unlocked when an owner of a locked
15290     part file saves his part file and loads another part file or leaves 
15300     CADKEY all together.  
15310        File locking is a virtual neccessity in a multi-user 
15320     environment.
15400     Will CADKEY be used in a multi-user environment (Y/N) (%s) ?
15410     CADKEY needs every user to have a unique user name to
15420     enable file locking.
15450     Enter unique user name (8 character maximum) (%s) :
15500 Choose dimension standard for CADKEY (%d) => 
15550     CADKEY allows users to control the individual attributes for 
15551     a dimension's text, witness lines and leader lines.
15552     Do you wish to control dimension attribute settings (Y/N) (%s) ?
16100 Enter default path for PART files: 
16101 Enter default path for PATTERN files: 
16102 Enter default path for PLOT files: 
16103 Enter default path for CADL files: 
16104 Enter default path for MACRO files: 
16105 Enter default path for NOTE files: 
16106 Enter default path for SUPPORT files: 
16107 Enter default path for HELP files:
16108 Enter default path for CDE files:
16109 Enter default path for DWG files:
16110 Enter default path for DXF files: 
16111 Enter default path for DOCUMENTATION files:
16121 Enter default path for LISP files:
16200 Default Language Selection
16201 Enter language selection (%d) => 
17100 Enter default macro library file name (%s) : 
17101 Enter start-up macro file name (%s) : 
17102 Enter default CDE file name(s) (%s) : 
171021 Additional functionality can be provided by loading CADKEY Dynamic
171022 Extension (CDE) modules. If you are using CDE modules they may be
171023 loaded automatically when CADKEY starts by designating the name of
171024 the CDE modules here. If you are using more than one CDE module the
171025 names must be comma (,) separated. To remove the list of CDE names 
171026 enter a single space.
20001 ;graphics device driver name
20002 ;graphics device mode
20003 ;graphics X resolution (pixels)
20004 ;graphics Y resolution (pixels)
20005 ;device palette type: 0=dumb, 1=EGA/VGA, 2=RGB, 3=BGR (HALO Metheus)
20006 ;number of colors in device lookup table
20007 ;maximum red intensity integer code
20008 ;maximum green intensity integer code
20009 ;maximum blue intensity integer code
20010 ;monitor config 0=one 1=two, graphics primary 2=two, mono primary
20011 ;number of graphics device memory pages
20012 ;graphics binary screen save switch: 0=no, 1=yes
20013 ;graphics segment starting address: 0xffff=driver default
20014 ;graphics device attribute code: 0xffff=driver default
20015 ;physical screen X size (inches)
20016 ;physical screen Y size (inches)
20017 ;graphics cursor X size (inches)
20018 ;graphics cursor Y size (inches)
20019 ;graphics cursor color
20020 ;rubber banding color
20021 ;  The following configuration records have 4 values
20022 ;	1. border color
20023 ;	2. background color
20024 ;	3. draw/text color
20025 ;	4. border style: 0=none, 1=single, 2=double
20026 ;menu options window colors
20027 ;break window colors
20028 ;status window colors
20029 ;cursor tracking window colors
20030 ;history line colors
20031 ;prompt line colors
20032 ;system mode indicator colors
20033 ;pop up menus colors
20034 ;  The following configuration record has 4 values
20035 ;	1. border color for primary graphics viewport
20036 ;	2. border color for other graphics viewports
20037 ;	3. background color for all graphics viewports
20038 ;	4. border style for all graphics viewports
20039 ;viewport area colors
20040 ;minimum text height allowed (pixels)
20041 ;maximum text height allowed (pixels)
20042 ;minimum text width allowed (pixels)
20043 ;maximum text width allowed (pixels)
20044 ;menu text cursor: 0=inverse video, 1=arrow
20045 ;default viewport configuration layout
20046 ;	1 = single                    5 = 1 left, 2 right
20047 ;	2 = 2 vertical		      6 = 2 bottom, 1 top
20048 ;	3 = 2 horizontal              7 = 1 bottom, 2 top
20049 ;	4 = 2 left, 1 right           8 = four
20050 ;maximum allowable number of viewports
20051 ;spacing between viewports for auto viewport placement (inches)
20052 ;display axes on entry: display viewport, construction viewport
20053 ;curve segmentation coarseness: 1.0=coarsest, 5.0=finest
20054 ;maximum number of horizontal and vertical grid points
20055 ;prompt marker color and size (inches)
20056 ;minimum increment size for sketching
20057 ;max number of entities to display while dynamically rotating part
20058 ;CADKEY input device
20059 ;CADL input device
20060 ;device driver
20061 ;device mode
20062 ;resolution (units/inch)
20063 ;device size (inches)
20064 ;minumum units
20065 ;cursor area X/Y min/max (inches)
20066 ;function area X/Y min/max (inches)
20067 ;# cols/rows of func area boxes
20068 ;button codes
20069 ;reversal flags
20070 ;device initialization
20071 ;ASCII format
20072 ;binary format
20073 ;plotter paper X size (inches)
20074 ;plotter paper Y size (inches)
20075 ;plotter pen width (mm)
20076 ;plotter X offset (inches)
20077 ;plotter Y offset (inches)
20078 ;plotter curve tolerance
20079 ;plotter sorting option
20080 ;plotter color map
20081 ;plotter communications configuration word
20082 ;plotter pen speed (cm/sec)
20083 ;plotter output port or file name
20084 ;printer paper X min (inches)
20085 ;printer paper Y min (inches)
20086 ;printer paper X max (inches)
20087 ;printer paper Y max (inches)
20088 ;printing pixel mode: 0=B/W,  1=Color
20089 ;printer output port or filename
20090 ;printer pixel width
20091 ;default part file pathname
20092 ;default pattern file pathname
20093 ;default plot file pathname
20094 ;default CADL file pathname
20095 ;default DXF file pathname
20096 ;default NOTE file pathname
20097 ;default HELP file pathname
20098 ;default data base scratch files pathname
20099 ;default system scratch file pathname
20100 ;default macro library file pathname
20101 ;size for SYSCMD and system buffer (K)
20102 ;0=inches, 1=millimeters, 2=feet, 3=centimeters, 4=yards, 5=meters
20103 ;CADL default decimal precision
20104 ;maximum number of CADL statement labels
20105 ;maximum number of register variables
20106 ;chain selection tolerance
20107 ;min. acceptable trimming intersection accuracy
20108 ;maximum font size (K)
20109 ;default macro library file name
20110 ;start-up macro name
20111 ;entity selection highlighting style
20112 ;auto-save time interval: 0=off, >0=seconds
20113 ;auto-save part name
20114 ;Reserved for future use
20115 ;Character set: 0=8 bit ASCII, 1=16 bit Kanji
20116 ;spacing between non-graphics viewports (inches)
20117 ;Path for CADKEY support files
20118 ;number of text rows for graphics device
20119 ;null func button value
20120 ;port device
20121 ;device communication configuration
20122 ;amount of memory to free when executing shell
20123 ;use EMM to store CADKEY image during shell (0=no; 1=yes)
20124 ;default language code
21000 ;plotter clip limit X min (millimeters)
21010 ;plotter clip limit Y min (millimeters)
21020 ;plotter clip limit X max (millimeters)
21030 ;plotter clip limit Y max (millimeters)
21040 ;file locking status: (0=disable, 1=enable)
21041 ;default CDE file pathname
21042 ;start-up cde name(s)
21043 ;graphics cde name
21044 ;maximum database memory pool size
21045 ;default DWG file pathname
21046 ;Dimensioning standard (0=ANSI, 1=DIN, 2=ISO, 3=JIS)
21047 ;default documentation file pathname
21048 ;User controlled dimension attributes (0=no, 1=yes)
21050 ;default LISP file pathname
25000 Cursor 
25010 Function
25020 Cur/Func
25030 F1
25040 F2
25050 F3
25060 F4
25070 F5
25080 F6
25090 F7
25100 F8
25110 F9
25120 F10
25130 Enter/CR
25140 ESC
25150 ALT-A
25160 ALT-B
25170 ALT-C
25180 ALT-D
25190 ALT-E
25200 ALT-F
25210 ALT-G
25220 ALT-H
25230 ALT-I
25240 ALT-J
25250 ALT-K
25260 ALT-L
25270 ALT-M
25280 ALT-N
25290 ALT-O
25300 ALT-P
25310 ALT-Q
25320 ALT-R
25330 ALT-S
25340 ALT-T
25350 ALT-U
25360 ALT-V
25370 ALT-W
25380 ALT-X
25390 ALT-Y
25400 ALT-Z
25410 CTRL-A
25420 CTRL-B
25430 CTRL-C
25440 CTRL-D
25450 CTRL-E
25460 CTRL-F
25470 CTRL-G
25480 CTRL-H
25490 CTRL-I
25500 CTRL-J
25510 CTRL-K
25520 CTRL-L
25530 CTRL-M
25540 CTRL-N
25550 CTRL-O
25560 CTRL-P
25570 CTRL-Q
25580 CTRL-R
25590 CTRL-S
25600 CTRL-T
25610 CTRL-U
25620 CTRL-V
25630 CTRL-W
25640 CTRL-X
25650 CTRL-Y
25660 CTRL-Z
25670 -VERIFY-
30 The color settings are invalid for the selected graphics device.
31 Do you wish to change them now (%c) ?
90 Are you sure you want to exit without saving changes (%c) ? 
99 *** Saving CONFIG.DAT file ***
999
