Geoworks Ensemble 2.0 
Geoworks May 1993

     * Minimum Hardware:
          + 286 CPU (386 recommended)
          + CGA display and adapter
          + 1 megabyte memory
          + 15 megabytes free disk space
          + Floppy drive compatible with host PC
          + Available serial port
     * Minimum Software:
          + MSDOS 3.0 or DR DOS 5.0
            
5 - Disks, use 1.2Mb or 1.44Mb floppies
Unzip each to a new or newly formatted floppy
You must install from floppy for this to
install. If you get an error during installation
be sure to have a printer attached to LPT 1,
seems if you don't you can get an error even if
no printer driver is installed.

Labels for disks:
Disk1= Geos_1
Disk2= Geos_2
Disk3= Geos_3
Disk4= Geos_4
Disk5= Geos_5



Troubleshooting startup:
Q: During Setup I get a divide by "0" error.

A: Make sure you have a printer connected and turned on.
   Or change the line in GEOS.INI that reads:
   continueSetup = true     to read:
   continueSetup = false
   and install the printer thru Geos and not Setup.

Q: When I try to start GEOS, I get a message saying that GEOS is
   unable to find /userdata/fonts
   
A: This could be any of several things. GEOS interacts with the
   hardware at a very low level, and it doesn't work well with anything
   that redirects the drives. Specifically:
     * Windows 32 bit file access SOMETIMES causes problems.
     * Networked drives cause problems for GEOS system files, although
       you can usually save data to a networked drive.
     * DOS emulation under Linux or Macintosh causes problems because
       GEOS tries to directly interact with hardware that just isn't
       there.

Q: I switched from MS-DOS/PC-DOS to DR-DOS and GEOS won't load, even
   after i run SETUP. What am I doing wrong?
   
A: Make sure that you have FILES=120 or MORE. DR-DOS uses files
   differently and needs more available. NWDOS USUALLY works with about
   50 files open.


Enjoy.....Ho !