[next] [prev] [prev-tail] [tail] [up]

#### $ASMMODE : Assembler mode (Intel 80x86 only)

The {$ASMMODE XXX} directive informs the compiler what kind of assembler it can expect in an asm block. The XXX should be replaced by one of the following:

att
  Indicates that asm blocks contain AT&T syntax assembler.
intel
  Indicates that asm blocks contain Intel syntax assembler.
direct
  Tells the compiler that asm blocks should be copied directly to the assembler file.

These switches are local, and retain their value to the end of the unit that is compiled, unless they are replaced by another directive of the same type. The command-line switch that corresponds to this switch is -R.

The default assembler reader is the AT&T reader.

[next] [prev] [prev-tail] [front] [up]