[next] [prev] [prev-tail] [tail] [up]

### 10.3 Optimization switches

This is where the various optimizing switches and their actions are described, grouped per switch.

-On:
  with n = 1..3: these switches activate the optimizer. A higher level automatically includes all lower levels.
  - Level 1 (-O1) activates the peephole optimizer (common instruction sequences are replaced by faster equivalents).
  - Level 2 (-O2) enables the assembler data flow analyzer, which allows the common subexpression elimination procedure to remove unnecessary reloads of registers with values they already contain.
  - Level 3 (-O3) enables uncertain optimizations. For more info, see -Ou.
-OG:
  This causes the code generator (and optimizer, IF activated), to favor faster, but code-wise larger, instruction sequences (such as ”subl $4,%esp”) instead of slower, smaller instructions (”enter $4”). This is the default setting.
-Og:
  This one is exactly the reverse of -OG, and as such these switches are mutually exclusive: enabling one will disable the other.
-Or:
  This setting causes the code generator to check which variables are used most, so it can keep those in a register.
-Opn:
  with n = 1..3: Setting the target processor does NOT activate the optimizer. It merely influences the code generator and, if activated, the optimizer:
  - During the code generation process, this setting is used to decide whether a jump table or a sequence of successive jumps provides the best performance in a case statement.
  - The peephole optimizer takes a number of decisions based on this setting, for example it translates certain complex instructions, such as

                  movzbl (mem), %eax|

    to a combination of simpler instructions

                  xorl %eax, %eax
                  movb (mem), %al

    for the Pentium.
-Ou:
  This enables uncertain optimizations. You cannot use these always, however. The previous section explains when they can be used, and when they cannot be used.

[next] [prev] [prev-tail] [front] [up]