;Top of File
begin
   type Display;Display
   dprompt Select your screen display card:
   mincnt 1
   maxcnt 2
end
begin
   name VGA;Display
   device Video Graphics Array
   file  L13VEGAS
   desc  Select this card if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to any kind of 
   desc  monitor.
   mneed  VGABUND
end
begin
   type VGABUND
   dprompt Select a VGA screen display mode:
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  VGA25B;VGABUND
   device 80x25 color
   id    80,90
   file  VGAS25CC.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a color monitor
   desc  and want to display the standard
   desc  80 characters across and
   desc  25 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO019LAA
end
begin
   name  VGA34B;VGABUND
   device 80x34 color
   id    80,70
   file  VGAS34CC.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a color monitor
   desc  and want to display
   desc  80 characters across and
   desc  34 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO014LCA
end
begin
   name  VGA60B;VGABUND
   device 80x60 color
   id    80,40
   file  VGAS60CC.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a color monitor
   desc  and want to display
   desc  80 characters across and
   desc  60 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO008LDA
end
begin
   name  VGA25M;VGABUND
   device 80x25 monochrome
   id    80,90
   file  VGAS25MM.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a monochrome
   desc  monitor and want to display
   desc  the standard 80 characters
   desc  across and 25 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO019LAA
end
begin
   name  VGA34M;VGABUND
   device 80x34 monochrome
   id    80,70
   file  VGAS34MM.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a monochrome
   desc  monitor and want to display
   desc  80 characters across and 
   desc  34 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO014LCA
end
begin
   name  VGA60M;VGABUND
   device 80x60 monochrome
   id    80,40
   file  VGAS60MM.VBD
   desc  Select this mode if you have
   desc  a Video Graphics Array (VGA)
   desc  connected to a monochrome
   desc  monitor and want to display
   desc  80 characters across and 
   desc  60 lines down.
   uses  FBC021LAA,FBC042LAA,FBC008LBA,FBO008LDA
end
begin
   name IBMEGA;Display
   device Enhanced Graphics Adapter
   file  L13VEGAS
   desc  Select this card if you have an
   desc  Enhanced Graphics Adapter (EGA)
   desc  that has 256 KB of memory and is
   desc  connected to any kind of monitor.
   mneed  EGABUND
   uses  FBC016LCA,FBC016LCA,FBC031LCA,FBC008LBA
end
begin
   name IBME64C;Display
   device EGA (64K) - color monitor
   file  L13VE64C
   desc  Select this card if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) that has either 64 KB
   desc  or 128 KB of memory and is
   desc  connected to a color monitor.
   mneed  E64BUND
   uses  FBC016LCA,FBC016LCA,FBC031LCA,FBC008LBA
end
begin
   name IBME64M;Display
   device EGA (64K) - monochrome monitor
   file  L13VE64M
   desc  Select this card if you have an
   desc  Enhanced Graphics Adapter (EGA)
   desc  that has only 64 KB of memory
   desc  and is connected to a monochrome
   desc  monitor.
   mneed  E64MUND
   uses  FBC016LCA,FBC016LCA,FBC031LCA,FBC008LBA
end
begin
   type EGABUND
   dprompt Select an EGA screen display mode:
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  EGA25B;EGABUND
   device 80x25 color
   id    80,70
   file  EGAS25CC.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a color
   desc  monitor and want to display
   desc  the standard 80 characters
   desc  across and 25 lines down.
   uses  FBO014LCA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name  EGA43B;EGABUND
   device 80x43 color
   id    80,40
   file  EGAS43CC.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a color
   desc  monitor and want to display
   desc  80 characters across and
   desc  43 lines down.
   uses  FBO008LDA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name  EGAM25;EGABUND
   device 80x25 monochrome
   id    80,70
   file  EGAS25MM.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a monochrome
   desc  monitor and want to display
   desc  the standard 80 characters
   desc  across and 25 lines down.
   uses  FBO014LCA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name  EGA43M;EGABUND
   device 80x43 monochrome
   id    80,40
   file  EGAS43MM.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a monochrome
   desc  monitor and want to display 
   desc  80 characters across and
   desc  43 lines down.
   uses  FBO008LDA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name  EGA25PL;EGABUND
   device 80x25 plasma
   id    80,70
   file  EGAS25PL.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a plasma
   desc  display and want to display
   desc  the standard 80 characters
   desc  across and 25 lines down.
   uses  FBO014LCA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name  EGA43PL;EGABUND
   device 80x43 plasma
   id    80,40
   file  EGAS43PL.VBD
   desc  Select this mode if you have
   desc  an Enhanced Graphics Adapter
   desc  (EGA) connected to a plasma
   desc  display and want to display
   desc  80 characters across and
   desc  43 lines down.
   uses  FBO008LDA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   type E64BUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  EGAL25;E64BUND
   device 80x25
   file  EGAS25LC.VBD
   uses  FBC008LBA,FBC016LCA,FBC031LCA,FBO008LDA
end
begin
   type E64MUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  E64M25;E64MUND
   device 80x25
   file  EGAS25MM.VBD
   uses  FBO014LCA,FBC031LCA,FBC016LCA,FBC008LBA
end
begin
   name CGA;Display
   device Color Graphics Adapter
   desc  Select this card if you have
   desc  a Color Graphics Adapter (CGA)
   desc  connected to any kind of 
   desc  monitor.  This card will
   desc  display full-screen graphs
   desc  and worksheets, but will
   desc  not display a graph and
   desc  worksheet at the same time.
   file  L13VCGAF
   need  CGABUND
   uses  FBC010LBA,FBC018LBA,FBC008LBA,FBC008LBA,FBC010LBA,FBC018LBA
end
begin
   type CGABUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  CGAB1;CGABUND
   device Color Text \ Color Charts
   file  CGAF25CC.VBD
   uses  FBC010LBA,FBC018LBA,FBC008LBA
end
begin
   name CGAWIN;Display
   device CGA for Windows
   desc  Select this card if you
   desc  have a Color Graphics
   desc  Adapter (CGA) and will be
   desc  using Microsoft Windows
   desc  Version 3 or above.
   file  L13VCGAH
   need  CGAWINBUND
   uses  FBC010LBA,FBC018LBA,FBC008LBA,FBC008LBA,FBC010LBA,FBC018LBA
end
begin
   type CGAWINBUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  CGAWINB1;CGAWINBUND
   device 80x25
   file  CGAF25CC.VBD
   uses  FBC010LBA,FBC018LBA,FBC008LBA
end
begin
   name MDA;Display
   device Monochrome Display Adapter
   file  L13VMDAF
   desc  Select this card if you have
   desc  a Monochrome Display Adapter.
   desc  A Monochrome Display Adapter
   desc  displays text in one color and
   desc  does not display graphs.
   need  MDABUND        
end
begin
   type MDABUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  MDAB;MDABUND
   device 80x25
   file  MDAF25MM.VBD
end
begin
   name TOSHIBA;Display
   device Toshiba 3100
   desc  Select this card if you
   desc  have an older model of the
   desc  Toshiba 3100. This will
   desc  display full-screen graphs
   desc  and worksheets, but will
   desc  not display a graph and
   desc  worksheet at the same time.
   file  L13VCGAF
   need  TOSHIBABUND
   uses  FBC010LBA,FBC018LBA,FBC008LBA,FBC008LBA,FBC010LBA,FBC018LBA
end
begin
   type TOSHIBABUND
   nselect
   mincnt 1
   maxcnt 2
end
begin
   name  TOSHB1;TOSHIBABUND
   device 80x25 plasma
   file  CGAF25MM.VBD
   uses  FBC010LBA,FBC018LBA,FBC008LBA
end
begin
   type Printer;Printer
   mprompt Select your printer manufacturer:
   dprompt Select your printer model or model series:
   mincnt 0
   maxcnt 16
   usemfgr
end
begin
   name  APPLE1;Printer
   file  L13PPSC0
   mfgr  Apple
   device  Apple LaserWriter
   desc  Select this model if you
   desc  have an Apple LaserWriter
   desc  printer.
   need  APPLEBUND
end
begin
   type APPLEBUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  APPLEB1;APPLEBUND
   device Times & Helvetica
   file  PS00ALW0.PBD
end
begin
   name  APPLE2;Printer
   file  L13PPSC0
   mfgr  Apple
   device  Apple LaserWriter Plus
   desc  Select this model if you have
   desc  an Apple LaserWriter Plus
   desc  printer.
   need  APPLEPBUND
end
begin
   type APPLEPBUND
   dprompt Select an Apple LaserWriter Plus font option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  APPLEPB1;APPLEPBUND
   device Times & Helvetica
   file  PS00ALW0.PBD
   desc  Select this option if you
   desc  have an Apple LaserWriter
   desc  Plus printer and want
   desc  to use "Times Roman" and
   desc  "Helvetica" typefaces.
end
begin
   name  APPLEPB2;APPLEPBUND
   device Bookman & Avant Garde
   file  PS00ALWP.PBD
   desc  Select this option if you
   desc  have an Apple LaserWriter
   desc  Plus and want to use
   desc  the "ITC Bookman" and
   desc  "ITC Avant Garde Gothic"
   desc  typefaces.
end
begin
   name  CANONBJP3;Printer
   file  L13PCOMN
   mfgr  Canon
   device BJ-10sx/10ex/10e (Proprinter)
   desc  Select this model series if you
   desc  have a Canon Bubble Jet printer
   desc  model BJ-10sx, 10ex, or 10e
   desc  which is set to Proprinter mode
   desc  (mode 1 on the 10sx and 10ex).
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed BJP3BUND
   uses  BJP3USE
end
begin
   type BJP3FILE
   dprompt Select a file
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  BJP3USE;BJP3FILE
   file  L13PCBJP
end
begin
   type BJP3BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PRO3BND1;BJP3BUND
   file  CBJIBPP2.PBD
   id	 180,180,360,360
   device Courier & Prestige Elite
   desc  Select this option if you
   desc  have a Canon Bubble Jet printer
   desc  model BJ-10sx, 10ex, or 10e
   desc  which is set to Proprinter mode
   desc  and want to use the
   desc  resident fonts "Courier"
   desc  and "Prestige Elite".
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  PRO3BND2;BJP3BUND
   file  CBJIBPP9.PBD
   id	 180,180,360,360
   device Legal (8.5" x 14")
   desc  Select this option if you have
   desc  a Canon Bubble Jet printer
   desc  model BJ-10sx, 10ex, or 10e
   desc  which is set to Proprinter mode
   desc  and wish to print on Legal
   desc  size paper or transparencies.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  CANONBJP2;Printer
   file  L13PCOMN
   mfgr  Canon
   device BJ-20/200/230 (Proprinter)
   desc  Select this model series if you
   desc  have a Canon Bubble Jet printer
   desc  model BJ-20, 200, or 230 which is
   desc  set to Proprinter mode (mode 1).
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed BJP2BUND
   uses  BJP2USE
end
begin
   type BJP2FILE
   dprompt Select a file
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  BJP2USE;BJP2FILE
   file  L13PCBJP
end
begin
   type BJP2BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PRO2BND1;BJP2BUND
   file  CBJIBPP2.PBD
   id	 180,180,360,360
   device Courier & Prestige Elite
   desc  Select this option if you
   desc  have a Canon Bubble Jet printer
   desc  model BJ-20, 200, or 230 which
   desc  is set to Proprinter mode and
   desc  want to use the resident
   desc  fonts "Courier" and
   desc  "Prestige Elite".
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  PRO2BND2;BJP2BUND
   file  CBJIBPP9.PBD
   id	 180,180,360,360
   device Legal (8.5" x 14")
   desc  Select this option if you have
   desc  a Canon Bubble Jet printer
   desc  model BJ-20, 200, or 230 which
   desc  is set to Proprinter mode and
   desc  wish to print on Legal size
   desc  paper or transparencies.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  CANONBJP;Printer
   file  L13PCOMN
   mfgr  Canon
   device BJ-300/330 (Proprinter)
   desc  Select this model series if you
   desc  have a Canon BubbleJet printer
   desc  model BJ-300 or BJ-330 which is
   desc  set to Proprinter mode.
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed BJPBUND
   uses  BJPUSE
end
begin
   type BJPFILE
   dprompt Select a file
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  BJPUSE;BJPFILE
   file  L13PCBJP
end
begin
   type BJPBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PROBND1;BJPBUND
   file  CBJIBPP1.PBD
   id	 180,180,360,360
   device Courier & Letter Gothic
   desc  Select this option if you
   desc  have a Canon Bubble Jet
   desc  (BJ-300 or BJ-330) which
   desc  is set to Proprinter
   desc  mode and want to use the
   desc  resident fonts "Courier"
   desc  and "Letter Gothic".
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  PROBND2;BJPBUND
   file  CBJIBPP2.PBD
   id	 180,180,360,360
   device Courier & Prestige Elite
   desc  Select this option if you
   desc  have a Canon Bubble Jet
   desc  (BJ-300 or BJ-330) which
   desc  is set to Proprinter mode
   desc  and want to use the
   desc  resident fonts "Courier"
   desc  and "Prestige Elite".
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  PROBND9;BJPBUND
   file  CBJIBPP9.PBD
   id	 180,180,360,360
   device Legal (8.5" x 14")
   desc  Select this option if you
   desc  have a Canon Bubble Jet 
   desc  (BJ-300 or BJ-330) which is
   desc  set to Proprinter mode
   desc  and wish to print on Legal
   desc  size paper or transparencies.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  BJC_600;Printer
   file  L13PCOMN
   mfgr  Canon
   device BJC-600 Color (Extended Mode)
   desc  Select this model if you
   desc  have a Canon BJC-600
   desc  color printer which is
   desc  set to Extended mode.
   mneed  BJC600BUND
   uses  BJC600USE
end
begin
   type BJC600BUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  BJC600PAPR;BJC600BUND
   device Plain Paper
   file  CNBJC6P.PBD
   id	 180,180,360,360
   desc  Select this option if you 
   desc  have a Canon BJC-600 and you
   desc  want to print on Plain paper
   desc  and use the resident font
   desc  "Courier" in 10 or 12 Pitch.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  BJC600COAT;BJC600BUND
   device Coated Paper
   file  CNBJC6C.PBD
   id	 180,180,360,360
   desc  Select this option if you 
   desc  have a Canon BJC-600 and you
   desc  want to print on Coated paper
   desc  and use the resident font
   desc  "Courier" in 10 or 12 Pitch.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  BJC600COTB;BJC600BUND
   device Coated Paper (Enhanced Black)
   file  CNBJC6CE.PBD
   id	 180,180,360,360
   desc  Select this option if you 
   desc  have a Canon BJC-600 and you
   desc  want to print on Coated paper
   desc  with Enhanced Black and use 
   desc  the resident font "Courier" 
   desc  in 10 or 12 Pitch.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   name  BJC600TRAN;BJC600BUND
   device Transparencies
   file  CNBJC6T.PBD
   id	 180,180,360,360
   desc  Select this option if you 
   desc  have a Canon BJC-600 and you
   desc  want to print on Transparencies
   desc  and use the resident font
   desc  "Courier" in 10 or 12 Pitch.
   uses  FAI030LAA,FAJ040LAA,FAA030LAA,FAC040LAA
   uses  AI060LAA,AI120LAA,AJ080LAA,AA060LAA,AA120LAA,AC080LAA
end
begin
   type  BJC600FILE
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  BJC600USE;BJC600FILE
   file  L13PBJC6
end
begin
   name  CANONBJC;Printer
   file  L13PCOMN
   mfgr  Canon
   device BJC-800 Color
   desc  Select this model if you
   desc  have a Canon BJC-800
   desc  color printer.
   mneed  BJCBUND
   uses  L13PEPLQ
end
begin
   type BJCBUND
   dprompt Select a Canon BJC-800 printer option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  BJCMBUN;BJCBUND
   file  CANBJCM.PBD
   id    180,180,360,180
   device Monospaced Letter (8.5"x11")
   desc  Select this option if you
   desc  have a Canon BJC-800 printer
   desc  with monospaced text and
   desc  Letter size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  BJCMGBUN;BJCBUND
   file  CANBJCMG.PBD
   id    180,180,360,180
   device Monospaced Legal (8.5"x14")
   desc  Select this option if you
   desc  have a Canon BJC-800 printer
   desc  with monospaced text and
   desc  Legal size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  BJCMLBUN;BJCBUND
   file  CANBJCML.PBD
   id    180,180,360,180
   device Monospaced Ledger (11"x17")
   desc  Select this option if you
   desc  have a Canon BJC-800 printer
   desc  with monospaced text and
   desc  Ledger size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  BJCPBUN;BJCBUND
   file  CANBJCP.PBD
   id    180,180,360,180
   device Proportional Letter (8.5"x11")
   desc  Select this option if you
   desc  have a Canon BJC-800 printer
   desc  with proportionally spaced
   desc  text and Letter size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  BJCPGBUN;BJCBUND
   file  CANBJCPG.PBD
   id    180,180,360,180
   device Proportional Legal (8.5"x14")
   desc  Select this option if you have
   desc  a Canon BJC-800 printer with
   desc  proportionally spaced text
   desc  and Legal size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  BJCPLBUN;BJCBUND
   file  CANBJCPL.PBD
   id    180,180,360,180
   device Proportional Ledger (11"x17")
   desc  Select this option if you
   desc  have a Canon BJC-800 printer
   desc  with proportionally spaced
   desc  text and Ledger size paper.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  CANON;Printer
   file  L13PCANR
   mfgr  Canon
   device LBP-4, 8 Series
   desc  Select this model series
   desc  if you have a Canon LBP-4,
   desc  LBP-8II, or LBP-8III laser
   desc  printer with standard memory.
   need  CANONBUND
   uses  CANONUSE
end
begin
   type CANONFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  CANONUSE;CANONFILE
   file  L13PCNLR
end
begin
   type CANONBUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  CANONB1;CANONBUND
   device printer
   id    300,300
   file  CNLR4RP.PBD
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
end
begin
   name  CAPSLIII;Printer
   file  L13PCLBP
   mfgr  Canon
   device  LBP-4, 8III added mem
   desc  Select this model if you have
   desc  a Canon LBP-4 or LBP-8III
   desc  printer with at least 1.5MB
   desc  of printer memory.
   desc  
   desc  This driver selection will use
   desc  CaPSL III technology supported
   desc  by 1.5MB of memory for faster
   desc  printing of high-density 
   desc  full-page graphics.
   need  CAPSL3BUND
   uses  CANWID
end
begin
   type CAPWIN
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  CANWID;CAPWIN
   file  L13PCLBP.WID
end
begin
   type CAPSL3BUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  CAPSL3B2;CAPSL3BUND
   device Dutch & Swiss
   file  CLBPFINT.PBD
   desc  Select this option if you
   desc  have a Canon LBP-4 or
   desc  LBP-8III printer and want
   desc  to use "Dutch" and "Swiss"
   desc  typefaces.
end
begin
   name  CAPSL3B1;CAPSL3BUND
   device Courier & Elite
   file  CLBPFPLS.PBD
   desc  Select this option if you
   desc  have a Canon LBP-4 Lite,
   desc  LBP-4 Plus, or LBP-8 III
   desc  Plus printer and want to
   desc  use the resident typefaces
   desc  "Courier" and "Elite".
end
begin
   name  CITGX;Printer
   file  L13PCOMN
   mfgr  Citizen
   device  GX Series
   desc  Select this model series if
   desc  you have a Citizen GX Series
   desc  printer.
   mneed  GXBUND
   uses  EPSONMXUSE
end
begin
   type GXBUND
   dprompt Select a Citizen GX Series printer:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  GXBWBUN;GXBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   device B&W 
   desc  Select this option if you
   desc  have a Citizen GX series
   desc  B&W printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  GXCBUN;GXBUND
   file  EPDTEXC.PBD
   id    120,72,120,72
   device Color
   desc  Select this option if you
   desc  have a Citizen GX series 
   desc  Color printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  CITGSX;Printer
   file  L13PCOMN
   mfgr  Citizen
   device  GSX Series
   desc  Select this model series if
   desc  you have a Citizen GSX Series
   desc  printer.
   mneed GSXBUND
   uses  L13PEPLQ,PANUSE
end
begin
   type GSXBUND
   dprompt Select a Citizen GSX Series printer:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  GSXBWM;GSXBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device B&W Monospaced
   desc  Select this option if you
   desc  have a GSX series B&W printer
   desc  and want to use monospaced
   desc  text and normal-density
   desc  graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  GSXBWP;GSXBUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device B&W Proportional
   desc  Select this option if you
   desc  have a GSX series B&W printer
   desc  and want to use proportionally
   desc  spaced text and high-density
   desc	 graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  GSXCM;GSXBUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device Color Monospaced
   desc  Select this option if you
   desc  have a GSX series Color printer
   desc  and want to use monospaced 
   desc  text and normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  GSXCP;GSXBUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device Color Proportional
   desc  Select this option if you
   desc  have a GSX series Color printer
   desc  and want to use proportionally
   desc  spaced text and high-density
   desc  graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  CITW240;Printer
   file  L13PCOMN
   mfgr  Citizen
   device GSX 240
   desc  Select this if you have a
   desc  Citizen GSX 240 printer. 
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed CIT240BUND
   uses  CITWTR240USE
end
begin
   type CITW240FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  CITWTR240USE;CITW240FILE
   file  L13PEPP2
end
begin
   type CIT240BUND
   dprompt Select a Citizen GSX 240
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  CIT240BBUN;CIT240BUND
   file  EPP2570.PBD
   id    180,180,360,360
   device B&W
   desc  Select this option if you
   desc  have a Citizen GSX 240 
   desc  B&W printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  CIT240CBUN;CIT240BUND
   file  EPP2C.PBD
   id    180,180,360,360
   device Color
   desc  Select this option if you
   desc  have a Citizen GSX 240 
   desc  Color printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  CIT48;Printer
   file  L13PCOMN
   mfgr  Citizen
   device PN-48
   desc  Select this model if
   desc  you have a Citizen PN-48
   desc  notebook printer.
   mneed CIT48BUND
   uses  L13PEPLQ,PANUSE
end
begin
   type CIT48BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  CIT48M1;CIT48BUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device Notebook printer
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  EPAL1LAS;Printer
   file  L13PHPCM
   mfgr  Epson
   device  ActionLaser 1000
   desc  Select this device if you
   desc  have an Epson ActionLaser 1000
   desc  laser printer.
   need  EPAL1BUND
   uses  HPUSE2
end
begin
   type EPAL1BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  EPAL1NCART;EPAL1BUND
   id    150,150,300,300
   file  HPLJ2NOH.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  EPA15LAS;Printer
   file  L13PHP3C
   mfgr  Epson
   device  ActionLaser 1500 
   desc  Select this model if you have
   desc  an Epson ActonLaser 1500
   desc  laser printer. 
   mneed  EPA15BUND
   uses  L13PHPL3
end
begin
   type EPA15BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  EPA15NCART;EPA15BUND
   id    150,150,300,300
   file  HPLJ3NHP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA,FAJ033LAA
end
begin
   name  EPSFX;Printer
   file  L13PCOMN
   mfgr  Epson
   device FX/MX/JX/EX Series
   desc  Select this model series if you
   desc  have an Epson FX, MX, JX 
   desc  or EX Series printer.
   mneed  MXBUND
   uses  EPSONMXUSE
end
begin
   type MXBUND
   dprompt Select an Epson model series and option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  FX80BUN;MXBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   device FX Model
   desc  Select this option if you
   desc  have an Epson FX series printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  NUMX80BUN;MXBUND
   file  EPDTMX.PBD
   id    120,72,120,72
   device MX Model
   desc  Select this option if you
   desc  have an Epson MX series printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  JX80BUN;MXBUND
   file  EPDTJX.PBD
   id    120,72,120,72
   device JX Color Model
   desc  Select this option if you
   desc  have an Epson JX series Color
   desc  printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  EX80BUNB1;MXBUND
   file  EPDTEX.PBD
   id    120,72,120,72
   device EX B&W Model
   desc  Select this option if you
   desc  have an Epson EX series  
   desc  B&W printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  EX80BUNB2;MXBUND
   file  EPDTEXC.PBD
   id    120,72,120,72
   device EX Color Model
   desc  Select this option if you
   desc  have an Epson EX series 
   desc  Color printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  EPSLQ;Printer
   file  L13PCOMN
   mfgr  Epson
   device  LQ Series
   desc  Select this model series if you
   desc  have an Epson LQ Series printer.
   mneed LQBUND
   uses  L13PEPLQ,PANUSE
end
begin
   type LQBUND
   dprompt Select an Epson LQ model and option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  LQ800B2;LQBUND
   file  EPLQL80M.PBD
   id    180,180,180,180
   device 800/850, 1000/1050 Monospaced
   desc  Select this option if you
   desc  have an Epson LQ-800/850 or 
   desc  LQ-1000/1050 printer and want
   desc  to use monospaced text and
   desc	 normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQ800B1;LQBUND
   file  EPLQL80P.PBD
   id    180,180,180,180
   device 800/850, 1000/1050 Proportional
   desc  Select this option if you
   desc  have an Epson LQ-800/850 or
   desc  LQ-1000/1050 printer and want
   desc  to use proportionally spaced
   desc  text and high-density graphics.  
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQ1500B1;LQBUND
   file  EPLQL15P.PBD
   id    180,180,180,180
   device 1500
   desc  Select this option if you
   desc  have an Epson LQ-1500 printer.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQ2500B1;LQBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device 2500/2550 B&W Monospaced
   desc  Select this option if you
   desc  have an Epson LQ-2500 or 2550 B&W 
   desc  printer and want to use monospaced
   desc  text and normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQ2500B2;LQBUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device 2500/2550 B&W Proportional
   desc  Select this option if you
   desc  have an Epson LQ-2500 or 2550
   desc  B&W printer and want to use
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQMONO;LQBUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device 2500/2550 Color Monospaced
   desc  Select this option if you
   desc  have an Epson LQ-2500 or 2550 
   desc  Color printer and want to
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  LQPROP;LQBUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device 2500/2550 Color Proportional
   desc  Select this option if you
   desc  have an Epson LQ-2500 or 2550
   desc  Color printer and want to
   desc  use proportionally spaced
   desc  text and high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  EPESCP2;Printer
   file  L13PCOMN
   mfgr  Epson
   device  ESC/P2 Series
   desc  Select this model series if you
   desc  have an Epson ESC/P2 Series
   desc  printer.
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed  P2BUND
   uses  ESCP2USE
end
begin
   type ESCP2FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name ESCP2USE;ESCP2FILE
   file L13PEPP2
end
begin
   type P2BUND
   dprompt Select an Epson ESC/P2 Series Printer:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  P2BWBUN;P2BUND
   file  EPP2570.PBD
   id    180,180,360,360
   device B&W 
   desc  Select this option if you
   desc  have an Epson ESC/P2 B&W
   desc  series printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA,FAC033LAA
end
begin
   name  P2CBUN;P2BUND
   file  EPP2C.PBD
   id    180,180,360,360
   device Color
   desc  Select this option if you
   desc  have an Epson ESC/P2 Color
   desc  series printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA,FAC033LAA
end
begin
   name  HPDJ;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet
   desc  Select this model if you
   desc  have an HP DeskJet printer.
   need  HPDJBUND
   uses  L13PHPDJ
end
begin
   type HPDJBUND
   dprompt Select an HP DeskJet cartridge option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name NDJBUND;HPDJBUND
   device No cartridge
   id    150,150,300,300
   file  HPDJNO.PBD
   desc  Select this option if you
   desc  want to use an HP DeskJet
   desc  with no cartridge
   desc  installed.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name LDJBUND;HPDJBUND
   device Landscape cartridge
   id    150,150,300,300
   file  HPDJLS.PBD
   desc  Select this option if you
   desc  want to use an HP DeskJet
   desc  with the 22707K Landscape
   desc  cartridge installed.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  HPDJ500P;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet Portable
   desc  Select this model if you
   desc  have an HP DeskJet Portable
   desc  printer.
   need  HP500PBUND
   uses  L13PHPDJ
end
begin
   type HP500PBUND
   dprompt Select an HP DeskJet Portable option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name HP5PPBUN;HP500PBUND
   device Paper
   id    150,150,300,300
   file  HPDJ500.PBD
   desc  Select this option if you
   desc  want to print on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name HP5PTBUN;HP500PBUND
   device Transparency
   id    150,150,300,300
   file  HPDJ500T.PBD
   desc  Select this option if 
   desc  you want to print on  
   desc  a transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin	    
   name  HPDJ310;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet 310
   desc  Select this model if you
   desc  have an HP DeskJet 310
   desc  printer.
   need  HP310BUND
   uses  DJ310USE
end
begin
   type  DJ310FILE
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  DJ310USE;DJ310FILE
   file  L13PHPDC
end
begin
   type HP310BUND
   dprompt Select an HP DeskJet 310 option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name HP31PBUN;HP310BUND
   device Paper
   id    150,150,300,300
   file  HPDJ5CP.PBD
   desc  Select this option if you
   desc  want to print color text
   desc  and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name HP31TBUN;HP310BUND
   device Transparency
   id    150,150,300,300
   file  HPDJ5CT.PBD
   desc  Select this option if you
   desc  want to print color text
   desc  and graphics on a transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  HPDJ500+;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet+, 500, 510, 520
   desc  Select this model if you
   desc  have an HP DeskJet Plus,
   desc  HP Deskjet 500, 510, or 520
   desc  printer.
   need  HPDJ500BUND
   uses  L13PHPDJ
end
begin
   type HPDJ500BUND
   dprompt Select an HP DeskJet option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name HDJBUND5001;HPDJ500BUND
   device Paper
   id    150,150,300,300
   file  HPDJ500.PBD
   desc  Select this option if you want to
   desc  print text and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name HDJBUND5002;HPDJ500BUND
   device Transparency
   id    150,150,300,300
   file  HPDJ500T.PBD
   desc  Select this option if you want
   desc  to print text and graphics on a
   desc	 transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  HPDJ500C;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet 500C, 550C
   desc  Select this model if you
   desc  have an HP DeskJet 500C or 550C
   desc  printer.
   need  HP500CBUND
   uses  DJ500CUSE
end
begin
   type  DJ500CFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  DJ500CUSE;DJ500CFILE
   file  L13PHPDC
end
begin
   type HP500CBUND
   dprompt Select an HP DeskJet 500C or 550C option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name HP5CPBUN;HP500CBUND
   device Paper
   id    150,150,300,300
   file  HPDJ5CP.PBD
   desc  Select this option if you
   desc  want to print color text 
   desc  and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name HP5CTBUN;HP500CBUND
   device Transparency
   id    150,150,300,300
   file  HPDJ5CT.PBD
   desc  Select this option if you
   desc  want to print color text
   desc  and graphics on a transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  HPDJ560C;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet 560C
   desc  Select this model if you
   desc  have an HP DeskJet 560C
   desc  printer.
   need  HP560CBUND
   uses  DJ560CUSE
end
begin
   type  DJ560CFILE
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  DJ560CUSE;DJ560CFILE
   file  L13PHPDC
end
begin
   type HP560CBUND
   dprompt Select an HP DeskJet 560C option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name HP56PNBUN;HP560CBUND
   device Paper
   id    150,150,300,300
   file  HPDJ56PN.PBD
   desc  Select this option if you
   desc  want to print color text
   desc  and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name HP56TNBUN;HP560CBUND
   device Transparency
   id    150,150,300,300
   file  HPDJ56TN.PBD
   desc  Select this option if you
   desc  want to print color text
   desc  and graphics on a transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  HPDESKJETC;Printer
   file  L13PCOMN
   mfgr  HP
   device DeskJet 1200C (/Print)
   desc  Select this model if you
   desc  have an HP DeskJet 1200C and
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc  
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed  DJETCBUND
   uses  DJETCUSE
end
begin
   type DJETCFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  DJETCUSE;DJETCFILE
   file  L13PPXL3
end
begin
   type DJETCBUND
   dprompt Select an HP DeskJet 1200C option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  DJETC1;DJETCBUND
   device Letter (8.5" x 11")
   id    150,150,300,300
   file  PJXL300.PBD
   desc  Select this option if you
   desc  want to use an HP DeskJet 1200C
   desc  with 8 1/2"x11" paper.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  DJETC3;DJETCBUND
   device Legal (8.5" x 14")
   id    150,150,300,300
   file  PJXL301.PBD
   desc  Select this option if
   desc  you want to use Legal  
   desc  size paper.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  DJETC4;DJETCBUND
   device A4  (210mm x 297mm)
   id    150,150,300,300
   file  PJXL303.PBD
   desc  Select this option if you
   desc  want to use A4 size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PCL5C;Printer
   file  L13PCL5C
   mfgr  HP
   device  DeskJet 1200C (PCL5 Wysiwyg)
   desc  Select this model if you
   desc  have an HP DeskJet 1200C and
   desc  want to best use Wysiwyg to print
   desc  text and graphics (:Print) and
   desc  best use 1-2-3 to print graphs
   desc  (/Print [B,E,P] Image).
   desc  This selection uses high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  PCL5CBUND
   uses  PCL5WID
end
begin
   type PCL5CBUND
   dprompt Select a DeskJet 1200C option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PCL5BC1;PCL5CBUND
   device Letter (8.5" x 11")
   file  DJCTHT.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  PCL5BC2;PCL5CBUND
   device Legal (8.5" x 14")
   file  DJCTHG.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  PCL5BC3;PCL5CBUND
   device A4 (210mm x 297mm)
   file  DJCTH4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name  HPLAS;Printer
   file  L13PCOMN
   mfgr  HP
   device  LaserJet
   desc  Select this model if you
   desc  have an HP LaserJet printer.
   mneed  HPBUND
   uses  HPUSE
end
begin
   type HPFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPUSE;HPFILE
   file  L13PHPL1
end
begin
   type HPBUND
   dprompt Select an HP LaserJet cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPNCART;HPBUND
   device No cartridge
   id    75,75
   file  HPLJ1NOL.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet 
   desc  with no cartridge installed.
   uses  FAA012LAA,FAA025LAA,FAC017LAA,FAJ017LAA,FAI012LAA,FAI025LAA
end
begin
   name  HP9ZCART;HPBUND
   device Z Microsoft 1A
   id    75,75
   file  HPLJ1ZLO.PBD
   desc  Select this option if you
   desc  want to use an HP
   desc  LaserJet with a 92286Z
   desc  Microsoft 1A HP Font cartridge
   desc  (Z cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAC017LAA,FAJ017LAA,FAI012LAA,FAI025LAA
end
begin
   name  HP9JCART;HPBUND
   device J Math Elite
   id    75,75
   file  HPLJ1JLO.PBD
   desc  Select this option if you
   desc  want to use an HP
   desc  LaserJet with a 92286J
   desc  Math Elite HP Font cartridge
   desc  (J cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAC017LAA,FAJ017LAA,FAI012LAA,FAI025LAA
end
begin
   name  HP9FCART;HPBUND
   device F TmsRmn2
   id    75,75
   file  HPLJ1FLO.PBD
   desc  Select this option if you
   desc  want to use an HP
   desc  LaserJet with a 92286F
   desc  TmsRmn2 HP Font cartridge
   desc  (F cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAC017LAA,FAJ017LAA,FAI012LAA
   uses  FAI025LAA
end
begin
   name  HPPLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet+, 500+
   desc  Select this model series if
   desc  you have an HP LaserJet Plus
   desc  or HP LaserJet 500+ with
   desc  standard memory.
   mneed  HPPBUND
   uses  HPUSE2
end
begin
   type HPPBUND
   dprompt Select an HP LaserJet Plus or 500+ cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPPNAMCART;HPPBUND
   device No cartridge
   id    75,75,150,150,300,300
   file  HPLJPNOL.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  with no cartridge installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPP9ZCART;HPPBUND
   device Z Microsoft 1A
   id    75,75,150,150,300,300
   file  HPLJZLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  with a 92286Z Microsoft 1A
   desc  HP Font cartridge 
   desc  (Z cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPP9JCART;HPPBUND
   device J Math Elite
   id    75,75,150,150,300,300
   file  HPLJPJLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  with a 92286J Math Elite
   desc  HP Font cartridge
   desc  (J cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPP9FCART;HPPBUND
   device F TmsRmn2
   id    75,75,150,150,300,300
   file  HPLJPFLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  with a 92286F TmsRmn2 HP
   desc  Font cartridge (F cartridge)
   desc  installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPPAMLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet+, 500+ added mem
   desc  Select this model series if
   desc  you have an HP LaserJet Plus
   desc  or HP LaserJet 500+ that has
   desc  added memory.
   desc
   desc  This selection allows
   desc  high-density full-page graphics.
   mneed  HPPAMBUND
   uses  HPUSE2
end
begin
   type HPPAMBUND
   dprompt Select an HP LaserJet Plus or 500+ cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPPAMNCART;HPPAMBUND
   device No cartridge
   id    150,150,300,300
   file  HPLJPNOH.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet 
   desc  Plus or HP LaserJet 500+
   desc  that has added memory with
   desc  no cartridge installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPPAM9ZCART;HPPAMBUND
   device Z Microsoft 1A
   id    150,150,300,300
   file  HPLJZHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or HP LaserJet 500+
   desc  that has added memory with a 
   desc  92286Z Microsoft 1A HP Font
   desc  cartridge (Z cartridge)
   desc  installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPPAM9JCART;HPPAMBUND
   device J Math Elite
   id    150,150,300,300
   file  HPLJPJHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  that has added memory with
   desc  a 92286J Math Elite HP
   desc  Font cartridge (J cartridge)
   desc  installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPPAM9FCART;HPPAMBUND
   device F TmsRmn2
   id    150,150,300,300
   file  HPLJPFHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Plus or an HP LaserJet 500+
   desc  that has added memory with
   desc  a 92286F TmsRmn2 HP Font
   desc  cartridge (F cartridge)
   desc  installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPS2LAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet Series II
   desc  Select this model series if you
   desc  have an HP LaserJet Series II
   desc  that has standard memory.
   mneed  HPS2BUND
   uses  HPUSE2
end
begin
   type HPS2BUND
   dprompt Select an HP LaserJet Series II cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPS2NCART;HPS2BUND
   device No cartridge
   id    75,75,150,150,300,300
   file  HPLJNOLO.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet 
   desc  Series II with no cartridge
   desc  installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPS29ZCART;HPS2BUND
   device Z Microsoft 1A
   id    75,75,150,150,300,300
   file  HPLJZLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II with a 92286Z 
   desc  Microsoft 1A HP Font
   desc  cartridge (Z cartridge)
   desc  installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPS29JCART;HPS2BUND
   device J Math Elite
   id    75,75,150,150,300,300
   file  HPLJ2JLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II with a 92286J
   desc  Math Elite HP Font 
   desc  cartridge (J cartridge)
   desc  installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPS29FCART;HPS2BUND
   device F TmsRmn2
   id    75,75,150,150,300,300
   file  HPLJ2FLO.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II with a 92286F
   desc  TmsRmn2 HP Font cartridge
   desc  (F cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPS2AMLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet Series II added mem
   desc  Select this model series if
   desc  you have an HP LaserJet Series II
   desc  that has added memory.
   desc
   desc  This selection allows
   desc  high-density full-page graphics.
   mneed  HPS2AMBUND
   uses  HPUSE2
end
begin
   type HPS2AMBUND
   dprompt Select an HP LaserJet Series II cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPS2AMNCART;HPS2AMBUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ2NOH.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet 
   desc  Series II that has added
   desc  memory with no cartridge
   desc  installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPSAM29ZCART;HPS2AMBUND
   device Z Microsoft 1A
   id    150,150,300,300
   file  HPLJZHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II that has added
   desc  memory with a 92286Z 
   desc  Microsoft 1A HP Font
   desc  cartridge (Z cartridge)
   desc  installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPSAM29JCART;HPS2AMBUND
   device J Math Elite
   id    150,150,300,300
   file  HPLJ2JHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II that has added
   desc  memory with a 92286J Math
   desc  Elite HP Font cartridge
   desc  (J cartridge) installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HPSAM29FCART;HPS2AMBUND
   device F TmsRmn2
   id    150,150,300,300
   file  HPLJ2FHI.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet
   desc  Series II that has added
   desc  memory with a 92286F TmsRmn2
   desc  HP Font cartridge
   desc  (F cartridge) installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HP2PLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet IIP
   desc  Select this model if 
   desc  you have an HP LaserJet IIP
   desc  with standard memory.
   mneed  HP2PBUND
   uses  L13PHPLP
end
begin
   type HP2PBUND
   dprompt Select an HP LaserJet IIP cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HP2PNCART;HP2PBUND
   device No cartridge
   id    75,75,150,150,300,300
   file  HPLJ2NLP.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet IIP
   desc  with no cartridge installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HP2P9ZCART;HP2PBUND
   device Z Microsoft 1A
   id    75,75,150,150,300,300
   file  HPLJ2ZLP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286Z Microsoft 1A HP Font
   desc  cartridge (Z cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HP2P9JCART;HP2PBUND
   device J Math Elite
   id    75,75,150,150,300,300
   file  HPLJ2JLP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286J Math Elite HP Font 
   desc  cartridge (J cartridge) installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end                     
begin
   name  HP2P9FCART;HP2PBUND
   device F TmsRmn2
   id    75,75,150,150,300,300
   file  HPLJ2FLP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286F TmsRmn2 HP Font
   desc  cartridge (F cartridge)
   desc  installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HP2PAMLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LaserJet IIP added mem
   desc  Select this model series if 
   desc  you have an HP LaserJet IIP
   desc  that has added memory.
   desc
   desc  This selection allows
   desc  high-density full-page graphics.
   mneed  HP2PAMBUND
   uses  L13PHPLP
end
begin
   type HP2PAMBUND
   dprompt Select a HP LaserJet IIP cartridge option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HP2PNCARTAM;HP2PAMBUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ2NHP.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet IIP
   desc  with no cartridge installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HP2P9ZCARTAM;HP2PAMBUND
   device Z Microsoft 1A
   id    150,150,300,300
   file  HPLJ2ZHP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286Z Microsoft 1A HP Font
   desc  cartridge (Z cartridge) installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HP2P9JCARTAM;HP2PAMBUND
   device J Math Elite
   id    150,150,300,300
   file  HPLJ2JHP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286J Math Elite HP Font 
   desc  cartridge (J cartridge) installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HP2P9FCARTAM;HP2PAMBUND
   device F TmsRmn2
   id    150,150,300,300
   file  HPLJ2FHP.PBD
   desc  Select this option if you
   desc  want to use an HP LaserJet IIP
   desc  with a 92286F TmsRmn2 HP Font
   desc  cartridge (F cartridge) installed.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  HP3PAMLAS;Printer
   file  L13PHPCM
   mfgr  HP
   device  LJ III Series standard mem
   desc  Select this model series if you
   desc  have an HP LaserJet III Series
   desc  that has standard memory (512KB).
   mneed  HP3PAMBUND
   uses  HPUSE2
end
begin
   type HP3PAMBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HP3PNCARTAM;HP3PAMBUND
   device No cartridge
   id    75,75,150,150
   file  HPLJNOLO.PBD
   desc  Select this option if you 
   desc  want to use an HP LaserJet III
   desc  Series with no cartridge installed.
   uses  FAA012LAA,FAA025LAA,FAA050LAA,FAC017LAA,FAC033LAA,FAJ017LAA
   uses  FAJ033LAA,FAI012LAA,FAI025LAA,FAI050LAA
end
begin
   name  HPS3AMLAS;Printer
   file  L13PHP3C
   mfgr  HP
   device  LJ III Series (/Print)
   desc  Select this model series if you
   desc  have an HP LaserJet III Series
   desc  that has added memory and you
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed  HPS3AMBUND
   uses  L13PHPL3
end
begin
   type HPS3AMBUND
   dprompt Select an HP LaserJet III Series option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPS3AMNCART;HPS3AMBUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ3NHP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PCL5R;Printer
   file  L13PCL53
   mfgr  HP
   device  LJ III Series (PCL5 Wysiwyg)
   desc  Select this model if you
   desc  have an HP LaserJet III Series
   desc  and want to best use Wysiwyg to
   desc  print text and graphics (:Print)
   desc  and best use 1-2-3 to print
   desc  graphs (/Print [B,E,P] Image).
   desc  This selection uses high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  PCL53BUND
   uses  PCL5WID
end
begin
   type PCL53BUND
   dprompt Select a LaserJet III Series option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PCL5BR1;PCL53BUND
   device Letter (8.5" x 11")
   file  LJ3THT.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  PCL5BR2;PCL53BUND
   device Legal (8.5" x 14")
   file  LJ3THG.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  PCL5BR3;PCL53BUND
   device A4 (210mm x 297mm)
   file  LJ3TH4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name  HP3Si;Printer
   file  L13PHP3S
   mfgr  HP
   device  LJ III Si (/Print)
   desc  Select this model if you
   desc  have an HP LaserJet III Si and
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed  HP3SIBUND
   uses  L13PHPL3
end
begin
   type HP3SIBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HP3SICART;HP3SIBUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ3NIP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PCL5I;Printer
   file  L13PCL5I
   mfgr  HP
   device  LJ III Si (PCL5 Wysiwyg)
   desc  Select this model if you
   desc  have an HP LaserJet III Si and
   desc  want to best use Wysiwyg to print
   desc  text and graphics (:Print) and
   desc  best use 1-2-3 to print graphs
   desc  (/Print [B,E,P] Image).
   desc  This selection uses high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  PCL5IBUND
   uses  PCL5WID
end
begin
   type PCL5IBUND
   dprompt Select an HP LaserJet III Si option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PCL5BI1;PCL5IBUND
   device Letter (8.5" x 11")
   file  LJITHT.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  PCL5BI2;PCL5IBUND
   device Legal (8.5" x 14")
   file  LJITHG.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  PCL5BI3;PCL5IBUND
   device A4 (210mm x 297mm)
   file  LJITH4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name  HPLJ4;Printer
   file  L13PHP3S
   mfgr  HP
   device  LJ 4 Series (/Print)
   desc  Select this model series if you
   desc  have an HP LaserJet 4 Series and
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed  HPLJ4BUND
   uses  L13PHPL3
end
begin
   type HPLJ4BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPLJ4CART;HPLJ4BUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ3NIP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PCL5E;Printer
   file  L13PCL54
   mfgr  HP
   device  LJ 4 Series (PCL5 Wysiwyg)
   desc  Select this model series if you
   desc  have an HP LaserJet 4 Series and
   desc  want to best use Wysiwyg to print
   desc  text and graphics (:Print) and
   desc  best use 1-2-3 to print graphs
   desc  (/Print [B,E,P] Image).
   desc  This selection uses high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  PCL54BUND
   uses  PCL5WID
end
begin
   type PCL54BUND
   dprompt Select an HP LaserJet 4 Series option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PCL5BE1;PCL54BUND
   device Letter (8.5" x 11")
   file  LJ4THT.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  PCL5BE2;PCL54BUND
   device Legal (8.5" x 14")
   file  LJ4THG.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  PCL5BE3;PCL54BUND
   device A4 (210mm x 297mm)
   file  LJ4TH4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name  HPPNTJET;Printer
   file  L13PCOMN
   mfgr HP
   device  PaintJet
   desc  Select this model if you have
   desc  an HP PaintJet printer.
   mneed  PAINTJETBUND
   uses  JETUSE
end
begin
   type JETFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  JETUSE;JETFILE
   file  L13PHPPJ
end
begin
   type PAINTJETBUND
   dprompt Select an HP PaintJet option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PNTJET1;PAINTJETBUND
   device Paper (8.5" x 11")
   id    90,90,180,180
   file  HPPJPAPR.PBD
   desc  Select this option if you
   desc  want to use an HP PaintJet
   desc  with 8 1/2"x11" paper.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTJET2;PAINTJETBUND
   device Transparency (8.5" x 11")
   id    90,90,180,180
   file  HPPJTRAN.PBD
   desc  Select this option if you
   desc  want to use an HP PaintJet
   desc  with 8 1/2"x11" transparencies.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  HPPNTXL;Printer
   file  L13PCOMN
   mfgr HP
   device  PaintJet XL
   desc  Select this model if you have
   desc  an HP PaintJet XL printer.
   mneed  PNTJETXLBUND
   uses  JETXLUSE
end
begin
   type JETXLFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  JETXLUSE;JETXLFILE
   file  L13PHPPX
end
begin
   type PNTJETXLBUND
   dprompt Select an HP PaintJet XL option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PNTXL1;PNTJETXLBUND
   device Paper Letter (8.5" x 11")
   id    90,90,180,180
   file  HPPXPAPR.PBD
   desc  Select this option if 
   desc  you want to use Letter
   desc  size paper.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTXL2;PNTJETXLBUND
   device Transparency Letter (8.5" x 11")
   id    90,90,180,180
   file  HPPXTRAN.PBD
   desc  Select this option if 
   desc  you want to use Letter
   desc  size paper transparencies.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTXL3;PNTJETXLBUND
   device Paper Legal (8.5" x 14")
   id    90,90,180,180
   file  HPPXPA1.PBD
   desc  Select this option if
   desc  you want to use Legal  
   desc  size paper.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTXL4;PNTJETXLBUND
   device Transparency Legal (8.5" x 14")
   id    90,90,180,180
   file  HPPXTR1.PBD
   desc  Select this option if 
   desc  you want to use Legal 
   desc  size transparencies.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTXL5;PNTJETXLBUND
   device Paper Ledger (11" x 17")
   id    90,90,180,180
   file  HPPXPA2.PBD
   desc  Select this option if you
   desc  want to use an HP 
   desc  PaintJet XL with paper.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  PNTXL6;PNTJETXLBUND
   device Transparency Ledger (11" x 17")
   id    90,90,180,180
   file  HPPXTR2.PBD
   desc  Select this option if
   desc  you want use Ledger
   desc  size transparencies.
   uses  FAI017LAA,FAI033LAA,FAJ022LAA,FAA017LAA,FAA033LAA,FAC022LAA
   uses  FAI030LAA,FAI060LAA,FAJ040LAA,FAA030LAA,FAA060LAA,FAC040LAA
end
begin
   name  HP3PAMPXL;Printer
   file  L13PCOMN
   mfgr  HP
   device  PaintJet XL300 (/Print)
   desc  Select this model if you
   desc  have an HP PaintJet XL300 and
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed  HP3PXLBUND
   uses  HP3PXLUSE
end
begin
   type HP3PXLFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HP3PXLUSE;HP3PXLFILE
   file  L13PPXL3
end
begin
   type HP3PXLBUND
   dprompt Select an HP PaintJet XL300 option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PJXL3B0;HP3PXLBUND
   device Letter (8.5" x 11")
   id    150,150,300,300
   file  PJXL300.PBD
   desc  Select this option if you
   desc  want to use Letter size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PJXL3B1;HP3PXLBUND
   device Legal (8.5" x 14")
   id    150,150,300,300
   file  PJXL301.PBD
   desc  Select this option if you
   desc  want to use Legal size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PJXL3B2;HP3PXLBUND
   device Ledger (11" x 17")
   id    150,150,300,300
   file  PJXL302.PBD
   desc  Select this option if you
   desc  want to use Ledger size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PJXL3B3;HP3PXLBUND
   device A4  (210mm x 297mm)
   id    150,150,300,300
   file  PJXL303.PBD
   desc  Select this option if you
   desc  want to use A4 size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PJXL3B4;HP3PXLBUND
   device A3  (297mm x 420mm)
   id    150,150,300,300
   file  PJXL304.PBD
   desc  Select this option if you
   desc  want to use A3 size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PJXL3B5;HP3PXLBUND
   device B4  (257mm x 364mm)
   id    150,150,300,300
   file  PJXL305.PBD
   desc  Select this option if you
   desc  want to use B4 size 
   desc  paper or transparencies.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PCL5X;Printer
   file  L13PCL5X
   mfgr  HP
   device  PaintJet XL300 (PCL5 Wysiwyg)
   desc  Select this model if you
   desc  have an HP PaintJet XL300 and
   desc  want to best use Wysiwyg to print
   desc  text and graphics (:Print) and
   desc  best use 1-2-3 to print graphs
   desc  (/Print [B,E,P] Image).
   desc  This selection uses high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  PCL5XBUND
   uses  PCL5WID
end
begin
   type PCL5XBUND
   dprompt Select an HP PaintJet XL300 option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PCL5BX1;PCL5XBUND
   device Letter (8.5" x 11")
   file  PJXTHT.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  PCL5BX2;PCL5XBUND
   device Legal (8.5" x 14")
   file  PJXTHG.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  PCL5BX3;PCL5XBUND
   device Ledger (11" x 17")
   file  PJXTHD.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  ledger sized paper.
end
begin
   name  PCL5BX4;PCL5XBUND
   device A4 (210mm x 297mm)
   file  PJXTH4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name  PCL5BX5;PCL5XBUND
   device A3 (297mm x 420mm)
   file  PJXTH3.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  A3 sized paper.
end
begin
   name  PCL5BX6;PCL5XBUND
   device B4 (257mm x 364mm)
   file  PJXTHB4.PBD
   desc  Select this option if you
   desc  have enhanced PCL5 and
   desc  want to use "Times Roman"
   desc  and "Universe" typefaces with
   desc  B4 sized paper.
end
begin
   name  HPQT;Printer
   file  L13PCOMN
   mfgr  HP
   device ThinkJet
   desc  Select this model if you
   desc  have an HP ThinkJet printer.
   need  HPQTBUND
   uses  QTUSE
end
begin
   type QTFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  QTUSE;QTFILE
   file  L13PHPTJ
end
begin
   type HPQTBUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  QTBUND;HPQTBUND
   device printer
   id    96,96,192,96
   file  HPTJTG.PBD
   uses  FAA017LAA,FAA033LAA,FAC022LAA,FAJ022LAA,FAI017LAA,FAI033LAA
end
begin
   name  HPPL7440;Printer
   file  L13PHPPL
   mfgr  HP
   device ColorPro 7440A Plotter
   desc  Select this model if you have
   desc  an HP ColorPro 7440A Plotter.
   need  HPPL7440BUND
   uses  FCOMROM,FCOMITA,FSIMROM,FDUPROM,FTRIROM,FTRIITA
end
begin
   type HPPL7440BUND
   dprompt Select an HP ColorPro 7440A Plotter option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name P7440PBUND;HPPL7440BUND
   device Paper (8.5" x 11")
   file  HPPL40P.PBD
   desc  Select this option if you
   desc  want to use an HP ColorPro
   desc  7440A Plotter with 8 1/2"x11"
   desc  paper.
end
begin
   name P7440TBUND;HPPL7440BUND
   device Transparency (8.5" x 11")
   file  HPPL40T.PBD
   desc  Select this option if you
   desc  want to use an HP ColorPro
   desc  7440A Plotter with 8 1/2"x11"
   desc  transparencies.
end
begin
   name  HPPL7475;Printer
   file  L13PHPPL
   mfgr  HP
   device 7475A Plotter
   desc  Select this model if you
   desc  have an HP 7475A Plotter.
   need  HPPL7475BUND
   uses  FCOMROM,FCOMITA,FSIMROM,FDUPROM,FTRIROM,FTRIITA
end
begin
   type HPPL7475BUND
   dprompt Select an HP 7475A Plotter option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name P74751BUND;HPPL7475BUND
   device Paper (8.5" x 11")
   file  HPPL75PN.PBD
   desc  Select this option if you
   desc  want to use an HP 7475A
   desc  Plotter with 8 1/2"x11"
   desc  paper.
end
begin
   name P74752BUND;HPPL7475BUND
   device Paper (11" x 17")
   file  HPPL75PL.PBD
   desc  Select this option if you
   desc  want to use an HP 7475A
   desc  Plotter with 11"x17"
   desc  paper.
end
begin
   name P74753BUND;HPPL7475BUND
   device Transparency (8.5" x 11")
   file  HPPL75TN.PBD
   desc  Select this option if you
   desc  want to use an HP 7475A
   desc  Plotter with 8 1/2"x11"
   desc  transparencies.
end
begin
   name  HPPL7550M;Printer
   file  L13PHPPL
   mfgr  HP
   device 7550A Plotter manual feed
   desc  Select this model if you
   desc  have an HP 7550A Plotter and
   desc  want to use it with manual
   desc  paper feed.
   need  H7550MBUND
   uses  FCOMROM,FCOMITA,FSIMROM,FDUPROM,FTRIROM,FTRIITA
end
begin
   type H7550MBUND
   dprompt Select an HP 7550A Plotter option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name M75501BUND;H7550MBUND
   device Paper (8.5"x11")
   file  HPPL5PNM.PBD
   desc  Select this option if you
   desc  want to use an HP 7550A
   desc  Plotter with 8 1/2"x11"
   desc  paper.
end
begin
   name M75502BUND;H7550MBUND
   device Paper (11"x17")
   file  HPPL5PLM.PBD
   desc  Select this option if you
   desc  want to use an HP 7550A
   desc  Plotter with 11"x17"
   desc  paper.
end
begin
   name M75503BUND;H7550MBUND
   device Transparency
   file  HPPL5TNM.PBD
   desc  Select this option if you
   desc  want to use an HP 7550A
   desc  Plotter with 8 1/2"x11" 
   desc  transparencies.
end
begin
   name  HPPL7550A;Printer
   file  L13PHPPL
   mfgr  HP
   device 7550A Plotter auto feed
   desc  Select this model if you have
   desc  an HP 7550A Plotter and want
   desc  to use it with automatic
   desc  paper feed.
   need  H7550ABUND
   uses  FCOMROM,FCOMITA,FSIMROM,FDUPROM,FTRIROM,FTRIITA
end
begin
   type H7550ABUND
   dprompt Select an HP 7550A Plotter option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name A75501BUND;H7550ABUND
   device Paper (8.5"x11")
   file  HPPL5PNA.PBD
   desc  Select this option if you
   desc  want to use an HP 7550A
   desc  Plotter with 8 1/2"x11"
   desc  paper.
end
begin
   name A75503BUND;H7550ABUND
   device Transparency (8.5"x11")
   file  HPPL5TNA.PBD
   desc  Select this option if you
   desc  want to use an HP 7550A
   desc  Plotter with 8 1/2"x11"
   desc  transparencies.
end
begin
   name  IBM4019;Printer
   file  L13PIBCM
   id    300,300,300,300
   mfgr  IBM
   device 4019 LaserPrinter Series
   desc  Select this model series if you
   desc  use an IBM 4019 LaserPrinter
   desc  Series printer.
   mneed 4019BUN
   uses  4019USE
end
begin
   type 4019FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4019USE;4019FILE
   file  L13PIB49
end
begin
   type 4019BUN
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4019BUN1;4019BUN
   file  IBMLJ419.PBD
   id    300,300,300,300
   device No Cartridge
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA050LAA,FAA100LAA,FAC066LAA
end
begin
   name  IBM4029;Printer
   file  L13PIBCM
   id    300,300,300,300
   mfgr  IBM
   device 4029 LaserPrinter Series
   desc  Select this model series if you
   desc  use an IBM 4029 LaserPrinter
   desc  Series printer.
   mneed 4029BUN
   uses  4029USE
end
begin
   type 4029FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4029USE;4029FILE
   file  L13P4029
end
begin
   type 4029BUN
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4029BUN1;4029BUN
   file  IBM4029.PBD
   id    300,300,300,300
   device No Cartridge
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA050LAA,FAA100LAA,FAC066LAA
end
begin
   name  IBM4037;Printer
   file  L13PIBCM
   id    300,300,300,300
   mfgr  IBM
   device LP 4037-5E
   desc  Select this model series if you
   desc  use an IBM LP 4037-5E printer.
   mneed 4037BUN
   uses  4037USE
end
begin
   type 4037FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4037USE;4037FILE
   file  L13P4029
end
begin
   type 4037BUN
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  4037BUN1;4037BUN
   device No Cartridge
   id    300,300,300,300
   file  IBM4029.PBD
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA050LAA,FAA100LAA,FAC066LAA
end
begin
   name  IBM4039R;Printer
   file  L13PHP3S
   mfgr  IBM
   device 4039 LP Series (/Print)
   desc  Select this model series if you
   desc  have an IBM 4039 LP Series and
   desc  want to best utilize the 1-2-3
   desc  capabilities for printing ranges
   desc  of data (/Print [B,E,F,P] Range).
   desc  
   desc  This selection uses 300dpi final
   desc  quality and 150dpi draft quality
   desc  and provides the fastest output
   desc  speed possible for your printer.
   mneed I4039RBUN
   uses  I4039RUSE
end
begin
   type I4039RFILE
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  I4039RUSE;I4039RFILE
   file  L13PHPL3
end
begin
   type I4039RBUN
   dprompt Select an IBM 4039 LP Series option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  I4039RBUN1;I4039RBUN
   device No Cartridge
   id    150,150,300,300
   file  HPLJ3NIP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  IBMPCL5I;Printer
   file  L13PCL5I
   mfgr  IBM
   device  4039 LP Series (PCL5 Wysiwyg)
   desc  Select this model series if you
   desc  have an IBM 4039 LP Series and
   desc  want to best use Wysiwyg to print
   desc  text and graphics (:Print) and
   desc  best use 1-2-3 to print graphs
   desc  (/Print [B,E,P] Image).
   desc  This selection allows high-density
   desc  full-page graphics and provides
   desc  the highest quality resolution at
   desc  the fastest output speed possible
   desc  for your printer.
   need  IBMPCL5IBUND
   uses  PCL5WID
end
begin
   type IBMPCL5IBUND
   dprompt Select an IBM 4039 LP Series option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  IBMPCL5BI1;IBMPCL5IBUND
   device Letter (8.5" x 11")
   file  LJITHT.PBD
   desc  Select this option if you
   desc  want to use "Times Roman" and
   desc  "Universe" typefaces with
   desc  letter sized paper.
end
begin
   name  IBMPCL5BI2;IBMPCL5IBUND
   device Legal (8.5" x 14")
   file  LJITHG.PBD
   desc  Select this option if you
   desc  want to use "Times Roman" and
   desc  "Universe" typefaces with
   desc  legal sized paper.
end
begin
   name  IBMPCL5BI3;IBMPCL5IBUND
   device A4 (210mm x 297mm)
   file  LJITH4.PBD
   desc  Select this option if you
   desc  want to use "Times Roman" and
   desc  "Universe" typefaces with
   desc  A4 sized paper.
end
begin
   name IBM4701;Printer
   file L13PCOMN
   mfgr IBM
   device 4070 IJ
   desc  Select this model if
   desc  you have an IBM 4070 IJ.
   mneed  IBM4701BND
   uses  L13PIBPP
end
begin
   type IBM4701BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IBM4701B1;IBM4701BND
   file  CANPPROM.PBD
   id    180,180,360,180
   uses  FAI012LFA,FAI024LFA,FAJ016LFA,FAA012LFA,FAA024LFA,FAC016LFA
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name IBM4072;Printer
   file L13PCOMN
   mfgr IBM
   device 4072 ExecJet
   desc  Select this model if you
   desc  have an IBM 4072 ExecJet.
   need  IBM4072BND
   uses  L13PIBPP
end
begin
   type IBM4072BND
   dprompt Select an IBM 4072 ExecJet option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IB4072M;IBM4072BND
   device Monospaced
   file  IBM4072M.PBD
   id    180,180,360,180
   desc  Select this option if you 
   desc  have an IBM ExecJet 4072 
   desc  printer and want to use 
   desc  monospaced text and normal-density
   desc  graphics.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  IB4072P;IBM4072BND
   device Proportional
   file  IBM4072P.PBD
   id    180,180,360,180
   desc  Select this option if you 
   desc  have an IBM ExecJet 4072 
   desc  printer and want to use 
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  IBM4076;Printer
   file  L13PCOMN
   mfgr  IBM
   device 4076 IJ
   desc  Select this model if you have
   desc  an IBM 4076 IJ printer.
   need  IJ4BUN
   uses  IJ4USE
end
begin
   type  IJ40FIL
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IJ4USE;IJ40FIL
   file  L13PHPDJ
end
begin
   type IJ4BUN
   dprompt Select an IBM 4076 IJ option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name I4076PBUND;IJ4BUN
   device Paper
   id    150,150,300,300
   file  HPDJ500.PBD
   desc  Select this option if you want to
   desc  print text and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name I4076TBUND;IJ4BUN
   device Transparency
   id    150,150,300,300
   file  HPDJ500T.PBD
   desc  Select this option if you want
   desc  to print text and graphics on a
   desc  transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  IBMPT;Printer
   file  L13PCOMN
   mfgr  IBM
   device 5183 Portable
   desc  Select this model if you have
   desc  an IBM 5183 Portable printer.
   mneed IBMPTBUND
   uses  L13PEPLQ,PANUSE
end
begin
   type IBMPTBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IBMPTM1;IBMPTBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device printer
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name IBM2380;Printer
   file L13PCOMN
   mfgr IBM
   device PPS-II 2380 Series
   desc  Select this if you
   desc  have an IBM PPS-II 2380
   desc  Series printer.
   need  IBM2380BND
   uses  L13PIBPP
end
begin
   type IBM2380BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IB2380M;IBM2380BND
   file  IBM4226M.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name IBM2390;Printer
   file L13PCOMN
   mfgr IBM
   device PPS-II 2390 Series
   desc  Select this if you
   desc  have an IBM PPS-2390
   desc  Series printer.
   need  IBM2390BND
   uses  L13PIBPP
end
begin
   type IBM2390BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IB2390M;IBM2390BND
   file  IBM2390M.PBD
   id    180,180,360,180
   uses  FAA030LAA,FAA030LGA,FAA060LAA,FAA060LGA,FAC040LAA,FAC040LGA
   uses  FAI030LGA,FAI060LAA,FAI060LGA,FAJ040LAA,FAJ040LGA,FAI030LAA
   uses  FAI017LIA,FAI033LIA,FAJ022LIA,FAA017LIA,FAA033LIA,FAC022LIA
end
begin
   name IBMPRO;Printer
   file L13PCOMN
   mfgr IBM
   device Proprinter
   desc  Select this model if you
   desc  have an IBM Proprinter.
   need  IBMPROBND
   uses  L13PIBPP
end
begin
   type IBMPROBND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PROB1;IBMPROBND
   device printer
   file  IBPPRO.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name IBMPROII;Printer
   file  L13PCOMN
   mfgr IBM
   device Proprinter II, XL
   desc  Select this model series if
   desc  you have an IBM Proprinter II
   desc  or an IBM Proprinter XL.
   need  IBMPROIIBND
   uses  L13PIBPP
end
begin
   type IBMPROIIBND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PROB2;IBMPROIIBND
   device printer
   file  IBPPROII.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name IBMPROX;Printer
   file L13PCOMN
   mfgr IBM
   device Proprinter X24/XL24
   desc  Select this model series if
   desc  you have an IBM Proprinter X24
   desc  or an IBM Proprinter XL24.
   mneed  IBMPROXBND
   uses  L13PIBPP
end
begin
   type IBMPROXBND
   dprompt Select an IBM Proprinter X24/XL24 option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PROB3;IBMPROXBND
   device Monospaced
   file  IBPPROII.PBD
   id    120,72,120,72
   desc  Select this option if you 
   desc  want to use an IBM
   desc  Proprinter X24/XL24 with
   desc  monospaced text and
   desc  normal-density graphics.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  PROB4;IBMPROXBND
   device Proportional
   id    180,180,360,180
   file  IBPPRO24.PBD
   desc  Select this option if you 
   desc  want to use an IBM
   desc  Proprinter X24/XL24 with
   desc  proportionally spaced
   desc  text and high-density
   desc  graphics.
   uses  FAA030LAA,FAA030LGA,FAA060LAA,FAA060LGA,FAC040LAA,FAC040LGA
   uses  FAI030LGA,FAI060LAA,FAI060LGA,FAJ040LAA,FAJ040LGA,FAI030LAA
   uses  FAI017LIA,FAI033LIA,FAJ022LIA,FAA017LIA,FAA033LIA,FAC022LIA
end
begin
   name IBMPS1;Printer
   file L13PCOMN
   mfgr IBM
   device PS/1, PS/1+
   desc  Select this model series if
   desc  if you have an IBM PS/1 or
   desc  an IBM PS/1+.
   mneed  IBMPS1BND
   uses  L13PIBPP
end
begin
   type IBMPS1BND
   dprompt Select an IBM PS/1, PS/1+ option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PS1B4;IBMPS1BND
   device Monospaced
   file  IBPPROII.PBD
   id    120,72,120,72
   desc  Select this option if you 
   desc  want to use an IBM PS/1
   desc  or an IBM PS/1+ with
   desc  monospaced text and
   desc  normal-density graphics.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  PS1B5;IBMPS1BND
   device Proportional
   id    180,180,360,180
   file  IBPPRO24.PBD
   desc  Select this option if you 
   desc  want to use an IBM PS/1
   desc  or an IBM PS/1+ with
   desc  proportionally spaced text
   desc  and high-density graphics.
   uses  FAA030LAA,FAA030LGA,FAA060LAA,FAA060LGA,FAC040LAA,FAC040LGA
   uses  FAI030LGA,FAI060LAA,FAI060LGA,FAJ040LAA,FAJ040LGA,FAI030LAA
   uses  FAI017LIA,FAI033LIA,FAJ022LIA,FAA017LIA,FAA033LIA,FAC022LIA
end
begin
   name IBMGRPH;Printer
   file L13PCOMN
   mfgr IBM
   device Graphics Printer
   desc  Select this model if you
   desc  have an IBM Graphics
   desc  Printer Model 5152.
   need  IBMGRPHBND
   uses  GRPHUSE
end
begin
   type GRPHFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  GRPHUSE;GRPHFILE
   file  L13PIBGP
end
begin
   type IBMGRPHBND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  GRPHB1;IBMGRPHBND
   device 5152
   file  IBGP5152.PBD
   id    120,72,120,72
   uses  FAA012LHA,FAA024LHA,FAC016LHA,FAI012LHA,FAI024LHA,FAJ016LHA
end
begin
   name IBMQUICK;Printer
   file L13PCOMN
   mfgr IBM
   device Quickwriter
   desc  Select this if you
   desc  have an IBM Quickwriter printer.
   need  IBMQUICKBND
   uses  L13PIBPP
end
begin
   type IBMQUICKBND
   dprompt Select an IBM Quickwriter option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IBQUICKM;IBMQUICKBND
   device Monospaced
   file  IBMQKM.PBD
   id    120,72,240,72
   desc  Select this option if you 
   desc  have an IBM Quickwriter printer
   desc  and want to use monospaced text
   desc  and normal-density graphics.
   uses  FAI012LFA,FAI024LFA,FAJ016LFA,FAA012LFA,FAA024LFA,FAC016LFA
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  IBQUICKP;IBMQUICKBND
   device Proportional
   file  IBMQKP.PBD
   id    120,72,240,72
   desc  Select this option if you 
   desc  have an IBM Quickwriter printer
   desc  and want to use proportionally
   desc  spaced text and high-density
   desc  graphics.
   uses  FAI012LFA,FAI024LFA,FAJ016LFA,FAA012LFA,FAA024LFA,FAC016LFA
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name IBMQW1;Printer
   file L13PCOMN
   mfgr IBM
   device Quietwriter I
   desc  Select this model if you
   desc  have an IBM Quietwriter I.
   need  IBMQW1BND
   uses  QW1USE
end
begin
   type QW1FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  QW1USE;QW1FILE
   file  L13PIBQ1
end
begin
   type IBMQW1BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  QW1B1;IBMQW1BND
   device printer
   id    60,72,120,72
   file  IBQ1QW1.PBD
   uses  FAA012LFA,FAA012LHA,FAA024LFA,FAA024LHA,FAC016LFA,FAC016LHA
   uses  FAI012LFA,FAI012LHA,FAI024LFA,FAI024LHA,FAJ016LFA,FAJ016LHA
end
begin
   name IBMQW2;Printer
   file L13PCOMN
   mfgr IBM
   device Quietwriter II
   desc  Select this model if you
   desc  have an IBM Quietwriter II.
   need  IBMQW2BND
   uses  L13PIBQ2
end
begin
   type IBMQW2BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  QW2B1;IBMQW2BND
   device printer
   file  IBQ2QW2.PBD
   id    120,72,120,72
   uses  FAA012LHA,FAA024LHA,FAC016LHA,FAI012LHA,FAI024LHA,FAJ016LHA
end
begin
   name IBMQW3;Printer
   file L13PCOMN
   mfgr IBM
   device Quietwriter III
   desc  Select this model if you 
   desc  have an IBM Quietwriter III.
   need  IBMQW3BND
   uses  L13PIBQ2
end
begin
   type IBMQW3BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  QW3B1;IBMQW3BND
   device printer
   file  IBQ2QW3.PBD
   id    120,72,120,72
   uses  FAA012LHA,FAA024LHA,FAC016LHA,FAI012LHA,FAI024LHA,FAJ016LHA
end
begin
   name IBM4226;Printer
   file L13PCOMN
   mfgr IBM
   device 4226
   desc  Select this model if you
   desc  have an IBM 4226.
   need  IBM4226BND
   uses  L13PIBPP
end
begin
   type IBM4226BND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  IB4226M;IBM4226BND
   file  IBM4226M.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  PIN;Printer
   file  L13PCOMN
   mfgr  NEC
   device  Pinwriter Series
   desc  Select this model series if
   desc  you have a NEC Pinwriter
   desc  Series printer.
   mneed  NECBUND
   uses  NECUSE
end
begin
   type NECFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  NECUSE;NECFILE
   file  L13PNEC
end
begin
   type NECBUND
   dprompt Select a NEC Pinwriter option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  NECBUND1;NECBUND
   device B&W Gothic
   file  NECBWGO.PBD
   id    180,180,360,180
   desc  Select this option if you
   desc  want to use a NEC Pinwriter
   desc  for B&W printing with
   desc  "Gothic" typeface and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  NECBUND2;NECBUND
   device Color Gothic
   file  NECCOLGO.PBD
   id    180,180,360,180
   desc  Select this option if you
   desc  want to use a NEC Pinwriter
   desc  for color printing with
   desc  "Gothic" typeface and 
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  NECBUND3;NECBUND
   device B&W Courier
   file  NECBWCO.PBD
   id    180,180,360,180
   desc  Select this option if you
   desc  want to use a NEC Pinwriter
   desc  for B&W printing with
   desc  "Courier" typeface and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  NECBUND4;NECBUND
   device Color Courier
   file  NECCOLCO.PBD
   id    180,180,360,180
   desc  Select this option if you
   desc  want to use a NEC Pinwriter
   desc  for color printing with
   desc  "Courier" typeface and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  OKI84;Printer
   file  L13PCOMN
   mfgr Okidata
   device  ML 84, 92/93
   desc  Select this model series if
   desc  you have an Okidata Microline
   desc  84, 92, or 93 printer.
   need  OKI84BUND
   uses  L13POK84
end
begin
   type OKI84BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OKI84GEN;OKI84BUND
   device printer
   id    72,72,72,72
   file  OK849293.PBD
   uses  FAA012LAA,FAA025LAA,FAC017LAA,FAJ017LAA,FAI012LAA,FAI025LAA
end
begin
   name  OKI192;Printer
   file  L13PCOMN
   mfgr Okidata
   device  ML 192/193
   desc  Select this model series if
   desc  you have an Okidata Microline
   desc  192 or 193 printer.
   need  OKI192BUND
   uses  L13POK84
end
begin
   type OKI192BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OKI192GEN;OKI192BUND
   device printer
   id    120,72,120,72
   file  OK192193.PBD
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  OKI294;Printer
   file  L13PCOMN
   mfgr Okidata
   device  ML 290I Series
   desc  Select this model series if
   desc  you have an Okidata Microline
   desc  292I, 293I, or 294I printer.
   need  OKI294BUND
   uses  294USE
end
begin
   type 294FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  294USE;294FILE
   file  L13POK29
end
begin
   type OKI294BUND
   dprompt Select an Okidata Microline 290I Series option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  294BUND;OKI294BUND
   device B&W
   id    120,72,120,72
   file  OK290I.PBD
   desc  Select this option if you
   desc  want to use an Okidata Microline
   desc  292I, 293I, or 294I printer
   desc  for B&W printing.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  294CBUND;OKI294BUND
   device Color
   id    120,72,120,72
   file  OK290IC.PBD
   desc  Select this option if you
   desc  want to use an Okidata Microline
   desc  292I, 293I, or 294I printer
   desc  for color printing.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  OKIX93;Printer
   file  L13PCOMN
   mfgr  Okidata
   device  ML 292 and 293 
   desc  Select this model series if you
   desc  have an Okidata Microline
   desc  292 or 293 printer.
   mneed  OKX93BUND
   uses  EPSONMXUSE
end
begin
   type OKX93BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OKX93BUN;OKX93BUND
   file  EPDTFX.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  OKI32X;Printer
   file  L13PCOMN
   mfgr  Okidata
   device  ML 320 and 321
   desc  Select this model series if you
   desc  have an Okidata Microline
   desc  320 or 321 printer.
   mneed  OK32XBUND
   uses  EPSONMXUSE
end
begin
   type OK32XBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OK32XBUN;OK32XBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  OKI380;Printer
   file  L13PCOMN
   mfgr  Okidata
   device  ML 380/390/391/393/395/590/591
   desc  Select this model series if
   desc  you have an Okidata Microline
   desc  380, 390, 390+, 391, 391+,
   desc  393, 393+, 395, 590 or 591.
   mneed OKI380BUND
   uses  L13PEPLQ,PANUSE
end
begin
   type OKI380BUND
   dprompt Select an Oki ML 380/390/391/393/395/590/591 option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OKI380B1;OKI380BUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device B&W Monospaced
   desc  Select this option if you
   desc  have an Oki ML 380, 
   desc  390/391/393/395/590/591
   desc	 Series printer and want to
   desc  use monospaced text and 
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  OKI380B2;OKI380BUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device B&W Proportional
   desc  Select this option if you
   desc  have an Oki ML 380, 
   desc  390/391/393/395/590/591
   desc	 Series printer and want to
   desc  use proportionally spaced 
   desc  text and high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  OKI380C1;OKI380BUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device Color Monospaced
   desc  Select this option if you
   desc  have an Oki ML 380, 
   desc  390/391/393/395/590/591
   desc	 Series printer with a Color
   desc  option and want to
   desc  use monospaced text and 
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  OKI380C2;OKI380BUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device Color Proportional
   desc  Select this option if you
   desc  have an Oki ML 380, 
   desc  390/391/393/395/590/591
   desc	 Series printer with a Color
   desc  option and want to use
   desc  proportionally spaced text
   desc  and high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  OKOL4LAS;Printer
   file  L13PHPCM
   mfgr  Okidata
   device  Laser OL-400, 800
   desc  Select this model series if
   desc  you have an Oki Laser OL-400
   desc  OL-400e or OL-800 Laser printer
   need  OKOL4BUND
   uses  HPUSE2
end
begin
   type OKOL4BUND
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  OKOL4NCART;OKOL4BUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ2NOH.PBD
   desc  Select this option if you 
   desc  want to use an Oki Laser 
   desc  OL-400, OL-400e, OL-800
   desc  with no cartridge.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  PAN1695;Printer
   file  L13PCOMN
   mfgr  Panasonic
   device  KX-P 9 Pin Series
   desc  Select this model series if you
   desc  have a Panasonic printer model
   desc  KX-P1080, 1080i, 1180, 1180i,
   desc  KX-P1091, 1091i, 1092, 1092i,
   desc  KX-P1191, 1592, 1595, 1695, or
   desc  KX-P2180.
   mneed  PANBUND
   uses  PANUSE
end
begin
   type PANFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANUSE;PANFILE
   file  L13PEPDT
end
begin
   type PANBUND
   dprompt Select a Panasonic 9-pin model option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PAN9BBUN;PANBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   device B&W
   desc  Select this for Panasonic KX-P
   desc  9 Pin Series B&W printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  PAN9CBUN;PANBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   device Color
   desc  Select this for Panasonic KX-P
   desc  9 Pin Series Color printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  PANLQ;Printer
   file  L13PCOMN
   mfgr  Panasonic
   device  KX-P 24 Pin Series
   desc  Select this model series if you
   desc  have a Panasonic printer model 
   desc  KX-P1123, 1124, 1124i,
   desc  KX-P2123, 2124, or 2624.
   mneed PANLQBUND
   uses  PANLQUSE,PANUSE
end
begin
   type PANLQFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANLQUSE;PANLQFILE
   file  L13PEPLQ
end
begin
   type PANLQBUND
   dprompt Select a Panasonic 24-pin model option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANLQB1;PANLQBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device B&W Monospaced
   desc  Select this option if you
   desc  want to use B&W text
   desc  and normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  PANLQB2;PANLQBUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device B&W Proportional
   desc  Select this option if you want
   desc  to use B&W proportionally spaced
   desc  text and high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  PANLQC1;PANLQBUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device Color Monospaced
   desc  Select this option if you
   desc  want to use color with text
   desc  and normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  PANLQC2;PANLQBUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device Color Proportional
   desc  Select this option if you
   desc  want to use color with
   desc  proportionally spaced text
   desc  and high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  PANKXP3;Printer
   file  L13PCOMN
   mfgr  Panasonic
   device KX-P3123, 3124, 3624
   desc  Select this if you have
   desc  a Panasonic printer model
   desc  KX-P3123, 3124, or 3624.
   desc
   desc  Draft mode 180x180 dpi
   desc  Final mode 360x360 dpi
   mneed  PANKXP3BUND
   uses  PANKXP3USE
end
begin
   type PANKXP3FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANKXP3USE;PANKXP3FILE
   file  L13PEPP2
end
begin
   type PANKXP3BUND
   dprompt Select a Panasonic Printer
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANKXPB3BUN;PANKXP3BUND
   file  EPP2570.PBD
   id    180,180,360,360
   device B&W
   desc  Select this for a Panasonic
   desc  KX-P3123, 3124, or 3624
   desc  B&W printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  PANKXPC3BUN;PANKXP3BUND
   file  EPP2C.PBD
   id    180,180,360,360
   device Color
   desc  Select this for a Panasonic
   desc  KX-P3123, 3124, or 3624
   desc  color printer.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  PANL24LAS;Printer
   file  L13PHPCM
   mfgr  Panasonic
   device  KX-P4450i Laser Printer
   desc  Select this device if you
   desc  have a Panasonic KX-P4450i
   desc  Laser printer.
   need  PANL24BUND
   uses  HPUSE2
end
begin
   type PANL24BUND
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PANL24NCART;PANL24BUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ2NOH.PBD
   desc  Panasonic KX-P4450i Laser
   desc  printer with no cartridge.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  POSTSCRIPT1;Printer
   file  L13PPSC0
   mfgr  PostScript
   device  PostScript
   desc  Select this if you have an Adobe
   desc  PostScript compatible B&W or Color
   desc  printer/option, for example:
   desc  
   desc  Apple LaserWriter, Epson EPL-7500,
   desc  HP LJ II PostScript Cartridge,
   desc  IBM 4019/4029 LaserPrinter Option,
   desc  Okidata OL-840, QMS PS-410,
   desc  Panasonic KX-P4455, or
   desc  TI Microlaser PS 17/35.
   need  PSCO1BUND
end
begin
   type PSCO1BUND
   dprompt Select a Postscript printer font option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  PSCOBL1;PSCO1BUND
   device Times & Helvetica
   file  PS00COW0.PBD
   desc  Select this option if you
   desc  have a PostScript printer
   desc  and want to use "Times Roman"
   desc  and "Helvetica" typefaces.
end
begin
   name  PSCOBL2;PSCO1BUND
   device Bookman & Avant Garde
   file  PS00COWP.PBD
   desc  Select this option if you
   desc  have a PostScript printer
   desc  and want to use "ITC Bookman"
   desc  and "ITC Avant Garde" typefaces.
end
begin
   name  POSTSCRIPT2;Printer
   file  L13PPS00
   mfgr  PostScript
   device  PostScript Level 2
   desc  Select this if you have an Adobe
   desc  PostScript Level 2 compatible
   desc  B&W or Color printer/option,
   desc  for example: 
   desc  
   desc  Apple LaserWriter IIf/IIg,
   desc  HP LJ III Cartridge Plus, 
   desc  HP LJ 4 Series, HP DJ 1200C/PS,
   desc  IBM 4039 LaserPrinter, QMS PS-860,
   desc  NEC SilentWriter2-95, or
   desc  Tektronix Color Phaser II/III PXi.
   need  PSCO2BUND
end
begin
   type PSCO2BUND
   dprompt Select a PostScript Level 2 font option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  PSCOB1;PSCO2BUND
   device Times & Helvetica
   file  PS00COW0.PBD
   desc  Select this option if you
   desc  have a PostScript printer
   desc  and want to use "Times Roman"
   desc  and "Helvetica" typefaces.
end
begin
   name  PSCOB2;PSCO2BUND
   device Bookman & Avant Garde
   file  PS00COWP.PBD
   desc  Select this option if you
   desc  have a PostScript printer
   desc  and want to use "ITC Bookman"
   desc  and "ITC Avant Garde" typefaces.
end
begin
   name  POSTSCRIPT;Printer
   file  L13PEPSF
   mfgr  PostScript
   device  PostScript EPSF
   desc  Select this if you require
   desc  printing to a standard
   desc  Encapsulated PostScript file.
   need  EPSFBUND
end
begin
   type EPSFBUND
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name  EPSFB;EPSFBUND
   device Encapsulated PostScript
   file  PS00ALW0.PBD
end
begin
   name  STLS5LAS;Printer
   file  L13PHP3C
   mfgr  Star
   device  LS-5 Laser Printer
   desc  Select this model series if
   desc  you have a Star LS-5 Laser
   desc  Printer. 
   mneed  STLS5BUND
   uses  L13PHPL3
end
begin
   type STLS5BUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  STLS5NCART;STLS5BUND
   id    150,150,300,300
   file  HPLJ3NHP.PBD
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA,FAJ033LAA
end
begin
   name  STARPRN;Printer
   file  L13PCOMN
   mfgr Star
   device NX-1000 Series
   desc  Select this model series if
   desc  you have a Star NX-1000 Series
   desc  printer.
   mneed  STAR1000
   uses  1000USE
end
begin
   type 1000FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  1000USE;1000FILE
   file  L13PSTAR
end
begin
   type STAR1000
   dprompt Select a Star NX-1000 model:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  STAR10001;STAR1000
   device NX-1000 B&W
   id    120,72,120,72
   file  ST1000BW.PBD
   desc  Select this option if you
   desc  have a Star NX-1000 B&W printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  STAR10002;STAR1000
   file  ST1000C.PBD
   id    120,72,120,72
   device NX-1000 Color
   desc  Select this option if you
   desc  have a Star NX-1000 Color
   desc  printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  STARFX;Printer
   file  L13PCOMN
   mfgr  Star
   device XR Series
   desc  Select this model series if you
   desc  have a Star XR 1000, 1500, 1020,
   desc  or 1520 Series printer.
   mneed  STARMXBUND
   uses  EPSONMXUSE
end
begin
   type STARMXBUND
   dprompt Select a Star XR model series option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  STXRBUN;STARMXBUND
   file  EPDTFX.PBD
   id    120,72,120,72
   device XR-1000 & 1500 B&W
   desc  Select this option if you
   desc  have a Star XR-1000 or
   desc  XR-1500 B&W  printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  STXRBUNB2;STARMXBUND
   file  EPDTEXC.PBD
   id    120,72,120,72
   device XR-1020 & 1520 Color
   desc  Select this option if you
   desc  have a Star XR-1020 or 1520
   desc  Color printer.
   uses  FAI012LHA,FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA
end
begin
   name  STARLQ;Printer
   file  L13PCOMN
   mfgr  Star
   device NX & XB Series
   desc  Select this model series if
   desc  you have a Star NX or XB
   desc	 2410, 2415, 2420, 2425 or 2430
   desc  Series printer.
   mneed STARLQBUND
   uses  L13PEPLQ,PANUSE
end
begin
   type STARLQBUND
   dprompt Select a Star NX or XB model and option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  ST800B2;STARLQBUND
   file  EPLQL80M.PBD
   id    180,180,180,180
   device NX-2410/2415/2430 Monospaced
   desc  Select this option if you
   desc  have a Star NX-2410, 2415,
   desc  2430 printer and want to
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  ST800B1;STARLQBUND
   file  EPLQL80P.PBD
   id    180,180,180,180
   device NX-2410/2415/2430 Proportional
   desc  Select this option if you
   desc  have a Star NX-2410, 2415,
   desc  2430 printer and want to use
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  ST25NXB1;STARLQBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device NX-2420 B&W Monospaced
   desc  Select this option if you
   desc  have a Star NX-2420 
   desc  B&W printer and want to 
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  ST25NXB2;STARLQBUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device NX-2420 B&W Proportional
   desc  Select this option if you
   desc  have a Star NX-2420 
   desc  B&W printer and want to use 
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  STNXMONO;STARLQBUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device NX-2420 Color Monospaced
   desc  Select this option if you
   desc  have a Star NX-2420 
   desc	 color printer and want to 
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  STNXPROP;STARLQBUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device NX-2420 Color Proportional
   desc  Select this option if you
   desc  have a Star NX-2420 
   desc	 color printer and want to use
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  ST2500B1;STARLQBUND
   file  EPLQL25M.PBD
   id    180,180,360,180
   device XB-2410/2415 B&W Monospaced
   desc  Select this option if you
   desc  have a Star XB-2410 or 2415
   desc  B&W printer and want to
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  ST2500B2;STARLQBUND
   file  EPLQL25P.PBD
   id    180,180,360,180
   device XB-2410/2415 B&W Proportional
   desc  Select this option if you
   desc  have a Star XB-2410 or 2415
   desc  B&W printer and want to use 
   desc  proportionally spaced text and
   desc  high-density graphics. 
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  STMONO;STARLQBUND
   file  EPLQL2MC.PBD
   id    180,180,360,180
   device XB-2420/2425 Color Monospaced
   desc  Select this option if you
   desc  have a Star XB-2420 or 2425
   desc	 color printer and want to
   desc  use monospaced text and
   desc  normal-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  STPROP;STARLQBUND
   file  EPLQL2PC.PBD
   id    180,180,360,180
   device XB-2420/2425 Color Proportional
   desc  Select this option if you
   desc  have a Star XB-2420 or 2425
   desc	 color printer and want to use
   desc  proportionally spaced text and
   desc  high-density graphics.
   uses  FAA060LAA,FAC040LAA,FAA030LAA,FAJ040LAA,FAI030LAA,FAI060LAA
end
begin
   name  TIUM;Printer
   file  L13PCOMN
   mfgr  Texas Instruments
   device TI microMarc
   desc  Select this model if you
   desc  have a TI microMarc
   desc  printer.
   need  TIUMBUND
   uses  L13PHPDJ
end
begin
   type TIUMBUND
   dprompt Select a TI microMarc option:
   nselect
   mincnt 0
   maxcnt 16    
end
begin
   name TIUMPBUND3000;TIUMBUND
   device Paper
   id    150,150,300,300
   file  HPDJ500.PBD
   desc  Select this option if you want
   desc  print text and graphics on paper.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name TIUMTBUND3000;TIUMBUND
   device Transparency
   id    150,150,300,300
   file  HPDJ500T.PBD
   desc  Select this option if you want
   desc  print text and graphics on a
   desc	 transparency.
   uses  FAI025LAA,FAI050LAA,FAJ033LAA,FAA025LAA,FAA050LAA,FAC033LAA
   uses  FAI100LAA,FAJ066LAA,FAA100LAA,FAC066LAA
end
begin
   name  TI850;Printer
   file  L13PCOMN
   mfgr  Texas Instruments
   device  TI 800 Series
   desc  Select this model series if you
   desc  have an 850 or 865 Series printer.
   mneed  TIBUND
   uses  TI850USE
end
begin
   type TIFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  TI850USE;TIFILE
   file  L13PTI80
end
begin
   type TIBUND
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  TIBUN;TIBUND
   file  TI850.PBD
   id    60,72,120,72
   device 850 or 865 Printer
   uses  FAI012LFA,FAI024LFA,FAJ016LFA,FAA012LFA,FAC016LFA,FAI012LHA
   uses  FAI024LHA,FAJ016LHA,FAA012LHA,FAA024LHA,FAC016LHA,FAA024LFA
end  
begin
   name  TIUW24LAS;Printer
   file  L13PHPCM
   mfgr  Texas Instruments
   device  TI microWriter
   desc  Select this device if you
   desc  have a TI microWriter
   desc  laser printer.
   need  TIUW24BUND
   uses  HPUSE2
end
begin
   type TIUW24BUND
   dprompt Select a
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  TIUW24NCART;TIUW24BUND
   device No cartridge
   id    150,150,300,300
   file  HPLJ2NOH.PBD
   desc  TI microWriter laser
   desc  printer with no cartridge.
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   name  TOSHPRN;Printer
   file  L13PCOMN
   mfgr Toshiba
   device  P351 Series
   desc  Select this model series if
   desc  you have a Toshiba P351 Series
   desc  printer.
   mneed  TOSH351
   uses  351USE
end
begin
   type 351FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  351USE;351FILE
   file  L13PTO35
end
begin
   type TOSH351
   dprompt Select a Toshiba P351 Series option: 
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  TOSH351B;TOSH351
   device B&W P351
   id    180,180
   file  TO351NO.PBD
   desc  Select this option if you
   desc  have a Toshiba P351 B&W printer.
   uses  FAA030LAA,FAA060LAA,FAC040LAA,FAI030LAA,FAI060LAA,FAJ040LAA
end
begin
   name  TOSH351C;TOSH351
   file  TO351C.PBD
   id    180,180
   device Color P351C
   desc  Select this option if you
   desc  have a Toshiba P351C color
   desc  printer.
   uses  FAA030LAA,FAA060LAA,FAC040LAA,FAI030LAA,FAI060LAA,FAJ040LAA
end
begin
   name  XEROX;Printer
   file  L13PXRX
   mfgr  Xerox
   device 4045
   desc  Select this model if you have
   desc  a Xerox 4045 Printer.
   need  XEBUN
   uses  XRX45USE
end
begin
   type XRX45FILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  XRX45USE;XRX45FILE
   file  L13PXE40
   uses  FAA025LAA,FAA050LAA,FAA100LAA,FAC033LAA,FAC066LAA,FAJ033LAA
   uses  FAJ066LAA,FAI025LAA,FAI050LAA,FAI100LAA
end
begin
   type XEBUN
   dprompt Select a Xerox 4045 printer option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  XEB1;XEBUN
   device Resident USA
   file  XE40B1.PBD
   id    150,150,300,300
   desc  Select this option if you
   desc  want to use a US Xerox 4045
   desc  with Titan10 & XCP14
   desc  resident fonts.
end
begin
   name  XEB2;XEBUN
   device Resident EUR
   file  XE40B2.PBD
   id    150,150,300,300
   desc  Select this option if you
   desc  want to use a European 
   desc  Xerox 4045 with Titan12
   desc  & XCP12.5 resident fonts
   desc  or US Xerox 4045 with soft
   desc  fonts. See the Xerox printer
   desc  documentation for details.
end
begin
   name  GENERIC;Printer
   file  L13PCOMN
   mfgr  Generic
   device  Generic Printer
   desc  This selection supports 
   desc  printers whose manufacturer
   desc  was not listed on the 
   desc  previous screen. This 
   desc  selection lets you print
   desc  text but not graphs.
   mneed  GENBUND
   uses  GENUSE
end
begin
   type GENFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  GENUSE;GENFILE
   file  L13PGC
end
begin
   type GENBUND
   dprompt Select a Generic Printer option:
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  NBCKBUND;GENBUND
   device No Backspacing Capability
   file  GC__NOBS.PBD
   desc  Select this option if your
   desc  printer is NOT capable of
   desc  backspacing.
end
begin
   name  BCKBUND;GENBUND
   device Backspacing Capability
   file  GC__BS.PBD
   desc  Select this option if
   desc  your printer is capable
   desc  of backspacing.
end
begin
   type NULBUND
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  NUL;NULBUND
   file  NUL
end
begin
   type PLRIFILE
   dprompt Select an Print Link RI file
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  DRRI;PLRIFILE
   file  DR123TXT.RI
end
begin 
   type Country;Country
   dprompt Select a collating sequence:
   mincnt 1
   maxcnt 1
end
begin
   name  CNTRY1;Country
   file  L123USF
   device  Numbers First
   desc  Select this option if you
   desc  want 1-2-3 to sort numbers
   desc  before letters during a
   desc  Data Sort command.
   need  CNTRYBUND
end
begin
   name  CNTRY2;Country
   file  L123USL
   device  Numbers Last
   desc  Select this option if you
   desc  want 1-2-3 to sort numbers
   desc  after letters during a
   desc  Data Sort command.
   need  CNTRYBUND
end
begin
   name  CNTRY3;Country
   file  L123USA
   device  ASCII
   desc  Select this option if
   desc  you want 1-2-3 to sort
   desc  in ASCII order.
   need  CNTRYBUND
end
begin
   type CNTRYBUND
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  CNTRYNUL;CNTRYBUND
   file  NUL
end
begin 
   type PRT_850
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  CONV850;PRT_850
   file  L13PPTF
   device  850 Converter
   need  NULBUND
end
begin 
   type PRT_PIC
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  PIC;PRT_PIC
   file  L13FPIC
   device  Pic
   need  PICBUND
end
begin
   type PICBUND
   dprompt Select an Pic feature
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  PICFILE;PICBUND
   file  L13FPIC.FBD
end
begin 
   type PRT_META
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  META;PRT_META
   file  L13FMETA
   device  Metafile
   need  METABUND
end
begin
   type METABUND
   dprompt Select an Meta feature
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  METAFILE;METABUND
   file  L13FMETA.FBD
end
begin 
   type PRINT_LINK
   dprompt Select your printer communications option:
   nselect
   mincnt 1
   maxcnt 16
end
begin
   name PAR1;PRINT_LINK
   file L13LPLNK
   device Parallel
   need PAR1BUND
   uses DRRI
end
begin
   type PAR1BUND
   dprompt Select a bundle:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name PAR1BUN;PAR1BUND
   file LNKLPT1.LBD
   device 1
   uses DRRI
end
begin
   name SER1;PRINT_LINK
   file L13LSLNK
   device Serial
   need SER1BUND
   uses DRRI
end
begin
   type SER1BUND
   dprompt Select a bundle:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name SER1BUN;SER1BUND
   file LNKCOM1.LBD
   device 1
   uses DRRI
end
begin
   name PAR2;PRINT_LINK
   file L13LPLNK
   device Parallel
   need PAR2BUND
   uses DRRI
end
begin
   type PAR2BUND
   dprompt Select a bundle:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name PAR2BUN;PAR2BUND
   file LNKLPT2.LBD
   device 2
   uses DRRI
end
begin
   name SER2;PRINT_LINK
   file L13LSLNK
   device Serial
   need SER2BUND
   uses DRRI
end
begin
   type SER2BUND
   dprompt Select a bundle:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name SER2BUN;SER2BUND
   file LNKCOM2.LBD
   device 2
   uses DRRI
end
begin
   name DOSDEV;PRINT_LINK
   file L13LDLNK
   device Output Device
   need DOSDEVICE
   uses DRRI
end
begin 
   type DOSDEVICE
   dprompt Select the DOS Device you wish to use:
   nselect
   mincnt 1
   maxcnt 5
end
begin
   name DOS1;DOSDEVICE
   file LNKLPT1.LBD
   device LPT1
   uses DRRI
end
begin
   name DOS2;DOSDEVICE
   file LNKLPT2.LBD
   device LPT2
   uses DRRI
end
begin
   name DOS3;DOSDEVICE
   file LNKLPT3.LBD
   device LPT3
   uses DRRI
end
begin
   name COM1;DOSDEVICE
   file LNKCOM1.LBD
   device COM1
   uses DRRI
end
begin
   name COM2;DOSDEVICE
   file LNKCOM2.LBD
   device COM2
   uses DRRI
end
begin 
   type KEYBOARD
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  KEYBRD;KEYBOARD
   file  LTSKIBM
   device  Keyboard
   need  NULBUND
end
begin 
   type SOFTFLT
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  SOFT;SOFTFLT
   file  LTSSFP
   device  Software Floating Point
   need  NULBUND
end
begin 
   type NW
   dprompt Select a required driver:
   nselect
   mincnt 1
   maxcnt 1
end
begin
   name  NETWORK;NW
   file  LTSNW
   device  Network
   need  NULBUND
end
begin
   type FNT1
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC021LAA;FNT1
   file BC021LAA.LRF
end
begin
   type FNT2
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC042LAA;FNT2
   file BC042LAA.LRF
end
begin
   type FNT3
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBO019LAA;FNT3
   file BO019LAA.LRF
end
begin
   type FNT4
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC010LBA;FNT4
   file BC010LBA.LRF
end
begin
   type FNT5
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC018LBA;FNT5
   file BC018LBA.LRF
end
begin
   type FNT6
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC036LBA;FNT6
   file BC036LBA.LRF
end
begin
   type FNT7
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBO016LBA;FNT7
   file BO016LBA.LRF
end
begin
   type FNT8
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC016LCA;FNT8
   file BC016LCA.LRF
end
begin
   type FNT9
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC031LCA;FNT9
   file BC031LCA.LRF
end
begin
   type FNT10
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBO014LCA;FNT10
   file BO014LCA.LRF
end
begin
   type FNT11
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC016LDA;FNT11
   file BC016LDA.LRF
end
begin
   type FNT12
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC031LDA;FNT12
   file BC031LDA.LRF
end
begin
   type FNT13
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBO008LDA;FNT13
   file BO008LDA.LRF
end
begin
   type FNT14
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA012LAA;FNT14
   file AA012LAA.LRF
end
begin
   type FNT15
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA017LAA;FNT15
   file AA017LAA.LRF
end
begin
   type FNT16
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA025LAA;FNT16
   file AA025LAA.LRF
end
begin
   type FNT17
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA030LAA;FNT17
   file AA030LAA.LRF
end
begin
   type FNT18
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA033LAA;FNT18
   file AA033LAA.LRF
end
begin
   type FNT19
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA050LAA;FNT19
   file AA050LAA.LRF
end
begin
   type FNT20
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA060LAA;FNT20
   file AA060LAA.LRF
end
begin
   type FNT21
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA100LAA;FNT21
   file AA100LAA.LRF
end
begin
   type FNT22
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC017LAA;FNT22
   file AC017LAA.LRF
end
begin
   type FNT23
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC022LAA;FNT23
   file AC022LAA.LRF
end
begin
   type FNT24
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC033LAA;FNT24
   file AC033LAA.LRF
end
begin
   type FNT25
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC040LAA;FNT25
   file AC040LAA.LRF
end
begin
   type FNT26
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC066LAA;FNT26
   file AC066LAA.LRF
end
begin
   type FNT27
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ017LAA;FNT27
   file AJ017LAA.LRF
end
begin
   type FNT28
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ022LAA;FNT28
   file AJ022LAA.LRF
end
begin
   type FNT29
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ033LAA;FNT29
   file AJ033LAA.LRF
end
begin
   type FNT30
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ040LAA;FNT30
   file AJ040LAA.LRF
end
begin
   type FNT31
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ066LAA;FNT31
   file AJ066LAA.LRF
end
begin
   type FNT32
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI012LAA;FNT32
   file AI012LAA.LRF
end
begin
   type FNT33
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI017LAA;FNT33
   file AI017LAA.LRF
end
begin
   type FNT34
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI025LAA;FNT34
   file AI025LAA.LRF
end
begin
   type FNT35
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI030LAA;FNT35
   file AI030LAA.LRF
end
begin
   type FNT36
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI033LAA;FNT36
   file AI033LAA.LRF
end
begin
   type FNT37
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI050LAA;FNT37
   file AI050LAA.LRF
end
begin
   type FNT38
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI060LAA;FNT38
   file AI060LAA.LRF
end
begin
   type FNT39
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI100LAA;FNT39
   file AI100LAA.LRF
end
begin
   type FNT40
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA012LFA;FNT40
   file AA012LFA.LRF
end
begin
   type FNT41
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA024LFA;FNT41
   file AA024LFA.LRF
end
begin
   type FNT42
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC016LFA;FNT42
   file AC016LFA.LRF
end
begin
   type FNT43
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI012LFA;FNT43
   file AI012LFA.LRF
end
begin
   type FNT44
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI024LFA;FNT44
   file AI024LFA.LRF
end
begin
   type FNT45
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ016LFA;FNT45
   file AJ016LFA.LRF
end
begin
   type FNT46
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA030LGA;FNT46
   file AA030LGA.LRF
end
begin
   type FNT47
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA060LGA;FNT47
   file AA060LGA.LRF
end
begin
   type FNT48
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC040LGA;FNT48
   file AC040LGA.LRF
end
begin
   type FNT49
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI030LGA;FNT49
   file AI030LGA.LRF
end
begin
   type FNT50
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI060LGA;FNT50
   file AI060LGA.LRF
end
begin
   type FNT51
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ040LGA;FNT51
   file AJ040LGA.LRF
end
begin
   type FNT52
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA012LHA;FNT52
   file AA012LHA.LRF
end
begin
   type FNT53
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA024LHA;FNT53
   file AA024LHA.LRF
end
begin
   type FNT54
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC016LHA;FNT54
   file AC016LHA.LRF
end
begin
   type FNT55
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI012LHA;FNT55
   file AI012LHA.LRF
end
begin
   type FNT56
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI024LHA;FNT56
   file AI024LHA.LRF
end
begin
   type FNT57
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ016LHA;FNT57
   file AJ016LHA.LRF
end
begin
   type FNT58
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA017LIA;FNT58
   file AA017LIA.LRF
end
begin
   type FNT59
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAA033LIA;FNT59
   file AA033LIA.LRF
end
begin
   type FNT60
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAC022LIA;FNT60
   file AC022LIA.LRF
end
begin
   type FNT61
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAJ022LIA;FNT61
   file AJ022LIA.LRF
end
begin
   type FNT62
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI017LIA;FNT62
   file AI017LIA.LRF
end
begin
   type FNT63
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FAI033LIA;FNT63
   file AI033LIA.LRF
end
begin
   type FNT64
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC008LBA;FNT64
   file BC008LBA.LRF
end
begin
   type FNT65
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC014LDA;FNT65
   file BC014LDA.LRF
end
begin
   type FNT66
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FBC016LBA;FNT66
   file BC016LBA.LRF
end
begin
   type FNT67
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FCOMROM;FNT67
   file COMROM.LVF
end
begin
   type FNT68
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FCOMITA;FNT68
   file COMITA.LVF
end
begin
   type FNT69
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FSIMROM;FNT69
   file SIMROM.LVF
end
begin
   type FNT70
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FDUPROM;FNT70
   file DUPROM.LVF
end
begin
   type FNT71
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FTRIROM;FNT71
   file TRIROM.LVF
end
begin
   type FNT72
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name FTRIITA;FNT72
   file TRIITA.LVF
end
begin
   type  FNT74
   nselect
   mincnt 0
   maxcnt 1
end
begin
   name  PCL5WID;FNT74
   file  PCL5.WID
end
;-------------------------------------------------------------------------
;	Canon BJ-Series ALL printers - SOFT fonts - in Proprinter mode
;-------------------------------------------------------------------------
begin
   type CBJPFONT
   dprompt
   nselect
   mincnt 0
   maxcnt 50
end
begin
   name AI060LAA;CBJPFONT
   file AI060LAA.LRF
end
begin
   name AI120LAA;CBJPFONT
   file AI120LAA.LRF
end
begin
   name AJ080LAA;CBJPFONT
   file AJ080LAA.LRF
end
begin
   name AA060LAA;CBJPFONT
   file AA060LAA.LRF
end
begin
   name AA120LAA;CBJPFONT
   file AA120LAA.LRF
end
begin
   name AC080LAA;CBJPFONT
   file AC080LAA.LRF
end
;COMMON DRIVER DDL'S
begin
   type BPPCMFIL
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PIBPP;BPPCMFIL
   file  L13PIBPP
end
begin
   type PEPCMFIL
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PEPLQ;PEPCMFIL
   file  L13PEPLQ
end
begin
   type MXFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  EPSONMXUSE;MXFILE
   file  L13PEPDT
   uses  FAA012LFA,FAA024LFA,FAC016LFA,FAI024LFA,FAJ016LFA
end
begin
   type  PHPCMFIL
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PHPDJ;PHPCMFIL
   file  L13PHPDJ
end
begin
   type PIBCMFIL
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PIBQ2;PIBCMFIL
   file  L13PIBQ2
end
begin
   type HPFILE2
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  HPUSE2;HPFILE2
   file  L13PHPLJ
end
begin
   type HP2PFIL
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PHPLP;HP2PFIL
   file  L13PHPLP
end
begin
   type POKCMFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13POK84;POKCMFILE
   file  L13POK84
end
begin
   type HP3PAMFILE
   nselect
   mincnt 0
   maxcnt 16
end
begin
   name  L13PHPL3;HP3PAMFILE
   file  L13PHPL3
end




