
    Release Notes for PowerMeter v2.02 - May 01, 1995
    ___________________________________________________________

    The version number has been updated to 2.02.
    
    Support for Pentium Machines has now been implemented.

    Support for Machines up to 100 mhz. now fully supported.

    The database has not been changed, still using format 1.5.

    Displays rated (standard) CPU speeds if measured within +/- 2%.
    (e.g, A 486/33 measured at 32.98MHz would display 33.00MHz)

    Corrects "divide by zero" errors during tests.

    Corrected problem with Help Files 

    ---------------------------------------------------------------------
    Revision History
    
    Version 1.81

    The version number has been updated to 1.81.

    The database has not been changed, still using format 1.5.

    For calculation of MIPs, the manifest constant 'VAX_DHRYSTONE' was 
    changed to 1757 (per Intel document order # 240734-001 release 1.0 
    Feb 1990). [This effective with version 1.8. We receive a lot of 
    questions about this issue and results versus Version 1.7. Power 
    Meter Version 1.8 and up are correct. This pertains to 80386 and 
    higher processors.]

    Mouse support was added.

    Displays rated (standard) CPU speeds if measured within +/- 2%.
    (e.g, A 386/33 measured at 32.98MHz would display 33.00MHz)

    Now shows warning message and exits if running from a write 
    protected diskette.

    Corrects "divide by zero" errors during SYSTEM and BATTERY tests.

    The file I/O tests no longer display 'Insufficient Disk Space' on 
    large drives (MR ??).

    Floppy drives now show as 360KB / 720KB  (MR B011)

    Fixed drives now show as integer values and drive size is within one 
    cylinder of size shown by "FE".  (MR B011)

    Corrected problem with Visual Quality Tests - mode 0 (MR B007)

    Corrected problem when exitting to DOS & changing directory
        (MR B012 & MR B035)

    Corrected problem with Help Files (MR B017)

    ---------------------------------------------------------------------

    NOTE For Generating GRAPHS:

    In utilities, generation of comma-separated-value (CSV) file was 
    corrected.  The CSV file contains the following fields:

            "SYSTEM ID"
            "CPU"
            "NPU"
            "MHz"
            "SysTest PMUs"  - aggregate system test on DRIVE C ONLY
            "CPUTest PMUs"  - aggregate CPU test
            "DiskTest PMUs" - aggregate disk test on DRIVE C ONLY
            "VideoTest PMUs"- aggregate video test
                
    Output file no longer contains leading spaces and numeric values 
    only contain one digit after the radix (eg. 317.2).  Additionally, 
    in CSV file, if any of the aggregate tests was NOT run, a '*' 
    character precedes the title else a SPACE (' ') precedes the title.

    *** END of PMREAD.ME ***
