DOS/32 Advanced DOS Extender - Programmer's Reference 3.49 - DOS function 0FF91h - DOS/32 Advanced Allocate High Memory Block
In: | AX = 0FF91h EBX = size of memory block in bytes
Out: | if successful: CF clear EBX = linear address of allocated memory block ESI = handle of allocated memory block if failed: CF set
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. b) This function is equal to DPMI function 0501h except that it uses 32-bit registers instead of 16:16-bit pair of registers. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.