DOS/32 Advanced DOS Extender - Programmer's Reference 2.41 - DPMI function 0702h - Mark Page as Demand Paging Candidate Notifies the DPMI host that a range of pages may be placed at the head of the page-out candidate list, forcing these pages to be replaced ahead of other pages even if the memory has been accessed recently. The contents of the pages will be preserved.
In: | AX = 0702h BX:CX = starting linear address of pages to mark as paging candidates SI:DI = size of region to mark (bytes)
Out: | if successful: CF clear if failed: CF set AX = error code 8025h - invalid linear address (range unallocated)
Notes: a) DOS/32 Advanced DPMI will perform no action on this function and will always return with carry flag clear. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.