DOS/32 Advanced DOS Extender - Programmer's Reference 3.56 - DOS function 0FF98h - DOS/32 Advanced Map Physical Memory
In: | AX = 0FF98h EBX = physical address of memory ESI = size of region to map
Out: | if successful: CF clear EBX = linear address that can be used to access physical memory if failed: CF set
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. b) This function is equivalent to DPMI function 0800h except that it uses 32-bit registers instead of 16:16-bit pair of registers. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.