DOS/32 Advanced DOS Extender - Programmer's Reference 3.09 - DOS function 34h - Get InDOS Flag Address
In: | AH = 34h
Out: | ES:EBX = address of InDOS flag
Notes: a) The selector returned in ES register will be zero selector, ie readable/writeable data selector with Base=0. This is an internal to DOS/32 Advanced selector which may NOT be freed or modified under any circumstances. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.