DOS/32 Advanced DOS Extender - Programmer's Reference 2.22 - DPMI function 0205h - Set Protected Mode Interrupt Vector Sets the address of protected mode handler for the specified interrupt into the interrupt vector.
In: | AX = 0205h BL = interrupt number CX:EDX = selector:offset of exception handler
Out: | if successful: CF clear if failed: CF set AX = error code 8022h - invalid selector
Notes: a) The value passed in CX should be a valid protected mode code selector, not a real mode segment address. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.