DOS/32 Advanced DOS Extender - Programmer's Reference 5.02 - Mouse function 000Ch - Define Interrupt Subroutine Parameters
In: | AX = 000Ch ECX = call mask ES:EDX = far pointer to interrupt routine
Out: | -
Notes: a) This function will use a real mode callback that was allocated by the DOS/32 Advanced at startup to pass the control from real mode mouse handler to your protected mode interrupt handler. b) Calling this function with zero values in ES:EDX (0000:00000000h) will uninstall your protected mode interrupt handler. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.