DOS/32 Advanced DOS Extender - Programmer's Reference 2.58 - API function 05h - Get Access to Protected Mode Virtual Stacks
In: | AL = 05h
Out: | BX = writeable data selector ECX = size of one protected mode virtual stack EDX = pointer to the current top of protected mode virtual stack ESI = pointer to base of protected mode virtual stacks
Notes: a) Selector returned in BX is a writeable data selector that should be used to access needed variables/addresses. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.