DOS/32 Advanced DOS Extender - Programmer's Reference 3.46 - DOS function 0FF89h - DOS/32 Advanced Get Configuration Info
In: | AX = 0FF89h
Out: | EAX = 49443332h ('ID32') (if the function is supported) EBX = DOS/32 Advanced version number ECX = DOS/32 Advanced Low Buffer size (in bytes) EDX = DOS/32 Advanced Configuration bits ESI = pointer to DOS/32 Advanced Configuration Header "ID32" FS = selector that can be used to access Configuration Header "ID32"
Notes: a) This call is specific to DOS/32 Advanced DOS Extender only, and is not supported by standard DOS. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.