DOS/32 Advanced DOS Extender - Programmer's Reference 2.55 - API function 02h - Get Access to Internal Interrupt Buffers
In: | AL = 02h
Out: | BX = writeable data selector ESI = pointer to interrupt switches EDI = pointer to 1-st interrupt buffer
Notes: a) Selector returned in BX is a writeable data selector that should be used to access needed variables/addresses. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.