DOS/32 Advanced DOS Extender - Programmer's Reference 3.06 - DOS function 25h - Set Interrupt Vector
In: | AH = 25h AL = INT vector DS:EDX = selector:offset of interrupt handler
Out: | if successful: CF clear if failed: CF set
Notes: a) This function sets a protected mode interrupt vector and is equivalent to DPMI function 0205h. b) This function will indicate an error (set carry flag) if the selector passed in DS was an invalid selector. Copyright © Supernar Systems, Ltd. 1996-2002 All Rights Reserved.