MWSUPPRT.TXT    17-Oct-95

                METAWINDOW VERSION 5 SUPPORTED VIDEO ADAPTERS

                       Metagraphics Software Corporation
- - - Advanced Graphic Programming Tools For DOS and DOS Protected-Mode - - -


The following is a partial list of the graphics cards and display modes
supported by MetaWINDOW.  We pride ourselves in supporting virtually every
popular graphics adpater on the market.  If your card is not on this list, 
please call and check with us.  Chances are we support it already, or will
soon have it available.  Please let us know if you have any questions
or comments (email: sales@metagraphics.com).


  LEGEND:  o  Supported in all MetaWINDOW products.
           *  32/65K-color supported with MetHICOLOR.
           !  Hardware acceleration supported with MetACCEL.
     !!NEW!!  New adaptor support with MetaWINDOW V5.

Alphebetic listings by graphic card vendor:

-------------------------------------
ACTIX SYSTEMS INC.
3060 Tasman Drive
Santa Clara, CA 95054
U.S.A
Phone: 408-986-1625
Fax: 408-986-1646

  Actix GE32+ (S3 801/805, ISA/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
ADEX

  Adex, 8514A
    !  256-color 8514A: 1024x768

-------------------------------------
ADT

  ADT, AcuView 8514/A Plus
    !  256-color 8514: 640x480, 800x600, 1024x768

-------------------------------------
AHEAD SYSTEMS

  Ahead, V-500B
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

  Ahead, VGA Wizard
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32k-color SVGA: 640x480

-------------------------------------
ATI TECHNOLOGIES INC.
33 Commerce Valley Drive East
Thornhill, Ontario L3T 7N6
Canada
Phone: 905-882-2600
Fax: 905-882-2620
BBS: 905-764-9404
Email: sales@atitech.ca
Web: http://www.atitech.ca
Ftp: ftp://ftp.atitech.ca/pub/support
CompuServe: GO ATI, LIB 17

  ATI, VGA Wonder XL24 (ATI 18800/28800; VESA Bios TSR: vv222.zip)
  ATI, VGA Wonder XL
  ATI, VGA Wonder Plus
  ATI, VGA Integra
  ATI, VGA Wonder
    o  Standard VGA modes
    o  16-color  SVGA: 800x600
    o  256-color SVGA: 640x480, 800x600, 1024x768

  ATI, Graphics Ultra (ATI Mach 8; VESA Bios TSR: vv222.zip)
  ATI, Graphics Vantage
  ATI, 8514-Ultra
  ATI, VGA-Wonder GT
    o  Standard VGA modes
    o  16-color  SVGA: 800x600
    o  256-color SVGA: 640x480, 800x600, 1024x768
    !  256-color Mach8: 640x480, 800x600, 1024x768

  ATI, Graphics Wonder (ATI Mach32; ISA/VLB; VESA Bios TSR: vv222.zip)
  ATI, Graphics Ultra Plus
  ATI, Graphics Ultra Pro
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768, 1280x1024
    o  256-color Mach32: 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600

  ATI, Graphics Pro Turbo (ATI Mach64; ISA/PCI/VLB; VESA Bios TSR: 64vbe101.zip)
  ATI, Graphics Xpression
  ATI, Winturbo
  ATI, Winboost
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
BOCA RESEARCH
6413 Congress Avenue
Boca Raton, FL  33487
Phone: 407-997-6227
Fax: 407-997-0918
BBS: 407-241-1601
Email: 75300.2672@compuserve.com
CompuServe: 75300,2672 -or- GO BOCA (Lib 2)


  Boca, SuperVGA (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
CARDINAL TECHNOLOGIES
1827 Freedom Road
Lancaster, PA 17601
Phone: 717-293-3000
Fax: 717-293-3104
FaxBack: 800-775-0899

  Cardinal, SnapPlus (ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  65k-color SVGA: 640x480, 800x600

  Cardinal, 400
  Cardinal, 500
  Cardinal, 600
  Cardinal, 700
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32k-color SVGA: 640x480

  Cardinal, VideoSpectrum (Cirrus GD5426/GD5428; ISA/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600

  Cardinal, WarpSpeed (Weitek P9000)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
CHIPS & TECHNOLOGIES
3050 Zanker Road
San Jose, CA 95134
Phone: 408-434-0600
Fax: 408-434-9315

  Chips & Technologies, 82c45x (ISA)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x350, 640x480

-------------------------------------
CIRRUS LOGIC
3100 West Warren Avenue
Fremont, CA 94538
Phone: 510-252-6000
Fax: 510-252-6070
BBS: 510-440-9080
CompuServe: GO CIRRUS (Lib 18)

  Cirrus Logic, 5422 (ISA)
  Cirrus Logic, 5428 (VLB)
  Cirrus Logic, 5226 (VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x350, 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600 (2Mb)

-------------------------------------
COMPAQ COMPUTER CORPORATION

  Compaq, Advanced VGA
    o  Standard VGA modes
    o  16-color  SVGA: 800x600
    o  256-color SVGA: 640x350, 640x480

  Compaq, Portable
  Compaq, Portable III (plasma)
    o  Standard CGA modes
    o  2-color: 640x400 (III)

  Compaq, QVision 
    o  16-color  SVGA: 800x600
    o  256-color SVGA: 640x350, 640x480

  Compaq, QVision 1280 (Compaq V32; EISA/ISA)
  Compaq, QVision 1280/P+ (Compaq V64; PCI)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x350, 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600 (2Mb)

  Compaq, QVision 2000 (Matrox MGA II; PCI)
  Compaq, QVision 2000+ (Matrox MGA II; PCI)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x350, 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
COMPUADD

  CompuAdd, Hi-Res VGA (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
DEFINICON

  Definicon, HiRes 1024 (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
DIAMOND MULTIMEDIA INC.
2880 Junction Avenue
San Jose, CA  95134
Phone: 408-325-7000
Fax: 408-325-7070
BBS: 408-325-7175
AOL: DIAMOND
CompuServe:  GO DMNDONLINE
Email: sales4u@diamondmm.com
Web: http://www.diamondmm.com
Ftp: ftp://ftp.diamondmm.com/pub

  Diamond, Speedstar (Tseng ET4000)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480

  Diamond, Speedstar Pro (Cirrus GD5426; ISA; VESA Bios TSR: cl542x.zip)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600

  Diamond, Speedstar Pro SE
  (Cirrus GD5430; PCI/VLB; VESA Bios TSR: cl542x.zip)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

  Diamond, Stealth (S3 924, ISA)
  Diamond, Stealth Pro (S3 968)
  Diamond, Stealth 24 (S3 805, VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

!!NEW!!
  Diamond, Stealth SE (S3 Trio32; PCI/VLB; VESA Bios TSR: ROM )
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

!!NEW!!
  Diamond, Stealth64 DRAM (S3 Vision864; PCI/VLB; VESA Bios TSR: ROM)
!!NEW!!
  Diamond, Stealth64 VRAM (S3 Vision964; PCI/VLB; VESA Bios TSR: ROM)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768 (1280x1024 VRAM)

  Diamond, Stealth64 Graphics 2001 (ARK 2000PV; PCI; VESA Bios TSR: ROM)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

!!NEW!!
  Diamond, Stealth64 Video (S3 Vision968; PCI/VLB; VESA Bios TSR: ROM)
!!NEW!!
  Diamond, Stealth64 Video 3200 (S3 Vision968; PCI/VLB; VESA Bios TSR: ROM)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

  Diamond, Viper (Weitek P9000; PCI/VLB; VESA Bios TSR: wdvesa.zip)
  Diamond, Viper SE (Weitek P9001; PCI/VLB; VESA Bios TSR: wdvesa.zip)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
DIGITAL EQUIPMENT CORPORATION

!!NEW!!
  DEC, Venturis (S3 Trio32; PCI/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
EIZO

  Eizo, BD-B07 (ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600

  Eizo, MD-B10 (ET3000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

-------------------------------------
EVEREX MICROSYSTEMS
48431 Milmont Drive
Fremont, CA 94538
Phone: 415-683-2230


  Everex, 623 Viewpoint VRAM (ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600

  Everex, 678 Viewpoint (ET3000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

  Everex, EV625 (ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
FORESIGHT DESIGN

  Foresight, VGA-16 (ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
GENOA 
75 East Trimble Road
San Jose, CA 95131
Phone: 408-432-9123
Fax: 408-432-0997
BBS: 408-943-1231
Email: 71333.3543@compuserve.com
CompuServe: 71333,3543 -or- GO GENOA (Lib 9)

  Genoa, SuperVGA 5000 (ISA)
  Genoa, SuperVGA 6000 (ISA)
  Genoa, SuperVGA 7900 Multimedia (ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

  Genoa, 8000 (S3 928; ISA)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
HEADLAND 

  See Video Seven

-------------------------------------
HERCULES COMPUTER TECHNOLOGY
3839 Spinnaker Court
Fremont, CA 94538
Phone: 510-623-6050
Fax: 510-623-1112
BBS: 510-623-7449
Email: 71333.2532@compuserve.com
CompuServe: 71333,2532 -or- GO HERCULES (Lib 8)

  Hercules Graphics Card (HGC)
    o  2-color: 720x348

-------------------------------------
HEWLETT PACKARD

  Hewlett Packard, Ultra VGA (S3 928)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
IBM

  IBM, CGA
    o  2-color:  640x200

  IBM, EGA
    o  2-color:  640x200, 640x350
    o  16-color: 320x200, 640x200, 640x350

  IBM, VGA
    o  2-color:   640x200, 640x350
    o  16-color:  320x200, 640x200, 640x350, 640x480
    o  256-color: 320x200

  IBM, 8514/A
    !  256-color 8514A: 1024x768

  IBM, XGA
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
IPS

  IPS, Overview 1024
    !  256-color 8514: 640x480, 800x600, 1024x768

-------------------------------------
MATROX GRAPHICS INC.
1025 St. Regis Boulevard
Doeval, Quebec H9P 2T4
Canada
Phone: 514-969-6330
Fax: 514-969-6363
FaxBack: 514-685-0174
Email: 72662.1164@compuserve.com
CompuServe: 72662,1164 -or- GO MATROX (Lib 16)

  Matrox, Impression Plus
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

  Matrox, Magnum
  Matrox, 8514 Xtra
    !  256-color 8514A: 640x480, 800x600, 1024x768

  Matrox, MGA Impression (MGA; ISA/PCI)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

  Matrox, MGA Millennium (MGA-2064W; PCI)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
MAXIM

  Maxim, 8514
    !  256-color 8514A: 1024x768

-------------------------------------
MICRONICS 

  See Orchid Technology

-------------------------------------
NATIONAL DESIGN INC.

  NDI, AT600 (S3 968)
  NDI, Warp 10 (S3 968)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
NUMBER NINE VISUAL TECHNOLOGY
18 Hartwell Avenue
Lexington, MA 02173
Phone: 408-325-7000
Fax: 408-325-7070
BBS: 408-325-7175
Email: sales@nine.com
Web: http://www.nine.com
Ftp: ftp://ftp.nine.com/pub

  Number Nine, Imagine 128 (#9 Imagine128; PCI)
  Number Nine, Imagine 128 Pro (#9 Imagine128; PCI)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

!!NEW!!
  Number Nine, 9FX Motion 771 (S3 Vision968; PCI/VLB)
!!NEW!!
  Number Nine, 9FX Motion 531 (S3 Vision968; PCI/VLB)
!!NEW!!
  Number Nine, 9FX Motion 330 (S3 Trio64; PCI/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
OAK TECHNOLOGY INC.

  Oak, OTI-037
  Oak, OTI-067
  Oak, OTI-077
  Oak, OTI-087
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480

-------------------------------------
ORCHID TECHNOLOGY
232 Warren Avenue
Fremont, CA 94539
Phone: 510-683-0300
Fax: 510-490-9312
BBS: 510-683-0327
FaxBack: 510-661-3199
CompuServe: GO ORCHID

  Orchid, Fahrenheit 1280 (S3 928; ISA)
  Orchid, Fahrenheit 1280 Plus (S3 801/805; ISA/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

!!NEW!!
  Orchid, Fahrenheit 64 (S3 Vision864; PCI/VLB; VESA: ROM Bios)
!!NEW!!
  Orchid, Fahrenheit Pro64 (S3 Vision964; PCI/VLB; VESA: ROM Bios)
!!NEW!!
  Orchid, Fahrenheit ProVideo64 (S3 Vision968; PCI/VLB; VESA: ROM Bios)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024 (4Mb)

  Orchid, Kelvin 64 (Cirrus 5434; ISA/PCI/VLB)
  Orchid, Kelvin EZ (Cirrus 5430; ISA/PCI/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024 (2Mb)
    *  65K-color VESA: 640x480, 800x600, 1024x768 (2Mb)

  Orchid, Designer (Tseng ET3000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

  Orchid, ProDesigner II (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
PARADISE (Western Digital)
800 East Middlefield Road
Mountain View, CA 94943
Phone: 415-960-3360
Fax: 415-968-1974

  Paradise, VGA (PVGA1A; ISA)
  Paradise, VGA Plus (PVGA1A; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600

  Paradise, VGA 1024 (ISA)
  Paradise, VGA Professional (ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600
    o  256-color SVGA: 640x480

  Paradise, 8514A Plus (ISA)
    !  256-color 8514A: 1024x768

  Paradise, Windows Accelerator (WD90C31; ISA/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
PHOTON

  Photon, Viper (8514; ISA)
    o  Standard VGA modes
    !  256-color 8514: 640x480, 800x600, 1024x768

  Photon, XV 70/70 DLX (S3; ISA)
    o  Standard VGA modes
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
PIXELWORKS

  Pixelworks, WhirlWIN (8514; ISA)
    o  Standard VGA modes
    !  256-color 8514: 640x480, 800x600, 1024x768

-------------------------------------
PRIAM

  Priam, VGA Eclipse (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
RADIUS INC.
215 Moffet Park Drive
Sunnyvale, CA 94089
Phone: 408-541-6100
Fax: 408-541-6190
Email: 76004.2155@compuserve.com
CompuServe: 76004,2155 -or- GO RADIUS

  Radius, Multiview (ISA)
    o  Standard VGA modes
    o  2-color: 1024x768
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768

-------------------------------------
S3 INCORPORATED
2880 San Tomas Expwy
Santa Clara, CA 95051-0981
Phone: 408-980-5400
Fax: 408-980-5444
BBS: 408-654-5676
Email: sales@s3.com

  S3, 86C801
  S3, 86C805
  S3, 86C928
  S3, 86C911
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600, 1024x768

!!NEW!!
  S3, Trio32
!!NEW!!
  S3, Trio64
!!NEW!!
  S3, Vision864
!!NEW!!
  S3, Vision868
!!NEW!!
  S3, Vision964
!!NEW!!
  S3, Vision968
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
SIGMA DESIGNS
47900 Bayside Parkway
Fremont, CA 94538
Phone: 510-770-0100
Fax: 510-770-0110
CompuServe: GO SIGMA

  Sigma Designs, VGA Legend (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
SPEA
CompuServe: GO SPEA

!!NEW!!
  Spea, V7-Mercury (S3 928; ISA/PCI/VLB) 
!!NEW!!
  Spea, V7-Mercury Lite (S3 928; PCI) 
!!NEW!!
  Spea, V7-Mercury Pro (S3 928; ISA/VLB) 
!!NEW!!
  Spea, V7-Mercury P-64 (S3 Vision964; PCI/VLB) 
!!NEW!!
  Spea, V7-Mercury P-64 V (S3 Vision968; PCI/VLB) 
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

!!NEW!!
  Spea, V7-Mirage (S3 801/805; ISA/VLB) 
!!NEW!!
  Spea, V7-Mirage P-32 (S3 Trio32; PCI/VLB) 
!!NEW!!
  Spea, V7-Mirage P-64 (S3 Vision964; PCI/VLB) 
!!NEW!!
  Spea, V7-Mirage P-64 V (S3 Vision968; PCI/VLB) 
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

  Spea, V7-Vega (Cirrus CL542x; ISA/VLB)
  Spea, V7-Vega Pro (Trident 9440; PCI/VLB)
  Spea, V7-Vega Plus (Advance Logic ALG2228/2301; PCI/VLB)
  Spea, V7-Vega Video (Advance Logic ALG2302; PCI/VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

-------------------------------------
STB SYSTEMS, INC.
1651 North Glenville
Richardson, TX 75085
Phone: 214-234-8750
Fax: 214-234-1306
BBS: 214-437-9615
CompuServe:  75300,1664 -or- GO STBSYS
Email: sales@stb.com
Web: http://www.stb.com
Ftp: ftp://ftp.stb.com

  STB, Horizon (Cirrus 542X; ISA/VLB; VESA Bios TSR: CL542x.zip)
  STB, Horizon + (Cirrus 5430; ISA/PCI/VLB; VESA Bios TSR: CL542x.zip)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768

  STB, Lightspeed (Tseng W32P; VLB)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

  STB, Nitro 64 (Cirrus 5434; ISA/PCI; VESA Bios TSR: CL542x.zip)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024 (2Mb)
    *  65K-color VESA: 640x480, 800x600, 1024x768 (2Mb)

  STB, PowerGraph VGA (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

!!NEW!!
  STB, PowerGraph 64 (S3 Trio64; PCI/VLB) 
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768

!!NEW!!
  STB, Velocity 64V (S3 Vision968; PCI/VLB) 
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    !  256-color   S3: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

  STB, WIND/X (S3 86C928)
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768
    !  256-color   S3: 640x480, 800x600, 1024x768

-------------------------------------
SWAN

  Swan, SuperVGA (Tseng ET4000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
TECMAR

  Tecmar, VGA/AD (ET3000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

-------------------------------------
TOSHIBA

  Toshiba, 3100 Portable (WD90C30)
    o  Standard CGA modes
    o  2-color: 640x400

-------------------------------------
TRIDENT

  Trident, Impact SuperVGA (Trident 8900; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768

  Trident, 9000 SuperVGA (Trident 9000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768
    *  65K-color VESA: 640x480, 800x600

-------------------------------------
TSENG LABS

  Tseng Labs, ET3000 SuperVGA (Tseng ET3000; ISA)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480

  Tseng Labs, ET4000 SuperVGA (Tseng ET4000; ISA/VLB)
    o  Standard VGA modes
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x350, 640x480, 800x600, 1024x768
    *  32K-color SVGA: 640x480

-------------------------------------
VESA
2150 N First St, Suite 440
San Jose, CA 95131-2029
Phone: 408-435-0333
Fax: 408-435-8225

  VESA, SuperVGA
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  32K-color VESA: 640x480, 800x600, 1024x768, 1280x1024
    *  65K-color VESA: 640x480, 800x600, 1024x768, 1280x1024

-------------------------------------
VIDEO 7

  Video 7, VEGA VGA
    o  Standard VGA modes
    o  16-color  SVGA: 800x600

  Video 7, FastWrite
  Video 7, VRAM
  Video 7, 1024i
    o  Standard VGA modes
    o  2-color   SVGA: 1024x768
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480

  Video 7, VRAM II (HT209; ISA)
    o  Standard VGA modes
    o  2-color   SVGA: 1024x768
    o  16-color  SVGA: 800x600, 1024x768
    o  256-color SVGA: 640x480, 800x600, 1024x768

-------------------------------------
WESTERN DIGITAL
800 East Middlefield Road
Mountain View, CA 94043
Phone: 415-960-3360
Fax: 415-968-1974

  Western Digital, WD90c31
  Western Digital, WD90c33
    o  Standard VGA modes
    o  16-color  VESA: 800x600, 1024x768
    o  256-color VESA: 640x480, 800x600, 1024x768

  Western Digital, 8514A (ISA)
    !  256-color 8514A: 640x480, 800x600, 1024x768

-----------------------------------------------------------------------------

  ************************************************************************
  *  NOTICE - While we have attempted to be as accurate as possible in   *
  *  compiling the information contained in this document, Metagraphics  *
  *  disclaims responsibility for any inaccuracies, errors or omissions  *
  *  contained herein.  Metagraphics reserves the right to update these  *
  *  specifications at any time without notice.                          *
  ************************************************************************

Copyright (C) 1995 Metagraphics Software Corporation


FOR MORE INFORMATION -               Toll Free:        800-332-1550
                                     Phone:            408-622-8950
  METAGRAPHICS CORPORATION           Fax:              408-622-8955
  200 Clock Tower Place, Suite 201E  BBS:              408-622-8945
  PO Box 222235                      CompuServe Mail:  74774,221
  Carmel, CA 93923                   CompuServe Forum: GO METAGR (LIB 12)
  U.S.A.                             Internet:         sales@metagraphics.com
                                     Internet ftp:     ftp.metagraphics.com
                                 
  Metagraphics Internet Web Site:    http://www.metagraphics.com

A wealth of information on Metagraphics products, demonstrations and
sample programs is available via Metagraphics BBS at 408-622-8945, and
through Metagraphics Internet Web site at:

      http://www.metagraphics.com    (also:  ftp://ftp.metagraphics.com)

/* End of File - MWSUPPRT.TXT */

