To get 256 user crack and MajorTCP/IP v2.00-8 to work.

First, install Worldgroup 2.0.
Don't specify and activation code yet.
Drop to dos after installation.
Copy the GALGSBL.DLL file I gave you into your BBS directory.
Boot up the bbs again.

Second, activation code.
Use this activation code for your bbs: 97epewcyf

Third, disabling unneeded modules.
Choose option #7 on your bbs main menu.
Choose WGSDMOD, 4th line down, and disable the following modules:

Forms-to-file Web Add-on
ISP via SLIP/CSLIP/PPP
MHS Importer/Exporter
Rlogin Server
SMTP Services
TCP/IP for Worldgroup
Telnet Server
Web Forms to E-mail
World-Wide Web Server

Fourth, Hardware setup and MajorTCP/IP installation.
INSTALL TCP/IP PACK NOW!
Choose option #1 on your main bbs menu.
This is the hardware setup.
Make channel group #1 TELNET lines.
Starting channel # is 1 and # of channels make 16.
Leave channel group #2 through #15 <NONE>
Channel group 16 set this up for your modem
set starting channel # to FF
and # of channels to 1.
Go down to the bottom where the file TCPLIBM.MSG file starts.
Choose yes to the first question.
2nd question: PPP
3rd question: FF
4th question: your modem dialout string for your inet provider
5th question: YES
6th question: your username on your inet provider
7th question: your password on your inet provider
8th question: 1
9th question: connect
10th question: 0
11th question: 0.0.0.0
12th question: 1024
13th question: 0.0.0.0
14th question: 0.0.0.0
15th question: YES
16th question: 50
17th question: anything
18th question: anything.com
19th and on: leave them alone!!

Fifth, activation codes for MajorTCP/IP.
choose option #3 on main bbs menu.
find TCPLIBM.MSG.
Activation code is JVHHTKTB
incoming activation code is ZIR-YECK
thats it for this one.

Sixth, menu tree.
setup a few options on your menu tree.
On top menu create an internet menu.
on internet menu create telnet, rlogin, ftp, and slip server.
choose module telnet for telnet
choose module rlogin for rlogin
choose module ftp for ftp
choose module tcp/ip slip server for slip server

Seventh, boot up your bbs.
fire up the board and let it dial to your inet provider.. THIS SHOULD WORK.
try telnetting from your bbs.
look in your audit trail, this is where it tells you the ip that has been
assigned to you.
Try telnetting from your bbs to your bbs.
If this does NOT work or if i have left out something, contact me somehow!!
hehehhe.. have fun!



[4:09] <sextronix> [18:41] <`JJJ> <digger-> Sylvain Miller
[4:09] <sextronix> [18:41] <`JJJ> <digger->  3145 Coderre
[4:09] <sextronix> [18:41] <`JJJ> <digger->  St-Hubert, 
[4:09] <sextronix> [18:41] <`JJJ> <digger->  J3Y 4P1
[4:09] <sextronix> [18:41] <`JJJ> <digger->  [514] 443-5727
[4:09] <sextronix> [18:41] <`JJJ> <digger->  5258948752073161
[4:09] <sextronix> [18:41] <`JJJ> <digger->  07/98
