                          Paradise VESA 1.00 Driver

VESA.EXE is a TSR program that provides support for the VESA BIOS calls.
Type 'VESA' on the DOS command line before running an application using
a VESA compatible driver.

This VESA driver works to VESA spec. 1.00 on the following Paradise boards:

VGA+

VGA+16

VGA PROF.

VGA1024

This VESA program will determine the amount of video memory and the video
chip present (PVGA1A and 90C00). As a result will respond correctly for the
video modes supported by the board. If you don't have a VGA board with either
of these chips then don't use this program. The bios for the subsequent
chips have the VESA support so they don't require the VESA program.

Window B is disabled for this driver.  A future version will support 32k
windows when Window B is enabled.

The window granularity is 4K, so 64K Banks are 16 times 4K.

