
The design requirements of the A13 (Cruiser Tank) called for the A10 to have
additional armor placed on the hull and turret. With this, it still had
good speed and carried a 2lb gun. Most of these tanks were used in the
1940 France campaign and North Africa. While the armor was improved on the 
turret, the side and rear were weakened, to increase speed.


