VetUsers
Init Ail
Found DRIVER in dig.ini file
Found SB16.DIG
Chose snd card SB16.DIG
Switch on cardType is 2 SB16/AWE32
Switch on cardType is 3 SBLASTER
HALF DMA SIZE 2048
half DMA size 2048 
DMA latency 43.000000 
Sample rate 43900, Hardware rate 44100
Minimum sample buffer size = 16896 bytes
Min sample buffer size = 33792 bytes
Play the movie
SoundAvail=1 -> start frameCallback & SfxSndTrk
No problem  Exited
