PLATFORM TYPE:     TANGO CLASS LONG-RANGE SUBMARINES

SPEED:             18KTS DIVED
MANNING LEVEL:     70
DIMENSIONS:        300 x 29.5 x 23 FT
DISPLACEMENT:      3900 SUBMERGED
POWERPLANT:        3 DIESEL ENGINES 6,000 HP
                   3 ELECTRIC MOTORS 6,000 HP
DEPTH:             1,310 FT

MISSILES:          (ASW) SS-N-15

TORPEDO TUBES:     10  21 IN (533mm) 6 BOW + 4 STERN

RADARS:
    (SURFACE SRCH):    SNOOP TRAY (I-BAND)

COUNTERMEASURES:
    (ESM):             SQUID HEAD
                       BRICK PULP
                       QUAD LOOP (D/F-BANDS)

SONARS:                SHARK TEETH HULL-MOUNTED, PASSIVE/
                       ACTIVE SEARCH AND ATTACK
                       LARGE ARRAY MOUNTED ABOVE TORPEDO
                       TUBES; ALSO A BOW-MOUNTED DOME

COUNTRIES:             CIS
COMMENTS:              TANGO CLASS HAS LARGER INTERNAL HULL
                       CAPACITY THAN THE FOXTROT CLASS

 
