 Init. Strings for Many Common Modems
         Brought to you by:
            Frank Baris
======================================

Aceex Modem 1496
AT&Q0S46=136S48=128S36=1S37=9&K0\Q3

USR Sportster 14.4k.  
ATZ^M&M0&B0&K0&H0&N6S27=32S15=24

14.4k internal ZOOM faxMODEM VFP
ATZ^M&Q6S46=136S48=128S36=1S37=9N0&K0

Boca M1440i (internal):
ATS48=0S37=9S46=136%C0%E0%M0&K0&Q0&R1&C1&D2\G0\N1N0

Boca 14.4k (internal):
AT&C0N0S37=9&K0W0&Q0S36=3S48=128%C0

Boca 14.4 Fax/Modem
AT S46=0 S37=9 N0 &Q0 &D2 &K4

Boca 14.4k (external):
AT &F S0=1 S36=0 &K0 &Q6N0S37=9 &D2

Boca 14.4k:
AT S46=0 S37=9 N0 &Q0 &D2 &K0 %C0

Cardinal 14.4k v.32bis, v.42bis Fax/Modem:
AT &F N0 S37=9 &Q0 &D2 \N1

Digicom Systems (DSI) (softmodem):
AT Z \N0 &D2 &K0 S48=48

Digicom Systems Scout Plus:
ATZ*E0*N3*M0*S0*F0&D2

Gateway Telepath:
AT &F S37=9 %C0 &K0 &Q6 \G0

Gateway Telepath 14.4k:
AT S46=0 S37=9 N0 &Q0 &D2 &K0 %C0

Gateway Telepath I:
AT S0=1 &N6 &K0 &M0

Gateway Telepath II:
AT S0=1 S37=9 %C0 &Q0 &K0

Generic v.32bis 14.4k Fax/Modem:
AT \N0 %C0 B8

Generic 14.4k Fax/Modem:
AT S46=0 S37=9 N0 &Q0 &D2 %C0 \G0 &K0

GVC 14.4k (internal):
AT &F B8 \Q0

Hayes 28.8k V.FAST Modem:
AT &Q6 &K S37=9 N %C0 \N0

Infotel 144I:
AT&Q0 S37=9 N0 &D2

Infotel 14.4:
&F0 \N1 &D2 S37=F8

Intel 14.4k:
AT \N0 %C0 \Q0 B8

Intel 14.4k (internal):
AT Z B8 Q1 \C0 \N1 %C0 \V "H

Microcom AX:
&F \N1 \Q0 &D2

Microcom QX/4232bis:
AT %C0 \N0

Netcomm M7F:
AT &E &K0 B0 \V0 X4 &D2 \N1 \Q0 #J0 #Q9 %C0

Nokia ECM 4896M Trellis V.32:
AT Z %C0 /N0

Nuvotel IFX 14.4 (internal):
&F \N1 &D2 

Practical Peripherals 14400FX v.32bis:
AT Z S46=0 &Q0 &D2

Practical Peripherals 14400FX v.32bis:
AT S46=0 &Q0 &K0 &D2

Supra:
AT &F0 S46=136 %C0

Supra (external):
AT &K &Q &D \N1

Supra 14.4k v.32bis:
AT &F S46=136 &Q0 &D2

Supra 14.4k v.32bis:
AT &K &Q &D \N1

Telepath 14.4k:
AT &F&M0&K0&N6&H0 S0=1

Twincomm DFi 14.4:
AT&F &Q0 %C0 S37=9 &D2

UDS V.3223:
&F \N1 \Q &D2

UDS Fastalk 32BX:
&F0 \N1 &D2

USR Courier v.32bis:
ATS0=1 S7=60 E1 Q0 V1 &C1 &D2 &H0 &K0 &M0 &N6 &A3

USR Courier HST/DS 16.8k:
First reset the modem in a communication program with AT&F&W
AT X4 B0 &A0 &B0 &H2 &I0 &K0 &M0 &N6a

USR DS v.32bis v.42bis (external):
AT&m0&n6&a0&r1&h0&k0&i0&s0&b1x1

USR Sporster 9600:
AT&M0&K0&N6

USR Sportster 14.4k Fax/Modem USING ERROR CORRECTION:
AT S0=1 S7=60 E1 QO V1 &C1 &D2 &K0 &N6 &A3

USR Sportster 14.4k Fax/Modem (internal):
AT &F&M0&K0&N6&H0

USR Sportster 14.4k (internal):
AT &F &B1 &H0 &I0 &K0 &M0 &N6 &R1

USR Sportster 14.4k:
ATS0=1S7=60E1Q0V1&C1&D2&K0&N6&A3

USR Sportster 14.4k:
AT &F0 &K0 &M0 &N6 &H0 &I0 &B1 &R1

USR Sportster 14,000 Fax Modem:
AT S0=2 &N6 &K0 &M0 &I0 &H0 &R1 &A0 V1 X4

USR 14.4k:
AT &F&A0&K0&M0

USR 14.4k
AT &K0 &H0 &D0 &I0 &R1

USR 14.4k Dual Standard
ATB0&R1&B1&N6Q0X4&A0&D2&H0&I0&K0&M0M1

USR (model?):
&F E1 V1 X4 &C1 &D2 &N0             

ViVa 14.4k:
AT&F&Q6\N0%C0&D2N0S37=9

ViVa modem (internal):
&F&Q6\N0%C0&D2N0S37=9

Zoltrix model 14/14 VE:
AT S0=Q0 V1 &C1 &D2 W2 &Q0

Zoom 14.4k VFX:
AT&Q6S37=9N0%C\N0

Zoom 14.4k VFX:
AT&Q6S37=11N0%C&K0

Zoom OEM Modem:
AT&Q6S37=9N0&K0

Zyxel U-1496E:
AT Z &N4 &K0


Extras Known to Work
========================
AT&Fs46=0&Q0&D2&W

AT&F%C0&D2&W

AT&F&Q0%C0&D2&W

AT &F S46=0 S48=0 S23=187 &Q0 &D2 \J0 &W

AT&F S46=0 &Q0 &D2 S37=F8 %C0 &W

AT&F S46=0 S48=0 &Q0 &D2 S37=F8 %C0 &W

AT&FE0V1X0S46=0&Q0&D2&W

AT &F \N0 \Q0 -J0 "H0 B8 E0

ATF&D2&K0&M0&N6       

ATZ&D2&K0&M0&N6       

AT %C0 "H0 \N0 \Q0

