CMaze PC v1.00 Notes
====================
The Crystal Maze must be run from a hard drive. To install it, insert CMaze
disk 0 into the floppy drive and type install.
To run it, change directory to that containing the cmaze executables. The 
hardware setup may be refined with the given setup utility.

Pressing any key during joystick calibration will cancel the calibration
test, but will also disable the joystick as an auxiliary input device!
