*****************************************************************************
                               Virtual Karts
                                 11/13/95
                               Version  1.0
*****************************************************************************


                 Thank you for purchasing Virtual Karts



DOS
------------
1.  For those of you with an 8Mb system running DOS, you have two options.
You can still set up a 512Kb smartdrv disk cache, which will speed up loading
times considerably. (NOTE:  smartdrv defaults normally to a 2Mb disk cache;
you will need to change this if you are running an 8Mb system.  The other
option, is to remove smartdrv from your autoexec.bat or config.sys (thus
freeing the amount of memory that smartdrv requires).


Windows 95
------------
1.  You still need a VESA driver to run Virtual Karts (yes, even under
Windows 95).  Some video cards come equiped with the VESA drivers on the
card, so you may not need to load a VESA driver.  If you do not have
a VESA driver, you can either call the manufacturer of your video card
and request a VESA driver, or you can use the shareware VESA driver that
we have provided on the CD.  The shareware UniVBE software is made by
SciTech and is good for a free 21 day trial period.  Please register
with SciTech if you choose to use this product. In the UniVBE directory,
there is a zip file that contains a shareware VESA driver.  You can unzip
this file to your hard drive and follow the directions contained within
readme.txt provided with UniVBE.

2.  We have supplied a .pif file for your convenience.  You may need
to change the command line and working directory in the program properties
depending on the drive letter of your CD-ROM.  The file attributes of the
.pif files are set to read only.  If you copy these files to your hard disk,
you will need to change the file attribute to read and write (this can be
done in the Win95 Explorer).

3.  Virtual Karts MUST BE RUN IN FULL-SCREEN mode.  It will not run in
window mode (Use ALT-ENTER to go to full-screen mode.)

Video Notes
------------
1.  If you experience problems with the opening animation, you can run an
alternate animation.  To run the alternate animation set the MPSVID
environment variable.  This is done by putting the following statement in
your autoexec.bat file.

	 SET MPSVID=1


Sound Notes
------------
1.  The Ensoniq SoundScape and Win95:  We have encountered problems with this
card running from a "DOS box" in Win95.  It was fixed by getting rid of the
old Win 3.1 and DOS drivers and replacing them with native Win95 drivers
from Ensoniq.  These drivers can be downloaded from Ensoniq's Web site or
BBS.

2.  Gravis Ultra Max:  There is a problem with this card using 16-bit DMA
channels on some systems.  Selecting an 8-bit DMA (0,1,3) will solve the
problem.  We've also had trouble getting stereo to work, therefore only
mono support is offered at this time.

3.  SoundBlaster Pro and DOS\Win95:  Auto-Dectection will not recognize this
card.  This card will work properly if you manually change the
sound parameters in the configuration menu (manually set the sound card
to SoundBlaster Pro).

4.  If the auto-detection displays a card different from what you know is
in the system, check to see if the installed card is compatible with what
auto-detection is reporting.  We've been surprised to see auto-detect
reporting a Microsoft Sound System on some computers when we thought we had
SoundBlasters.  In many cases, auto-detect will report the best option
available. However, you can still change the selection manually if you're not
satisfied.

5.  If you have problems with your sound card under Win95, make sure that
you are using the latest drivers for that sound card.  We have seen
Win 3.1 sound drivers, not work under Win95.  Check with the manufacturer
of your sound card for the most recent (Win95) sound drivers.


6.  It is possible that sound auto-detection will lock-up or "hang" on
some systems.  If the auto-detection does not work properly, please use
the manual sound configuration.  Manual sound configuration is done by
clicking on the sound buttons in the sound configuration menu.  Please
make sure you set the proper Sound Board, Address, IRQ, and DMA.



Controllers
------------
1.  CH Pro Pedals should be set to plane mode.


Network Play
------------
1.  This game requires that you have an IPX driver loaded to run in network
play.  You do not actually have to be logged into a network to run the
game in network mode.

2.  Shifter Karts can not be chosen in network mode.


