Fast Attack
Troubleshooting Guide
for PC's using DOS 5.0 and higher or Windows 95
revised 3/6/96


Sierra Technical Support provides this documentation as a reference to 
Sierra customers using Sierra software products. Sierra Technical 
Support makes reasonable efforts to ensure that the information contained 
in this documentation is accurate. However, Sierra makes no warranty, 
either express or implied, as to the accuracy, effectiveness, or 
completeness of the information contained in this documentation.

SIERRA ON-LINE, INC. DOES NOT WARRANTY OR PROMISE 
THAT THE INFORMATION HEREIN WILL WORK WITH ANY OR 
ALL COMPUTER SYSTEMS. SIERRA DOES NOT ASSUME ANY 
LIABILITY, EITHER INCIDENTAL OR CONSEQUENTIAL, FOR 
THE USE OF THE INFORMATION HEREIN, INCLUDING ANY 
AND ALL DAMAGE TO OR LOST USE OF COMPUTER 
HARDWARE OR SOFTWARE PRODUCTS, LOSS OF 
WARRANTIES, OR LOST DATA BY THE CUSTOMER OR ANY 
THIRD PARTY. NO ORAL OR WRITTEN INFORMATION OR 
ADVICE GIVEN BY SIERRA, ITS EMPLOYEES, DISTRIBUTORS, 
DEALER OR AGENTS SHALL CHANGE THE RESTRICTION OF 
LIABILITY OR CREATE ANY NEW WARRANTIES. IN NO CASE 
SHALL SIERRA'S LIABILITY EXCEED THE PURCHASE PRICE 
OF THE SIERRA SOFTWARE PRODUCT.



TABLE OF CONTENTS

SECTION 1 - HARDWARE REQUIREMENTS
SECTION 2 - INSTALLATION PROCEDURES
SECTION 3 - COMMON INSTALLATION PROBLEMS
SECTION 4 - COMMON GAME PROBLEMS
SECTION 5 - COMMON SOUND PROBLEMS
SECTION 6 - DOS BOOT DISK INSTRUCTIONS 
SECTION 7 - WINDOWS 95 BOOT DISK INSTRUCTIONS
SECTION 8 - IF YOU STILL HAVE PROBLEMS
SECTION 9 - SOUND CARD DRIVER INFORMATION

SECTION 1 - HARDWARE REQUIREMENTS

REQUIRED
486DX33
8 MB RAM
2X Speed CD ROM drive
1MB hard drive space (2MB compressed)
MS-DOS 5.0 or higher
SVGA (640x480x256)
Mouse
Sound card with DAC

RECOMMENDED FOR BEST PERFORMANCE
Pentium
16 MB RAM
Quad speed CD ROM
Local Bus Video
Sound Blaster or 100% compatible


SECTION 2 - INSTALLATION PROCEDURES 

DOS Installation
1. Before installing the game, make sure that your computer is turned on 
and that the MS-DOS prompt is showing. The prompt should look 
like this C> or like this C:\> (the letter may be different if you are 
installing to a different drive). Exit completely out of any other 
program you may have running such as Windows or DOS Shell.
2. Insert the Fast Attack CD into your CD-ROM drive. Change to your 
CD-ROM drive by typing the letter of your CD-ROM drive followed 
by a colon, and then press <ENTER>. For example, if “D” is your 
CD-ROM drive, type D: and press <ENTER>.
3. Type INSTALL and press <ENTER>. Follow the on-screen 
instructions to complete the installation.
4. By default, the installation program will create a directory on your C: 
drive called SIERRA\FAST and place all game files in that directory.
5. The game will prompt you for sound and field war (video) 
configurations. This will only occur when you have newly installed 
the game. You must run each setup before you can play Fast Attack. 
6. To play Fast Attack after you have installed the program, change to 
the SIERRA\FAST directory on your hard drive by typing 
CD\SIERRA\FAST and pressing <ENTER>.
7. From the game directory, type FAST and press <ENTER> to begin 
the game.
 
You may reconfigure your sound setup after you have installed the game. 
To do so, change to your Fast Attack game directory, as explained in Step 
5 above, type SOUNDSET and press <ENTER>. Then follow the on-
screen instructions.

Windows 95 Installation
1. Insert the Fast Attack CD into your CD-ROM drive. After a few 
seconds, a window will automatically appear on your Desktop and 
ask you if you would like to install Fast Attack/
2. Choose "Yes, please" and follow the on-screen instructions.

To play Fast Attack from Windows 95 after installation, insert the CD in 
your CD-ROM drive. It will ask you if you want to play Fast Attack. 
Click on "yes".

NOTE: Fast Attack may not play properly if any other programs are 
running in Windows 95. Make sure no other programs are running, 
including screen savers and virus scanners BEFORE you start Fast 
Attack.

If no window appears after putting the CD in the drive, you may have 
Autoplay disabled in Windows 95. To re-enable it, click on your Start 
button, go to Settings, then Control Panel. From Control Panel, double-
click on the System icon. Choose the Device Manager tab, then find the 
section labeled "CD-ROM". Click the plus (+) next to CD-ROM, then 
click the name of the CD-ROM beneath it. Then click the "Properties" 
button. When the Properties window comes up, choose the "Settings" tab. 
In the "Options" section, put a check mark next to "Auto insert 
notification". Then click "Apply" and "OK". Follow the on-screen 
directions (you may need to restart Windows 95). Now when you insert 
the Fast Attack CD, a window should automatically appear.

If you have trouble installing Fast Attack under Windows 95, we 
recommend booting your system in MS-DOS mode and installing the 
game following the instructions below.


SECTION 3 - COMMON INSTALLATION PROBLEMS

Problem: In Windows 95, when you insert the CD, you never get a 
message asking if you want to play Fast Attack.
Solution: You need to enable the Autoplay feature of Windows 95. Click 
on your Start button, go to Settings, then Control Panel. From Control 
Panel, double-click on the System icon. Choose the Device Manager tab, 
then find the section labeled "CD-ROM". Click the plus (+) next to CD-
ROM, then click the name of the CD-ROM beneath it. Then click the 
"Properties" button. When the properties window comes up, choose the 
"Settings" tab. In the "Options" section, put a check mark next to "Auto 
insert notification". Then click "Apply" and "OK". Follow the on-screen 
directions (you may need to restart Windows 95). Now when you insert 
the Fast Attack CD, a window should automatically appear.

Problem: After typing INSTALL, a row of dots goes across the screen 
and stops. The computer is locked up with this row of dots appearing on 
the screen.
Solution: The dots indicate the hardware detection portion of the 
installation program. You can bypass the hardware detection (and 
therefore the lockup) by typing INSTALL /M. If this entry doesn't work, 
try INSTALL /F. One of these entries should get you past the lockup. If 
this does not work, create a boot disk using the boot disk instructions 
included with this document. After booting up with the boot disk, install 
the game.


SECTION 4 - COMMON GAME PROBLEMS

Problem: You receive a message: "ERROR: Initializing Mouse Could 
Not Find Mouse on System"
Solution: There is no mouse driver installed in DOS. A mouse driver 
must be installed before the game will run. Check your mouse 
documentation for loading instructions.

Problem: When you start the game, the program crashes with a 
DOS/4GW error and/or large text fills the screen.
Solution: This is caused by a memory conflict, usually with a memory 
manager (such as EMM386, QEMM, etc.). Running the game from a 
boot disk will usually correct this problem. Use the game's INSTALL 
program to create a boot disk. If you experience problems, create a boot 
disk using the appropriate instructions in Sections 6 or 7. 

Problem: "EMM386 Error 06 ... " The error number may vary.
Solution: This is caused by a memory conflict. Running the game from 
the boot disk will usually correct this problem. Use the INSTALL 
program to create a boot disk. If you experience problems, please see the 
boot disk instructions in Sections 6 or 7. 

Problem: You get an "Error reading Drive D" or "Unable to read drive 
D:"(drive letter will vary depending on your CD drive letter). The error 
may occur at the beginning of the game or randomly throughout the 
program.
Solution: The most common reason for a "read error" is a dirty or 
scratched CD. You should check the CD to make sure that there are no 
smudges, fingerprints, scratches or cracks on it.  If you see any smudges 
on the CD, clean it off with a soft cloth and try it again. 

If this doesn't work, the problem may lie with the CD ROM drivers. You 
should make sure that you are using the latest version (v2.23) of 
MSCDEX in your AUTOEXEC.BAT. If you're using DOS 6.2 or higher, 
use the MSCDEX in your C:\DOS directory; this one is version 2.23. If 
you're using Windows 95 and running the game in MS-DOS mode, you 
should be using the MSCDEX in your C:\WINDOWS\COMMAND 
directory; this one is version 2.25. You should also check with the CD 
ROM drive manufacturer to make sure that you have the latest version of 
their CD drivers. Outdated or incompatible drivers can also cause this 
type of problem.

This error can also be caused by a defective CD. The easiest way to get a 
new CD is to exchange it at the store where you bought the game. If they 
are unable to exchange the game, Sierra will replace it for you. Please see 
your game documentation for information CD replacement.

Problem: You experience random lockups during the game, or your 
computer reboots during the middle of game play. Sometimes you receive 
memory errors or other problems when playing Fast Attack. 
Solution: This is caused by a memory conflict. Running the game from a 
boot disk will usually correct this problem. Use the game's INSTALL 
program to create a boot disk. If you experience problems, please see the 
boot disk instructions in Sections 6 or 7.

Problem: The graphics in the game are distorted or have lines running 
through them.
Solution: This problem can have three causes. The first, and most 
common, is that the game is experiencing a memory conflict. Running the 
game from a boot disk should correct this problem. Use the Install 
program to create a boot disk or follow the appropriate instructions in 
Sections 6 or 7. The second cause is an incompatible VESA driver. Make 
sure that you are using the VESA driver appropriate for your video card. 
Check your video card documentation for details. This problem can also 
be caused by an incompatible mouse driver. Some DOS mouse drivers 
don't handle VESA (SVGA-resolution) applications well. Try switching 
to a Microsoft or Logitech mouse driver. Sierra recommends Microsoft 
8.20 or higher, or Logitech 6.1 or higher. If you are running the game in 
Windows 95, be sure that no other programs are running.

Problem: You are unable to make any selections from the Weapons 
Launch Console.
Solution: Be persistent, but make sure you don't randomly click the 
mouse about the screen because this may cause the game to lockup. 
Sometimes, though, you must double-click on an option before it will 
become selected. The process to launch a torpedo is rather lengthy so 
make sure you have followed the necessary steps in the manual, and if 
double-clicking still doesn't select your choices, then the game may have 
locked up. 

If you don't see your question listed in this document: Most difficulties 
with Fast Attack, including lockups and Fatal or Panic errors can be 
resolved by simply running the game with a boot disk. Please see Sections 
6 and 7 for detailed boot disk instructions. Incompatible or outdated sound 
card and VESA drivers can also cause lockups and errors. You should 
make sure that you are using the latest versions of your sound card and 
video drivers. Contact your sound and video card manufacturers to obtain 
the latest drivers. If you are experiencing problems in Windows 95, restart 
the computer in DOS mode and run the game in that environment.


SECTION 4 - COMMON SOUND PROBLEMS

Problem: You get the message: "Sound System Fault Invalid Driver ID" 
when you attempt to start the game.
Solution:  This error is referring to the fact that one of the sound settings 
has not been selected (DIGITAL, MIDI, or both). The game will not start 
if you leave either setting as "NO DIGITAL DEVICE" or "NO MIDI 
DEVICE". Although a Sound Card is not listed as one of the minimum 
requirements on the box, the game will not play without one.

Problem: When running the game, you get no sound and/or music.
Solution: This is usually caused by either incorrect sound settings in the 
program or insufficient free memory. First, check your sound settings for 
the game. If you're running under Windows 95, consult your Windows 95 
documentation on how to change and configure sound drivers. If you're 
running under DOS, run the SOUNDSET program from the 
\SIERRA\FAST directory. Select Set Sound and follow the on screen 
instructions Note that many Sound Blaster-compatible cards can also 
emulate the Microsoft Sound System. If the Sound Blaster setting doesn't 
work, check your sound card documentation to see if your card can 
emulate the Microsoft Sound System, then set the card up for that mode 
and re-run the SOUNDSET program. If you're sure that all of your 
settings are correct in SOUNDSET, you may not have enough available 
memory to run the game with full music and sound effects under your 
current configuration. Running the game from a boot disk should correct 
this problem. Use the Install program to create a boot disk or use the boot 
disk instructions in Sections 6 and 7.

NOTE: NOTE: Some sound drivers do not support sound correctly when 
running DOS applications under Windows 95. This usually occurs when 
the sound card is not directly supported by Windows 95, which forces you 
to use the Windows 3.1 drivers for the sound card. Common symptoms of 
this are lockups or simply no sound. You should be able to get around this 
by restarting your computer in MS-DOS mode (with a boot disk, if 
necessary) and running the game from DOS. If you continue to experience 
problems with sound after booting from a boot disk, check your sound 
card documentation to make sure that you have all of the necessary lines 
in the CONFIG.SYS and AUTOEXEC.BAT files, or contact your sound 
card manufacturer for details or information on updated Windows 95 
drivers.

Problem: While playing the game, the sound slows down or drops out, or 
the video sequences become choppy and slow.
Solution: This is often caused by insufficient available memory. Running 
the game from a boot disk should correct this problem. Use the Install 
program to create a boot disk or use the boot disk instructions in Sections 
6 or 7. If you are running in Windows 95 make sure no other applications 
are running. This includes screen savers, virus scanners and anything 
using sound..


SECTION 6 - DOS BOOT DISK INSTRUCTIONS

IMPORTANT NOTE: Please read the entire instructions prior to 
starting at Step 1.

The easiest way to make a boot disk is to use the boot disk maker 
provided with Fast Attack. To use the boot disk maker type INSTALL 
from your CD-ROM drive prompt (usually D:>). Go to the blue screen 
and select Make Bootable Floppy Disk from the menu and press 
<ENTER>. Follow the on screen instructions.

TO MAKE A BOOT DISK MANUALLY
If the boot disk maker is not successful you can try to make one manually 
by following these instructions.

STEP 1 - FORMATTING THE DISK
To make a boot disk, you must system format a high density diskette in 
the A: drive. This procedure will transfer the "system files" to the disk and 
allow the computer to boot up correctly. The disk must be in the A: drive; 
the computer will not boot from the B: drive. At a DOS prompt, type the 
FORMAT command as follows:

FORMAT A: /S <ENTER>

If you get a "Bad command or file name" error message, type: 

PATH=C:\DOS <ENTER>

Then retype the FORMAT command above. If you receive the error 
again, the MS-DOS FORMAT command may not be on your system, or 
it may have been renamed. Programs such as PC Tools and Norton Disk 
Utilities sometimes rename the FORMAT command to prevent accidental 
loss of data. If you are using a program of this type, check your 
documentation to find out how to format a SYSTEM DISK, then proceed 
to Step 2. 

STEP 2 - LOCATING THE MOUSE DRIVER
You must load a mouse driver into memory or Fast Attack will not run. 
There are two kinds of mouse drivers available: those that load in the 
CONFIG.SYS file and those that load in the AUTOEXEC.BAT file. 
CONFIG.SYS mouse drivers have an extension of .SYS (MOUSE.SYS) 
and AUTOEXEC.BAT drivers have either a .COM or .EXE extension 
(MOUSE.COM, MOUSE.EXE). You must load at least one of these 
drivers, but it is not necessary to load them all. 

If you do not know where the mouse drivers are located on your system, 
the command below should help you locate them. Type the following at 
the C:\ prompt:

DIR MOUSE* /S <ENTER>

This command will cause the system to search all subdirectories for a file 
called MOUSE. If the system locates a MOUSE file, it will display the 
path where the file is located. For example, if the MOUSE.COM file is 
located in a C:\MOUSE directory, the system will display:

Directory of C:\MOUSE
	MOUSE.SYS		55160 	03-10-92	3:10a
	MOUSE.COM		56408	03-10-03	6:00a

If this procedure does not locate a MOUSE file, your mouse driver may 
have a different name; some common names for mouse drivers are 
IMOUSE, GMOUSE and HPMOUSE. Your should check your mouse 
documentation for the exact file names and how to install them. 

Once you have located the mouse driver, you must copy it to the boot 
disk. The following example assumes that the mouse drivers are located in 
the C:\MOUSE directory as shown above. To copy the MOUSE files to 
the boot disk, type:

COPY C:\MOUSE\MOUSE.* A: <ENTER>

Substitute the appropriate path and file names for your mouse drivers in 
the command above. After you press ENTER, you should see a message 
indicating that some files were copied.

STEP 3 - LOCATING THE CD ROM DEVICE DRIVER
The CD ROM drive requires a device driver loaded in the CONFIG.SYS 
file. This driver must be loaded correctly or you will be unable to access 
your CD ROM drive. To make sure that the device driver loads correctly 
on the boot disk, look at the CONFIG.SYS on the hard drive and copy the 
driver line from there. To display the CONFIG.SYS, type the following at 
a DOS prompt:

CD\ <ENTER>
EDIT CONFIG.SYS <ENTER>

The CONFIG.SYS file will display on the screen. Look for the line that 
loads the CD ROM device driver. The line should look something like 
this:

DEVICE=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220
DEVICEHIGH=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220
DEVICEHIGH /L:14652 =C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220

The device driver in your CONFIG.SYS may differ slightly from those 
listed above. Carefully write down the line for use in your boot disk. 

To exit the CONFIG.SYS, press the <ALT>, <F>, then <X> keys.

If you have a SCSI CD ROM drive, there may be an additional driver in 
your CONFIG.SYS that must be loaded for the CD ROM device drivers 
to load correctly. Check your CD drive documentation for more 
information. 

NOTE: If you cannot locate the driver in your CONFIG.SYS file, check 
your CD-ROM drive documentation, or contact the drive's manufacturer.

STEP 4 - LOCATING THE MSCDEX CD ROM EXTENSION 
In addition to the CD ROM device driver in the CONFIG.SYS, your CD 
ROM drive requires MSCDEX, the Microsoft extension for CD ROM 
drives. If this extension is not loaded correctly in the AUTOEXEC.BAT, 
you will be unable to access your CD ROM drive. To display the 
AUTOEXEC.BAT, type the following at a DOS prompt:

CD\ <ENTER>
EDIT AUTOEXEC.BAT <ENTER>

The AUTOEXEC.BAT file will display on the screen. Look for the line 
that loads MSCDEX. It should look something like this:

C:\DOS\MSCDEX /D:MSCD001
LH C:\DOS\MSCDEX /D:MSCD001 
LOADHIGH /L:14429 C:\DOS\MSCDEX /D:MSCD001

The MSCDEX line in your AUTOEXEC.BAT may differ slightly from 
the ones above. Carefully write down the line for use in your boot disk. 

To exit the AUTOEXEC.BAT, press the <ALT>, <F>, then <X> keys.

STEP 5 - LOCATING THE SOUND CARD DRIVERS
Many sound cards have drivers or initialization lines that must be loaded 
in the AUTOEXEC.BAT or CONFIG.SYS.  Some sound cards that 
require these drivers or initialization routines are the SoundBlaster 16, 
MAD16 and the Aria 16.

At the end of these Boot Disk Instructions, you will find a section labeled 
"Sound Cards". These tables contain the sound card lines for many 
common sound cards. Check to see if your sound card is on the list. If it 
is, you will need to add the appropriate lines to the AUTOEXEC.BAT 
and/or CONFIG.SYS on your boot disk. If your sound card is not listed, 
you should check your documentation for information on what needs to 
load in the AUTOEXEC.BAT and CONFIG.SYS. 

STEP 6 - CREATING THE CONFIG.SYS FILE
To create the CONFIG.SYS file on the boot disk, type the following at a 
DOS prompt:

A: <ENTER>
CD\ <ENTER>
EDIT CONFIG.SYS <ENTER>

This will display the blank (usually blue) screen of the DOS Editor. Enter 
the following lines:

DEVICE=C:\WINDOWS\HIMEM.SYS 
DOS=HIGH,UMB 
FILES=30
BUFFERS=20 

If you're using MOUSE.SYS to load your mouse, add the following line:

DEVICE=A:\MOUSE.SYS 

Now add the CD ROM device driver as you wrote it down in the 
"Locating the CD ROM Device Driver" section above. The device driver 
should look something like this:

DEVICE=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220 

If you need to load any sound card drivers, copy them from the "Sound 
Cards" section now. The following example lines are for the SoundBlaster 
16:

DEVICE=C:\SB16\DRV\CTSB16.SYS /UNIT=0 /BLASTER=A:220 I:5 D:1 H:5 
DEVICE=C:\SB16\DRV\CTMMSYS.SYS

Save the file by pressing <ALT>, <F>, then <S>. Exit the file by pressing 
<ALT>, <F>, then <X>.

STEP 7 - CREATING THE AUTOEXEC.BAT FILE
To create the AUTOEXEC.BAT file on the boot disk, type the following 
at a DOS prompt:

A: <ENTER>
CD\ <ENTER>
EDIT AUTOEXEC.BAT <ENTER>

This will display the blank (usually blue) screen of the DOS Editor. Enter 
the following lines:

@ECHO OFF
C:\ 
SET COMSPEC=C:\COMMAND.COM 
PROMPT SIERRA BOOT DISK $_$P$G 
PATH=C:\;C:\DOS;C:\SIERRA 
C:\DOS\SMARTDRV

If you are using the MOUSE.COM or MOUSE.EXE file to load your 
mouse, add the appropriate line:

A:\MOUSE.COM

Now add the MSCDEX line as you write it down in the "Locating the 
MSCDEX CD ROM Extension" section. For example:

C:\DOS\MSCDEX /D:MSCD001 

If you need to run any sound card initialization programs or load any 
drivers, copy them from the "Sound Cards" section

now. The following example lines are for the SoundBlaster 16:

SET BLASTER=A220 I5 D1 H5 T6 
SET SOUND=C:\SB16
SET MIDI=SYNTH:1 MAP:E 
C:\SB16\SB16SET /M:220 /VOC:220 /CD:220 /MIDI:220 /LINE:220 
C:\SB16\DIAGNOSE /S 

Save the file by pressing <ALT>, <F>, then <S>. Exit the file by pressing 
<ALT>, <F>, then <X>.

STEP 8 - REBOOT THE SYSTEM AND START THE GAME
Reboot your system by pressing the <RESET> button on your computer 
or by using the <CTRL> <ALT> <DELETE> key sequence on your 
keyboard. Start the game by typing the following at the C:> prompt:

CD\SIERRA\FAST <ENTER>
FAST <ENTER>


SECTION 7 - WINDOWS 95 BOOT DISK INSTRUCTIONS 

IMPORTANT NOTE: Please read all instructions before beginning this 
procedure.

STEP 1 - FORMATTING THE DISK
To make a boot disk, you must system format a high density diskette in 
the A: drive. This procedure will transfer the "system files" to the disk and 
allow the computer to boot up correctly. The disk must be in the A: drive; 
the computer will not boot from the B: drive. 

To format a disk in Windows 95, put the disk in the drive, open My 
Computer, then right click on the A: icon. From the pop-up menu, select 
Format. Under "Format type" select Full; under "Other options", choose 
Copy system files. Click on Start. 

After the disk is formatted, you must copy the MSDOS.SYS file from the 
hard drive to the floppy disk. To do this, leave the floppy disk in the drive, 
open Windows Explorer and find the MSDOS.SYS file in the root of the 
C: drive. Right click on the file, then select Send to from the pop-up 
menu. Send the file to the A: drive. 
NOTE: If you don't see the MSDOS.SYS file in Explorer, the file is 
hidden. To make the file visible, select View, Options, then Show all 
files. If you do not wish the hidden files to remain visible, you can hide 
them again after you've made the boot disk by choosing View, Options, 
Hide files of this type.

STEP 2 - LOCATING THE CD ROM DEVICE DRIVER
The CD ROM drive requires a device driver loaded in the CONFIG.SYS 
file. This driver must be loaded correctly or you will be unable to access 
your CD ROM drive. To make sure that the device driver loads correctly 
on the boot disk, look at the CONFIG.SYS on the hard drive and copy the 
driver line from there. To display the CONFIG.SYS, click on the Start 
button, then choose Run. In the command line, type SYSEDIT. The 
SYSEDIT window will appear. Click on the CONFIG.SYS title bar to 
display the CONFIG.SYS file. Look for the line that loads the CD ROM 
device driver. The line should look something like this:

DEVICE=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220
DEVICEHIGH=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220
DEVICEHIGH /L:14652 =C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220

The device driver in your CONFIG.SYS may differ slightly from those 
listed above. Carefully write down the line for use in your boot disk. 

If you have a SCSI CD ROM drive, there may be an additional driver in 
your CONFIG.SYS that must be loaded for the CD ROM device drivers 
to load correctly. Check your CD drive documentation for more 
information. 

NOTE: If you cannot find your CD ROM driver in the CONFIG.SYS 
file, you may need to look in the CONFIG.DOS file. To access this file, 
choose Start, Run, then type NOTEPAD C:\CONFIG.DOS. If you still 
cannot locate the driver, check your CD ROM drive documentation or 
contact the drive's manufacturer. 

STEP 3 - LOCATING THE MSCDEX CD ROM EXTENSION 
(May be optional - See Note below)
NOTE: If your CD ROM drive has native 32-bit Windows 95 drivers, 
you will NOT need to load MSCDEX.EXE on your boot disk. If you are 
unable to access your CD ROM drive if MSCDEX is not loaded, contact 
your system manufacturer or CD ROM drive manufacturer for Windows 
95 CD ROM drivers. In the meantime, you can use these instructions to 
load MSCDEX in the AUTOEXEC.BAT file on your boot disk.

In addition to the CD ROM device driver in the CONFIG.SYS, your CD 
ROM drive requires MSCDEX, the Microsoft extension for CD ROM 
drives. If this extension is not loaded correctly in the AUTOEXEC.BAT, 
you will be unable to access your CD ROM drive. To make sure that 
MSCDEX loads correctly on the boot disk, use SYSEDIT to look at the 
AUTOEXEC.BAT on your C: drive and copy the MSCDEX line from 
there. It should look something like this:

C:\DOS\MSCDEX /D:MSCD001
LH C:\DOS\MSCDEX /D:MSCD001 
LOADHIGH /L:14429 C:\DOS\MSCDEX /D:MSCD001

The MSCDEX line in your AUTOEXEC.BAT may differ slightly from 
the ones above. Carefully write down the line for use in your boot disk. 

If you cannot find the MSCDEX line in the AUTOEXEC.BAT file, then 
most likely you do not need to load it to access your CD ROM drive in 
Windows 95. Skip this step and continue to Step 4.

STEP 4 - CREATING THE CONFIG.SYS FILE
To create the CONFIG.SYS file on the boot disk, choose Start, Run, then 
type NOTEPAD A:\CONFIG.SYS in the command line field. This will 
start the Windows Notepad program. In the new Notepad screen, enter the 
following lines:

DEVICE=C:\WINDOWS\HIMEM.SYS 
DOS=HIGH,UMB 
FILES=30
BUFFERS=20 

Add the CD ROM device driver as you wrote it down in the "Locating the 
CD ROM Device Driver" section. The device driver should look 
something like this:

DEVICEHIGH=C:\DRV\CDROMDRV.SYS /D:MSCD001 /P:220 

Save the file by clicking on File, Save. Close Notepad by clicking on File, 
Exit.

STEP 5 - CREATING THE AUTOEXEC.BAT FILE
To create the AUTOEXEC.BAT file on the boot disk, choose Start, Run, 
then type NOTEPAD A:\AUTOEXEC.BAT in the command line field. 
This will start the Windows Notepad program. In the new Notepad screen, 
enter the following lines:

@ECHO OFF
C:\ 
SET COMSPEC=C:\COMMAND.COM 
PROMPT SIERRA BOOT DISK $_$P$G 
PATH=C:\;C:\DOS;C:\SIERRA 

If necessary, add the line loading MSCDEX that you wrote down in Step 
3.

Save the file by clicking on File, Save. Close Notepad by clicking on File, 
Exit.

STEP 6 - REBOOT THE COMPUTER AND RUN THE GAME
Leave the disk in the drive and restart the computer by clicking on Start, 
Shut Down., then Restart the computer. The computer will now re-boot 
with the boot disk. When Windows 95 restarts, start Fast Attack.


SECTION 8 - IF YOU STILL HAVE PROBLEMS
If you continue to experience problems, or if you have any questions 
concerning any of the above steps, Sierra Technical Support will be happy 
to assist you. You can reach Technical Support at (206) 644-4343 
between 8:15 am and 4:45 pm, Monday through Friday. We can also be 
reached by fax at (206) 644-7697 or by mail at the following address:

Sierra On-Line Technical Support
PO Box 85006
Bellevue, WA 98015-8506

In Europe, please contact our office in England. The Customer Service 
number is (44) 1734-303171, between 
9:00 am and 5:00 pm, Monday through Friday.  The BBS number is (44) 
1734-304227 and the fax number 
is (44) 1734-303201. Customer Service can also be reached at the 
following address:

Sierra On-Line Limited
4 Brewery Court
The Old Brewery
Theale, Reading, Berkshire
RG7 5AJ UNITED KINGDOM

You can also contact our Technical Support Team on one of the following 
services:

Sierra BBS		(206) 644-0112 
CompuServe		GO SIERRA
America Online		KEYWORD SIERRA
Internet                http://www.sierra.com
			support@sierra.com
If you decide to write or fax, please provide the following information so
that Sierra Technical Support can assist you as efficiently as possible:

Name:
Fax number:
Phone number:
Address:

Game name, version number and S/N number (from disk #1 or CD hub): 

What problem are you having?  Be VERY specific.  Is there an 
error message?  What is it?  Where does it occur? Does it happen 
the same way each time?





Floppy or CD?

Are you playing in Windows or DOS?

Type of computer (386, 486, etc.)

Brand of video card (Trident, Diamond, etc.)

Amount of RAM (4 meg, 8 meg, etc.)

DOS version (MS-DOS 6.0, PC-DOS 6.2, etc.)

Windows version (3.1, WFWG, Win95, etc.)

Brand of sound card and sound card settings (SoundBlaster Pro, 
Forte16, Mozart, etc.  Please be VERY specific with the brand 
name. Sound card settings include DMA, IRQ and I/" values.)

Any disk compression?  What kind? (Doublespace, Stacker, etc.)

Any third-part memory manager?  What kind?  (QEMM, 386MAX, 
etc.)

Largest executable program size or bytes free after booting with the 
boot disk. (Type MEM to find out.) 

What have you tried so far?  (Boot disk, no sound, etc.)



Please attach copies of your CONFIG.SYS and AUTOEXEC.BAT 
from your hard drive and the boot disk.




SOUND CARD DRIVER INFORMATION 

NOTE:  The sound card drivers and initialization lines in this section are
the default settings for these devices.  You should check your AUTOEXEC.BAT
and CONFIG.SYS on your hard drive to see if you are using any non-default
settings.


ADLIB
        AUTOEXEC.BAT
        NONE

        CONFIG.SYS
        NONE

This is a MIDI card only and will not play most sound 
effects.


ARIA 16 - Common on IBMs
        AUTOEXEC.BAT
        SET ARIA=C:\ARIA
        SET BLASTER=A220 I5 D1 T5
        C:\DOS\SOUNDCLT.COM*

        CONFIG.SYS
        DEVICE=C:\ARIA\BIN\SOUNDCFG.SYS
        DEVICE=C:\ARIA\BIN\SNDSAVER.SYS
        
*This line is not always present.


ATI STEREO FXCD
        AUTOEXEC.BAT
        SET ATI_SND=C:\SFXCD

        CONFIG.SYS
        NONE


AUDIO ROCK IT 16
        AUTOEXEC.BAT
        NONE

        CONFIG.SYS
        NONE


AUDIO 16 BY AZTECH
        AUTOEXEC.BAT
        C:\GB2KAUDIO\UTILITY\GWBVOL
        SET BLASTER=*
        SET SOUND=*

        CONFIG.SYS
        NONE

*Check your AUTOEXEC.BAT on the hard drive for
the SET BLASTER and SET SOUND parameters.


BOCA SOUND EXPRESS
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1 T5

        CONFIG.SYS
        DEVICE=C:\SE1440\CSACMOD1.EXE


BREVE TECHNOLOGIES
        AUTOEXEC.BAT
        C:\BRV16F\DOSDRV\INIT16
        C:\BRV16F\DOSDRV\MIXER

        CONFIG.SYS
        NONE


CRYSTAL CLEAR WAVE TABLE BY CRYSTAL LAKE
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1 T5
        C:\CCLEAR\CSACMAX1.COM*
        C:\CCLEAR\CSACHMX1.COM**

        CONFIG.SYS
        DEVICE=C:\CCLEAR\CSAMOD1.EXE -S***

*Enables Soundblaster compatibility.
**Add /ON to enable Soundblaster compatibility, /OFF to disable it.
***Use -S for Soundblaster mode and -W for Windows Sound System mode.


DIAMOND
        AUTOEXEC.BAT
        SET BLASTER=*
        SET SOUND16=C:\DIAMOND
        C:\DIAMOND\SNDINIT /B**

        CONFIG.SYS
        NONE

*Check your AUTOEXEC.BAT on the hard drive for the SET BLASTER parameters.
**Use /C for Soundblaster mode and /B for Microsoft Sound System mode.


DIAMOND LX
        AUTOEXEC.BAT
        SET SOUND=C:\SONIC
        SET BLASTER=A220 I5 D1 T5
        C:\SONIC\MZTVOL.EXE
        C:\SONIC\MZTINIT WSS*
        C:\SONIC\MTZINIT.SYS

        CONFIG.SYS
        NONE

*Use WSS for Windows Sound System mode and SB for Soundblaster mode.


DSP16
        AUTOEXEC.BAT
        SET BLASTER=*

        CONFIG.SYS
        NONE

*Check your AUTOEXEC.BAT on the hard drive for the SET BLASTER parameters.


ENSONIQ SOUNDSCAPE - Common on Gateways
Driver version 1.10 dated 11/31/94
        AUTOEXEC.BAT
        SET BLASTER=A220 Ixx Dx
        SET SNDSCAPE=C:\SNDSCAPE
        C:\SNDSCAPE\SSINIT FM*
        C:\SNDSCAPE\VSB_EMM.COM**

        CONFIG.SYS
        DEVICE=C:\DOS\EMM386.EXE***

*Use FM for FM synth, GM for General MIDI and MT32 for Roland MT32 emulation.
**Can help with Soundblaster emulation. Requires the EMM386 line in the CONFIG.SYS
***Necessary for the VSB_EMM.COM line in the AUTOEXEC.BAT


ENSOMIQ SOUNDSCAPE - Common on Gateways
Driver version 1.20.02 dated 12/19/94
        AUTOEXEC.BAT
        SET BLASTER=A220 Ixx Dx
        SET SNDSCAPE=C:\SNDSCAPE
        C:\SNDSCAPE\SSINIT /I*
        C:\SNDSCAPE\VSB_EMM.COM**

        CONFIG.SYS
        DEVICE=C:\DOS\EMM386.EXE***

*/I enables FM synth and General MIDI emulation.
Run MT32.EXE to enable Roland MT32 emulation.
**Can help with Soundblaster emulation. Requires the EMM386 line in the CONFIG.SYS
***Necessary for the VSB_EMM.COM line in the AUTOEXEC.BAT


ESS AUDIO DRIVE - Common on Compaqs
        AUTOEXEC.BAT            
        NONE     

        CONFIG.SYS
        DEVICE=C:\CPQDOS\VOLCTRL.EXE*
        DEVICE=C:\PCAUDIO\VOLCTRL.EXE**

*Loads the DOS mixer. <Ctrl/Right Shift> turns up the volume, <Ctrl/Left Shift>
turns it down.
**Necessary to load Windows mixer.


FORTE 16 - Common on Packard Bells
        AUTOEXEC.BAT
        SET BLASTER=*
        SET GALAXY=*
        SET SOUND=C:\FORTE16
        C:\FORTE16\UTILITY\EMUTSR

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for these settings.
**Enables the Soundblaster emulation.


FUSION 16
        AUTOEXEC.BAT
        SET BLASTER=*

        CONFIG.SYS
        DEVICE=C:\SPECTRUM\MVSOUND.SYS D: Q:**

*Check the AUTOEXEC.BAT on your hard drive for these settings.
**D: is the DMA channel and Q: is the IRQ setting


GALANT
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        NONE


GALAXY - See Multi-Media Pro 16


GATEWAY 2000 AUDIO DRIVE
        AUTOEXEC.BAT
        C:\G2KAUDIO\UTILITY\GWBVOL
        SET BLASTER=A220 I5 D1 T5
        SET SOUND=C:\G2KAUDIO

        CONFIG.SYS
        NONE

This sound card will autoconfigure itself to Soundblaster or Microsoft
Sound System mode.


GOLDEN SOUND BY TOPEK
        AUTOEXEC.BAT
        C:\GS16\GS-ENV PC:\GS16ES

        CONFIG.SYS
        NONE


GRAVIS ULTRASOUND OR GRAVIS ACE
        AUTOEXEC.BAT
        SET ULTRASND=*
        SET ULTRADIR=*
        C:\ULTRASND\ULTRINIT
        SBOS.BAT**
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for complete SET lines for the GUS.
**The SBOS.BAT line must be loaded to enable the card's Soundblaster
emulation. This line is not needed for the ACE.


IBM PS/1
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        NONE


ISP 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET ISP16=C:\ISP16
        C:\ISP16\ISPINIT /B/M*

        CONFIG.SYS
        NONE
*Use /B switch for SB mode
*Use /M switch for  Microsoft Sound System mode



JAZZ 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        DEVICE=C:\JAZZ\JAZZ.SYS D:* Q:*

*D:  DMA CHANNEL.
*Q:  IRQ SETTING.
Specific values and directories may change



MAD 16
        AUTOEXEC.BAT
        SET MAD16=C:\MAD16
        SET BLASTER=A220 I5 D1 
        C:\MAD16\M16INIT /B /M*

        CONFIG.SYS
        NONE

*Use /B switch for Soundblaster  mode.  Use /M switch for Microsoft Sound
System Mode



MAGIC S20 - Common on Acers
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET SOUND16=C:\MAGICS20
        C:\MAGICS20\SNDINIT /B /M*

        CONFIG.SYS
        NONE

*Use /B switch for Soundblaster  mode.  Use /M switch for  Microsoft Sound
System Mode



MAGITEC GREEN 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        NONE



MEDIA CONCEPT
        AUTOEXEC.BAT
        SET MC=C:\MC

        CONFIG.SYS
        NONE



MEDIA VISION DELUXE
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        C:\MEDVSN\VBEAI.COM

        CONFIG.SYS
        DEVICE=C:\MEDVSN\PROS.SYS



MEDIA VISION PREMIUM 3D SCSI2
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        DEVICE=C:\MEDVSN\PA3D.SYS
        DEVICE=MINI406A.SYS



MMCD16W
        AUTOEXEC.BAT
        SET BLASTER=*
        SET SOUND=C:\MMCD16W
        SET GALAXY=*

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT for the SET BLASTER and SET GALAXY parameters



MONTE CARLO BY TURTLE BEACH
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        C:\MCARLO\MCHKMIX

        CONFIG.SYS
        DEVICE=C:\MCARLO\MCMODE -S -W*

*Use -S switch for SB mode
*Use -W switch for  Microsoft Sound System Mode



MOZART SOUND CARD Common on Canons
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET SOUND=C:\MOZART
        C:\MOZART\MTZVOL.EXE

        CONFIG.SYS
        DEVICE=C:\MOZART\MZTINIT.SYS WSS /530*

*WSS /530 Puts the card into WSS mode port 530



MULTI-MEDIA PRO 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET GALAXY=*
        SET SOUND=C:\MMP16P

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the full SET GALAXY line.



MW WAVE - Common on IBM Thinkpads
        AUTOEXEC.BAT
        SET BLASTER=
        SET MWPATH=C:\MWD\MANAGER;C:\MWD\MWGAMES*
        SET MWROOT=C:\MWD
        MWGAMES=ON**

        CONFIG.SYS
        NONE

*This is all one line.
**ON turns on Soundblaster emulation and OFF turns it off.



ORCHID GAMEWAVE
        AUTOEXEC.BAT
        SET BLASTER=*
        SET SOUND=*
        C:\GW32\GW32.EXE

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the complete SET SOUND and
SET BLASTER lines.



ORCHID SOUNDWAVE
        AUTOEXEC.BAT
        SET BLASTER=*
        SET SOUND=*
        C:\SW32\SW32.EXE

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the complete SET SOUND and
SET BLASTER lines.



PHILLIPS
        AUTOEXEC.BAT
        NONE

        CONFIG.SYS
        NONE



PRO AUDIO SPECTRUM 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        DEVICE=C:\SPECTRUM\MVSOUND.SYS D:*Q:*

*D:  DMA CHANNEL.      Q:  IRQ SETTING.
<DIR> may be PROAUDIO on older drivers.



PRO SONIC
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        DEVICE=C:\PROSONIC\PROSYS.SYS



SC400
        AUTOEXEC.BAT
        SET SOUND=C:\SC400
        SET BLASTER=A220 I5 D1
        C:\SC400\UTILITY\SNDINIT /B

        CONFIG.SYS
        NONE



SGBAS16
        AUTOEXEC.BAT
        SET BLASTER=*
        SET SOUND=C:\SGBAS16
        SET GALAXY=*

        CONFIG.SYS
        DEVICE=C:\SGBAS16\DRIVERS\EEPRO.SYS

*Check the AUTOEXEC.BAT on your hard drive for the complete SET GALAXY and
SET BLASTER lines.



SOUNDBLASTER AWE 32 
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET SOUND=C:\SB16
        C:\SB16\SB16SET /P/Q
        C:\SB16\DIAGNOSE /S*
        C:\SB16\AWEUTIL /S

        CONFIG.SYS
        DEVICE=C:\SB16\DRV\CTSB16.SYS   /UNIT=0 /BLASTER=A:220 I:5 D:1 H:5
        DEVICE=C:\SB16\DRV\CTMMSYS.SYS**

*May be SBCONFIG on older cards.
**This line is only required to enable the sound card's CD-ROM interface.



SOUNDBLASTER PRO
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET SOUND=C:\SBPRO*
        C:\SBPRO\SBP_SET*

        CONFIG.SYS
        NONE

*On newer cards the drivers and such may look like 
the SB16 except loading out of a different directory.



SOUNDBLASTER 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1 H5 T6
        SET SOUND=C:\SB16
        SET MIDI=SYNTH:1 MAP:E
        C:\SB16\SB16SET*
        C:\SB16\DIAGNOSE /S**

        CONFIG.SYS
        DEVICE=C:\SB16\DRV\CTSB16.SYS /UNIT=0 /BLASTER=A:220 I:5 D:1 H:5
        DEVICE=C:\SB16\DRV\CTMMSYS.SYS***

*Check the AUTOEXEC.BAT on your hard drive for the complete SB16SET line.




SOUND EXPRESSION BY BOCA
        AUTOEXEC.BAT
        SET BLASTER=
        C:\CE1440\CSACMAX1.COM*
        C:\CE1440\CSACHMX1.COM**

        CONFIG.SYS
        DEVICE=C:\SE1440\CSACMOD1.EXE -S -W***

*Enables Soundblaster compatibility.
**/ON turns on Soundblaster compatibility, /OFF turns it off.
***-S for Soundblaster mode and -W for Windows Sound System mode.




SOUND EZ - See Mad 16



SOUND FX PLUS
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SOUND=C:\MMSUP

        CONFIG.SYS
        NONE




SOUNDMAND BY LOGITECH
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1

        CONFIG.SYS
        DEVICE=C:\SOUNDMAN\MVSOUND.SYS




SOUND 16A - Common on Packard Bells 1 OF 2**
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET GALAXY=*
        C:\SOUND16A\UTILITY\SETMODE /MSS**
        SET SOUND16=C:\SOUND16A

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the complete SET GALAXY line.
**Use /SB switch for SB mode. Use /MSS switch for Microsoft Sound System Mode.




SOUND 16A - Common on Packard Bells 2 OF 2**
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET GALAXY=*
        C:\AUDIO\SNDINIT.EXE /B**
        SET SOUND16=C:\AUDIO

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the complete SET GALAXY line.
**Use /B switch for SB mode
**Use /M switch for  Microsoft Sound System Mode




SOUND 144 - Common on Packard Bells
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET GALAXY=*
        SET SOUND=SOUND144
        C:\SOUND144\UTILITY\SETMODE /SBP**

        CONFIG.SYS
        NONE

*Check the AUTOEXEC.BAT on your hard drive for the complete SET GALAXY line.
**Use /SBP for Soundblaster mode and /MSS for Microsoft Sound System mode.




STRAUSS
        AUTOEXEC.BAT
        NONE

        CONFIG.SYS
        NONE





TROPEZ BY TURTLE BEACH 
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        C:\TROPEZ\DOSAPPS\SETUPSND*
        C:\TROPEZ\DOSAPPS\TZMODE -S*

        CONFIG.SYS
        DEVICE=C:\TROPEZ\DOSAPPS\TZMODE**

*Windows will disable these lines, so they will need to be run again
if Windows is started and shut down.  Use -S for Soundblaster mode and -W
for Windows Sound System mode on the TZMODE line.
**This line is necessary if the sound card is also 
acting as the CD-ROM controller.




VIBRA 16
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1 H5 T6
        SET SOUND=C:\VIBRA16
        SET MIDI=*
        C:\VIBRA16\DIAGNOSE /S**
        C:\VIBRA16\MIXERSET /P/Q

        CONFIG.SYS
        DEVICE=C:\VIBRA16\DRV\VIBRA16.SYS
        DEVICE=C:\VIBRA16\DRV\CTMMSYS.SYS

*Check the AUTOEXEC.BAT on your hard drive for the complete SET MIDI line.
**Older cards may use SBCONFIG instead of DIAGNOSE.




VOYETRA SOUND
        AUTOEXEC.BAT
        SET BLASTER=A220 I5 D1
        SET ISP16=ISP16*
        C:\ISP16\ISPINIT /B

        CONFIG.SYS
        NONE

*May be SET ISP16=VOYETRA




WAVERIDER BY AZTECH
        AUTOEXEC.BAT
        SET BLASTER=
        SET SOUND=C:\WAVRIDER
        SET GALAXY=
        C:\WAVRIDER\DRIVERS\WAVERIDE.EXE
        C:\WAVRIDER\SETMODE /SBP*

        CONFIG.SYS
        NONE

*Use /SBP for Soundblaster mode and /MSS for Microsoft Sound System mode.


