REM                       MK II WCS file for
REM        GAMMA Wing v1.3 (C) 1994 Rockland Software Productions
REM                       gamma.adv version 3.1
REM               Written and Tested by Norman Barrows 7/94
REM
REM  Base Switch Settings
REM  Black Hat switch = Digital
REM  Red Switch       = analog
REM
GAME 0 100            REM analog throttle
REM
BTN UB tab            REM Upper button   - toggle target
BTN MB ent            REM Middle button  - toggle weapon
BTN LB w              REM Lower button   - toggle semi/fullauto
REM
BTN 1 s               REM shields
BTN 2 /U c /M t /D e  REM dmg display    - targeting      - eject
BTN 3 /U f /M d /D z  REM fix dmg        - togl displays  - distress signal
BTN 4 /U x /M h /D p  REM wpn links      - hyper          - pause
BTN 5 /U o /M a /D !  REM orders         - autopilot      - self destruct
BTN 6 /U m /M g /D l  REM tactical map   - guncamera      - land me
REM
BTN HU 1              rem hat up        view fwd
BTN HR 3              rem hat right     view right
BTN HD 5              rem hat down      view behind
BTN HL 7              rem hat left      view left
REM
REM This file works ONLY with the NEW chip and MICROCODE for the MARK II WCS!
REM If you do not have the NEW chip and MICROCODE, contact THRUSTMASTER at
REM (503) 639-3200 and find out how to get the upgrade!!!
REM How can you tell if you have the new chip and microcode?  From the
REM C:\MARK2 DOS prompt, type: DIR MK2LOAD.EXE then hit ENTER. If you receive
REM the message: "File not found", then you have the OLD microcode version
REM that uses the program DOWNLOAD.EXE to load files into the WCS MARK II.
REM
