Nerves of Steel 
Quick Start

ATTENTION WINDOWS 95 USERS:
Please read installation instructions below.
MS-DOS users please skip ahead to the MS-DOS Systems: Nerves of Steel 
Installation Instructions section.

Windows 95 Systems: Nerves of Steel Installation Instructions
Nerves of Steel is not a Windows 95 game, however, you may install and 
run Nerves of Steel on a Windows 95 system by shutting down Windows 
and rebooting your system in MS-DOS mode.  

Here are the steps to follow for installing Nerves of Steel:
1. Click on the Start button and from the menu choose Shut Down.
2. Select the third choice which is Restart computer in MS-DOS mode.
3. When you reach MS-DOS mode, you will see the C:\Windows\> prompt.
4. Type cd\ [ENTER] to get to a C:\> prompt
5. To install the Nerves of Steel CD-ROM, place the Nerves of Steel disc in 
any CD-ROM drive and log onto that drive.  You will then type:
install  ( source drive )  ( destination drive )
For example, if you placed the disc in drive D: you would type:
d: [ ENTER]
install d: c:

6. Follow the on-screen directions for completing the CD-ROM installation.  

Systems with Windows 95 Pre-installed
If your computer system came with Windows 95 already installed, you may 
need to check to ensure that your computer manufacturer has setup your 
CD-ROM drive to run in MS-DOS mode.  If this information isn't disclosed 
in your computer system's instruction manual, please follow these 
instructions:

1. While in MS-DOS mode, log onto your CD-ROM drive.  Example: d: 
[ENTER] 
2. You should see a D:\> prompt or the letter which represents your CD-
ROM designation.
3. If you get an Invalid Drive Specification message, you will need to 
contact you computer manufacturer for instructions on how to load the 
appropriate CD-ROM drivers for MS-DOS mode.
4. If you do get a CD-ROM prompt, type dir [ENTER] to ensure that the 
CD-ROM drive is working properly.  If you receive a directory listing on 
the screen, your CD-ROM drive is working properly.  If you do not receive 
a directory listing, please contact you computer  for instructions on how to 
load the appropriate CD-ROM drivers for MS-DOS mode.

Windows 95 Systems: Nerves of Steel Loading Instructions

1. Start your system in MS-DOS mode as outlined in steps 1-4 under the 
Windows 95 Systems: Nerves of Steel Loading Instructions section above.
2. Type the following:
cd\nos [ENTER]
nos [ENTER]

VERY IMPORTANT: If you encounter difficulties when installing or 
loading Nerves of Steel, please run the README.BAT file included on 
this CD to access the complete USERS GUIDE, or follow the printing 
instructions detailed at the end of this file.

MS-DOS Systems: Nerves of Steel Installation Instructions
To install the Nerves of Steel CD-ROM, place the Nerves of Steel disc in 
any CD-ROM drive and log onto that drive.  You will then type:
install  ( source drive )  ( destination drive )
For example, if you placed the disc in drive D: you would type:
d: [ ENTER]
install d: c:

Then, follow the on-screen directions for completing the CD-ROM 
installation.  

MS-DOS Systems: Nerves of Steel Loading Instructions
1. Log onto the hard drive partition which contains the Nerves of Steel 
subdirectory.  
Example: c: [ENTER]

2. Type the following:
cd\nos [ENTER]
nos [ENTER]

VERY IMPORTANT: If you encounter difficulties when installing or 
loading Nerves of Steel, please run the README.BAT file included on 
this CD to access the complete USERS GUIDE, or follow the printing 
instructions detailed below.

************* IF YOU WISH TO PRINT THIS QUICK START TO A PRINTER ************

1.  Make sure that the printer is turned on and has paper.    

2.  Log on to the CD ROM drive
	Example: D:

3. Type QUICKPRN [Enter] and the QUICK START GUIDE will begin to print.

********* IF YOU WISH TO PRINT THE COMPLETE USERS GUIDE TO A PRINTER *********

1.  Make sure that the printer is turned on and has paper.    

2.  Log on to the CD ROM drive
	Example: D:

3. Type PRINT [Enter] and the complete USERS GUIDE will begin to print.


