                                                                      .
                                                                      |
                                                         -   -- ÄÄÄ-ÄÄÅÄ- -
         ±²ÛÛÛÛ² ±²ÛÛÛ²± ²ÛÛÛÛ²± ²ÛÛÛÛ²± ±²ÛÛÛÛ²   °±² ²ÛÛÛ²± °±² °±² ³
         ²ÛÜÜÜÛÛ ²ÛÜÜÜÛ² ÜÜÜÜÜÛ² ÛÛ   Û² ²ÛÜÜÜÛÛ    ²Û ÛÛÜÜÛ²  ²Û  ²Û |
         ²Û ²ÛÜÜ ²ÛÜÜ Û² ²ÛÜÜÜÜÜ ²ÛÜÜÜÛ² ²Û ²ÛÜÜ    ²Û   ÜÜÛ²  ²Û  ²Û :
         ±² ±²Û² ±²ÛÛ Û± ±²ÛÛÛÛ² ±²ÛÛÛ²± ±² ±²Û²    ±²   ²Û²±  ±²  ±² .

 ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
 ³                                BLUE FORCE!                                 ³
 ÃÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÂÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ´
 ³ Supplier  : <*> MARAUDER <*>        ³ Publisher : Tsunami                  ³
 ³ Cracker   : N/A                     ³ Graphics  : VGA                      ³
 ³ Rel. Date : 15TH JUNE 1993          ³ Soundcard : Roland/Adlib/Sound Blast ³
 ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÁÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ


               TechRAZOR Installation Guide for EASY installation:
               ~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

        For those of you who have done this before, no need to read on, just
        do a standard SUBST install.. For those of you who asked me time and
        time again to explain the install procedure, read on!

        1. Create a TEMPORARY directory, example:

                MD C:\TEMP <ENTER>

        2. Unzip all 8 disks into that directory, example:

                PKUNZIP A:*.ZIP C:\TEMP <ENTER>

        3. Repeat the above step 8 times, once per disk.

        4. Creat a substitute drive, example:

                SUBST B: C:\TEMP <ENTER>

        5. Switch to that virtual drive, example:

                B: <ENTER>

        6. Perform the quick installation, example:

                INSTALL <ENTER>

 If port 330 is occupied in your computer, or if you have a SCSI card, or
 if for any reason your computer locks at the first screen, install with a

 INSTALL /A to disable autodetection of the Sound Blaster.  Install the
 game using the PC Speaker, then, during game play, select F6 to switch to
 your sound card.  The next time you play, the game will start with the right
 soundcard.

 If you are having trouble, contact me via FelonyNet, and I'll be happy to
 help!

 Oh, yeah, here are some POLICE CODES that might help you out:

                10-1    Radio Reception - POOR
                10-2    Radio Reception - GOOD
                10-4    Received Message
                10-13   Weather Check
                10-15   Prisoner in Custody
                10-27   Subject Check
                10-35   Back-Up requested
                10-97   Arrived at Scene
                10-98   Cleared Scene; Available for Call
                10-99   Emergency; Officer needs Assistance

           
           ENJOY this rather awesome RAZOR 1911 USA Release!


                                        -<*> MARAUDER <*>-


