		      CorelSCSI Pro! Version 1.0
---------------------------------------------------------------------

This file contains the following information about 
CorelSCSI Pro version 1.0:

- the information you require if you're a DOS or Windows
  user upgrading to CorelSCSI Pro from CorelSCSI version 1.2 
  or earlier.

- the list of ASPI managers provided with CorelSCSI Pro

- the instructions for installing ASPI managers that aren't
  provided with CorelSCSI Pro

- the syntax you require if you're using a Future Domain host adapter

- the last-minute product information for Windows users

- the last-minute product information for DOS users

- the Corel Technical Support numbers


UPGRADING FROM CORELSCSI VERSION 1.2 OR EARLIER
=================================================

If you're upgrading from CorelSCSI for DOS or Windows 
version 1.2 or earlier, you must remove any system patches 
before installing CorelSCSI Pro. You remove patches using  
the CorelSCSI software.

To remove a patch

1. At the command prompt, type PATCH.
2. Select the Remove Patch option.


ASPI MANAGERS INCLUDED WITH CORELSCSI PRO
=========================================

The installation includes the ASPI manager for many SCSI
interface cards. The installation installs the ASPI you select.

The installation includes the following ASPI managers:
 
   Card Type                       ASPI Version      File Name
   -------------------------------------------------------------
   Corel Generic ASPI for
   BusLogic & Adaptec (154X,164X)  1.03              ASPIDRV.SYS      
   Corel LS2000                    1.00              ASPILS_D.SYS

   Always AL-500                   1.00              ASPILS_D.SYS
   Always IN-2000                 461-12             ASPIDRVR.SYS
			     
   DPT                             001.K             DPTDDL.SYS

   FDC ASPI Interface              1.00              ASPIFCAM.SYS
   FDC TMC-950 CAM driver          1.02              DCAM950.EXE
   FDC TMC-18XX CAM driver         1.03              DCAM1800.EXE

   UltraStor 14                    2.00              USPI14.SYS
   UltraStor 24                    1.04              USPI24.SYS


INSTALLING ASPI MANAGERS NOT PROVIDED WITH CORELSCSI PRO
========================================================

If the ASPI manager for your card isn't included with the 
installation, you must install your card's ASPI manager and
load it in your CONFIG.SYS file before installing CorelSCSI.

To load an ASPI manager in your CONFIG.SYS file

1. Copy the ASPI manager from the diskette provided with your 
   SCSI card to your hard drive.

2. Add the device driver line to the CONFIG.SYS file using
   the following syntax:

	 DEVICE=C:\xxxx.SYS

   where xxxx indicates the name of your ASPI manager.

3. Reboot the system before you start the CorelSCSI installation.
   While the system is rebooting, you should look for status 
   messages from the ASPI manager. If the status indicates 
   unsuccessful installation, the CorelSCSI device driver won't 
   function.


ABOUT FUTURE DOMAIN HOST ADAPTER(S)
===================================

 TMC-950 HOST ADAPTER
 --------------------
 DCAM950 can support multiple adapters. The TMC-950 adapter requires 
 that you specify the memory location of the adapter and the IRQ 
 setting of the adapter using the following command line  syntax:
							       
     DEVICE=DCAM950.EXE /MEM IRQ [/MEM IRQ [/MEM IRQ]]           
							       
 The default setting for a single adapter looks like this:
							       
     DEVICE=DCAM950.EXE /CA00 5                                  

 Valid memory locations for the TMC-950 are CA00, C800, CE00 and DE00.

 Valid IRQ's are 3, 4, 5, 10, 11, 12, 14, and 15.


 TMC-18XX HOST ADAPTER
 ---------------------
 The TMC-18XX host adapter does not require any command 
 line settings:                      
							       
   DEVICE=DCAM1800.EXE                                         


PRODUCT INFORMATION FOR WINDOWS USERS
=====================================

  About the Corel Wallpaper Flipper
  --------------------------------

  The Corel Wallpaper Flipper utility automatically
  changes your wallpaper background each time you start Windows. 
  The utility uses BMP files that you select as the background.

  To select the BMP files you want used as wallpaper

  1. Double-click the Corel Wallpaper Flipper icon in the
     CorelSCSI Pro Utilities window. 

  2. Select the files you want to use as wallpaper images and
     then select [Add].
      -- or --
     Select [Add All].

  3. Select the Random Order checkbox if you want the images 
     displayed in different sequences.

  4. Select the Tile Wallpaper checkbox if you want multiple images 
     of the current BMP file displayed.

  5. Select [OK].

  To turn off the wallpaper flipper 

  1. Select [Disable] from the wallpaper flipper window.


  About the Corel TWAIN Device Driver
  -----------------------------------

  CorelSCSI Pro for Windows provides a device driver for scanning 
  images into TWAIN-compliant graphics applications. This section
  provides information about how to improve the scanning speed of 
  this device driver and how to use supplemental device drivers.

  You can improve the scanning speed of the Corel TWAIN device
  driver by pre-allocating memory.

  The program GRABMEM.EXE located in the WINDOWS\TWAIN\CORTWAIN 
  directory pre-allocates a 32K block of memory.

  The program must be run before starting Windows. To run the 
  program, you can place the following line in your AUTOEXEC.BAT:

    c:\windows\twain\cortwain\grabmem.exe

  You can also run the program by creating a batch file called 
  WINSTART.BAT and placing the file in your WINDOWS directory.  
  WINSTART.BAT must include the following lines:

    @echo off
    c:\windows\twain\cortwain\grabmem.exe


  Using Supplemental Device Drivers
  ---------------------------------

  Using supplemental device drivers, some other manufacturers' 
  scanners can be supported. These device drivers are located in the 
  WINDOWS\TWAIN\CORTWAIN\OEMTWAIN directory.

  The supplemental device driver takes the form of an MS-DOS device 
  driver, often used in conjunction with the manufacturer's own device 
  driver. Only one of these other scanners may be used at a time.

  Scanner         Associated Files
  -------         ------------------------------------------------
  EPSON 300C      EPSON.DOC describes the setup procedure.
                  EPSON.SYS is the required MS-DOS device driver.

  MICROTEK 600Z   MICROTEK.EXE file is the required MS-DOS 
                  device driver.
  
  MICROTEK        MICROTEK.DOC describes the setup procedure if 
                  you're using MSCAN.SYS.

  ScanMakerII     DOSDRVR.DOC describes the setup procedure if 
                  you're using MSCSI.SYS.

  HP ScanJet      HPSCANER.DOC describes the setup procedure.

  HP ScanJet Plus HPSCANER.EXE is the required MS-DOS device driver.

  HP ScanJet IIc  HPSCANER.EXE is the required MS-DOS device driver.

  Logitech        HHSCAND.SYS is the required MS-DOS device driver.

  ScanMan 256     SAPI.EXE is the required MS-DOS device driver.
                  HHSCAND.DOC describes the setup procedure.
                  SAPI.DOC describes the setup procedure.
 
  Support for Kodak PhotoCD
  -------------------------

  The Corel CD-ROM device driver for DOS and Windows (CUNI_ASP.SYS) 
  currently supports Kodak PhotoCD with the following drives:

  Single session       Multi session
  --------------       -------------
  Chinon CDS435        Chinon CDS535
  NEC CDR73            NEC CDR74-1
  NEC CDR73M           NEC CDR84-1
  NEC CDR74            Panasonic CR-532
  NEC CDR83            Philips CDD-521
  NEC CDR83M           Smart & Friendly HS-2200 i/e
  NEC CDR84            Sony CDU-561
  Sony CDU-541         Teac CD-50
  Sony CDU-6211        Texel DM-3024K
  Texel DM-5024        Texel DM-5024K
  Texel DM-3024        Toshiba XM3301 (with multi session upgrade)
  Toshiba XM3301       Toshiba XM3401


  Other drives may be capable of reading Kodak PhotoCD, but have
  not been tested by Corel.


  CorelSCSI BACKUP 
  ----------------
		 
  The Catalog Files Path option in Preferences defines where 
  catalog files created by the Backup utility are stored. 
  If you change this location, you must restart the application
  before the new setting takes effect.

  CorelSCSI Backup can read tapes written with SY-TOS.  If you 
  want to restore tapes written with SY-TOS, you must add some 
  information to the [CorelSCSI Backup] section of your 
  CRLSCSI.INI file. This file is located in the CorelSCSI Pro 
  installation directory.

  To restore SY-TOS tapes, add the following line:

     bSyTOS=1

  If the tapes were written with a version of SY-TOS later 
  than version 1.32, you must also add the following:

     bSyTOS_132=0

  NOTE: You must remove these lines from the CRLSCSI.INI
  file if you want to restore tapes written with the Corel
  backup utilities CTBACKUP or WTBACKUP.

  When you format tapes using the Backup utility, you have the
  option of using error correction code. Only QIC tape drives 
  support error correction code. If you aren't using a QIC tape
  drive, make sure that you don't mark the Error Correction Code
  selection box.

  CorelSCSI Backup can read tapes written with SY-TOS.  If you 
  want to restore tapes written with SY-TOS, you must add some 
  information to the [CorelSCSI Backup] section of your 
  CRLSCSI.INI file. This file is located in the CorelSCSI Pro 
  installation directory.

  To restore SY-TOS tapes, add the following line:

     bSyTOS=1

  If the tapes were written with a version of SY-TOS later 
  than version 1.32, you must also add the following:

     bSyTOS_132=0

  NOTE: You must remove these lines from the CRLSCSI.INI
  file if you want to restore tapes written with the Corel
  backup utilities CTBACKUP or WTBACKUP.


PRODUCT INFORMATION FOR DOS USERS
=================================

  Support for Kodak PhotoCD
  -------------------------

  The Corel CD-ROM device driver for DOS and Windows (CUNI_ASP.SYS) 
  currently supports Kodak PhotoCD with the following drives:

  Single session       Multi session
  --------------       -------------
  Chinon CDS435        Chinon CDS535
  NEC CDR73            NEC CDR74-1
  NEC CDR73M           NEC CDR84-1
  NEC CDR74            Panasonic CR-532
  NEC CDR83            Philips CDD-521
  NEC CDR83M           Smart & Friendly HS-2200 i/e
  NEC CDR84            Sony CDU-561
  Sony CDU-541         Teac CD-50
  Sony CDU-6211        Texel DM-3024K
  Texel DM-5024        Texel DM-5024K
  Texel DM-3024        Toshiba XM3301 (with multi session upgrade)
  Toshiba XM3301       Toshiba XM3401


  Other drives may be capable of reading Kodak PhotoCD, but have
  not been tested by Corel.

  CorelSCSI BACKUP 
  ----------------
		 
  When you format tapes using the Backup utility, you have the
  option of using error correction code. Only QIC tape drives 
  support error correction code. If you aren't using a QIC tape
  drive, make sure that you don't mark the Error Correction Code
  selection box.

  CorelSCSI Backup can read tapes written with SY-TOS.  If you 
  want to restore tapes written with SY-TOS, you must add some 
  information to the [CorelSCSI Backup] section of your 
  CRLSCSI.INI file. This file is located in the CorelSCSI Pro 
  installation directory.

  To restore SY-TOS tapes, add the following line:

     bSyTOS=1

  If the tapes were written with a version of SY-TOS later 
  than version 1.32, you must also add the following:

     bSyTOS_132=0

  NOTE: You must remove these lines from the CRLSCSI.INI
  file if you want to restore tapes written with the Corel
  backup utilities CTBACKUP or WTBACKUP.


  Changes to the DBACKUP Command
  ------------------------------

  The command syntax for the CorelSCSI Pro for DOS DBACKUP command
  has changes since the Users' Manual was printed.

  The following switch has been added to the DBACKUP command syntax:

    /i<rhsa>

  This switch specifies the attributes to ignore. For example,

     /irs 
   
  backs up all files except read-only and system files. By default, 
  all files are backed up.


  The following DBACKUP switch has been changed:

    /d<path>

  This switch is now specified as 

    /dp<path>



CORELSCSI PRO TECHNICAL SUPPORT
===============================

If you have any suggestions or questions about this product that 
your distributor can't answer, contact: 


      CorelSCSI Technical Support  
      ---------------------------
      Voice:      (613) 728-1010
      CompuServe: type GO COREL

