

  APAR INFORMATION
  ________________





                      o   IR99523

                          Several items were included in this APAR:

                          -   Corrections to HELP and MESSAGE files.
                          -   Late-breaking National Language Support cor-
                              rections.
                          -   HP-PCL image printing enhancements.
                          -   Reinstalls require deleting of print queues
                              first.
                          -   Additional application print support.

                          APAR initially fixed in PTF UR38483

                      o   IR99461 - Type Transformer

                          Several items were included in this APAR:

                          -   Missing token names on the begin & end structured
                              fields.
                          -   Incorrect Hebrew character mappings and missing
                              Cyrillic Greek character mappings.
                          -   Same character set filename generated for dif-
                              ferent Type-1 fonts.
                          -   Time out error during host upload.
                          -   Storing multiple fonts into an AS/400 folder.
                          -   Incorrect copyright statement.

                          APAR initially fixed in PTF UR38483

                      o   IR99524

                          PSF/2 does not work with OS/2 32-bit Graphics Engine.

                          APAR initially fixed in PTF UR38483

                      o   IR99676

                          The following HP-PCL enhancements have been added:

                          -   Printing in color with HP-PCL data stream
                              printers that support color.
                          -   Better printer memory emulation.
                          -   Support for offset stacking.
                          -   More flexible mapping of bins from an AFPDS data
                              stream to actual printer trays.
                          -   Allow specifications of media, and logical and
                              printable area.

                          APAR initially fixed in PTF UR38637

                      o   IR99715

                          Message AIN0396E indicating SQL problem. SQL error
                          SQL0180N.

                          APAR initially fixed in PTF UR38637

                      o   IR22337

                          For USA only, 4019 default paper size is Letter
                          instead of A4.

                          APAR initially fixed in PTF UR39260

                      o   IR22334

                          4019 devices may overprint at left margin.

                          APAR initially fixed in PTF UR39260

                      o   IR22430

                          Help panel used wrong word for button name.

                          APAR initially fixed in PTF UR39260

                      o   IR99810

                          DPF fonts being deleted from printer between jobs.

                          APAR initially fixed in PTF UR39260

                      o   IR22335

                          ACIF print support.

                          APAR initially fixed in PTF UR39260

                      o   IR22429

                          BCOCA and GOCA objects not being positioned
                          correctly.

                          APAR initially fixed in PTF UR39260

                      o   IR22298

                          LU Alias for Host Receiver does not allow same
                          characters as Communications Manager for the name.

                          APAR initially fixed in PTF UR39260

                      o   IR22431

                          Remove FILE option from list of ports for OS/2
                          2.0 for device type 4019.

                          APAR initially fixed in PTF UR39260

                      o   IR22475

                          Fix DBCS problem which was causing a PSF/2 trap
                          when printing jobs received via DPF.

                          APAR initially fixed in PTF UR39260

                      o   IR22560

                          Fix ASCII Landscape parameter not being accepted
                          when printing from the Print Submitter.

                          APAR initially fixed in PTF UR39260

                      o   IR22564

                          Fix lock that is taking too long for Channel driver
                          with OS/2 2.1

                          APAR initially fixed in PTF UR39260

                      o   IR22336

                          Update PENNANT Logo.

                          APAR initially fixed in PTF UR39825

                      o   IR22499

                          Upload fonts to VSE and AIX.

                          APAR initially fixed in PTF UR39825

                      o   IR22501

                          Font GRID width error in 300 pel fonts.  Fixes the
                          formula for calculating Font Width (GRID width) in
                          certain font character sets.  We recommend that you
                          re-generate all 300-pel fonts that were previously
                          created using Type Transformer.

                          APAR initially fixed in PTF UR39825

                      o   IR22502

                          Several Type Transformer items were included in this
                          APAR:

                          -   Remove C-PLI runtime library prerequisite for
                              storing fonts to VM or MVS
                          -   Disallow a blank library name in the Store to
                              AS/400 Panel.
                          -   Expand the maximum length of the typeface name
                              displayed in various panels, from 32 to 128
                              characters.
                          -   Disallow simultaneous stores to multiple hosts.
                          -   Type 1 character name to IBM name (GCGID)
                              mapping changes for conformity to the Greek
                              Standards Authority for Printing.
                          -   Added Cyrillic Greek and Hebrew character lists.
                          -   Summary report now displays large FGID values
                              correctly.
                          -   Detect maximum baseline extents greater than
                              256 pels.
                          -   Detect character increments greater than 255 pels
                              for characters in the 90 and 270 degree rotations.
                          -   Online help fixes for French version of Type
                              Transformer.

                          APAR initially fixed in PTF UR39825

                      o   IR22566

                          AFPDS Windows Device Driver may create AFPDS records
                          too long for uploading to host systems.

                          APAR initially fixed in PTF UR39825

                      o   IR22739

                          Can't restart a job at current page after printer
                          intervention.

                          APAR initially fixed in PTF UR39825

                      o   IR22878

                          Provide additional exit programs for the samples
                          directory for Post Script.

                          APAR initially fixed in PTF UR39825

                      o   IR22879

                          New functions for using PSF/2 with NOVELL networks,
                          with DOS.

                          APAR initially fixed in PTF UR39825

                      o   IR22895

                          Add a "FILE" option to the list of printer ports
                          available for 4019 device type.

                          APAR initially fixed in PTF UR39825

                      o   IR23083

                          Delete private resources when no longer needed
                          without having to bring Spool Manager down.

                          APAR initially fixed in PTF UR39825

                      o   IR23321

                          A job with a host form that is not selected is
                          printed via the DPF spool.  Wrong criteria being
                          used for determining which jobs to print.

                          APAR initially fixed in PTF UR40232

                      o   IR23398

                          If an option is not selected for a temporary
                          operator message, a bad default is returned.
                          This can also occur when a user selects an
                          option.

                          APAR initially fixed in PTF UR40232

                      o   IR23425

                          HP-PCL, PPDS printers have a variety of problems
                          when printing from the host, or LAN.  The output
                          is incorrect.

                          APAR initially fixed in PTF UR40232

                      o   IR23445

                          PAGES datastream support for Japan.

                          APAR initially fixed in PTF UR40232

                      o   IR23451

                          Control panel fixes for FORMDEF that doesn't
                          stay changed after being changed.

                          APAR initially fixed in PTF UR40232

                      o   IR23466

                          When a new spool is created the DPF Class selected
                          to print was 'A', has been changed to '*'.

                          APAR initially fixed in PTF UR40232

                      o   IR23483

                          HP-PCL4 has new default FORMDEFs and new default
                          paper sizes.  Fixes a number of problems with
                          overlapping text, etc.

                          APAR initially fixed in PTF UR40232

                      o   IR23559

                          Job is duplex, and only one page is sent for each
                          duplex indicator (printing as simplex).  This causes
                          an out of storage indication, or trap condition.

                          APAR initially fixed in PTF UR40232

                      o   IR23611

                          Channel card in highest numbered slot, and with an
                          IRQ of 12 (via reference disk) get traps, and hangs.
                          This fixes most (but not all) of these problems.

                          APAR initially fixed in PTF UR40232

                      o   IR23735

                          Ship command line functions to create AFPDS 
                          documents, segments, and overlays from PostScript.

                          APAR initially fixed in PTF UR40232

                      o   IR24290

                          Type Transformer - DUVSREB reblocking program
                          generates a B37 ABEND on MVS.

                          APAR initially fixed in PTF UR40768

                      o   IR24287

                          Type Transformer - Miscellaneous fixes:
                          1) Selection multiple typefaces locks up system
                          2) SYS3175 System Message when performing the filter
                             function and no characters are left to be built
                             into a character set.

                          APAR initially fixed in PTF UR40768

                      o   IR24289

                          Type Transformer - Code Page names are padded
                          incorrectly in the coded font object.

                          APAR initially fixed in PTF UR40768

                      o   IR24292

                          When processing an ASCII image and creating IOCA,
                          a NACK from the printer at this time is not handled
                          correctly, and causes a TRAP D.

                          APAR initially fixed in PTF UR40768

                      o   IR24293

                          JISCII is not being invoked correctly on machine
                          with Japanese code pages.

                          APAR initially fixed in PTF UR40768

                      o   IR24217

                          Re-release of Core Outline fonts, contains
                          appearance improvements.

                          APAR initially fixed in PTF UR40768

                      o   IR23709

                          Formdef changes for Message, Accounting, and
                          Auditing exits.  This uses the least common
                          denominator in printable area so that all printers
                          can print generated text.

                          APAR initially fixed in PTF UR40768

                      o   IR24252

                          Support of new printers.

                          APAR initially fixed in PTF UR40768

                      o   IR24250

                          Migration of device profiles so that PSF/2 devices
                          do not need to be destroyed and recreated.

                          APAR initially fixed in PTF UR40768

                      o   IR24136

                          Redid Control Panel so everything is now indexed
                          off of attachment type.

                          APAR initially fixed in PTF UR40768

                      o   IR23886

                          WP transform required to be first in the list of 
                          transforms when it is used.

                          APAR initially fixed in PTF UR40768

                      o   IR23893

                          Screen focus not returned when message displayed
                          by Control Panel

                          APAR initially fixed in PTF UR40768

                      o   IR24015

                          Can't install third CSD diskette when PS and HPFS
                          are used.

                          APAR initially fixed in PTF UR40768

                      o   IR22963

                          Windows AFP driver fixes:
                          1) WINWORD footer outside of VPA
                          2) Page Segment generated incorrectly
                          3) TIFF file not used correctly
                          4) File option not handled correctly when disk is
                             full

                          APAR initially fixed in PTF UR40768

                      o   IR24137

                          New Windows AFP driver for Windows 3.1, generates
                          both image and text instead of just text.

                          APAR initially fixed in PTF UR40768

                      o   IR22880

                          JISCII Transform fixes:
                          1) First line garbled
                          2) Image data is shifted

                          APAR initially fixed in PTF UR40768

                      o   IR24028

                          Changing attributes of Print Driver in Lotus 
                          screen, did not change how job printed.

                          APAR initially fixed in PTF UR40768

                      o   IR24438

                          PTF UR40525 had problems with some EUI code.

                          APAR initially fixed in PTF UR40768

                      o   IR25357

                          The use of DosSleep by OS/2 has changed between
                          OS/2 1.3, and OS/2 2.1.  A fix was needed to
                          avoid hanging the keyboard and mouse.

                          APAR initially fixed in PTF UR41102

                      o   IR25378

                          OS/2 2.1 Service Pak1 caused some problems with
                          the INI files when they developed S H R attributes.

                          APAR initially fixed in PTF UR41102

                      o   IR25385

                          When a job is INTERRUPTED with DPF, the page ID
                          is saved, and will not be changed when Start Page
                          is modified in the Spool Manager Panels.

                          APAR initially fixed in PTF UR41102

                      o   IR25524

                          Added in new printer support.

                          APAR initially fixed in PTF UR41102

                      o   IR25523

                          Upload and Print support for AFPDS files.

                          APAR initially fixed in PTF UR41102

                      o   IR25522

                          Command Line Install support.

                          APAR initially fixed in PTF UR41102

                      o   IR25356

                          OS/2 problem with 16-bit applications can
                          occasionally cause memory to not be deallocated
                          in the PCL, PPDS support code.  Workaround was
                          coded.

                          APAR initially fixed in PTF UR41102

                      o   IR25498

                          PENNAFP Windows driver updated with extra printer
                          support, and some problem fixes

                          APAR initially fixed in PTF UR41102

                      o   IR25499

                          Control Panel would assume wrong default if LPT
                          port was not explicitly selected

                          APAR initially fixed in PTF UR41102

                      o   IR25521

                          IPDS Converter was not handling out of Resource
                          ID's correctly, and was trapping

                          APAR initially fixed in PTF UR41102

                      o   IR24852

                          Host Receiver was terminating incorrectly when
                          the number of resources in the virtual printer
                          was a multiple of 20 greater than 120

                          APAR initially fixed in PTF UR41102

                      o   IR24837

                          An SMO of an orientation different than the default
                          will cause some problems if the Host Receiver is
                          restarted and does an OPC.  AS/400 is using the
                          data incorrectly, and trunctaion occurs.  Make sure
                          the SMO is the default before doing an OPC under
                          all circumstances.

                          APAR initially fixed in PTF UR41102

                      o   IR23606

                          Removed bogus call to BPSHOAHO.DLL when someone
                          tries to use the Print to File feature with Print
                          Manager

                          APAR initially fixed in PTF UR41102

                      o   IR23655

                          AIN0221E after an Operator Intervention timer
                          does not allow PSF/2 to restart again.

                          APAR initially fixed in PTF UR41102

                      o   IR23487

                          When the ICON's are created, the working directory
                          is always on C:, and this causes problems if C:
                          is unformatted, and OS/2 is installed on D:

                          APAR initially fixed in PTF UR41102

                      o   IR23207

                          Rotated celled images had a problem coming out in
                          the correct orientation on a 4028

                          APAR initially fixed in PTF UR41102

                      o   IR24332

                          Resource Manager Asserts on Soft Page Segments that
                          are imbedded in Hard Overlays via ACIF

                          APAR initially fixed in PTF UR41102

                      o   IR24411

                          Host Receiver HAID files get corrupted, and that
                          causes an assert in the Host Receiver.  The cause
                          of this condition is a Power Off without shutdown

                          APAR initially fixed in PTF UR41102

                      o   IR24516

                          Postscript problem in handling a standard control

                          APAR initially fixed in PTF UR41102

                      o   IR24596

                          Bad Extended Attributes on the PMAFP.DRV file causes
                          OS/2 to corrupt its INI files when it traps.

                          APAR initially fixed in PTF UR41102

                      o   IR24932

                          G4 IOCA decompression assumes alignment of an image
                          when printing to a PCL or PPDS printer.

                          APAR initially fixed in PTF UR41102

                      o   IR24933

                          Reset Sequence is not correct between jobs, and
                          it shows up when printing to a Novell queue and
                          intermixing jobs from different sources.

                          APAR initially fixed in PTF UR41102

                      o   IR24934

                          Some overlay positioning problems when printing to
                          PCL and PPDS printers.

                          APAR initially fixed in PTF UR41102

                      o   IR25530

                          Host Reciever enters infinite loop ending in a 
                          Presentation Manager trap when terminating under
                          some special circumstances.

                          APAR initially fixed in PTF UR41102

