
                    AUDIO PLUS Last Information
                   ****************************

 1. INSTALLATION

 To install just execute the installation program, INSTALL.BAT,
 found on the diskette labeled "AUDIO PLUS Disk ". INSTALL.BAT
 will install all AUDIO PLUS files into your hard disk driver.

 To begin installation, follow these steps.

    1. Place the distribution disk labeled "AUDIO PLUS Disk " in
       floppy drive and change drive.
    2. Type " INSTALL " and press <Enter>.

 After INSTALL, you have to add the environment settings into your AUTOEXEC.BAT
 file, as: " SET BLASTER=A220 I7 D1 " If the AUDIO PLUS on default setting.

 The following files are contained in 1.2M diskette.

 AUDIO PLUS Disk -

 INSTALL.BAT       - AUDIO PLUS software installation program
 APTEST.EXE        - AUDIO PLUS card test program
 APUTIL.EXE        - Voice integrated program
 APPLAY.EXE        - Voice play program
 APREC.EXE         - Voice record program
 APSSR.EXE         - Change sampling rate program
 APTEST.VOC        - Voice sample file
 README            - This file
 APDEMO.BAT        - AUDIO PLUS demo program
 APDEMO.VOC        - AUDIO PLUS demo voice file
 APORGAN.EXE       - Organ program
 INSTALL2.BAT      - Wolf3D shareware game install program

 2. ENVIRONMENT

 Several parameters defined in AUTOEXEC.BAT file are described as follows.

 SET BLASTER= A220 I7 D1 T1

        Note: *  A  refers to I/O address setting
              *  I  refers to IRQ setting
              *  D  refers to DMA channel setting
              *  T  refers to AUDIO PLUS card type

 3. APDEMO

 APDEMO.BAT must run on your PC with VGA card and color monitor.
