New function keys:

F5 switches between absolute and relative coordinates coordinates
        absolute - uses a single origin on screen
        relative - origin changes with each item that is placed on screen

F6 redraw - refreshes the screen.

Additions  in 2D

Lenght and angle of the straight walls are shown in the coordinate line
at the bottom of the screen.  The radius of curved walls is also shown
in the coordinate line.

Additions in 2D

x,y,camera height, direction and vertical angle have been added to
the internal view camera parameters. These parameters help the user to
position the camera in 2D after creating a 3D image.
x and y are absolute coordinates, so the user should switch to
absolute coordinates (F5) in 2D if the user wants
to position the camera at the same place in 3D.

Wall and column heights are automatically set to level height. When the level
height is changed, the wall and column height will change assume that
height.  The program will not change the custom height walls and columns set
by the user unless they are modified individually.

Note on printers driver settings:
Printer driver settings should be set to:

On the HP LaserJet 4/4M:
"Print TruType as graphics"
Graphics Mode: Raster

Windows 3.1 is required with TrueType fonts installed.


