F-18 NO FLY ZONE(tm) 2.0
Designed and created by DOE ENTERTAINMENT(R).
Copyrighted(c) 1994, All Rights Reserved.

DOE ENTERTAINMENT
2412 Desert Oak Drive
Palmdale, Ca.
93550
USA

PLEASE READ THE FOLLOWING LICENSE AGREEMENT CAREFULLY! USAGE
OF THE GAME CONSTITUTES ACCEPTANCE OF THESE TERMS.

Terms & Conditions

LIMITED WARRANTY.
THIS SOFTWARE IS PROVIDED 'AS IS'.  ALL WARRANTIES, EITHER EXPRESSED OR
IMPLIED, ARE DISCLAIMED AS TO THE SOFTWARE AND ITS QUALITY PERFORMANCE,
MERCHANTABILITY, OR FITNESS FOR ANY PARTICULAR PURPOSE.  THE ENTIRE RISK
RELATING TO THE QUALITY AND PERFORMANCE OF THE SOFTWARE IS ASSUMED BY THE
USER.  IN NO EVENT WILL DOE ENTERTAINMENT(R) BE LIABLE FOR DIRECT,
INDIRECT, INCIDENTAL, OR CONSEQUENTIAL DAMAGES RESULTING FROM THE USE,
INABILITY TO USE, OR ANY DEFECT IN THE SOFTWARE.  IF THE SOFTWARE PROVES TO
HAVE DEFECTS, THE USER ASSUMES THE COST OF ANY NECESSARY SERVICING OR REPAIRS.

Copyright (c) 1994 DOE ENTERTAINMENT(R).
All rights reserved.  All rights of reproduction in other media reserved.


IDEAL SYSTEM :
	Windows 3.1  or WFW 3.1x
	486-33DX or better
	6 Megs of RAM
	Fast Video Card & Fast Video Driver (LOCAL BUS is BETTER)
	MOUSE or KEYBOARD or JOYSTICK
	VGA 256 COLORS ONLY
	5 MEGS of Free Hard Disk Space (for game)

MINIMUM SYSTEM :
	Windows 3.1  or WFW 3.1x
	386-33DX or better
	6 Megs of RAM
	Fast Video Card & Fast Video Driver (LOCAL BUS is BETTER)
	MOUSE or KEYBOARD or JOYSTICK
	VGA 256 COLORS ONLY
	5 MEGS of Free Hard Disk Space (for game)


     Optional game enhancements

	1-2 Meg drive CACHE software (like Norton Speed Cache, SMARTDRV)

	PERMANENT SWAP FILE

	32BITDISKACCESS ON      = Workgroup for Windows option

	VFAT enabled            = Workgroups for Windows option

	SOUND CARD 8 bit        = Plays MONO SOUND ONLY
	or
	SOUND CARD 16 bit       = Plays MONO or STEREO

	Joy Stick               = Supported by IBMJOY.DRV


FILES :
	F18NFZ.EXE      -- Game Directory you created   Example(C:\F18NFZ\F18NFZ.EXE)
	Ctl3D.DLL       -- Support file
	WaveMix.DLL     -- (same) 'Digital Sound file'  --
				   Special Thanks to  Angel Diaz. and
				   ToddLa & PatWil.
	Install.TXT     -- (same)  how the game should be installed
	Readme.TXT      -- (same)  what your looking at

	PlayDoe.INI     -- WINDOWS DIRECTORY !!!
			   Example(C:\WINDOWS\PlayDoe.INI)

	IBMJOY.DRV      -- WINDOWS SYSTEM DIRECTORY !!! Example(C:\WINDOWS\SYSTEM\IBMJOY.DRV)
	JOYSTICK.CPL    -- WINDOWS SYSTEM DIRECTORY !!! (same)

	License.TXT     -- Our Legal Contract You agreed to.
	File_id.diz     -- Brief File Description


SOUND :
	The PC SPEAKER DRIVER for Windows & DSOUND speaker driver:
	Will cause the animation to stop at every instance of playing a digital sound.

	If we fail to detect your sound system properly,
	you must push F2 on your keyboard to disable ALL DIGITAL SOUND !.

	OLD Wavemix.dll:
		If you purchased Microsoft Arcade! (cool games)
		Our wavemix.dll is NEWER. Theirs does not support STEREO,
		you must copy our wavemix.dll to your windows directory.
		All Ms Arcade games are compatible with our version.

	Microsoft Sound System:  (or similar 8 bit sound cards)
		Jittery animation:
			Simply press F9 and select Adjust Microsoft Sound.
			Then exit F18NFZ, and Restart Windows.

	Wave Mapper:
		If you want us to use a different wave device other than the
		default (first one we find) simply press F9 and select what
		wave device you want us to use.
		Then exit F18NFZ, and Restart F18NFZ.

	Delayed Sounds Fx's:
		Press F9 and check the option to REMIX.

	Clicking Noise:
		Edit the PlayDoe.INI (windows directory)
		and adjust the WaveBlocks to a higher number (MAX 6)
		Sound Blaster's & Audio Blaster cards need the latest
		drivers.


	Stereo!!!:
		You can set this option from F2 configure dialog.
		Once set, must restart F-18 NO FLY ZONE(tm).

	Mono-Sound:
		uncheck the Stereo option from F2 configure dialog.
		Once set, must restart F-18 NO FLY ZONE(tm).


	QSOUND:
		Follow the instructions in the Trouble Shooting Sound.


	No Sound:
		1) You system has no digital sound capabilities
		2) Could not determine sound card or wave device.
		   Follow the Trouble shooting sound instructions.

		3) Try F9 and choose another WAVE device.

		4) Check F2 is digital sound enabled.

		5) Check Speaker connections.


	Trouble Shooting Sound:
		1) Edit the PlayDoe.INI file (windows directory)
		   and adjust Showdevices to equal 1.
		   {example: Showdevices=1}

		2) Run F18NFZ and write down the displayed information.

		   Example:
			Device 1:SB16 Wave Out

		   This is the type of sound card you have.
		   Quit F-18 NO FLY ZONE.

		   Then add the following.

		   [name of card goes here]
		   Remix=1
		   GoodWavePos=0
		   WaveBlocks=6
		   SamplesPerSec=11

		   Run F-18 NO FLY ZONE and listen for a difference.



VIDEO   Performance:
	Some video cards have a slow animation capability.
	The only solution is to have less objects on the screen.
	You can adjust the amount of items by pressing F2 and selecting
	fewer items or disabling the animated options.

	You can change to Mono Sound instead of stereo.
	You can disable the Digital Music to increase speed.
	You can turn the sound off completely.


     ** We've balanced the game's speed for slow and fast video cards.
	However, it is unavoidable that the game will be very difficult on
	blazing fast video cards.


	Video Cards:
		Stealth VRAM -- You need the latest drivers
				or you'll lose mouse control.

				You'll need latest drivers to
				avoid garbage on game start up.

CONTROL:
	We support the mouse, keyboard and Joystick.
	All controls can be used with each other or at the same time.

	KEYBOARD:
		No known problems.

	MOUSE:
		Sluggish:
			Press F2 (configure dialog).
			Move scroll bar (control sensitivity)
			to the right until desired results.

	JOYSTICK:
		Sluggish;
			Press F2 (configure dialog).
			Move scroll bar (control sensitivity)
			to the right until desired results.


		The Joystick is supported through Microsoft's joystick driver.
		(not supported by Microsoft in any way)

		Please test your Joystick before playing

		If you do not have the driver,
		copy IBMJOY.DRV and JOYSTICK.CPL from the game directory
		to your windows system directory. example ( C:\WINDOWS\SYSTEM )

		Run F18NFZ and press F9 and select Adjust System file for
		Joystick. Quit F18NFZ, Restart Windows.

		To calibrate the Joystick, either go to your control panel
		or run F18NFZ and press F2. The Configure dialog must have
		JOYSTICK CHECKED, calibration dialog will appear.
		You must click 'OK' on configure dialog, for options to be saved.

	    *** If your joystick is not readable by this driver (IBMJOY.DRV),
	    *** then it is with regret, we cannot support your joystick.



Revisions:

	1.0     Initial Release

	2.0  	Updated all the dialogs
		Converted to control 3D
		Added Hard, Med, Easy Settings (F2)
		Added Load up status bar
		Added High score (F5)
		        	          
Special Notes:

	The Higher the Resolution the more room you'll have to run in.
	We've played from 640x480 to 1280x1024 resolutions.

	The game is easier if you choose 'less items' from F2 dialog.
	{on FAST video cards, this makes the game harder with Timer disabled}



STEREO****STEREO****STEREO****STEREO****STEREO
Stereo is disabled on shipping Demo and Release !!!!
You must either Run F18NFZ, press F2 and Change it, exit F18NFZ and Run
again.

Or you must edit the PlayDoe.INI FILE (in windows directory) and change
the 'StereoStatus=0' to 'StereoStatus=1', then run F-18 NO FLY ZONE.

NOTE: Stereo is a speed decrease in the game's performance;
      you can press F2 and lower the detail options to compensate.
      Or play the game in mono-sound.
      You can also turn the digital music off.

      Stereo is also a memory hog.
      If you are low on memory, set this option off.



Just in case, you want to know what we used to test and make this game...

	We used :
		Borland 3.1 C++

		CPU     Type   Ram  VIDEO
		---------------------------
		386-33 Dell    6    Cirrus True Color/256
		386-33 (clone) 6    Qvision Color 256
		486-33 (clone) 6    local bus video
		486-33 (ngate) 6    Farenhiet 1280
		486-33 (ngate) 8    Video 7
		486-33 (ngate) 16   Cirrus True Color/256
		486-66 (clone) 8    MACH 32
		486-66 (clone) 16   Ati Ultra
		486-66 (clone) 8    Stealth VRAM
		486-66 (clone) 16   cirrus True Color/256
		486-80 (clone) 20   ATI Ultra                   (yes 80mhz)
		486-80 (clone) 32   Volante (8Meg AT2000)       (yes 80mhz)
		586-75 (clone) 32   ATI MACH32
		586-66 IBM PS2 32   AIT MACH32


	      Sound Cards: {16 Bit Cards are better}

		Microsoft Sound System
		Compaq Sound System
		Sound Blaster
		Sound Blaster pro
		Sound Blaster 16
		Ati Stereo Sound FX
		Pro Audio Spectrum+
		Pro Audio Spectrum 16
		Gravis Ultra Sound
		Covox (or other DAC)
		MultiSound
		Thunder Board

	      Joystick Cards

		Sound Blaster's
		Stereo Fx's
		Pro Audio Spectrum's
		Gravis Joystick Game card.


(c) 1994 DOE ENTERTAINMENT(R). All Rights Reserved
All rights reserved.  All rights of reproduction in other media reserved.
DOE ENTERTAINMENT
2412 Desert Oak Drive
Palmdale, Ca.
93550
USA

