;
;	Modem Init String List for NavCIS Pro/TE/SE
; Updated May 9, 1994
;
; To add or edit, use the following format:
; Brand and modem model : Init string 1 : Init string 2 (optional) with
; a hard return at end... if there is no Init string 2, be SURE to include " :"
; after init string 1, then a hard return.
; 
; EXAMPLE (Init 1 only) Note, these examples are not valid init strings.
;    Zenith Laptop 2400 Int : ATZ&F0V1D2M0 :
;
; EXAMPLE (Init 1 and Init 2)
;    Steve's Portable : AT&F : ATM0V1X4&C1&D2S55=0
;
; If your modem does not work with the model listing provided, we suggest
; try BASIC, then CARRIER Off w/DTR Hangup, FACTORY DEFAULT and finally STANDARD.
; If it still does not work, try starting with the first choice and try each until
; you find one that works... usually 99% of all modem users can get good connection
; using one of these choices.
;
; NOTE: If you are connecting to CIS at 14.4k or higher, please do your
; best to turn on LAPM error correction... this is usually invoked using
; the \N4 command with the extended Hayes AT set.  See Intel SatisFAXion
; example with UART emulation below...
;
;Correct Modem Configuration for NavCIS - Setting Init Strings
;
;NavCIS currently connects with CIS using 8N1 port settings.
;To connect with a 14.4 node, make sure your max baud rate is set to
;19,200 bps.
;
;If you are using defined nodes(CONFIGURATION|NODES), make sure that
;the nodes are set to the appropriate baud rate.   NavCIS will strap
;most modems to the baud rate specified in either the node(if one is
;defined) or max baud rate settings(if no node is defined).
;
;The following is a listing of basic settings that NavCIS expects
;modem initialization strings to ensure:
;
;1) Reset modem to factory defaults. This is usually accomplished
;   with a reset string of AT&F.
;
;2) Disable data compression(apparently CIS does not support it).
;   Please note that V.42bis is V.42 with compression.  To disable
;   compression on some modems, you will need to specify the use of
;   V.42 and NOT V.42bis.
;
;3) Enable Error correction.   We recommend the use of V.42/LAPM
;   (not V.42bis) for 14400 bps connections and MNP4 for 2400 and
;   9600 bps.
;
;4) Enable Data Terminal Ready(DTR) and Data Carrier Detect(DCD)
;   monitoring.  These are usually enabled with the use of &D2 and
;   &C1 commands.
;
;5) Most important of all, Enable the use of RTS/CTS(Hardware) Flow
;   Control.  By doing this, XON/XOFF(Software) Flow Control should
;   be disabled.
;
;By following these directions, high speed access with NavCIS should
;work properly.
;
;
Accex DATEX-J : AT&F&C1&K3&Q0 : AT&N3X3M0S0=0
Aceex 1414 (Ext) : ATZ0S6=2S7=90S9=10 : ATS10=30S11=50X4
ATI 9600 : AT&F : ATV1M0&C1&D2
Basic : AT&F :
Bausch CN-3522SA : AT&F : ATV1&C1&D2
Best Data 14400 EC : AT&FS0=0Q0V1M0&C1&D2%C0\J0\Q3\N2
Cardinal 9600 : AT&F : ATM0V1X4&C1&D2S46=136W1S95=46
Carrier Off w/DTR Hangup : ATV1&C1&D2 :
Digicom Systems : AT&F : AT*E5*M2
Dowty Quattro : AT&FQ0V1X4&C1&D2 : AT&E4&K2&R0
Everex Evercom 24 (EV941) : ATZ : ATV1&D2
Factory Default : AT&F :
Factory Default w/DTR Hangup : AT&F : ATV1&D2
Gateway Telepath : AT&F&C1&D2 S11=50 S95=44 :
Gateway Telepath PCMCIA : AT&F&C1&D2\N3 : AT%C0&K3S95=44
Hayes Accura 144+Fax : AT&F : ATM0V1Q0&K3&Q0&C1&D2&S38=0
Hayes Optima 144+Fax : AT&F&C1&D2&Q9&K3 : ATS37=11S38=0S95=46S11=60V1
Hayes Smartmodem Optima 9600 : AT&FV1M0&C1&D2 :
Intel 144i : AT&F\N3%C0%E0"H0 :
Intel PCMCIA 144 : AT&F : AT\N2%C0%E0
Intel SatisFAX /400 : AT&F : AT\N2%C0%E0
Intel SatisFAX /400 (alt) : AT&F : AT\N4%C0%E0"H0
Intel SatisFAX /400 (w/UART & LAPM) : AT&F\N4"B=3M :
MegaHertz FMs,C,S : AT&F&C1&D2 : AT\N6\Q3%C0W1
MegaHertz PCMCIA CC3144 : AT&F&C1&D2&Q5 : AT&K3&S1%CW2S95=18
MegaHertz T3144 : AT&FM0&C1&D2 : AT\G\J\Q3\N3%C0
MegaHertz XJ1144 : AT&F&C1&D2&K3&S1 : AT&Q5&WW1
MegaHertz XJ1144 (alt) : AT&F&C1&D2&Q&K&S1W2 : ATS95=0\N\G0%C0&W
Pace Microlin fx : AT&F&C1&D2
Practical Modem 9600SA v32/v42bis : ATZ : ATM0V1
Practical Periph PM14400FXxx : AT&F1 : AT&Q8S95=44S46=0S36=4
QBlazer/Telebit - TQB1 : AT&F : AT&C1&D2S190=0
Quiet Standard : AT&F : ATM0V1
SupraFaxModem : AT&F2B0&Y0%C0%E1%G1&K3S95=44 :
SupraFaxModem (alt) : AT&FB0&Y0%C0%E1%G1&K3S95=44
TI Internal TI 9600v32bis/v42bis : AT&F&C1&D2\J0\Q3\N7W1 :
TI Internal TI (alt) : AT&C1&D2\J0\Q3\N3\V1 : AT%C3Q2S7=60S0=0
Twincom 14.4 External : AT&F&C1&D2N0 :
USR Dual Standard : AT&F&C1&D2M1X7S11=45 : AT&A3&B1&H1&R2&M4&N0&K3A
USR Dual Stand (alt) : AT&FQ0V1X4B0F1 : ATS27=128&K0&H1&M5
USR Sportster 14.4 Int : AT&F&H1&R2X4&B1M1&A3E1 :
USR Sportster 14.4 (Alt) : AT&F&A3&B1&S1&K3&H1&R2&W :
USR Sportster 14.4, TI : AT&F&C1&D2&R2&K0 : AT&M5&H1&A3X4
USR Worldport 14.4 : AT&F&H1&R2X4 : AT&B1M1&A3&S1
USR Worldport 14.4 (alt) : AT&F&A3&B1&S1&K3&H1&R2&W
ViVa 14.4 FaxModem : AT&F : AT\Q3\N6
ViVa 24m : AT&FC1&D2&R0\G1\J0\N3\Q3\V1\X1S11=55 :
Zoom Standard : AT&F&C1&D2 :
Zoom v32bis : AT&F : ATM0V1X4&C1&D2S46=136W1S95=46
Zoom FaxModem VFP : AT&FM0W1&C1&D2
Zoom (2400 specific) : AT&Q6S37=6 : ATN0M0W1
ZyXel 1496B : AT&F : ATL1M3S38=32
