
                        ²ÛÛ          AND
                        ²ÛÛßßßßß ßßßßßßßßßßßßßßßßßÛÛÛ
                        ±ÛÛ       ÛÛÛ    ÛÛ  ÛÛÛ  ²ÛÛ
                        ±ÛÛ   ÜÜÜ ²ÛÛ   ÜÛÛ  ²ÛÛ  °ÛÛ
                TRADERS °ÛÛ   ²ÛÛ ±ÛÛ Üß ÛÛ  ±ÛÛßßßß PLAYERS
                        °ÛÛ   °ÛÛ °ÛÛß   ÛÛ  °ÛÛ
                         ÛÛÜÜÜÛÛÛ  ÛÛ    ÛÛ  ÛÛß
       
ÚÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¿
³                   [ T A P   I N S T A L L   I N F O ]                     ³
ÀÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÙ

To create a diskette from the DSK file:

- Insert a blank diskette into the A: drive

- At a DOS prompt type "LOADDSKF <filename>.DSK A:" and press Enter
  (note that <filename> should be the name of the file that contains the
   original disk image.)

- Follow the instructions on the screen

Example:  If the disk image file you received is "AW701303.DSK" then you would
          type the following at a DOS prompt:

               LOADDSKF AW701303.DSK A:

          and then press Enter.

If you receive a message stating that an incorrect disk format was detected, it
means that the original disk image was on a different density disk than the one
you inserted in the A:  drive.  For example, if you inserted a high density
(1.44M) disk in the A:  drive and the disk image was created from a 720K disk
you would get the following error message:


     Target disk is wrong format

     Expecting 2 side(s) - 80 tracks -  9 sectors per track


To correct the problem simply replace the disk in drive A:  with the correct
density disk and re-enter the LOADDSK command at the DOS prompt.


                            -Valiance
                     TAP Senior / RTS Member
