May 1, 1995 (c) Copyright 1995 Palindrome Corporation. All
rights reserved.


     This file includes late-breaking information and important
     topics about Palindrome Storage Manager 4.0.

     Use this with your Storage Manager documentation.          

CONTENTS
========
1. SFT III Support
2. HSM Support
3. GFS and Near Line Set Support
4. Restoring Installation Volumes
5. Adding Administrators to the Admin List
6. AutoLoaders and Cleaning Cartridges
7. Windows Shells and NetWare 4.x
8. Using the same Library Name
9. Checking the NetWare Environment
10. PALSHELL Command Line options
11. Unfreed Resources on NetWare 4.1 Servers
12. Documentation Corrections
13. Vault Lead Time
14. DOS Workstation TSA and NetWare 4.x
15. List of Certified Devices


1. SFT III Support
==================
Because NDS cannot be loaded in the MS Engine and Storage Manager
NLMs must be loaded in the IO engine, Storage Manager does not
currently support version 4.0 of SFT III.

Both Novell and Palindrome are currently working on a solution to
this problem.

2. HSM Support
==============
The current version of Storage Manager does not support
Palindrome's HSM option. By sending in the PSM Update Coupon
included with the software, you will receive free HSM Software when
it is released.

3. GFS and Near Line Set Support
================================
If you are using the GFS rotation pattern, you cannot enable the
Near Line Set option in Device Manager.

4. Restoring Installation Volumes
==================================
If you have to restore an installation volume that contains
centralized File History Databases, you must also restore the File
History Database for each protected resource after restoring the
installation volume.
To restore File History Databases
1.   Access Resource Manager
2.   Tag protected resources
3.   Open the Operation menu and select Restore/History Database

5. Adding Administrators to the Admin List
==========================================
When adding Administrators to the Admin List, be aware that anyone
on the Admin list has equivalent rights to the auto login user. In
other words, administrators on the Admin list have the same NetWare
rights that the auto login user has.

6. AutoLoaders and Cleaning Cartridges
======================================
Do not install cleaning cartridges in AutoLoaders prior to
configuring a cleaning slot (using Device Manager). If you place a
cleaning cartridge in the AutoLoader prior to configuring a slot,
Storage Manager will load the cleaning cartridge in the tape drive
repeatedly, thereby expending the cartridge.


7. Windows Shells and NetWare 4.x
=================================
If you install Storage Manager on a NetWare 4.x server while
running Windows and then later install a Windows shell program
(such as Central Point's PC Tools), you must copy the unicode
tables from the WINDOWS\NLS directory to the shell program's root
directory.

For example, if your shell program's directory is \CPS, you must
create an NLS directory as a subdirectory to \CPS and copy the
UNI*.* files from the \WINDOWS\NLS directory to the \CPS\NLS
directory.

8. Using the same Library Name
==============================
If you change the name of your media library (library name), do not
use a library name you have already used.

If you use a previously used name (and erase or format tapes from
the original library), the labels of the erased/formatted tapes 
cannot be used again in your new library.

For example, if your original library name was ADMIN, and you used
ADMIN again as a library name later, if your format ADMIN:A:1 from
the original library, your new library will not create an ADMIN:A:1
and would start with ADMIN:A:2 (as if ADMIN:A:1 was retired or
forgotten). 

9. Checking the NetWare Environment
===================================
If you notice a negative impact on backup performance after
updating modules on the network, run PALCHECK.NLM. PALCHECK.NLM is
copied to the SYS:\SYSTEM directory of the installation server.
When run on the server, PALCHECK examines currently loaded NLMs and
makes recommendations based on what it finds.

10. PALSHELL Command Line options
=================================
PALSHELL.NLM allows you to perform command line operations at the
server console that you would normally perform from the Windows
interface.

Command line documentation for PALSHELL.NLM is included in
PALSHELL.TXT file in the \TOOLS directory on disk 4.

11. Unfreed Resources on NetWare 4.1 Servers
============================================
Due to a bug in NetWare 4.1, upon termination of some NLMs you will
see the following messages:

"xx-xx-xx  xx:xx:xx pm:    SERVER-4.10-2713                       
 Module did not release 1 resource                                
 Module: Palindrome Environment Checker                           
 Resource: Service Connections                                    
 Description: Service Connections"

"xx-xx-xx  xx:xx:xx pm:    SERVER-4.10-2715                       
 Module did not release 64 resources                              
 Module: Palindrome Environment Checker                           
 Resource: Small memory allocations                               
 Description: Alloc Memory (Bytes)"

The NLMs that are affected are:                                   
- PALCHECK.NLM                                                    
- PAL.NLM                                                         
- PALMEDIA.NLM                                                    
- PALSHELL.NLM                                                    
     
The resources will be left on Netware 4.1 servers when these NLMs
are loaded when a job queue does not exist.  When a job queue
exists, the problem will not occur. 

12. Documentation Corrections
=============================
General
-------
The telephone and fax numbers the United Kingdom and European
Headquarters (Palindrome U.K.) are:
     Phone     011 44 1344 360888
     FAX       011 44 1344 360910
     BBS       011 44 1344 360920

Installation Guide
------------------
Page 2-15
Trust mode is not enabled by leaving the password field blank in
the NET.CFG file. The only way to enable trust mode is to load
TSASMS.COM from the command line and specify the /T option.
(Correction)

When using Trust mode on 4.x servers, the user ADMIN is the only
user that can connect to the TSA on the workstation. This user must
be defined in the default bindery context for the server. (Addition)

Page 2-21
The auto login user does not require Write rights to the root
object of the NDS tree (unless backing up and restoring the entire
NDS tree). The auto login user must have Browse rights to the
entire NDS tree, however. (Correction)


Administrator's Guide
---------------------
>Page 3-6
The que card references for the media and device operations should
read:
To format media, see page 10-14 
To identify currently loaded media, see page 10-4
To add a device, see page 11-5 

>Page 8-22
File History Databases can be distributed to NetWare volume
resources only. (Clarification)

>Page C-6
Add to the assumptions: "The DOS partition on the server to be
recovered has at least 4MB free space."

>Page C-11
The \LOGIN\NLS directory only needs to be created for NetWare 4.1
servers.

>Page C-13
Step 6 should read: "From the SYS:\LOGIN\NLS directory ...."

PALFCOPY step should read: "Copy PALFCOPY.NLM from the \TOOLS
directory on your last installation diskette to the \RECOV\SYSTEM
directory."

>Page C-19
Step 4 (2nd paragraph) should read: C:\RECOV\SYSTEM

>Page C-20
Step 3 command statement should read: 
LOAD PALFCOPY C:\RECOV\*.*  SYS:  /S

>Page C-23
Second paragraph should read:
If the bindery does not exist, type Supervisor with no password in
the auto login user name and password fields. On 4.x servers, type
in the fully qualified name of the ADMIN user (for example,
.CN=ADMIN.OU=SALES).

>Page D-14
The Media Details tab has a new field. The Last Updated field
indicates the last time the media was used for a backup operation.
The Last Formatted field has been renamed Created On to indicate
when the media was created.

13. VAULT LEAD TIME
===================
If you increase the number of days to rotate media sets in Configuration 
Manager on the Scheduling Tab, you should make a corresponding change to the 
"Notice Required for Retrieving Off-Site Media" on the Off-Site Media Tab.
 
The following are Palindrome's recommendation for off-site notification:

	If rotating media sets...       Set off-site notice for:
	-------------------------       ------------------------
	Once per week                           14 days
	Twice per week                           7 days
	More than twice per week                 4 days


If you fail to adjust the off-site media notification, the off-site media 
advisor may suggest that the same media be taken off-site and retrieved from 
off-site at the same time.

14. DOS WORKSTATION TSA AND NETWARE 4.X
=======================================
If you specify trust mode when loading the DOS TSA on a DOS workstation, 
the user ADMIN is the only user that can connect to the TSA when adding the 
workstation to the Protected Resource List. This is a requirement for NetWare
4.x servers protecting DOS workstations only.

The user ADMIN does not need any special rights on the server but the user 
must be defined in the default bindery context for the server that 
the TSA is connecting to.  

If you do not want to create an ADMIN user, you can configure passwords on 
each workstation or not configure a password at all.

If you configure a password, you will be asked to specify
the password when adding the resource to the Protected Resource List.

If you do not configure a password, you can add the workstation to the 
Protected Resource List without being prompted to login.

15. LIST OF CERTIFIED DEVICES
=============================
The following is a list of certified devices as of May 1, 1995.
This list of devices is continually updated. Contact Palindrome for the most
recent Certified Device List.

SCSI TAPE DRIVES

DC 600/DC 2000                                  Firmware Supported            
--------------                                  -------------------                         
Archive Anaconda 2750                             5.0
Archive ST 350                                    5.0
Colorado Memory Systems PowerTape  4000           =4Y
Compaq 320/525mb                                  7 1A, 7 1G, 7 3J
Compaq 525mb ACA                                  7 1A, 7 1G, 7 3J
Compaq 51000HT                                    (Under review)
Exabyte EXB-2501/FS1G                             2200, 2400 
Exabyte EXB-2501C                                 7100, 7300
IBM 4120                                          IO4:38
Irwin 7300 Series                                 5.0
Legacy 500s                                       7 3J
Legacy 1100q                                      7 3J
Palindrome FAST 150                               Palin_001
Palindrome FAST 250                               Palin_001
Palindrome FAST 525                               7 1A, 7 1G, 7 3J
Tallgrass FS 1000                                 -3:07, -4:08
Tallgrass FS 2000                                 =5Y, =05:17
Tallgrass FS 3000                                 5.0
Tallgrass FS 3000e                                =5Y, =05:17
Tallgrass FS 4100                                 =5Y, =05:17
Tandberg 3800                                     -3:07, -4:08
Tandberg 3820                                     -3:07, -4:08
Tandberg 4100                                     =5Y, =05:17
Tandberg 4120                                     =5Y, =05:17
Tandberg 4200                                     =5Y, =05:17
Tandberg 4220                                     =5Y, =05:17
Tandberg 4222                                     =07:  
Tandberg Panther 525                              -3:07, -4:08
Tandberg Panther 1000                             =5Y, =05:17
Tandberg Panther 2000                             =5Y, =05:17
Tecmar 525ES                                      7 1A, 7 1G, 7 3J
Tecmar 1000ES                                     7 3J
Tecmar ProLine 525                                7 1A, 7 1G, 7 3J
Tecmar ProLine 1000                               7 3J
Wangtek 5150ES                                    -08
Wangtek 5525ES                                    7 1A, 7 1G, 7 3J
Wangtek 51000ES                                   7 3J
Wangtek 51000HT                                   (Under Review)


4mm, DDS DAT                                    Firmware Supported
------------                                    -------------------
ADIC DAT 2000a                                    8.09, 9.09, 10.7
ADIC DAT 8000a (DCLZ Comp.)                       8.09, 9.09, 10.7
Aiwa Corporation GD-201                           1.38, 1.47
Anthem Technology 35480 DAT (DCLZ Comp.)          8.09,9.09
Archive Python 4320NT                             2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73,2.96
Archive Python 4330NT                             2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Archive Python 4330XT                             2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Archive Python 4350XT                             2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Archive Python 4520NT                             2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Archive Python 4540NT                             2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Archive Python 4322NT (DCLZ Comp.)                3.58, 3.76, 4.45, 4.94, 
						  4.AH 
Archive Python 4322NP (DCLZ Comp.)                3.58, 3.76, 4.45, 4.94, 
						  4.AH
Archive Python 4352XP (DCLZ Comp.)                3.58, 3.76, 4.45, 4.94, 
						  4.AH
Archive Python 4542NT (DCLZ Comp.)                3.58, 3.76, 4.45,4.94, 
						  4.AH
Archive Python 4542NP (DCLZ Comp.)                3.58, 3.76, 4.45, 4.94, 
						  4.AH
Archive Turbo Python 4324NP (DCLZ Comp.)          4.45, 4.94, 4.AH
Archive Turbo Python 4324RP (DCLZ Comp.)          4.45,4.94, 4.AH 
Archive Turbo Python 4354XP (DCLZ Comp.)          4.28,4.45, 4.94, 4.AH
Archive Python 4326NP (DDS-2)                     4.98, 4.AH
Archive Python 4326RP (DDS-2)                     4.98, 4.AH
Archive Python 4356XP (DDS-2)                     4.98, 4.AH
Archive ST DAT                                    2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Archive ST 2000                                   2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Archive ST 4000 DAT (DCLZ Comp.)                  3.58, 3.76, 4.45, 4.94, 
						  4.AH
Colorado Memory Systems Power DAT 6000            8.09, 9.09,10.7 
Compaq 4322 DAT                                   2.19, 2.26, 2.54, 2.57, 
						  2.66,2.73, 2.96
Compaq 5.0gb DAT (DCLZ Comp.)                     3.58, 3.76, 4.45, 4.94, 
						  4.AH, 4.BG
Compaq 4/16 Turbo DAT (DDS-2)                     4.94A
Conner 2000DAT                                    2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Conner 4000DAT (DCLZ Comp.)                       3.58, 3.76, 4.45, 4.94, 
						  4.AH
Conner Python 4326NP (DDS-2)                      4.98, 4.AH
Conner Python 4356XP (DDS-2)                      4.98, 4.AH
Data General 28219 DAT                            4.94, 4.AH
Digital Equipment Corporation TLZ06               3.74, 4.AT, 4.BH0 
Digital Equipment Corporation TLZ06-VA            3.74, 4.AT, 4.BH0 
Digital Equipment Corporation TLZ07 (DDS-2)       4.AT, 4.BE0  
StorageWorks SWXTA-AA                             3.74, 4.AT
StorageWorks SWXTA-BA,BT                          4.BE0
Dynatek DAT 1300                                  8.09, 9.09, 10.7, 10.09 
Dynatek DAT 2000                                  8.09, 9.09, 10.7, 10.09
Dynatek DAT 2600 (DCLZ Comp.)                     8.09, 9.09, 10.7,10.09, 
						  11.12 
Dynatek DAT 4000 (DCLZ Comp.)                     8.09, 9.09, 10.7, 10.09, 
						  11.12 
Emerald 4mm RapidRecover                          1.8, 1.9, 2.1, 2.2
Emerald DAT 1000                                  8.09, 9.09, 10.7, 
Emerald DAT 2000                                  8.09, 9.09, 10.7, 
Emerald DAT 4000 (DCLZ Comp.)                     8.09, 9.09, 10.7, 10.09, 
						  11.12 
Exabyte EXB-4200/FS4000                           1.38, 212, 216
Exabyte EXB-4200C/FS4000DC                        1.24a, 1.26, 149, 217
Hewlett-Packard 35470A                            8.09, 9.09, 10.7, 10.09 
Hewlett-Packard 35480A (DCLZ Comp.)               8.09, 9.09, 10.7, 10.09, 
						  11.12 
Hewlett-Packard C1521E (DCLZ Comp.)               8.09, 9.09, 10.7, 10.09, 
						  11.12 
Hewlett-Packard C1533A (DDS-2)                    9312, 9401, 9403, 9406
Hewlett-Packard C1534A                            T503
Hewlett-Packard C1536A                            T503
Hewlett-Packard C2224B                            8.09, 9.09, 10.7, 10.09
Hewlett-Packard C2225A (DCLZ Comp.)               8.09, 9.09, 10.7, 10.09, 
						  11.12
Hewlett-Packard 2000e/C1520A/C1520E               8.09, 9.09, 10.7, 10.09, 
						  11.09
Hewlett-Packard JetStore 2000i/C1525A             8.09, 9.09, 10.7, 10.09
Hewlett-Packard JetStore 5000/C1524A (DCLZ Comp.) 8.09, 9.09, 10.7, 10.09, 
						  11.12
Hewlett-Packard JetStore 6000i/C1528A (DDS-2)     9401, 9403, 9406
Hewlett-Packard Jet Store 6000e/C1529A (DDS-2)    9401, 9403, 9406
Hewlett-Packard Sure Store 2000e/C1520F           10.7
Hewlett-Packard Sure Store 2000i/C1525F           10.7
Hewlett-Packard Sure Store 5000e/C1521F           10.7
Hewlett-Packard Sure Store 5000eU/C1551F          10.7
Hewlett-Packard Sure Store 5000i/C1526F           10.7
Hewlett-Packard Sure Store 6000e/C1529F           9503
Hewlett-Packard Sure Store 6000eU/C1552A          9503
Hewlett-Packard Sure Store 6000i/C1528F           9503
IBM 35480A                                        !C9  
IBM 4326NP/RP (DDS-2)                             4.75, 4.AC, 4.AP, 4.BK
Infinity DAT 2GB                                  8.09, 9.09, 10.7, 10.09,
						  11.09
Infinity DAT 8GB (DCLZ Comp.)                     8.09, 9.09, 10.7, 10.09,
						  11.12
Irwin 9131Se                                      2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Legacy 4000D                                      02.2
Legacy 8000D                                      1.1
Maynard MaynStream 1300DAT                        2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
Maynard MaynStream 2000DAT                        2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Maynard MaynStream 4000DAT (DCLZ Comp.)           3.58, 3.76, 4.45
Micro Design SE1300D                              8.09, 9.09, 10.7 
Micro Design SE2000D (HP 35480A)                  8.09, 9.09, 10.7, 10.09,
						  11.12
Micro Design  SE2000DF  (HP C1533A DDS-2)         9312, 9401, 9403, 9406
MicroNet CPKD-2000                                2.19, 2.26, 2.54, 2.57,
						  2.66, 2.73, 2.96
MicroNet MD-5000 (STAC Group Comp.)               101.2
Mountain FileSafe 1200                            1.8, 1.9, 2.1, 2.2
Mountain FileSafe 1200 Plus AT                    1.8, 1.9, 2.1, 2.2
Mountain FileSafe 1200 SA                         2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Mountain FileSafe 1200 Plus SA                    2.19, 2.26, 2.54, 2.57, 
						  2.66, 2.73, 2.96
Mountain FileSafe 1200-4 (DCLZ Comp.)             1.6, 1.8, 2.0
Palindrome FAST 1300                              2.26, 2.54, 2.57, 2.66,
						  2.73, 2.96
Palindrome FAST 2000                              2.26, 2.54, 2.57, 2.66,
						  2.73, 2.96, 
						  (EXB 4200) 1.38, 2.12, 
						  2.16
Palindrome FAST 2000C                             3.58, 3.76, 4.45, 4.94,
						  4.AH
Palindrome FAST 2000C Turbo (DCLZ Comp.)          4.28, 4.45, 4.94, 4.AH
Soltronics David I/2, I/5 (DCLZ Comp.)            8.09, 9.09, 10.7
Sony SDT-2000                                     2.09
Sony SDT-2000E                                    E326
Sony SDT-4000/4010 (DCLZ Comp.)                   2.09
Sony SDT-4000E                                    E326
Sony SDT-5000 (DDS-2)                             3.02, 3.26
Sony SDT-5200 (DDS-2  Non-Comp.)                  3.26
Storage Dimensions Tape 2000                      8.09, 9.09, SD21
Storage Dimensions Tape 4000 (DCLZ Comp.)         8.09, 9.09, 10.09
Storage Dimensions Tape 8000                      3.02
Storage Dimensions LANStor TapeArrayII (C1533A)   9406, 9503
Tallgrass FS 4000                                 1.8 (WangDAT), 1.14, 
						  1.16, (Exabyte 4200) 1.38, 
						  212a, 216
Tallgrass FS 4000DC (DCLZ Comp.)                  1.24a , 1.26, 1.49, 
						  217   (Exabyte 4200C)
Tecmar ProLine DATaVault 4000 (DCLZ Comp.)        1.6, 1.8, 2.0                 
WangDAT 1300                                      1.8, 1.9, 2.1, 2.2
WangDAT 1300XL                                    1.8, 1.9, 2.1, 2.2
WangDAT 3100                                      2.0, 2.2
WangDAT 3200 (DCLZ Comp.)                         1.6, 1.8, 2.0, 2.2
WangDAT 3400DX (DDS-2)                            1.0w, 1.1


8mm                                             Firmware Supported
---                                             ------------------
Alloy Retriever/2200                              2618, 2637, 263H
Conner 5000HS                                     446, 46G, 5E0, 6L0, 6X0
Contemporary Cybernetics CY-8200 (non-Comp.)      2618, 2637, 263H
Contemporary Cybernetics CY-8500 (non-Comp.)      446, 46G, 5E0, 6L0, 6X0
StorageWorks SWXTE-AA                             620, 6M0
StorageWorks SWXTE-AB                             620, 6M0
StorageWorks SWXTE-AC                             620, 6M0
Dynatek HSB 2300                                  2618, 2637, 263H
Dynatek HSB 5000                                  446, 46G, 5E0, 6L0, 6X0
Emerald VAST/2.2 gb                               2618, 2637, 263H
Emerald 5.0gb                                     415, 446, 46G, 5E0, 6L0
Exabyte EXB-8200                                  2618, 2637, 263H
Exabyte EXB-8200SX                                2535, 260H, 261A
Exabyte EXB-8500                                  446, 46G, 5E0, 6L0, 6X0
Exabyte EXB-8500C                                 620, 6J0, 730, 
Exabyte EXB-8205                                  620, 6M0, 730, 790
Exabyte EXB-8205XL                                790
Exabyte EXB-8505                                  620, 6M0, 730, 781
Exabyte EXB-8505XL/FS10G                          730, 781
IBM 8505                                          520B                
Irwin 9230Se                                      2618, 2637, 263H
Legacy 2000s                                      2618, 2637, 263H
Legacy 2005H                                      620, 6M0, 730, 790
Legacy 5000S                                      6L0, 6X0
Legacy 5005H                                      620, 6M0, 730, 781
Maynard Maynstream 2200HS+                        2535, 260H, 261A
Maynard Maynstream 5000HS                         446, 46G, 5E0, 6L0, 6X0
Mountain FileSafe 2100                            2618, 2637, 263H
Mountain FileSafe 5000 SA                         446, 46G, 5E0, 6L0, 6X0
Palindrome Standard 2200                          2618, 2637, 263H
Palindrome FAST 2200                              2535, 260H, 261A
Palindrome FAST 5000                              411, 415, 446, 46G, 5E0,
						  6L0, 6X0
Palindrome FAST 5000C                             620, 6M0, 730, 781
Storage Dimensions Tape 5000                      411, 415, 446, 46G, 5E0,
						  6L0, 6X0
Tallgrass FS 10G                                  6M0, 730
Tecmar THS-2200                                   2618, 2637, 263H
Tecmar ProLine 2200                               2618, 2637, 263H
TTI 8510  (8500 mode)                             46G, 5E0, 6L0
TTI 8510H  (8505 mode)                            5B0, 6M0, 730, 781
TTI 8512H  (8505 mode)                            6M0, 730, 781
Vistar VT5000                                     2618, 2637, 263H


Digital Linear Tape (DLT)                    Firmware Supported
-------------------------		     ------------------
Cipher T860                                       430E, 4314
Cipher T826                                       270E, 2714
Compaq DLT2000                                    971E
Conner T860                                       430E, 4314
Conner MS20DLT                                    9105 (Under review)
Digital Equipment Corporation TZ86/TZ86-VA        4314, 4316
Digital Equipment Corporation TZ86-VA             4314, 4316
Digital Equipment Corporation TZ87/TZ87N          930A, 9410, 9514 
Digital Equipment Corporation TZ88                C814 
Digital Equipment Corporation DLT2000             930A, 9410, 9514, 971E 
Digital Equipment Corporation DLT4000             C814
Quantum DLT2000                                   971E
Quantum DLT4000                                   C814
StorageWorks SWXTL-AA                             4314, 4316
StorageWorks SWXTL-BA                             9104, 930A
StorageWorks SWXTL-BT (table top)                 9104, 930A
TTI CTS-2110                                      930A, 9410


SCSI TAPE AUTOLOADERS

4mm DDS DAT                                      Firmware Supported
-----------                                      ------------------

ADIC DAT 1200C AutoChanger (HP 35480A)            0327, 0330, 0331, 0351, 
						  0354
ADIC DAT 1200D AutoChanger  (Archive Python drive)0414, 0420, 0421, 0451, 
						  0454, 0458
ADIC DAT 1200D AutoChanger  (C1533A) [8]          0327, 0330, 0331, 0351, 
						  0354, 0360
ADIC DAT 1200D AutoChanger  (SDT-5000 drive) [8]  0454, 0458
ADIC VLS 4mm [2]                                  2.10, 2.13, 2.22 (Under review) 
ArDAT DiamondBack (Python 28849-xxx)              4.63, 4.91
ArDAT Python Loader (Python 27460-xxx)            2.96
AIWA AL-D210 (Sony SDT-5000 drive)  [8,9]         1.01, 1.02
AIWA AL-D210 (Sony SDT-5000 drive)  [2,8,9]       1.01, 1.02
Compaq 4586 Turbo DAT Autoloader                  4.94C, 4.BG 
Conner 4586NP Python DDS-2:Loader                 4.AS
Digital Equipment Corporation TLZ6L               4.42, 4.91, 4.AT, 4.BH0
Digital Equipment Corporation TLZ6L-VA            4.42, 4.91, 4.AT, 4.BH0
Digital Equipment Corporation TLZ7L               4.BQD
StorageWorks  SWXTA-LA                            4.42, 4.91, 4.AT, 4.BH0 
StorageWorks  SWXTA-BL                            4.BQD
Dilog Libra-8 SA100                               C.8.
Emerald DAT Autoloader                            0327, 0330, 0331, 0351
Exabyte EXB-018 3                                 (Under review)
Hewlett-Packard  C1553A                           9401, 9403, 9406
Hewlett-Packard  SureStore Tape 12000e/C1561A     9403, 9406, 9503
Lago LS-340 2                                     6.2 (Under review) 
Legacy DAT Changer 48                             0451, 0454
Micro Design International   SE2000DC             9403, 9406                
Mountain DAT AutoChanger                          0413, 0414, 0420, 0421,
						  0451, 0454
Palindrome FAST 2000 AutoLoader                   0413, 0414, 0420,
						  0421, 0451, 0454
Palindrome FAST 2000C AutoLoader                  0413, 0414, 0420,
						  0421, 0451, 0454
Palindrome FAST 2000TC Turbo AutoLoader           0413, 0414, 0420, 0421, 
						  0451, 0454, 0458
Spectra 4000 (using HP C1533A) [3]                1.02, 2.0 (Under review)
Storage Tek 9704 [2]                              6.2 (Under review)
TapeWorks MiniChanger 400                         0.15
WangDAT LD4-3200                                  1.2, 2.0, 02.2


8mm                                             Firmware Supported
---                                             ------------------
ADIC VLS 8mm 2                                    2.10
Conner 10L-HS                                     2.6, 3.0.240, 3.1.1, 
						  3.1.24
Contemporary Cybernetics CY-CHS10i                2.6, 3.0.240, 3.1.1, 
						  3.1.24
Emeritus TapeWare/VTL-50gb                        2.6, 3.0.240, 3.1.1,
						  3.1.24
Exabyte EXB-10i Cartridge Handling Subsystem      2.6, 3.0.240, 3.1.1, 
						  3.1.24
Exabyte EXB-10e Cartridge Handling Subsystem      1.1.6, 1.2.33, 1.2.185
Exabyte EXB-10h Cartridge Handling Subsystem      1.5.1
Exabyte EXB-60 Cartridge Handling Subsystem [3]   3.4, 3.7
Exabyte EXB-120 Cartridge Handling Subsystem [3]  3.4.61
Exabyte EXB-210 Cartridge Handling Subsystem [3]  2.12.1, 3.1.36
Exabyte EXB-440 Cartridge Handling Subsystem [3]  3.1.8
Exabyte EXB-480 Cartridge Handling Subsystem [3]  3.1.8
Lago LS/380L DataWheel                            4.9, 5.2 
Legacy Autoloader 50                              1.2.185
Maynard MaynStream 10L-HS                         2.6, 3.0.240, 3.1.1,
						  3.1.24
Palindrome FAST 5000 AutoLoader                   2.6, 3.0.240, 3.1.1, 
						  3.1.24
Palindrome FAST 5000C AutoLoader                  1.1.6, 1.2.33, 1.2.185
QualStar TLS-42xx/44xx/46xx     [3,8]             (Under review)
SpectraLogic STL-6000 [2]                         1.85, 1.89, 1.90
SpectraLogic STL-8000 [2]                         1.85, 1.89, 1.90
Spectra 9000  [3,8]                               (Under review)
Storage Tek 9708   [2,8]                          4.9, 5.2, 6.1
Storage Tek 9711  [2,8]                           6.1

		    
Digital Linear Tape (DLT)                       Firmware Supported
-------------------------                       ------------------
Breece Hill Q7
Cipher L860                                       430E, 4314
Conner TZ867                                      4314, 4316
Conner TZ877                                      930A, 9410
Digital Equipment Corporation TZ867/TZ86-VA       4314, 4316
Digital Equipment Corporation TZ875/TZ875N        930A, 9410, 9514 
Digital Equipment Corporation TZ877               930A, 9514 
Digital Equipment Corporation TZ885               (Under review) 
Digital Equipment Corporation SZ107               930A, 9514
Digital Equipment Corporation DLT2500             930A, 9514 
Digital Equipment Corporation DLT2700             930A, 9514
Quantum DLT4500                                   (Under review)
Quantum DLT4700                                   (Under review)
StorageWorks SWXTL-BL,BM                          930A, 9410, 9514
StorageWorks SWXTL-BR,BP                          930A, 9514


OPTICAL DRIVES

Rewriteable/Multifunction/Worm 
------------------------------
Hewlett Packard C1716C
Hewlett Packard C1716T
IBM 0632ACA
IBM MTA 3127
IBM MTA 3230 
IBM 0632-CBD (Under review)
Maxoptix Tahiti I
Maxoptix Tahiti III T3-1300
Micro Design International 300R
Micro Design International 600MX
Micro Design International SE1000M
Micro Design International SE1300MX
Micro Design International SE128RH
Micro Design International SE230RH
Mitshita 7010
Panasonic LF-7010
Panasonic LF-7300
Panasonic LF-9000
Panasonic LS-5300A (Under review)
Pinnacle Micro PMO-650
Pinnacle Micro PMO-1300
Pinnacle Sierra 1.3GB  OHD-1300
Pinnacle Tahoe 230MB
Plasmon Data Systems RF-6800e
Plasmon Data Systems RF-6800i
Plasmon Data Systems RF-7010
Plasmon Data Systems RF-7010i
Plasmon Data Systems RF-7010X 
Plasmon Data Systems RF-7030e
Plasmon Data Systems RF-7030i
Ricoh RO-5031E HyperSpace
Ricoh RS-9200EX HyperSpace
Sharp JY-800  (Under review)
Sony SMO-C501-00G
Sony SMO-E502
Sony SMO-F521
Sony SMO-F331 
Sony WWD-931 


OPTICAL JUKEBOXES

Rewriteable/Multifunction
-------------------------
Hewlett Packard Model 10C  (C1713C) [2]
Hewlett Packard Model 10LC (C1718C)
Hewlett Packard Model 20LT (C1718T)
Hewlett Packard Model 20XT (C1100A)
Hewlett Packard Model 20T  (C1713T) [2]
Hewlett Packard Model 20C  (C1710C) [2]
Hewlett Packard model 40ST [2]  (Under review)
Hewlett Packard Model 40T  (C1700T) [2]
Hewlett Packard Model 60C  (C1714C) [2]
Hewlett Packard Model 100C  (C1715C) [2]
Hewlett Packard Model 120T  (C1704T) [2]
Hewlett Packard Model 200T  (C1705T) [2]
IDE MLS-LG-5
IDE PLS 7100
IDE 9000 [3]
Maxoptix Axxis [2]
Maxoptix  MaxLyb 6.5
Maxoptix  MaxLyb 13
Maxoptix  MaxLyb 26
Maxoptix  MaxLyb 52 [2]
Maxoptix  MaxLyb 60 [2]
Micro Design International LB  Library 5-5
Micro Design International LB Library 5-25  [2]
Micro Design International LB Library 5-16D
Micro Design International LB Library 5-10
Micro Design International LB Library 5-16
Micro Design International LB Library 5-88  [2]
Micro Design International LB Library 5-144  [2]
Micro Design International  SEL6DX
Micro Design International  SEL20DX 
Micro Design International  SEL20MX
Micro Design International  SEL41MX [2]
Micro Design International  SEL114MX [2]
Micro Design International  SEL187MX [2]
NKK N-520   [3]
Pinnacle Micro PMO-10GB
Pinnacle Micro PMO-20GB [2]
Pinnacle Micro PMO-60GB [2]
Pinnacle Micro PMO-94GB [2]
Pinnacle ALTA
Pinnacle ASPEN [2]
Pinnacle ALPINE [2]
Pinnacle MAMMOTH [2]
Plasmon Data Systems RF-10J
Plasmon Data Systems RF-llJM
Plasmon Data Systems RF-20JM
Plasmon Data Systems RF-25JM [2]
Plasmon Data Systems RF-40JM [2]
Plasmon Data Systems RF-50JM [2]
Plasmon Data Systems Multi I [2]
Plasmon Data Systems Multi II [2]
Plasmon Data systems Multi III [2]
Ricoh HyperSpace Shuttle
Sony  OSL-2000-10  (Under review)
Sony  OSL-2000-20 [2]  (Under review)
StorageWorks SWXOW-JA
StorageWorks SWXOW-JB

SCSI HOST ADAPTERS

ISA/EISA
--------
Adaptec AHA-1510
Adaptec AHA-1510A
Adaptec AHA-1520
Adaptec AHA-1522
Adaptec AHA-1530  (Under review)
Adaptec AHA-1540B
Adaptec AHA-1540C
Adaptec AHA-1540CF
Adaptec AHA-1542B
Adaptec AHA-1542C
Adaptec AHA-1542CF
Adaptec AHA-1740
Adaptec AHA-1740A
Adaptec AHA-1742
Adaptec AHA-1744
Adaptec AHA-2740
Adaptec AHA-2740A
Adaptec AHA-2740AT
Adaptec AHA-2740W  (Under review)
Adaptec AHA-2742 
Adaptec AHA-2742A 
Adaptec AHA-2742AT 
Adaptec AHA-2742W  (Under review)
Adaptec AHA-2840  (Under review)
Always IN-2000
Always AL-6000    (Under Review)
BusLogic BT-445C
BusLogic BT-445S
BusLogic BT-520
BusLogic BT-540CF
BusLogic BT-542B
BusLogic BT-542D 
BusLogic BT-545C
BusLogic BT-742A
BusLogic BT-746C 
BusLogic BT-747C                   
BusLogic BT-747D
BusLogic BT-757D
BusLogic BT-757S 
Compaq CPQ 94
Compaq CPQ 710
DPT SK 2011/90
DPT SK 2011/95
DPT SK 2012B/90
DPT SK 2012B/95
DPT PM 2021
DPT PM 2022 [6]      
DPT PM 2122 [6]      
Palindrome HAC-1510-A16
Palindrome HAC-1540B-A16
Palindrome HAC-1740-E16
ProComp  Pro-Master
Storage Dimensions SDC 3222B
Storage Dimensions SDC 3222F
Storage Dimensions SDC 1602B
Storage Dimensions SDC 1602F
Storage Dimensions SD 542


MCA/PCI
-------
Adaptec AHA-1640
Adaptec AHA-2940  [SCSI 2 Fast PCI]
Adaptec AHA-2940W  [SCSI 2 Fast -Wide PCI]   (Under review)
BusLogic BT-640A
BusLogic BT-646S 
BusLogic BT-646D
BusLogic BT-946C   [SCSI 2 Fast PCI]
IBM 84F8009  w/o cache  
IBM 66G1086 w/o cache   
IBM 84F8014 w/ cache    
IBM 61G2975 w/ cache   
IBM 82G2674   wide SCSI
IBM 53G0381   [SCSI 2 Fast PCI]  
Palindrome HAC-1640-M16
Palindrome HAC-640A-M16
Storage Dimensions SDC 3211B 
Storage Dimensions SDC 3211F

OTHER HOST ADAPTERS

Compaq ProLiant 1000
Compaq ProSigna
HP NetServer - LM Series
HP NetServer  - LS Series
IBM Host via Emprise Stage3  [4]
IBM Model 85 Server Family
NetFRAME SCSI IOP [7]
Tricord IIOP
Tricord Enhanced IIOP


[2]   Requires Palindrome Multi-Drive Autoloader software

[3]   For configurations using more than one drive, refer to #2 above

[4]   Contact Emprise for specific configuration information
[5]   Support provided with updated drivers available via Palindrome
      BBS
[6]   Does not support hard drive mirroring with Novell 3.11
[7]   Support of Novell 3.12 and 4.0x via update drives on Palindrome
      BBS
[8]   Using latest version of drive firmware
[9]   Power cycle unit after changing tapes


Note:  Because of hardware timing and operating system variations,
Palindrome recommends not attaching sequential media devices to the
same physical SCSI adapter used to control system hard drives 

Refer to Palindrome Tested Device Driver Configurations List for
SCSI adapter driver specific names and dates.
