[ver]
	4
[sty]
	
[files]
[charset]
	82
	ANSI (Windows, IBM CP 1252)
[revisions]
	0
[sequence]
	11
	0
	0
	0
	23
	3
	Numbered list
	0
	Bullet
	0
	Indnt bullet
	0
	Indnt caution
	0
	Indnt tip
	0
	Indnt note
	0
	Caution
	0
	Tip
	0
	Note
	0
	Browse
	0
	Keyword
	0
	Context
	0
	Title
	0
	Macros
	0
	Alink
	0
	Butnbar
	0
	Window
	0
	Win95 macros
	0
	Win31 macros
	0
	Build tag
	0
	_COND_IF
	0
	_COND_ELSE
	0
	_COND_ENDIF
[prn]
	PostScript Printer
[port]
	LPT3:
[lang]
	1
[fldnames]
	Field1
	Field2
	Field3
	Field4
	Field5
	Field6
	Field7
	Field8
[desc]
	
	
	
	
	
	801506550
	63
	780270025
	2075
	11
	0
	0
	0
	0
	
	
	
	
	
	
	1
[fopts]
	0
	1
	0
	0
	
	
[lnopts]
	2
	Body Text
	1
[docopts]
	5
	2
[GramStyle]
	
[ParaNum]
	1
[tag]
	Body Text
	2
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Ahead
	3
	[fnt]
		Arial
		220
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		240
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		2160
		3
		0
		1
		1
		1
		65
		10
		1
	[spec]
		0
		1
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead title
	4
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		79
		0
		3
		100
	[brk]
		80
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Chead title
	5
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead
	6
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		180
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Chead
	7
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Numbered list
	8
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		300
		300
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		5
		<*:>.
		0
		3
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Numbered list
	0
	0
[tag]
	1st lev para
	9
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		68
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	1st lev para
	0
	0
[tag]
	Bullet
	11
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		120
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Bullet
	2
	1
	160
	1
	400
	0
[tag]
	Indnt bullet
	12
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		420
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		16
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Indnt bullet
	0
	0
[tag]
	2nd lev para
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		600
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	2nd lev para
	0
	0
[tag]
	See also prnt
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also prnt
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Book art
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Book art
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Callout text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Callout text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Figure title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		40
		60
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Figure title
	0
	0
[tag]
	Chapter title
	0
	[fnt]
		Arial
		280
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		300
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Chapter title
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	1st pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	1st pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Right pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Right pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Left pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Left pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Table title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		60
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		7
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Table title
	0
	0
[tag]
	Table col hd
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		4
	[line]
		10
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		6
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table col hd
	0
	0
[tag]
	Table Text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table Text
	0
	0
[tag]
	See also hlp
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		40
		4
		180
		0
		3
		100
	[brk]
		96
	[line]
		9
		0
		3
		0
		1
		1
		1
		70
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	0
	120
[tag]
	See also btn
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		240
	[spc]
		24
		200
		4
		0
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Crossref
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		513
		3
		0
		300
		600
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Crossref
	0
	0
[tag]
	Indnt caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt caution
	0
	0
[tag]
	Indnt tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		324
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt tip
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Indnt note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt note
	0
	0
[tag]
	Caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Caution
	0
	0
[tag]
	Tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		324
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Tip
	0
	0
[tag]
	Note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Note
	0
	0
[tag]
	Mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		48
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Indnt mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		300
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Dhead
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		4
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Parameter
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Parameter
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Formula
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Formula
	0
	0
[tag]
	Browse
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		+
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Browse
	0
	0
[tag]
	Keyword
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		K
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Keyword
	0
	0
[tag]
	Context
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		#
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Context
	0
	0
[tag]
	Title
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		$
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Title
	0
	0
[tag]
	Macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		!
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Macros
	0
	0
[tag]
	Footnote
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		244
		0
	[spc]
		40
		2400
		3
		0
		0
		1
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		256
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Footnote
	0
	0
[tag]
	Alink
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		A
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Alink
	0
	0
[tag]
	Butnbar
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		0
		0
		3
		100
	[brk]
		48
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		\li-140 
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Butnbar
	0
	0
[tag]
	Window
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		>
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Window
	0
	0
[tag]
	Win95 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		W
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win95 macros
	0
	0
[tag]
	Win31 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		X
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win31 macros
	0
	0
[tag]
	Build tag
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		*
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Build tag
	0
	0
[tag]
	_COND_IF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		IF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ELSE
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ELSE
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ENDIF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ENDIF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[frm]
	14
	1572932
	960
	1160
	9429
	8407
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	8
	0
	0
	65280 31743
	[frmlay]
		9119
		8469
		3
		0
		0
		3
		1160
		0
		0
		2
		0
		0
		0
		0
		1
		840
		11400
		0
	[tbl]
		 8 3 200 86 3423 86 1 43 43
		[h]
			 0 210 86 2 0 3 0
			 1 864 86 2 0 1 0
			 2 633 86 2 0 1 0
			 3 844 86 2 0 1 0
			 4 1055 86 2 0 1 0
			 5 800 86 2 0 1 0
			 6 844 86 2 0 1 0
			 7 1266 86 2 0 1 0
		[e]
		[w]
			 0 1468 360 6 0
			 1 1934 360 6 0
			 2 3944 360 6 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@<+!>Parameter<-!>

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@<+!>Default Value<-!>

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@<+!>Explanation<-!>

>
			 1 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>drivername

>
			 1 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>elnkii$ or elnkii<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$

>
			 1 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><+!><:f180,,0,0,0>Required<-!><:f180,,0,0,0>. Identifies network interface card. elnkii$ identifies first card; elnkii<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$ identifies additional card where 
<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0> is 2 for second card, and so on.

>
			 2 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>interrupt 

>
			 2 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>3

<:S+-1>

>
			 2 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Indicates interrupt level of card. Value is integer from 2 to 5. On 286 and 386 computers, interrupt 9 is the same as 2.

>
			 3 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>ioaddress

>
			 3 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>300H

>
			 3 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Indicates the input-output address of network interface card; should match card's switch settings. Value is hexadecimal from 250H to 350H.

>
			 4 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>maxtransmits

>
			 4 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>8

>
			 4 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Indicates number of transmit queue entries for network interface card. For server, this value equals size of transmit window times max. number of sessions. Value is integer from 8 to 50.

>
			 5 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>netaddress

>
			 5 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><+!><:f180,,0,0,0>-

>
			 5 2 0 0 0 0 0 1 0 0 0 0
Overrides network address of card or driver; for use in cases where network has duplicate addresses. Value is 12-digit hexadecimal string enclosed in quotation marks.

>
			 6 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>transceiver

>
			 6 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><+"><:f180,,0,0,0>onboard

>
			 6 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Determines the kind of Ethernet media you are using: onboard (for thin Ethernet - BNC Connector) or External (for thick Ethernet - DIX Connector).

>
			 7 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>xmitbufs

>
			 7 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>2

>
			 7 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Indicates number of transmit buffers to allocate on network interface card. Allocating second transmit buffer may improve transmit performance although it reduces amount of memory available for storing received packets. Value is integer from 1
 to 2.

>
		[e]
	[tble]
[frm]
	10
	1572932
	960
	8765
	9446
	11617
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	10
	1
	0
	65280 31743
	[frmlay]
		9299
		8486
		3
		0
		0
		3
		8765
		0
		0
		2
		0
		0
		0
		0
		1
		1020
		11580
		0
	[tbl]
		 3 3 200 86 3423 86 1 43 43
		[h]
			 0 210 86 2 0 3 0
			 1 1286 86 2 0 1 0
			 2 1055 86 2 0 1 0
		[e]
		[w]
			 0 1468 360 6 0
			 1 2215 360 6 0
			 2 3944 360 6 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Parameter

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@Default Value

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@Explanation

>
			 1 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>drivername

>
			 1 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>elnk16$ or elnk16<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$

>
			 1 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><+!><:f180,,0,0,0>Required<-!><:f180,,0,0,0>. Identifies network interface card. elnk16$ identifies first card; elnki16<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$ identifies additional card where 
<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0> is 2 for second card, and so on. iobase 300H indicates the input-output base address of network interface card. Value is hexadecimal 200H to 3F0H.

>
			 2 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>netaddress<:f><:f180,,0,0,0> 

>
			 2 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>-

<:S+-1>

>
			 2 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Overrides network address of network interface card, for use in cases where a network has duplicate addresses. Value is 12-digit hexadecimal string enclosed in quotation marks. For example, "02608C010001".<:f>

>
		[e]
	[tble]
[frm]
	10
	1572932
	720
	1160
	9206
	5584
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	11
	2
	0
	65280 31743
	[frmlay]
		9479
		8486
		3
		0
		0
		3
		1160
		0
		0
		2
		0
		0
		0
		0
		1
		1200
		11760
		0
	[tbl]
		 5 3 200 86 3423 86 1 43 43
		[h]
			 0 210 86 2 0 3 0
			 1 1286 86 2 0 1 0
			 2 1055 86 2 0 1 0
			 3 800 86 2 0 1 0
			 4 600 86 2 0 1 0
		[e]
		[w]
			 0 1468 360 6 0
			 1 2249 360 6 0
			 2 3944 360 6 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Parameter

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@Default Value

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@Explanation

>
			 1 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>drivername

>
			 1 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>elnkmc$ or elnkmc<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$

>
			 1 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><+!><:f180,,0,0,0>Required<-!><:f180,,0,0,0>. Identifies network interface card. elnk16$ identifies first card; elnkimc<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0>$ identifies additional card where 
<+"><:f180,,0,0,0>n<-"><:f180,,0,0,0> is 2 for second card, and so on. iobase 300H indicates the input-output base address of network interface card. Value is hexadecimal 200H to 3F0H.

>
			 2 0 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>maxtransmits<:f><:f180,,0,0,0> 

>
			 2 1 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>12

<:S+-1>

>
			 2 2 8 0 0 0 0 1 0 0 0 0
<+@><:I0,0,0,0><:S+-1><:f180,,0,0,0>Indicates number of transmit queue entries for network interface card. For server, this value equals the size of transmit window time maximum number of sessions. Value is integer from 8 to 50.<:f>

>
			 3 0 0 0 0 0 0 1 0 0 0 0
netaddress

>
			 3 1 0 0 0 0 0 1 0 0 0 0
-

>
			 3 2 0 0 0 0 0 1 0 0 0 0
Overrides network address of network interface card, for use in cases where network has duplicate addresses. Value is 12-digit hexadecimal string enclosed in quotation marks.

>
			 4 0 0 0 0 0 0 1 0 0 0 0
slotnumber

>
			 4 1 0 0 0 0 0 1 0 0 0 0
<+">Default is lowest slot number with elnkmc<-">

>
			 4 2 0 0 0 0 0 1 0 0 0 0
Required for second elnkmc card. Second card must be in higher slot number. Value is integer from 1 to 8.

>
		[e]
	[tble]
[frm]
	10
	1573060
	960
	960
	9446
	6658
	0
	1
	1
	1 0 0 0 0 0 0
	0
	16777215
	12
	3
	0
	65280 31743
	[frmlay]
		12483
		8486
		1
		0
		0
		1
		960
		0
		0
		2
		0
		0
		0
		0
		1
		984
		6456
		0
	[tbl]
		 11 3 200 86 1440 0 1 43 43
		[h]
			 0 210 86 18 0 3 0
			 1 600 86 2 0 1 0
			 2 800 86 2 0 1 0
			 3 1000 86 2 0 1 0
			 4 1000 86 2 0 1 0
			 5 600 86 2 0 1 0
			 6 1800 86 2 0 1 0
			 7 400 86 2 0 1 0
			 8 800 86 2 0 1 0
			 9 400 86 2 0 1 0
			 10 800 86 2 0 1 0
		[e]
		[w]
			 0 1602 0 2 0
			 1 2608 0 2 0
			 2 4345 0 2 0
		[e]
		[data]
			 0 0 0 0 0 0 4352 1 0 0 0 0
@Table col hd@Parameter

>
			 0 1 0 0 0 0 4352 1 0 0 0 0
@Table col hd@Default Value

>
			 0 2 0 0 0 0 4352 1 0 0 0 0
@Table col hd@Explanation

>
			 1 0 0 0 0 0 0 1 0 0 0 0
drivername

>
			 1 1 0 0 0 0 0 1 0 0 0 0
ibmtok$ or ibmtokn$

>
			 1 2 0 0 0 0 0 1 0 0 0 0
Required. Identifies network interface card. ibmtok$ identifies first card; ibmtokn$ identifies additional card where n is 2 for second card, and so on.

>
			 2 0 0 0 0 0 0 1 0 0 0 0
maxtransmits

>
			 2 1 16 0 0 0 0 1 0 0 0 0
<+A>6

>
			 2 2 0 0 0 0 0 1 0 0 0 0
Indicates number of transmit queue entries for network interface card. For server, this value equals size of transmit window times maximum number of sessions. Value is integer from 6 to 50.

>
			 3 0 0 0 0 0 0 1 0 0 0 0
netaddress

>
			 3 1 0 0 0 0 0 1 0 0 0 0
-

>
			 3 2 0 0 0 0 0 1 0 0 0 0
Overrides network address of card or driver, for us in cases where a network has duplicate addresses. Value is 12-digit hexadecimal string enclosed in quotation marks. For strict IBM compatibility, only use digits 1-9.

>
			 4 0 0 0 0 0 4096 1 0 0 0 0
primary or alternate

>
			 4 1 0 0 0 0 4096 1 0 0 0 0
-

>
			 4 2 0 0 0 0 4096 1 0 0 0 0
Identifies driver assignments when using multiple cards. Remember to set different ROM addresses for each card. For detailed setting information for specific IBM Token Ring cards, see the documentation.

>
			 5 0 0 0 0 0 4096 1 0 0 0 0
product_id

>
			 5 1 0 0 0 0 4096 1 0 0 0 0
0110F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0F0

>
			 5 2 0 0 0 0 4096 1 0 0 0 0
Identifies specific network interface card. Value is string of up to 35 hexadecimal digits and must be an even number.

>
			 6 0 0 0 0 0 4096 1 0 0 0 0
ram (Adapter and Adapter II only)

>
			 6 1 0 0 0 0 4096 1 0 0 0 0
location immediately following read-only memory (ROM) on next appropriate boundary

>
			 6 2 0 0 0 0 4096 1 0 0 0 0
Indicates physical random access memory (RAM) location on network interface card if default location does not suffice. Value is hexadecimal number A000 - F000, located on an 8K boundary for Token Ring Adapter or 16K boundary for Token Ring Adapter II. For s
trict IBM compatibility, set primary RAM value to 0xD800 and alternate RAM value to 0xD400. For detailed setting information for specific IBM Token Ring cards, see the card documentation.

>
			 7 0 0 0 0 0 4096 1 0 0 0 0
recvbufs

>
			 7 1 16 0 0 0 4096 1 0 0 0 0
<+A>2

>
			 7 2 0 0 0 0 4096 1 0 0 0 0
Indicates number of receive buffers to use. Value is integer from 2 to 60.

>
			 8 0 0 0 0 0 4096 1 0 0 0 0
recvbufsize

>
			 8 1 16 0 0 0 4096 1 0 0 0 0
<+A>256

>
			 8 2 0 0 0 0 4096 1 0 0 0 0
Indicates size of receive buffers in bytes. Value is multiple of 8, from 256 to 17952. For detailed setting information for specific IBM Token Ring cards, see the card documentation.

>
			 9 0 0 0 0 0 4096 1 0 0 0 0
xmitbufs

>
			 9 1 16 0 0 0 4096 1 0 0 0 0
<+A>1

>
			 9 2 0 0 0 0 4096 1 0 0 0 0
Indicates number of transmit buffers to allocate. Value is integer 1 or 2.

>
			 10 0 0 0 0 0 4096 1 0 0 0 0
xmitbufsize

>
			 10 1 0 0 0 0 4096 1 0 0 0 0
-

>
			 10 2 0 0 0 0 4096 1 0 0 0 0
Indicates size of transmit buffers in bytes. Value is a multiple of 8, from 256 to 17952. For detailed setting information for specific IBM Token Ring cards, see the card documentation.

>
		[e]
	[tble]
[frm]
	4
	1573060
	720
	7768
	9180
	10395
	0
	1
	1
	1 0 0 0 0 0 0
	0
	16777215
	14
	4
	5376
	0 15872
	[frmlay]
		2099
		8460
		1
		0
		0
		1
		7768
		0
		0
		2
		0
		1
		1
		0
		1
		1164
		9362
		0
	[tbl]
		 9 4 200 86 2026 86 1 43 43
		[h]
			 0 210 86 2 0 4 0
			 1 200 86 2 0 4 0
			 2 200 86 2 0 4 0
			 3 200 86 2 0 4 0
			 4 200 86 2 0 4 0
			 5 200 86 2 0 4 0
			 6 200 86 2 0 4 0
			 7 200 86 2 0 4 0
			 8 200 86 2 0 4 0
		[e]
		[w]
			 0 2242 360 6 0
			 1 1541 360 6 0
			 2 1667 360 6 0
			 3 1527 360 6 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Network interface card

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@Vendor

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@Driver file name

>
			 0 3 0 0 0 0 0 1 0 0 0 0
@Table col hd@Network media

>
			 1 0 0 0 0 0 0 1 0 0 0 0
EtherLink II</n> (3C503)

>
			 1 1 0 0 0 0 0 1 0 0 0 0
3Com

>
			 1 2 0 0 0 0 0 1 0 0 0 0
elnkii.os2

>
			 1 3 0 0 0 0 0 1 0 0 0 0
Ethernet

>
			 2 0 0 0 0 0 0 1 0 0 0 0
EtherLink</n> 16 (3C507)

>
			 2 1 0 0 0 0 0 1 0 0 0 0
3Com

>
			 2 2 0 0 0 0 0 1 0 0 0 0
elnk16.os2

>
			 2 3 0 0 0 0 0 1 0 0 0 0
Ethernet

>
			 3 0 0 0 0 0 0 1 0 0 0 0
EtherLink/MC (3C523)

>
			 3 1 0 0 0 0 0 1 0 0 0 0
3Com

>
			 3 2 0 0 0 0 0 1 0 0 0 0
elnkmc.os2

>
			 3 3 0 0 0 0 0 1 0 0 0 0
Ethernet

>
			 4 0 0 0 0 0 0 1 0 0 0 0
Token Ring II

>
			 4 1 0 0 0 0 0 1 0 0 0 0
IBM

>
			 4 2 0 0 0 0 0 1 0 0 0 0
ibmtok.os2

>
			 4 3 0 0 0 0 0 1 0 0 0 0
Token Ring

>
			 5 0 0 0 0 0 0 1 0 0 0 0
Token Ring 16/4, A

>
			 5 1 0 0 0 0 0 1 0 0 0 0
IBM

>
			 5 2 0 0 0 0 0 1 0 0 0 0
ibmtok.os2

>
			 5 3 0 0 0 0 0 1 0 0 0 0
Token Ring

>
			 6 0 0 0 0 0 0 1 0 0 0 0
P1392

>
			 6 1 0 0 0 0 0 1 0 0 0 0
Proteon</n>

>
			 6 2 0 0 0 0 0 1 0 0 0 0
ndis39xr.os2

>
			 6 3 0 0 0 0 0 1 0 0 0 0
Token Ring

>
			 7 0 0 0 0 0 0 1 0 0 0 0
P1892

>
			 7 1 0 0 0 0 0 1 0 0 0 0
Proteon

>
			 7 2 0 0 0 0 0 1 0 0 0 0
ndis89xr.os2

>
			 7 3 0 0 0 0 0 1 0 0 0 0
Token Ring

>
			 8 0 0 0 0 0 0 1 0 0 0 0
P1990

>
			 8 1 0 0 0 0 0 1 0 0 0 0
Proteon

>
			 8 2 0 0 0 0 0 1 0 0 0 0
ndis990r.os2

>
			 8 3 0 0 0 0 0 1 0 0 0 0
Token Ring

>
		[e]
	[tble]
[lay]
	Standard
	1031
	[rght]
		12960
		10166
		1
		960
		1200
		3
		960
		720
		0
		1
		0
		1
		0
		2
		1
		960
		9446
		1
		1
		3120
	[lft]
		12960
		10166
		1
		720
		1200
		3
		960
		960
		0
		1
		0
		1
		0
		2
		1
		720
		9206
		1
		1
		3120
	[hlft]
	[lyfrm]
		1
		3008
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		3
	[frmlay]
		960
		10166
		1
		720
		180
		3
		0
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		2
		4674
	[txt]

>
	[hrght]
	[lyfrm]
		1
		11200
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		1
	[frmlay]
		960
		10166
		1
		900
		180
		3
		0
		780
		0
		1
		0
		1
		1
		0
		1
		900
		9386
		1
		2
		4674
	[txt]

>
	[flft]
	[lyfrm]
		1
		5056
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		4
	[frmlay]
		12960
		10166
		1
		720
		480
		3
		11940
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		3
		9900
	[txt]
@Left pg foot@<+@><:R1,1,3,8486,><:P19999,0,2->  Network Configuration Guide	Lotus Confidential

>
	[frght]
	[lyfrm]
		1
		13248
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		2
	[frmlay]
		12960
		10166
		1
		900
		480
		3
		11940
		780
		0
		1
		0
		1
		1
		0
		1
		900
		9386
		1
		3
		9900
	[txt]
@Right pg foot@<+@><:R1,1,3,8460,>Lotus Confidential	Running Lotus Notes on AppleTalk  <:P19999,0,2->

>
[elay]
[l1]
	0
[pg]
	11
	21 0 85 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	37 0 7 512 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	67 0 61 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	89 0 50 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	108 0 67 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	126 0 0 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	130 0 5 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 3 0 0
	135 0 5 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 5 0 0
	143 506 98 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	165 200 107 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	196 0 0 1025 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
[edoc]
@Chapter title@<:s><:#300,8486>Chapter 2 Running Lotus Notes on Apple Talk

@See also prnt@<:#600,8486>This chapter explains how to install and configure Lotus Notes AppleTalk software to enable communication between Notes servers for OS/2, Notes servers for Windows NT, and Notes Macintosh workstations.

@Ahead@<:#240,8486>About Notes and AppleTalk

<:s><:R1,1,1,5760,><:#400,8486>Notes servers and workstations use the Notes AppleTalk port driver to communicate on an AppleTalk network. These Notes servers and workstations can run on AppleTalk:

@Bullet@<:s><:R1,1,1,5760,><:#200,8486>OS/2 server

@Bullet@<:s><:R1,1,1,5760,><:#200,8486>Windows NT server

@Bullet@<:s><:R1,1,1,5760,><:#200,8486>Macintosh workstation

<:R><:#600,8486>Notes AppleTalk workstations on one type of network can communicate with Notes AppleTalk servers on other types of networks through AppleTalk routers that connect the Notes server to Ethernet or Token Ring networks.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>COMMAND from a Macintosh workstation cancels any AppleTalk network transaction.

@Bullet@<:R1,1,1,1224,><:#800,8486>An AppleTalk entity name has three components: the object, type, and zone, used by the AppleTalk Name Binding Protocol (NBP). For a Notes server, the object is the first 32 characters of the common name (CN=) portion of the Notes server name; the type is "L
otus Notes 1"; the zone is the default zone of the AppleTalk network to which the server is connected.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Notes does not support more than one AppleTalk port on a Notes Server

@Bullet@<:R1,1,1,1260,><:#600,8486>AppleTalk Phase 1 and AppleTalk Phase 2 can run on the same AppleTalk network only if the network is using Phase 1 to Phase 2 transition routers. This configuration is recommended only for highly experienced network engineers.

@Bullet@<:R1,1,1,1224,><:#600,8486>On a Macintosh, to avoid down time if the home server is temporarily unavailable, you can specify a preferred backup home server by selecting the Chooser, selecting the Lotus Notes icon, selecting an AppleTalk zone, and selecting a Notes server.

@Ahead@<:s><:R><:#240,8486><-!>About running Notes and AppleTalk on OS/2<-!>

<:R1,1,1,5760,><:#400,8486>Lotus Notes AppleTalk software provides an OS/2 protocol stack and an AppleTalk application program interface (API) which allow the Notes OS/2 server to communicate with Notes Macintosh workstations.

<:R1,1,1,5760,><:#1000,8486>Notes AppleTalk can coexist on a Notes OS/2 server with other Notes-supported network protocols (such as NetBIOS, Banyan VINES, TCP/IP, and Novell NetWare SPX). To connect to Notes Macintosh workstations on Notes platforms that do not support AppleTalk prot
ocols (such as Windows and UNIX), you must install a separate network, such as Novell NetWare, and the appropriate protocol driver software supplied with Notes software.

<:R><:#600,8486>If you are installing Notes AppleTalk within a network operating system that supports the Network Driver Interface Specification (NDIS) standard, you may be able to use some of your existing hardware and software.

@Bhead@<:s><:R1,1,1,1224,><:#220,8486>System requirements

@Bullet@<:R1,1,1,1224,><:#600,8486>A PC running OS/2 Release 3 or 2.1 on the same Ethernet or Token Ring network as the Macintosh computers that are using Notes, or connected to the Macintosh computers through AppleTalk routers.

@Bullet@<:R1,1,1,1224,><:#400,8486>An NDIS-compliant network card and NDIS card driver software for the network card (sometimes called NDIS media access control (MAC) drivers).

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Lotus Notes Server CD-ROM which contains the following files particular to AppleTalk:

@Indnt bullet@<:R><:#400,8486>ATALK2V2.OS2  The Notes AppleTalk protocol driver for OS/2 Release 3 (Warp) and Release 2.x that communicates with a specified network interface card.

@Indnt bullet@<:s><:R1,5,1,0,1,360,1,360,1,720,1,1080,><:#200,8486>Notes AppleTalk protocol drivers support AppleTalk Phase 2.

@Indnt bullet@<:R><:#200,8486>ATALKINI.EXE   A daemon program for the Notes AppleTalk protocol driver.

@Indnt bullet@<:#200,8486>ATALK.DLL   AppleTalk application program interface (API) used by Notes.

@Indnt bullet@<:#400,8486>ATK.MSG   The warning and error messages used by the Notes AppleTalk protocol driver, daemon program, and dynamic link library (DLL). 

@Indnt bullet@<:#600,8486>NETBIND.EXE   A program that causes the Protocol Manager driver to bind the NDIS-compliant network protocol drivers to the NDIS network card drivers. The card drivers must be bound before applications can use the network protocols.

@Indnt bullet@<:#400,8486>PROTMAN.OS2  Protocol Manager 2.0, the Protocol Manager driver that associates the NDIS-compliant network protocol drivers with the NDIS card drivers.

@Indnt bullet@<:#400,8486>PRO.MSG   A message file that contains the status and error messages reported by the Protocol Manager.

@Indnt bullet@<:R1,1,1,1224,><:#600,8486>PROH.MSG   A file that contains detailed information about Protocol Manager errors. For additional information on an error, type HELP PROxxxx at the server console,  where xxxx is the error number that the Protocol Manager displays.

@Indnt bullet@<:R1,1,1,1224,><:#400,8486><-">TPAUSE.EXE  A delay program used by the STARTUP.CMD file for some configurations to allow time for the NDIS-compliant protocol driver and NDIS card drivers to bind.<-">

@Bhead@<:s><:R1,1,1,1224,><:#220,8486><-!>Network interface cards for Notes AppleTalk on an OS/2 Notes server<-!>

<:R><:#800,8486>To run AppleTalk on a Notes OS/2 server, requires fully supports NDIS-compliant Ethernet and Token Ring network interface cards. Drivers for NDIS cards are available from most network card manufacturers, from bulletin board or information systems, or as par
t of the LAN Manager network operating system.

<:#600,8486>To enable Notes AppleTalk users to communicate with a Notes AppleTalk server on another type of network, you use an AppleTalk router to connect the Notes server to the Ethernet or Token Ring network that contains the other server.

<:#200,8486>The following table lists the NDIS-compliant cards that have been tested with Notes:

<:s><:R1,1,1,1224,><:t4>

@Ahead@<:s><:R1,1,1,1224,><-"><:p<* >><-">Setting up Notes and AppleTalk on OS/2

<:R><:#400,8486><-!>These are the basic procedures you must follow to set up a Notes server for OS/2 to run AppleTalk after you install an NDIS-compliant network interface card on the server:<-!>

<:s><:#400,8486>print only: Steps 1-6 are described in detail in this Chapter. Steps 7-9 are described in the Administrator's Guide.

@Numbered list@<:#400,8486>Create directories for NDIS driver and AppleTalk files on the Notes server, and copy those files into those directories.

@Numbered list@<:#200,8486>Edit the CONFIG.SYS file on the Notes server.

@Numbered list@<:#200,8486>Edit the STARTUP.CMD file on the Notes server.

@Numbered list@<:#200,8486>Create the PROTCOL.INI file on the Notes server.

@Numbered list@<:s><:#200,8486>Configure the error log for Notes AppleTalk.

@Numbered list@<:s><:#200,8486>Restart the Notes server and launch the Notes workstation.

@Numbered list@<:s><:#200,8486>Enable the network port for AppleTalk on the Notes server.

@Numbered list@<:#400,8486>Include the network name in the Notes Server document on the Notes Name & Address book (NAMES.NSF).

@Numbered list@<:s><:#200,8486>Restart the Notes server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,1,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>See related topics: Error log (AG), Installing Protocol Manager 2.0 on a Notes server for OS/2, Enabling a network port (AG), Editing the Notes server N&A book

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,2,1
@Build tag@@EndSection

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Print refs: Chapter 3, Notes and networks- Administrator's Guide

@Bhead title@<:R><:#220,8486>Step 1: Creating NDIS and AppleTalk directories on the Notes OS/2 server

<:#400,8486>Make sure you have installed an NDIS-compliant network interface card on the Notes server before you perform this task.

@Numbered list@<:#400,8486>Create two directories on the Notes server. One will hold NDIS driver files, and the other will hold AppleTalk files. You can use any name for these directories.

@Numbered list@<:#200,8486>Copy the NDIS driver file(s) into the NDIS directory.

@Numbered list@<:#400,8486>Copy all the files from the ATALK directory on the Lotus Notes Server for OS/2 CD-ROM into the AppleTalk directory.

<:#200,8486>

@Bhead title@<:#220,8486>Step 2: Editing the CONFIG.SYS file

<:#400,8486>To set up the Protocol Manager and the Notes AppleTalk driver on a Notes server for OS/2, you must edit the CONFIG.SYS file on the server as follows.

@Numbered list@<:#200,8486>Back up the CONFIG.SYS file so that you can begin again if you make a mistake.

@Numbered list@<:#200,8486>Open the CONFIG.SYS file in a text editor.

@Numbered list@<:#400,8486>Edit the DPATH statement to include the directories that contain the files PRO.MSGPR, OH.MSG, and ATK.MSG.

@Numbered list@<:#200,8486>Edit the LIBPATH statement to include the directory containing the ATALK.DLL file.

@Numbered list@<:#400,8486>Add DEVICE statement(s) to identify the location of the Protocol Manager, the network interface card driver, and to install the AppleTalk driver.

@Numbered list@<:s><:#200,8486>Add a RUN statement that starts the AppleTalk driver.<-#><-#><-#><-#>

@Numbered list@<:s><:#200,8486>Save the file.

<:#200,8486>If you are running OS/2 Release 3, your CONFIG.SYS file might look like this:

<:#200,8486>yy add Release 3 example

<:#200,8486>If you are running OS/2 2.1, your CONFIG.SYS file might look like this:

<:#600,8486>rem network card driver<**>DEVICE = c:\atalk\atalk2v2.os2<**>RUN = c:\atalk\atalkini.exe

<:s><:#200,8486>

@See also prnt@<:#200,8486>

@Bhead title@<:#220,8486>Step 3: Editing the STARTUP.CMD file

<:#600,8486>Add two lines to the STARTUP.CMD file. One line binds the Notes AppleTalk protocol driver to the NDIS card driver. The second line specifies the amount of time AppleTalk has to initialize. 45 seconds is recommended.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>d:\atalk\netbind.exe<**>d:\atalk\tpause.exe 45<**>notes server

<:R><:#600,8486>The tpause parameter equals the number of seconds to pause. This example shows the recommended pause of 45 seconds. The line "notes server" starts the Notes server program automatically when the server is powered on.

<:#200,8486>

@Bhead title@<:#220,8486>Step 4: Creating the PROTOCOL.INI file

<:#800,8486>Create the PROTOCOL.INI file in the Notes AppleTalk files directory you specified in the CONFIG.SYS file. PROTOCOL.INI should contain sections that identify each network interface card and protocol driver installed on the server. Each section has a heading 
in brackets, followed by parameters that identify the driver name and other parameters specific to the network interface card.

@Numbered list@<:s><:#200,8486>Enter a section to configure the network interface card.

@Numbered list@<:s><:#200,8486>Enter a section to configure the AppleTalk protocol driver.

<:#400,8486>In addition to the DriverName, the section must include parameters for Bindings and Port Type. You can also enter optional AppleTalk Driver Parameters, as necessary.

<:#800,8486>This example uses Microsoft section names, including the convention of ending card section names with "_NIF" and protocol section names with "_XIF". There are two sections in this example. The first section configures a 3Com Etherlink II network card and th
e second section configures the AppleTalk protocol driver for a 3Com Etherlink II card.

@Mono@<:#1600,8486><[>ELNKII_NIF]<**>DriverName = ELNKII$<**>Interrupt = 3<**>IOAddress = 0x300<**><[>ATALK_XIF]<**>DriverName = ATALK$<**>Bindings = ELNKII_NIF<**>PortType = EtherTalk

<:s><:#200,8486>where:

<:#400,8486>DriverName identifies the card driver file name (excluding the extension), followed by a $. You entered the card driver file name in the CONFIG.SYS file when you installed the network interface card.

<:s><:#200,8486>Interrupt is the interrupt specified for the card.

<:#200,8486>IOAddress is the hexadecimal value for the card's input/output address.

<:#200,8486>DriverName is the protocol driver file name (excluding the extension) followed by a dollar sign.

<:s><:#200,8486>Bindings is the section name of the network card that AppleTalk should use.

<:#400,8486>PortType identifies the type of port. In this case, it is either EtherTalk</n> (AppleTalk on Ethernet) or TokenTalk</n> (AppleTalk on Token Ring).

@Ahead@<:s><:#240,8486>About optional AppleTalk driver parameters

<:#400,8486>You must define each network interface card that Notes AppleTalk supports by entering valid parameters and values in the PROTOCOL.INI file. This defines the card you are using with Notes AppleTalk.

@Note@<:R1,1,1,360,><:#400,8486>For information on card parameters and values, see your network interface card documentation, or the sample PROTOCOL.INI file usually provided with the NDIS driver software that comes with the card.

@Bhead@<:R><:#220,8486>Aarp Retries

<:#800,8486>About AarpRetries specifies the number of retries that the AppleTalk address resolution protocol (AARP) uses to acquire a unique AppleTalk address. This parameter is useful on large networks where nodes have difficulty acquiring unique AppleTalk addresses. 
The AARP protocol reconciles addressing conflicts in networks with multiple sets of protocols. Valid values are 15 to 900; the default value is 15.

<:#200,8486>AarpRetries = value

@Bhead@<:#220,8486>Ddpchecksums

<:#600,8486>About DdpChecksums specifies whether or not checksums are generated for transmitted packets. If present, checksums on received packets are always verified. Valid values are "yes" or "no"; the default is "no."

<:#200,8486>DdpChecksums = value

@Note@<:s><:R1,1,1,360,><:#600,8486>This parameter is not used to configure a Notes server for an AppleTalk network with one or more zones. For further information on how to configure a Notes server for an AppleTalk network with one or more zones, see "Troubleshooting" later in this chapter.

@Bhead@<:R><:#220,8486>DefaultZone

<:#1200,8486>About DefaultZone specifies the AppleTalk zone in which the Notes server will appear. Use this parameter if you do not want the Notes server to reside in the default zone on the connected AppleTalk network. The default zone is determined by a router on the 
AppleTalk network. By placing the DefaultZone=  statement in the PROTOCOL.INI file, you allow the Notes server to appear in a different zone than determined by the router. A valid value for this parameter is the name of any AppleTalk zone present on the con
nected AppleTalk network.

<:#200,8486>DefaultZone = zone name

<:R1,1,1,360,><:#400,8486>In order for this feature to work, the zone must exist on the network (appear in the Chooser on a Macintosh workstation), and must be accessible on the directly-connected network.

<:R><:#200,8486>Example: This PROTOCOL.INI file has set the default zone to Zone 2.

@Mono@<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#2200,8486><[>PROTMAN]<**>  DRIVERNAME = PROTMAN$<**><[>ELNKMC_NIF]<**>  DRIVERNAME = ELNKMC$<**>  MAXTRANSMITS = 40<**>  SLOTNUMBER = 4 
<**><[>ATALK2_XIF]<**>  Bindings = ELNKMC_NIF<**>  DriverName = ATALK$<**>  PortType = EtherTalk<**>  DefaultZone = "ZONE2" 

@Bhead@<:R1,1,1,360,><:#220,8486>PortName

<:R1,1,1,360,><:#1600,8486>About PortName allows you to set the registered AppleTalk name for Notes AppleTalk software. When the Notes AppleTalk driver software starts up, it automatically registers a default AppleTalk name (PacerTalk) on the network. This default name is not the Not
es OS/2 server name, although you can use the Notes OS/2 server name as the port name. AppleTalk names can contain up to 16 valid characters; invalid characters are: @ (at sign), : (colon), and " (quotation mark). If the name contains a space or starts with
 a number, you must enclose it in quotation marks. The protocol software automatically adds a number to the end of the name to ensure that it is unique on the network. The default value is "PacerTalk." 

<:R><:#200,8486>PortName = "port name"

@Bhead@<:#220,8486>RecvBufs

<:#400,8486>About RecvBufs - specifies the number of buffers AppleTalk uses to receive packets from the network. Each buffer uses 640 bytes of memory. Valid values are 8 to 20; the default value is 20. 

<:#200,8486>RecvBufs = value

@Bhead@<:s><:#220,8486>About Selectors

<:#1000,8486>About Selectors specifies the number of OS/2 global descriptor table (GDT) selectors that AppleTalk uses. Each configured selector uses one GDT entry and locks 64K of memory into physical memory, preventing it from being swapped out. Lowering this value con
serves memory and lowers the number of Macintosh computers that the Notes OS/2 server can support. Valid values are 4 to 100; the default value is 14. 

<:s><:#200,8486>Selectors = value

@See also prnt@<:#200,8486>See also XferBufs

@Bhead@<:#220,8486>XferBufs

<:#600,8486>About XferBufs specifies the number of buffers that the NDIS receive lookahead function uses when receiving a packet. Each buffer uses 640 bytes of memory. This parameter should be the same as RecvBufs. Valid values are 8 to 20; the default value is 20. 

<:#200,8486>XferBufs = value

@Bhead@<:#220,8486>XmitBufs

<:#400,8486>About XmitBufs - specifies the number of buffers that AppleTalk uses to transmit packets onto the network. Each buffer uses 640 bytes of memory. Valid values are 8 to 40; the default value is 20. 

<:#200,8486>XmitBufs = value<:>

<:#200,8486>

@Chead title@<:#200,8486>Example: AppleTalk parameters for the 3Com EtherLink II Card

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:t0>

@Chead title@<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Example:  AppleTalk parameters for the 3Com EtherLink 16 card

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:t1>

@Chead title@<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Example:  AppleTalk parameters for the 3Com EtherLink/MC card

@Bhead@<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:t2>

@Chead title@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Example:  AppleTalk parameters for the IBM Token Ring card

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#1200,8486>The IBMTOK.OS2 driver supports these IBM Token Ring cards<**>IBM Token Ring Adapter<**>IBM Token Ring Adapter II\<**>IBM Token Ring Adapter/ A<**>IBM Token Ring 16/4 Adapter<**>IBM Token Ring 16/4 Adapter/A

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:t3>

@Bhead title@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#220,8486><:><-!>Step 5: Configuring the error log for AppleTalk

<:R><:#600,8486>You can control how the AppleTalk software logs warning and error messages in the Notes error log on the Notes server. The way you specify these parameters depends upon whether your networking software is Lan Manager-derived or non-Lan Manager-derived.

@Chead@<:#200,8486>Configuring the error log for AppleTalk on Lan Manager networks

<:#800,8486>AppleTalk messages on a Lan Manager network are written to the network operating system error log. To view the error log, use the utility provided with the network operating system. For example, in Microsoft LAN Manager, the error log can be read with the N
ET ADMIN command or with the NET ERROR command.

@Numbered list@<:#400,8486>Open the file in a text editor: LANMAN.INI for Microsoft LAN Manager and DEC PATHWORKS; and  IBMLAN.INI for IBM Extended Edition, LAN Server, or LAN Requester.

@Numbered list@<:s><:#200,8486>Enter the following lines in the configuration file:

@Indnt mono@<:#600,8486><[>AppleTalk]<**>WarningFreq = 1<**>ErrorFreq = 1<:>\

<:#1200,8486>WarningFreq and ErrorFreq control the frequency with which warnings and errors are logged. Each different message is logged only as often as the WarningFreq or ErrorFreq value. For example, if ErrorFreq is 5, an error which occurs 12 times will be logged on
 the 1st, 6th and 11th occurrences. If six different errors each occurred once, all would be logged. Not logging every occurrence of an error can prevent the error log from filling up with repeated messages. These parameters should be set to 1 when troubles
hooting, and to a higher value for normal operation. ??why does our example set them to 1?

<:#1400,8486>Even under normal operation, the AppleTalk stack might log some warning and error messages. For example, if a router on the network is misconfigured for a while, the OS/2 AppleTalk stack might log error messages to indicate conflicting information on the ne
twork, even though the operation of the AppleTalk stack continues unaffected. As another example, the protocol stack might drop some packets when under a peak load. The AppleTalk protocols will usually recover from such a situation without the application e
ven noticing, and the resulting warning or error messages which are logged do not indicate a real problem.

<:s><:#200,8486>Valid values are 1-16535. The default is to log every 10th warning and every 10th error.

@Chead@<:#200,8486>Configuring the error log for AppleTalk on non-Lan Manager networks

<:R1,1,1,1080,><:#800,8486>Examples of these networks are Novell NetWare, Banyan VINES, and Notes servers that are running only AppleTalk. On these systems, you can specify AppleTalk error log parameters in the CONFIG.SYS file by using OS/2 environment variables with the SET command 
in the format: set AppleTalk_parameter. The parameters are described below and are not case sensitive.

@Chead@<:R1,1,1,1080,><:#200,8486>Example:  Lines from CONFIG.SYS:

@Mono@<:R1,1,1,1080,><:#400,8486>set AppleTalk_LogFile=c:\notes\atalk.log<**>set AppleTalk_LogFileSize=100

<:R1,1,1,1080,><:#600,8486>AppleTalk messages on non-Lan Manager networks are written to a plain-text file. By default, this is the file ATALK.LOG in the root directory of the boot drive (usually C:), but the file name can be overridden with the LogFile parameter described below.

<:R1,1,1,1080,><:#600,8486>LogFile applies only to non-LAN Manager networks. This option specifies the path and name of the file in which to log warning and error messages. The default is ATALK.LOG in the root directory of the boot drive.

@Chead@<:s><:R1,1,1,1080,><:#200,8486>Example: (Non-LAN Manager network):

@Mono@<:R1,1,1,1080,><:#200,8486>set AppleTalk_LogFile=c:\notefile\atalk.log

<:R1,1,1,1080,><:#1000,8486>LogFileSize applies only to non-LAN Manager networks. This option specifies the maximum size of the log file, in Kilobytes. When the log file reaches the maximum size, the AppleTalk software logs a message warning that the log is full, and no additional err
ors are logged to the file. To resume logging, delete the log file, or use a text editor to delete some entries. Valid values are 0-2000 (file size in Kilobytes). The default value is 80.

@Chead@<:s><:R1,1,1,1080,><:#200,8486>Example (Non-LAN Manager network):

@Mono@<:R1,1,1,1080,><:#200,8486>set AppleTalk_LogFileSize=100

@Bhead title@<:s><:R><:#220,8486>Step 6: Restarting the Notes server

<:s><:#400,8486>Power down the server and launch the Notes workstation. You can now set up the port on the Notes server, and edit the Notes server name and address book to include the new network name.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,3,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG), Editing the Notes server N&A book

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,4,1
@Build tag@@EndSection

>

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Print refs: Chapter 3, Notes and networks- Administrator's Guide

@Ahead@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#240,8486>About running Notes and AppleTalk on Windows NT

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#1200,8486>You can run Notes and AppleTalk on the Notes Windows NT server. In order to run your Notes server for NT on AppleTalk, you must enable the Microsoft Windows NT server services for Macintosh. Enabling this service starts or enables the AppleTalk protocol on 
the server. You can set up services for Macintosh when you install the Windows NT server, or later. For information on how to do this, see the installation guide that came with your NT server software.

@Ahead@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#240,8486>Setting up Notes and AppleTalk on Windows NT

@Numbered list@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Set up Services for Macintosh on the NT server.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><-!><-!>Launch the Notes workstation program on your NT server.

@Numbered list@<:s><:R><:#200,8486>Enable the network port for AppleTalk.

@Numbered list@<:s><:#200,8486>Restart the NT server.

<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>This port may have already been enabled when you installed Notes on the NT server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,5,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,6,1
@Build tag@@EndSection

>

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Print refs: Install Guide for setting up first port, Admin Guide port setup info in Ch.3?

@Ahead@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#240,8486>About running Notes and AppleTalk on the Macintosh

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#600,8486>Notes Macintosh workstations can communicate using Notes AppleTalk without any additional networking software because Notes provides all the software necessary to enable a Notes AppleTalk port on the Macintosh.

@Ahead@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#240,8486>Setting up Notes and AppleTalk on the Macintosh

@Numbered list@<:s><:R><:#200,8486>Launch the Notes workstation program on your Macintosh workstation.

@Numbered list@<:s><:#200,8486>Enable the network port for AppleTalk.

@Numbered list@<:s><:#200,8486>Restart the Notes workstation.

<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>This port may have already been enabled when you installed Notes on the Macintosh.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486><-!><-!>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,7,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,8,1
@Build tag@@EndSection

>

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>Print refs: Install Guide for setting up first port, Admin Guide port setup info in Ch.3?

@Ahead@<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#240,8486>About example configuration files for AppleTalk

<:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#400,8486>This section provides sample CONFIG.SYS, and PROTOCOL.INI files for various network interface cards supported by Notes AppleTalk.

<:s><:R><:#200,8486>The following directories are used in these examples:

@Indnt bullet@<:R1,1,1,360,><:#200,8486>ATALK - location of ATALK files supplied on the Lotus Notes CD-ROM

@Indnt bullet@<:R1,1,1,360,><:#200,8486>NDISDRV- location of NDIS driver file

@Indnt bullet@<:s><:R1,1,1,360,><:#200,8486>NOTES - location of Notes executable file

@Indnt bullet@<:R1,1,1,360,><:#200,8486>NOTES\DATA - location of Notes data files

<:R><:#200,8486>

>

[Embedded]
00067156
