[ver]
	4
[sty]
	
[files]
[charset]
	82
	ANSI (Windows, IBM CP 1252)
[revisions]
	0
[prn]
	Apple LaserWriter II NT
[port]
	LPT2:
[lang]
	1
[fldnames]
	Field1
	Field2
	Field3
	Field4
	Field5
	Field6
	Field7
	Field8
[desc]
	
	
	
	
	
	801506545
	70
	780276418
	5269
	11
	0
	0
	0
	0
	
	
	
	
	
	
	1
[fopts]
	0
	1
	0
	0
	
	
[lnopts]
	2
	Body Text
	1
[docopts]
	5
	2
[GramStyle]
	
[ParaNum]
	1
[tag]
	Body Text
	2
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Ahead
	3
	[fnt]
		Arial
		220
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		240
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		2160
		3
		0
		1
		1
		1
		65
		10
		1
	[spec]
		0
		1
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead title
	4
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		79
		0
		3
		100
	[brk]
		80
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Chead title
	5
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead
	6
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		180
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Chead
	7
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Numbered list
	8
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		300
		300
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		5
		<*:>.
		0
		3
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Numbered list
	0
	0
[tag]
	1st lev para
	9
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		68
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	1st lev para
	0
	0
[tag]
	Bullet
	11
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		120
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Bullet
	2
	1
	160
	1
	400
	0
[tag]
	Indnt bullet
	12
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		420
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		16
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Indnt bullet
	0
	0
[tag]
	2nd lev para
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		600
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	2nd lev para
	0
	0
[tag]
	See also prnt
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also prnt
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Book art
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Book art
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Callout text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Callout text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Figure title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		40
		60
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Figure title
	0
	0
[tag]
	Chapter title
	0
	[fnt]
		Arial
		280
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		300
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Chapter title
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	1st pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	1st pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Right pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Right pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Left pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Left pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Table title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		60
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		7
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Table title
	0
	0
[tag]
	Table col hd
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		4
	[line]
		10
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		6
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table col hd
	0
	0
[tag]
	Table Text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table Text
	0
	0
[tag]
	See also hlp
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		40
		4
		180
		0
		3
		100
	[brk]
		96
	[line]
		9
		0
		3
		0
		1
		1
		1
		70
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	0
	120
[tag]
	See also btn
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		240
	[spc]
		24
		200
		4
		0
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Crossref
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		513
		3
		0
		300
		600
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Crossref
	0
	0
[tag]
	Indnt caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt caution
	0
	0
[tag]
	Indnt tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		324
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt tip
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Indnt note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt note
	0
	0
[tag]
	Caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Caution
	0
	0
[tag]
	Tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		324
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Tip
	0
	0
[tag]
	Note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Note
	0
	0
[tag]
	Mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		48
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Indnt mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		300
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Dhead
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		4
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Parameter
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Parameter
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Formula
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Formula
	0
	0
[tag]
	Browse
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		+
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Browse
	0
	0
[tag]
	Keyword
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		K
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Keyword
	0
	0
[tag]
	Context
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		#
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Context
	0
	0
[tag]
	Title
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		$
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Title
	0
	0
[tag]
	Macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		!
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Macros
	0
	0
[tag]
	Footnote
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		244
		0
	[spc]
		40
		2400
		3
		0
		0
		1
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		256
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Footnote
	0
	0
[tag]
	Alink
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		A
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Alink
	0
	0
[tag]
	Butnbar
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		0
		0
		3
		100
	[brk]
		48
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		\li-140 
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Butnbar
	0
	0
[tag]
	Window
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		>
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Window
	0
	0
[tag]
	Win95 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		W
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win95 macros
	0
	0
[tag]
	Win31 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		X
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win31 macros
	0
	0
[tag]
	Build tag
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		*
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Build tag
	0
	0
[tag]
	_COND_IF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		IF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ELSE
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ELSE
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ENDIF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ENDIF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[frm]
	1
	1573060
	960
	1558
	9427
	6387
	0
	1
	1
	1 0 0 0 0 0 0
	0
	16777215
	7
	0
	6399
	3 17408
	[frmlay]
		2597
		8467
		1
		0
		0
		1
		1558
		0
		0
		2
		0
		1
		1
		0
		1
		1104
		9302
		0
	[tbl]
		 16 2 200 86 4131 86 1 43 43
		[h]
			 0 210 86 2 0 2 0
			 1 200 86 2 0 2 0
			 2 200 86 2 0 1 0
			 3 200 86 2 0 1 0
			 4 200 86 2 0 1 0
			 5 200 86 2 0 1 0
			 6 400 86 2 0 1 0
			 7 200 86 2 0 2 0
			 8 200 86 2 0 1 0
			 9 200 86 2 0 1 0
			 10 200 86 2 0 1 0
			 11 200 86 2 0 1 0
			 12 200 86 2 0 2 0
			 13 200 86 2 0 1 0
			 14 200 86 2 0 2 0
			 15 200 86 2 0 1 0
		[e]
		[w]
			 0 2844 86 2 0
			 1 5408 86 2 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Notes server platform

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@LAN protocols supported

>
			 1 0 0 0 0 0 0 1 0 0 0 0
OS/2 Release 3.0 and 2.11

>
			 1 1 0 0 0 0 0 1 0 0 0 0
AppleTalk

>
			 2 1 0 0 0 0 0 1 0 0 0 0
Banyan Vines

>
			 3 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 4 1 0 0 0 0 0 1 0 0 0 0
Novell NetWare SPX

>
			 5 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 6 0 0 0 0 0 0 1 0 0 0 0
Windows 3.1 and Windows for Workgroups 3.11

>
			 6 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 7 0 0 0 0 0 0 1 0 0 0 0
Windows NT v3.5 and higher

>
			 7 1 0 0 0 0 0 1 0 0 0 0
AppleTalk

>
			 8 1 0 0 0 0 0 1 0 0 0 0
Banyan Vines

>
			 9 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 10 1 0 0 0 0 0 1 0 0 0 0
Novell NetWare and Microsoft SPX, Microsoft SPX II

>
			 11 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 12 0 0 0 0 0 0 1 0 0 0 0
UNIX Solaris 2.X

>
			 12 1 0 0 0 0 0 1 0 0 0 0
SPX

>
			 13 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 14 0 0 0 0 0 0 1 0 0 0 0
UNIX HP-UX

>
			 14 1 0 0 0 0 0 1 0 0 0 0
SPX

>
			 15 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
		[e]
	[tble]
[frm]
	6
	1573060
	720
	960
	9187
	2433
	0
	1
	1
	1 0 0 0 0 0 0
	0
	16777215
	14
	1
	6399
	3 17408
	[frmlay]
		2777
		8467
		1
		0
		0
		1
		960
		0
		0
		2
		0
		1
		1
		0
		1
		1284
		9482
		0
	[tbl]
		 20 2 200 86 4131 86 1 43 43
		[h]
			 0 210 86 2 0 2 0
			 1 200 86 2 0 2 0
			 2 200 86 2 0 1 0
			 3 200 86 2 0 1 0
			 4 200 86 2 0 1 0
			 5 400 86 2 0 1 0
			 6 200 86 2 0 1 0
			 7 200 86 2 0 1 0
			 8 200 86 2 0 1 0
			 9 200 86 2 0 2 0
			 10 200 86 2 0 1 0
			 11 200 86 2 0 1 0
			 12 200 86 2 0 1 0
			 13 200 86 2 0 1 0
			 14 400 86 2 0 1 0
			 15 200 86 2 0 1 0
			 16 200 86 2 0 2 0
			 17 200 86 2 0 1 0
			 18 200 86 2 0 2 0
			 19 200 86 2 0 1 0
		[e]
		[w]
			 0 2606 86 2 0
			 1 5646 86 2 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Notes workstation platform

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@LAN protocols supported

>
			 1 0 0 0 0 0 0 1 0 0 0 0
OS/2 Release 3.0 and 2.11

>
			 1 1 0 0 0 0 0 1 0 0 0 0
Banyan Vines

>
			 2 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 3 1 0 0 0 0 0 1 0 0 0 0
Novell NetWare SPX

>
			 4 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 5 0 0 0 0 0 0 1 0 0 0 0
Windows 3.1 and Windows for Workgroups 3.11

>
			 5 1 0 0 0 0 0 1 0 0 0 0
Banyan Vines

>
			 6 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 7 1 0 0 0 0 0 1 0 0 0 0
Novell NetWare SPX

>
			 8 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 9 0 0 0 0 0 0 1 0 0 0 0
Windows 95

>
			 9 1 0 0 0 0 0 1 0 0 0 0
AppleTalk (TBD)

>
			 10 1 0 0 0 0 0 1 0 0 0 0
Banyan Vines

>
			 11 1 0 0 0 0 0 1 0 0 0 0
NetBIOS, NetBEUI

>
			 12 1 0 0 0 0 0 1 0 0 0 0
Novell NetWare SPX, Microsoft SPX, Microsoft SPX II

>
			 13 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 14 0 0 0 0 0 0 1 0 0 0 0
Macintosh System 7.5 and higher

>
			 14 1 0 0 0 0 0 1 0 0 0 0
AppleTalk

>
			 15 1 0 0 0 0 0 1 0 0 0 0
TCP/IP (MacTCP)

>
			 16 0 0 0 0 0 0 1 0 0 0 0
UNIX - HP UX

>
			 16 1 0 0 0 0 0 1 0 0 0 0
SPX

>
			 17 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
			 18 0 0 0 0 0 0 1 0 0 0 0
UNIX - Solaris 2.X

>
			 18 1 0 0 0 0 0 1 0 0 0 0
SPX

>
			 19 1 0 0 0 0 0 1 0 0 0 0
TCP/IP

>
		[e]
	[tble]
[lay]
	Standard
	1031
	[rght]
		12960
		10166
		1
		960
		1200
		3
		960
		720
		0
		1
		0
		1
		0
		2
		1
		960
		9446
		1
		1
		3120
	[lft]
		12960
		10166
		1
		720
		1200
		3
		960
		960
		0
		1
		0
		1
		0
		2
		1
		720
		9206
		1
		1
		3120
	[hlft]
	[lyfrm]
		1
		3008
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		3
	[frmlay]
		960
		10166
		1
		720
		180
		3
		0
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		2
		4674
	[txt]

>
	[hrght]
	[lyfrm]
		1
		11200
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		1
	[frmlay]
		960
		10166
		1
		960
		180
		3
		0
		720
		0
		1
		0
		1
		1
		0
		1
		960
		9446
		1
		2
		4674
	[txt]

>
	[flft]
	[lyfrm]
		1
		5056
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		4
	[frmlay]
		12960
		10166
		1
		806
		480
		3
		11940
		900
		0
		1
		0
		1
		1
		0
		1
		806
		9266
		1
		3
		9900
	[txt]
@Left pg foot@<:R1,1,3,8486,><:P12,2,1->  Network Configuration Guide	Lotus Confidential

>
	[frght]
	[lyfrm]
		1
		13248
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		2
	[frmlay]
		12960
		10166
		1
		900
		480
		3
		11940
		806
		0
		1
		0
		1
		1
		0
		1
		900
		9360
		1
		3
		9900
	[txt]
@Right pg foot@<:R1,1,3,8460,>Lotus Confidential	Notes and Networks <:P11,1,1->

>
[elay]
[l1]
	0
[pg]
	11
	29 0 5 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	56 0 10 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	61 0 5 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 15 0 0
	79 0 5 512 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	101 0 0 0 0 0 0 40 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	130 0 95 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	146 0 48 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	170 0 71 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	190 0 82 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	215 349 46 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	230 0 0 1025 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
[edoc]
@Chapter title@<:s><:#300,8486>Chapter 1 Notes and networks

@See also prnt@<:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>Notes is a workgroup application that allows people to share information using networks. Notes servers and workstations can communicate over local area networks (LANs) and wide area networks (WANs). This book provides information about running Notes on LANs
.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Notes has networking services that support:

@Bullet@<:s><:R><:#200,8486>Sessions between Notes workstations and servers, and communication over those sessions

@Bullet@<:s><:#400,8486>A fall-back method for getting a list of Notes server names, which Notes usually gets from the user's mail server

@See also prnt@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>This chapter provides information on concepts relevant to Notes and local area networks. You should be familiar with Notes system and network administration. This book provides information on these topics from a Notes perspective and does not attempt to pro
vide general network information.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,1,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Table of LAN protocols supported by Notes servers by platform

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,2,1
@@EndSection

>

@See also prnt@<:R><:#200,8486>Print cross ref:

@See also prnt@<:R1,0,><:#400,8486>For information on using protocols such as X.PC and X.25 to run Notes on a wide area network, see the Lotus Notes Administrator's Guide.

@Ahead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>About network operating systems compatible with Notes

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>You set up your Notes system after you set up your network operating system. The following network operating systems are compatible with Notes:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>AppleTalk

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Banyan VINES

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>DEC PATHWORKS

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>FTP Software PC/TCP for OS/2

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM OS/2 EE LAN Requester for Ethernet

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM TCP/IP for OS/2

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Microsoft LAN Manager

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Novell NetWare NetBIOS emulator

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Novell NetWare Requester with SPX

@Ahead@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#240,8486>About network protocols

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#1000,8486>A protocol is a set of rules that govern how computers share information over a network. Some network protocols are proprietary, or developed for use and modification by a single organization, and some are industry standards. Often, a protocol starts off as
 proprietary, and when a substantial number of other computer hardware and software vendors create products that support that protocol, it becomes a standard.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,3,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Table of LAN protocols supported by Notes servers by platform

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,4,1
@@EndSection

>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>About network protocols compatible with Notes

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>Each network operating system is associated with a network protocol. A network protocol is a set of rules that defines how that operating system transfers information. The following network protocols are compatible with Notes:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>AppleTalk

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Banyan VINES

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>NetBIOS/NetBEUI

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>NetWare SPX

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>TCP/IP

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,5,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>See related topics: Table of LAN protocols supported by Notes servers by platform and Table of LAN protocols supported by Notes workstations by platform

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,6,1
@@EndSection

>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>Selecting a network protocol

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#800,8486>In many cases, people who purchase Notes buy Notes server and workstations that are compatible with an existing network operating system. If you are deciding which network operating system to buy or are adding a protocol to an existing Notes system, you sho
uld know that certain network protocols perform certain tasks better than other protocols:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>AppleTalk, Banyan VINES, and NetBIOS offer convenience and ease of use.

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>NetWare SPX offers high speed across local area networks.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>TCP/IP offers wide area routability, which simplifies LAN connections to wide area networks such as the Internet. TCP/IP is a very robust protocol and is the protocol on which the Internet is based.

<:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>No one protocol offers an optimal combination of convenience, wide area routability, and speed. Local access protocols may be different from the protocols used for cross-backbone database replication and mail routing.

@Ahead@<:s><:R1,1,1,360,><:#240,8486>About using Notes with single and multiple protocols

<:s><:R1,1,1,360,><:#600,8486>You can set up your Notes servers and workstations on one or more network protocols. Adding a protocol to your Notes system usually requires installing additional software, editing system files, and possibly adding network interface cards to your Notes serv
er.

<:s><:R1,1,1,360,><:#800,8486>The simpler the network configuration, the easier network and Notes system administration is. Also, the fewer protocols installed on a Notes system, the lower the network traffic and load. This is because each installed protocol occupies an amount of bandwi
dth on the network, so the fewer protocols installed, the less occupied bandwidth.

@Bullet@<:s><:R1,1,1,360,><:#400,8486>An example of using Notes with a single protocol is when Novell NetWare is installed on the Notes server.

@Bullet@<:R1,1,1,360,><:#400,8486>An example of using Notes with multiple network protocols is when AppleTalk and Banyan VINES are installed on the same Notes server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,7,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Running Notes on multiple protocols, About network interface cards

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,8,1
@@EndSection

>

<:R1,1,1,360,><:#200,8486>print ref:

@See also prnt@<:s><:R1,1,1,360,><:#200,8486>For more information on running Notes on multiple protocols, see Chapter 7.

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>Table of LAN protocols supported by Notes servers by platform

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,><:t0><:>

@Ahead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>Table of LAN protocols supported by Notes workstations by platform

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:t1>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>About setting up Notes servers and workstations on networks

<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#400,8486>Here's an overview of the process you should use to set up Notes servers and workstations on a network.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#400,8486>Install the network operating system. For detailed information, see the documentation that came with the network operating system.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#200,8486>Install network interface cards as needed on Notes servers.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#400,8486>Install Notes server or workstation software. For detailed information, see your Lotus Notes installation guides.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#400,8486>Install other software if necessary (for example, protocol manager), and make sure all network driver files have been installed and are in the correct directories.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#200,8486>Edit system configuration files as needed.

@Numbered list@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#200,8486>Set up additional Notes server and workstation ports as necessary.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Perform network access checks. Check server-to-server and server-to-workstation connections.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,9,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>See related topics: About network interface cards, Table of protocol standards supported by Notes network protocols, Administrator's Guide (port setup, network access checks)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,10,1
@@EndSection

>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Print only: This book covers the information you need to do in steps 4 and 5.

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>About Notes network drivers

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>Notes network drivers are software files that control network communication to and from Notes servers and workstations. In Notes, network driver files typically have a .DLL extension and are in the Notes directory.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>Each protocol requires its own network driver. Some network drivers are supplied with Notes server and workstation software and are installed automatically when you install Notes. Other network drivers come with network operating system software, and you mu
st install these separately.<-">

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:p<* >>About Notes network interface cards (NICs)

<:R1,1,1,5760,><:#1000,8486>A network interface card (NIC) provides the physical access between a Notes server or workstation and a network. A NIC typically plugs into an expansion slot on the computer and provides a connection for a network cable. The NIC contains processors that tra
nslate signals that pass between the network and the computer. NICs are directly associated with the network protocols you install on a Notes server or workstation. In fact, the network protocols are actually installed on the NIC.

<:R1,1,1,5760,><:#800,8486>The number of network protocols you can install on a NIC depends on which network protocols you are installing. Sometimes you can install only one protocol on a card; in other cases, you can install multiple protocols on a network interface card. How many p
rotocols you can install on a card depends on the protocol standards with which those protocols are compliant.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,11,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>See related topics: Table of protocol standards are supported by Notes network protocols, About Notes protocol standards, Running Lotus Notes on multiple protocols

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,12,1
@@EndSection

>

@Ahead@<:R1,1,1,5760,><:#240,8486>About network protocol standards

<:s><:R1,1,1,5760,><:#200,8486>Notes supports networks compatible with two protocol standards:

@Bullet@<:R1,1,1,5760,><:#200,8486>Network driver interface specification (NDIS)

@Bullet@<:R1,1,1,5760,><:#200,8486>Open data link interface (ODI)

<:R><:#400,8486>NDIS and ODI provide standard functions and calling interfaces that enable network drivers to work with network interface cards.

@Bhead@<:#220,8486>The NDIS network protocol standard

<:R1,1,1,1224,><:#400,8486>Notes supports Ethernet and Token Ring networks that use network drivers compliant with NDIS. You can install up to four NDIS-compliant network protocols on one network interface card.

<:R1,1,1,1224,><:#200,8486>The NDIS architecture has three main software components:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Protocol driver (usually provided by the protocol vendor)

@Bullet@<:s><:R1,1,1,1224,><:#400,8486>Protocol manager (usually provided by the protocol vendor) - enables the protocol driver and media access control (MAC) driver to communicate with each other.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Media access control driver - directly controls the network interface card.

<:R1,1,1,1224,><:#1000,8486>Protocol drivers form the top layer, the protocol manager forms the middle layer, and MAC drivers form the bottom layer of the protocol stack. This stack implements the protocols and drivers that link applications to specified network interface cards. NDIS 
driver software is available from most NIC manufacturers, from bulletin board systems, or as part of the Microsoft LAN Manager network operating system. 

@Bhead@<:R1,1,1,1224,><:#220,8486>The ODI network protocol standard

<:R1,1,1,1224,><:#1000,8486>ODI functionality enables multiple ODI-compliant protocol drivers to share a single card, and Novell's ODI NDIS Support (ODINSUP) drivers enable multiple protocol drivers that comply with NDIS or ODI to share a single card. Before ODI existed as a standard,
 you had to install a separate network driver and network interface card for each machine on a network. Using ODI, you can install more than one network protocol on a network interface card, and that card can support various machines on the network.

<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>Most of the Notes-supported protocol drivers do not support ODI and ODINSUP. Notes fully supports only the NDIS network protocol standard.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,13,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Table of protocol standards supported by Notes network protocols

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,14,1
@@EndSection

>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486>Table of protocol standards supported by Notes network protocols

<:R1,4,1,0,1,720,1,1440,1,2160,><:#800,8486>Unless the network operating system is Microsoft LAN Manager, a Notes server or workstation can run only one NetBIOS-based protocol at a time. LAN Manager is a NetBIOS-based network operating system and can run several protocols concurrently, such as NetBEU
I and TCP/IP. Lotus Notes can support one NetBIOS port enabled on each LAN Manager protocol stack.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#800,8486>Use these lists to determine the network protocol standards with which your network operating system is compliant. If the protocols are NetBIOS-based, the word NetBIOS appears in parentheses after the name of the protocol. Use that information to determine 
how many network interface cards you need to install in your servers and workstations.

@Bhead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#220,8486>NDIS standard protocols

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>AppleTalk

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Banyan VINES with NDIS drivers

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>DEC PATHWORKS (NetBIOS)

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>FTP Software PC/TCP (TCP/IP)

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM OS/2 EE LAN Requester for Ethernet  (NetBIOS)

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM OS/2 LAN Server (IBM NetBIOS)

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM TCP/IP

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Microsoft LAN Manager (NetBIOS)

@Bhead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#220,8486>ODI standard protocols

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Novell NetBIOS

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Novell NetWare SPX

@Bhead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#220,8486>Proprietary protocols

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Banyan VINES (IP)

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>IBM OS/2 EE LAN Requester for Token Ring (NetBIOS)

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,15,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: About Notes network interface cards

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,16,1
@@EndSection

>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486><:f220,BArial,0,0,0>About protocol manager software

<:R1,4,1,0,1,720,1,1440,1,2160,><:#1000,8486>Protocol manager software enables network protocol drivers in a multi-protocol system to communicate. When you add a protocol to a Notes system, you must install protocol manager software to support it. The actual software you install is different for each 
protocol. Most network protocol vendors supply the necessary protocol manager files with the protocol software. Typically, you install a protocol manager program for each protocol in a Notes system.

<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>print only ref:

<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>For specific protocol manager requirements and procedures, see the individual protocol chapter.

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#220,8486>Installing protocol manager software

<:s><:R><:#600,8486>To add network protocols to your Notes servers and workstations, you need to install software which will support these different network protocols. This software is known as protocol manager software. You need a protocol manager program for each set of prot
ocols on your Notes servers and workstations. 

<:#800,8486>Novell Inc. supplies a protocol manager - IPXODI.EXE - for use with its Novell NetWare IPX/SPX protocols. For use Windows 3.1 you need IPXODI.EXE 1.2 or later. Novell's optional software package, LAN Workplace for DOS, includes a protocol manager program fo
r using TCP/IP protocols with NetWare.

<:#1200,8486>Protocol manager software associates the protocol driver with the network interface card driver and, therefore, must be compatible with both.  Protocol Manager software must be compatible with the protocol driver and the network card driver. You install the
 new Protocol Manager software by editing the Notes server's CONFIG.SYS and STARTUP.CMD files, and creating the PROTOCOL.INI file. Where directory names are required, use the names you assigned to the directories when you created them; the names used in the
 samples are for example only.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Edit your system CONFIG.SYS file for the new Protocol Manager installation.<-">

@Numbered list@<:R1,1,1,1080,><:#1400,8486>Add a line to your system STARTUP.CMD file to bind the protocol driver to the NDIS card driver. You do not need to do this if you have installed protocols already using Microsoft's Protocol Manager Example: C:\ATALK\NETBIND.EXE<**><**>For a Notes AppleTalk 
installation, add the following line after the bind entry to specify the amount of time allowed for the protocol to initialize (45 seconds is recommended) 
<**>C:\ATALK\TPAUSE.EXE 45

@Numbered list@<:R1,1,1,1080,><:#400,8486>Create and edit a file called PROTOCOL.INI in your protocol files directory (C:\ATALK in the above example).

@Chead@<:R1,1,1,360,><:#200,8486>Editing CONFIG.SYS for a protocol manager installation

<:s><:R1,1,1,360,><:#400,8486>In order to install protocol manager you need. Add two DEVICE statements that identify the name and location of the protocol manager file and the network interface card. 

<:R1,1,1,360,><:#200,8486>There is an example of an edited CONFIG.SYS file in each protocol chapter.

@Chead@<:R1,1,1,360,><:#200,8486>Editing PROTOCOL.INI for a protocol manager installation

<:R1,1,1,1080,><:#1200,8486>In PROTOCOL.INI, enter a section, consisting of a heading in brackets, followed by parameters and values for each protocol or network card that you are installing. The PROTOCOL.INI examples here use Microsoft section names, including the convention of endin
g card section names with "_NIF" and protocol section names with "_XIF". Network interface card manufacturers usually provide a "stub" or section of a PROTOCOL.INI file with default values that you can copy into PROTOCOL.INI. The example section below confi
gures a 3Com EtherLink II card:

<:R1,1,1,1080,><:#800,8486><**><[>ELNKII_NIF]<**>DriverName = ELNKII$<**>Interrupt = 3<**>IOAddress = 0x300

<:R1,1,1,1080,><:#400,8486>DriverName is the card driver file name (excluding the extension), followed by a $. You enter the card driver file name in your CONFIG.SYS file when you install the network interface card.

<:s><:R1,1,1,1080,><:#200,8486>Interrupt is the interrupt time specified for the network card.

<:R1,1,1,1080,><:#200,8486>IOAddress is the card base input/output address.

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486><:f220,BArial,0,0,0>About protocol driver software

<:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>The protocol driver software loads and starts the protocol supplied by the network operating system and communicates with the NDIS protocol manager or ODI link support layer, or directly with a proprietary network interface card driver.

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#220,8486>Installing protocol driver software

<:R><:#600,8486>On a Notes OS/2 server, you install new protocol drivers by editing CONFIG.SYS and PROTOCOL.INI, using any text editor. Where directory names are required, use the names you assigned to the directories when you created them.

@Numbered list@<:#400,8486>Edit your system CONFIG.SYS file for the new protocol driver installation. 
<+!><+">??jump to "Editing CONFIG.SYS for the protocol driver installation"<-"><-!>

@Numbered list@<:R1,1,1,1080,><:#400,8486>Add a protocol driver section to the PROTOCOL.INI file. <+!><+">??jump to "Editing PROTOCOL.INI for a protocol driver installation"<-"><-!>

<:R1,1,1,1080,><:#200,8486>DriverName is the protocol driver file name (excluding the extension) followed by $.

<:s><:R1,1,1,1080,><:#200,8486>Bindings is the section name of the network card which the new protocol should use.

<:R1,1,1,1080,><:#400,8486>If you are installing Notes AppleTalk, add a line defining port type to the protocol driver section: EtherTalk (AppleTalk on Ethernet) or TokenTalk (AppleTalk on Token Ring). For example:  

<:R1,1,1,1080,><:#200,8486>PortType = EtherTalk

@Chead@<:R1,1,1,1080,><:#200,8486>Editing CONFIG.SYS for the protocol driver installation

@Numbered list@<:R1,1,1,1080,><:#400,8486>Add the directory containing the new protocol's Application Program Interface (API) file, with a .DLL extension (such as ATALK.DLL) to the LIBPATH statement.

@Numbered list@<:R1,1,1,1080,><:#400,8486>Add the directory containing the protocol driver message file (such as ATK.MSG) to the DPATH statement.

@Numbered list@<:R1,1,1,1080,><:#600,8486>Add a DEVICE statement to CONFIG.SYS to load the protocol driver file. This statement must follow the DEVICE statement that loads PROTMAN.OS2. The following example shows the additional statement, where C:\ATALK is the AppleTalk files directory.

<:R1,1,1,1080,><:#400,8486>REM network card driver<**>DEVICE = C:\ATALK\ATALK2v2.OS2

<:R1,1,1,1080,><:#400,8486>If you are installing Notes AppleTalk, add a RUN statement that starts the protocol driver executable (ATALKINI.EXE) after the DEVICE statement. For example:

<:R1,1,1,1080,><:#200,8486>RUN = C:\ATALK\ATALKINI.EXE

@Chead@<:R><:#200,8486>Editing PROTOCOL.INI for a protocol driver installation

<:R1,1,1,1080,><:#800,8486>The section consists of a heading, followed by parameters and values. The parameters should include DriverName and Bindings. Network interface card manufacturers usually provide a 'stub' or section of a PROTOCOL.INI file with default values that you can cop
y into PROTOCOL.INI. The example section below shows the lines to be added to PROTOCOL.INI for installing Notes AppleTalk on an Ethernet card:

<:R><:#600,8486><[>ATALK_XIF]<**>DriverName = ATALK$<**>Bindings = ELNKII_NIF

@Ahead@<:s><:#240,8486>About the Notes server error log

<:#600,8486>The Notes server error log lists network errors and warnings that can help you monitor network activity. In order to trap these system errors, you must configure the error log for each protocol by specifying error log parameters in the CONFIG.SYS file.

<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>print only ref:

<:R><:#200,8486>For specific error log parameters, see the individual protocol chapter.

@Bhead title@<:s><:#220,8486>Editing the error log for a network protocol

<:#600,8486>The error log file on the Notes OS/2 server lists network errors and warnings that help you monitor network activities. Configure the error log for the new protocol software by using the SET command to specify the error log parameters in CONFIG.SYS.

<:s><:#200,8486>Error log parameters are as follows:

<:#400,8486>LogFile specifies the path and name of the file in which to log error and warning messages. The default is PROTOCOL.LOG in the root directory of the startup drive (usually C:). 

<:#200,8486>Example: SET AppleTalk_LogFile=C:\NOTES\ATALK.LOG

<:#800,8486>LogFileSize specifies the maximum size of the log file, in Kilobytes. When the log file reaches the maximum size, the protocol software logs a message indicating that the log is full, and no additional errors are logged to the file. To resume logging, back 
up the log file, then delete it, or use a text editor to delete some entries. Valid values are 0 to 2000 (file size in Kilobytes); the default value is 80. 

<:#200,8486>Example: SET AppleTalk_LogFileSize=100

<:#1200,8486>ErrorFreq and WarningFreq control the frequency at which errors and warnings are logged. A particular message is logged only as often as the ErrorFreq or WarningFreq value. For example, if ErrorFreq is 5, an error that occurs 12 times is logged on the 1st, 
6th and 11th occurrences. If six different errors occur once each, all are logged. Limiting logging to specific numbered occurrences of an error can prevent the error log from filling up with repeated messages. These parameters should be set to 1 when troub
leshooting, and to a higher value for normal operation.

<:#800,8486>Protocol software may log some error and warning messages even under normal operation. For example, when a router on the network is temporarily misconfigured, the protocol software may log error messages reporting conflicting information on a network, even 
though operation continues unaffected. In another instance, the software might drop some packets when under a peak load, and log it as an error.

<:s><:#400,8486>Valid values for both warning and error frequency are 1 to 16535; the default is to log every 10th warning and every 10th error.

<:#200,8486>Example: SET AppleTalk_ErrorFreq=15

<:#600,8486>If you are installing Notes AppleTalk in an environment other than LAN Manager 2.1, AppleTalk protocol messages are written to a plain-text file. By default this is the file ATALK.LOG in the root directory of the startup drive (usually C:). You can view thi
s file with the OS/2 TYPE command, or with any text editor.

<:#800,8486>If you are installing the Notes AppleTalk software in a LAN Manager 2.1 environment, edit the error log for the new protocol software by setting the protocol error log parameters in the network operating system configuration file LANMAN.INI. To set the para
meters, create an AppleTalk section in LANMAN.INI, starting with a heading in square brackets, followed by the parameters. For example:

<:#600,8486><[>AppleTalk]<**>   WarningFreq = 1  <**>   ErrorFreq = 1

<:#400,8486>ErrorFreq and WarningFreq control the frequency at which warnings and errors are logged, as described above.

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486><:f220,BArial,0,0,0>About Notes network ports

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>Notes network ports are software switches that determine which network driver to use, based on the network communication needed by the Notes machine.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>There are two types of Notes network ports:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>COM ports - used with the Notes X.PC and X.25 drivers<-"> for remote (mobile) connections involving modems and wide area networks

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>LAN ports - used for LAN communications, work with Notes LAN protocols and drivers

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>You set up the first network port on a Notes server or workstation during Notes installation.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,17,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: About Notes network port information, Configuring a Notes network port (AG)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,18,1
@@EndSection

>

<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>print only refs: For more information on Notes LAN ports, see the Lotus Notes Administrator's Guide, Chapter 3, Communicating with Notes, About setting up Notes network ports

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>The Lotus Notes Administrator's Guide provides information on enabling additional Notes network ports (beyond the first one) and disabling Notes network ports.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486> For more information on setting up the first network port, see your Lotus Notes installation guides.

@Bhead title@<:R1,4,1,2390,1,2868,1,3347,1,3825,><:#220,8486>Checking the status of a Notes network port<:><-!>

<:s><:R1,1,1,0,><:#200,8486>There are two ways to check the status of a network port on a Notes server:

@Bullet@<:R1,1,1,0,><:#200,8486>Use the command SHOW PORT portname at the Notes server console.

@Bullet@<:R1,1,1,0,><:#200,8486>In Notes, select File - Notes Setup - Preferences, Ports, and ShowStatus.

<:s><:R1,1,1,0,><:#200,8486>To check the status of a network port on a Notes workstation, you can use only the second method.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,19,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Issuing server commands (AG), About (each protocol) port status

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,20,1
@@EndSection

>

<:R1,1,1,0,><:#200,8486>print ref: For an example of a port status for a particular protocol, see the protocol chapter.

@Ahead@<:s><:R1,4,1,2390,1,2868,1,3347,1,3825,><:#240,8486>Table of Notes network port parameters 

<:s><:R><:#400,8486>To monitor or troubleshoot network activity on a Notes server or workstation, start by using Notes to check the status of the network port. Here are what some of the parameters mean:

<:#400,8486><:f180,,0,0,0>Aborted transmissions - <:f><:f180,,0,0,0>Network transmissions that were canceled<:f><:f180,,0,0,0> . 
<:f><:f180,,0,0,0>May indicate problems with the network card. Run diagnostics and replace the card if necessary. 
<:f>

<:#1000,8486><:f180,,0,0,0>Adapter name table<:f> - <:f180,,0,0,0>N<:f><:f180,,0,0,0>ames by which the server 
<:f><:f180,,0,0,0>and applications running on it are known by non-Notes computers and applications on the network. A name can also be part of a NetBIOS group, identified in the table as "grp." (<:f><:f180,,0,0,0>Name 5 is the server name. The first 15 chara
cters are blank-space filled; the 16th character is a + sign.). <:f><:f180,,0,0,0>You need to know this format if the server will be communicating through a bridge that uses manual n<:f><:f180,,0,0,0>ame registration.

<:s><:#800,8486><:f180,,0,0,0>Adapter resources - <:f><:f180,,0,0,0>C<:f><:f180,,0,0,0>urrent status of the network adapter card. 
<:f><:f180,,0,0,0>You can use these statistics for fine-tuning network performance. For example, if the number of sessions in use is equal to the maximum number of sessions, you may want to increase the maximum number of sessions in the network configuratio
n file.<:f>

<:#1000,8486><:f180,,0,0,0>Adapter session table - <:f><:f180,,0,0,0>St<:f><:f180,,0,0,0>atus information about current network sessions. 
<:f><:f180,,0,0,0>You can see such information as the local session number (LSN), the state of the session (Listen pending, Session created), the<:f><:f180,,0,0,0> local and remote names, and the number of Receive and Send commands pending. On lines that co
ntain "Listen Pending" in the State column, an asterisk (*) in the Remote Name column means "receive connections from anyone."<:f>

<:s><:#800,8486><:f180,,0,0,0>Alignment errors - <:f><:f180,,0,0,0>Network alignment errors reported on this port - 
<:f><:f180,,0,0,0>Alignment errors occur when the number of bits received is not a multiple of 16, so the boundary between characters is ambiguous. This is considered a frame error and may require a new network interface card. It could also be caused by bad
ly formed data packets or a loose cable.<:f>

<:s><:#400,8486><:f180,,0,0,0>Available command blocks - <:f><:f180,,0,0,0>Number of NetBIOS control blocks available now - 
<:f><:f180,,0,0,0>If this drops to a low number, the Notes server may not be able to support additional users.<:f>

<:s><:#400,8486><:f180,,0,0,0>Collisions - <:f><:f180,,0,0,0>Network collision errors reported on this port. 
<:f><:f180,,0,0,0>Caused when packets on the network collide and are damaged; could be caused by a loose cable.<:f>

<:#800,8486><:f180,,0,0,0>CRC errors - <:f><:f180,,0,0,0>Number of cyclic redundancy check (CRC) errors reported on this port - 
<:f><:f180,,0,0,0>CRC is used for message transmission and reception verification. CRC errors mean that the CRC included in the frame does not match the<:f><:f180,,0,0,0> actual number of bits in the frame. CRC errors cause retransmissions and network degra
dation and can be caused by badly formed data packets or a loose cable on a network port.<:f>

<:s><:#400,8486><:f180,,0,0,0>Maximum sessions - <:f><:f180,,0,0,0>N<:f><:f180,,0,0,0>umber of sessions configured for this server. 
<:f><:f180,,0,0,0>Compare this to the number of sessions in use.<:f>

<:s><:#200,8486><:f180,,0,0,0>Network <:f><:f180,,0,0,0>unit status - <:f><:f180,,0,0,0>The<:f><:f180,,0,0,0> revision number of the network software<:f>

<:s><:#400,8486><:f180,,0,0,0>Number of packets dropped - <:f><:f180,,0,0,0>The network dropped packets,<:f><:f180,,0,0,0> because there was no buffer ready to receive them. Could be caused by insufficient link support buffers or<:f><:f180,,0,0,0> by transmissions from a f
ast <:f>

<:s><:#200,8486><:f180,,0,0,0>Packets received - <:f><:f180,,0,0,0>Number of network packets received on this port<:f>

<:s><:#200,8486><:f180,,0,0,0>Packets transmitted - <:f><:f180,,0,0,0>Number of network packets sent from this port<:f>

<:s><:#200,8486><:f180,,0,0,0>Reporting period - <:f><:f180,,0,0,0>Collection time for statistics<:f>

<:#600,8486><:f180,,0,0,0>Retransmissions - <:f><:f180,,0,0,0>Network transmissions that were retried. P<:f><:f180,,0,0,0>ackets are retransmitted when they don't reach their destination the first time. Causes include CRC errors, alignment errors, collisions, and abort
ed transmissions.<:f>

<:s><:#400,8486><:f180,,0,0,0>Session data packet size - <:f><:f180,,0,0,0>V<:f><:f180,,0,0,0>aries depending on the network. I<:f><:f180,,0,0,0>n NetWare, it is the maximum amount of data it can send in a single packet<:f>

<:s><:#600,8486><:f180,,0,0,0>Sessions in use - <:f><:f180,,0,0,0>Sessions that are active now. 
<:f><:f180,,0,0,0>If the number of sessions in use is equal to the maximum number of sessions, you may want to increase the maximum number of sessions in the network configuration file.<:f>

<:s><:#400,8486><:f180,,0,0,0>Total command blocks -<:f><:f180,,0,0,0>N<:f><:f180,,0,0,0>umber of total command blocks configured. 
<:f><:f180,,0,0,0>Should be set to 1-1/2 times the number of sessions.<:f>

<:s><:#400,8486><:f180,,0,0,0>Traffic and e<:f><:f180,,0,0,0>rror statistics - <:f><:f180,,0,0,0>Shows the<:f><:f180,,0,0,0> communications activity on the port. 
<:f><:f180,,0,0,0>Used to<:f><:f180,,0,0,0> troubleshoot network hardware or track network performance.

<:R1,4,1,2390,1,2868,1,3347,1,3825,><:#200,8486>

>

[Embedded]
00064241
