[ver]
	4
[sty]
	
[files]
[charset]
	82
	ANSI (Windows, IBM CP 1252)
[revisions]
	0
[sequence]
	9
	0
	0
	0
	23
	3
	Numbered list
	0
	Bullet
	0
	Indnt bullet
	0
	Indnt caution
	0
	Indnt tip
	0
	Indnt note
	0
	Caution
	0
	Tip
	0
	Note
	0
	Browse
	0
	Keyword
	0
	Context
	0
	Title
	0
	Macros
	0
	Alink
	0
	Butnbar
	0
	Window
	0
	Win95 macros
	0
	Win31 macros
	0
	Build tag
	0
	_COND_IF
	0
	_COND_ELSE
	0
	_COND_ENDIF
[prn]
	HP LaserJet III PostScript
[port]
	LPT2:
[lang]
	1
[fldnames]
	Field1
	Field2
	Field3
	Field4
	Field5
	Field6
	Field7
	Field8
[desc]
	
	
	
	
	
	801506562
	60
	780272848
	2792
	28
	0
	0
	0
	0
	
	
	
	
	
	
	1
[fopts]
	0
	1
	0
	0
	
	
[lnopts]
	2
	Body Text
	1
[docopts]
	5
	2
[GramStyle]
	
[ParaNum]
	1
[tag]
	Body Text
	2
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Ahead
	3
	[fnt]
		Arial
		220
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		240
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		2160
		3
		0
		1
		1
		1
		65
		10
		1
	[spec]
		0
		1
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead title
	4
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		79
		0
		3
		100
	[brk]
		80
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Chead title
	5
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead
	6
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		180
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Chead
	7
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Numbered list
	8
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		300
		300
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		5
		<*:>.
		0
		3
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Numbered list
	0
	0
[tag]
	1st lev para
	9
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		68
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	1st lev para
	0
	0
[tag]
	Bullet
	11
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		120
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Bullet
	2
	1
	160
	1
	400
	0
[tag]
	Indnt bullet
	12
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		420
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		16
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Indnt bullet
	0
	0
[tag]
	2nd lev para
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		600
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	2nd lev para
	0
	0
[tag]
	See also prnt
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also prnt
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Book art
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Book art
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Callout text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Callout text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Figure title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		40
		60
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Figure title
	0
	0
[tag]
	Chapter title
	0
	[fnt]
		Arial
		280
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		300
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Chapter title
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	1st pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	1st pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Right pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Right pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Left pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Left pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Table title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		60
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		7
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Table title
	0
	0
[tag]
	Table col hd
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		4
	[line]
		10
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		6
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table col hd
	0
	0
[tag]
	Table Text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table Text
	0
	0
[tag]
	See also hlp
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		40
		4
		180
		0
		3
		100
	[brk]
		96
	[line]
		9
		0
		3
		0
		1
		1
		1
		70
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	0
	120
[tag]
	See also btn
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		240
	[spc]
		24
		200
		4
		0
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Crossref
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		513
		3
		0
		300
		600
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Crossref
	0
	0
[tag]
	Indnt caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt caution
	0
	0
[tag]
	Indnt tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		324
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt tip
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Indnt note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt note
	0
	0
[tag]
	Caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Caution
	0
	0
[tag]
	Tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		324
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Tip
	0
	0
[tag]
	Note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Note
	0
	0
[tag]
	Mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		48
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Indnt mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		300
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Dhead
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		4
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Parameter
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Parameter
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Formula
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Formula
	0
	0
[tag]
	Browse
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		+
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Browse
	0
	0
[tag]
	Keyword
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		K
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Keyword
	0
	0
[tag]
	Context
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		#
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Context
	0
	0
[tag]
	Title
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		$
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Title
	0
	0
[tag]
	Macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		!
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Macros
	0
	0
[tag]
	Footnote
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		244
		0
	[spc]
		40
		2400
		3
		0
		0
		1
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		256
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Footnote
	0
	0
[tag]
	Alink
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		A
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Alink
	0
	0
[tag]
	Butnbar
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		0
		0
		3
		100
	[brk]
		48
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		\li-140 
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Butnbar
	0
	0
[tag]
	Window
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		>
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Window
	0
	0
[tag]
	Win95 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		W
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win95 macros
	0
	0
[tag]
	Win31 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		X
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win31 macros
	0
	0
[tag]
	Build tag
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		*
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Build tag
	0
	0
[tag]
	_COND_IF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		IF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ELSE
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ELSE
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ENDIF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ENDIF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[frm]
	2
	1573060
	900
	3909
	9386
	6392
	0
	1
	1
	1 0 0 0 0 0 0
	0
	16777215
	5
	0
	2304
	0 65280
	[frmlay]
		4417
		8486
		1
		0
		0
		1
		3909
		0
		0
		2
		0
		1
		1
		0
		1
		864
		9062
		0
	[tbl]
		 5 5 200 86 1603 86 1 43 43
		[h]
			 0 410 86 2 0 2 0
			 1 200 86 2 0 5 0
			 2 600 86 2 0 1 0
			 3 400 86 2 0 1 0
			 4 400 86 2 0 1 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Notes Platform

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@DEC PATHWORKS

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@IBM LAN Server

>
			 0 3 0 0 0 0 0 1 0 0 0 0
@Table col hd@Novell NetBIOS

>
			 0 4 0 0 0 0 0 1 0 0 0 0
@Table col hd@Microsoft NETBEUI

>
			 1 0 0 0 0 0 0 1 0 0 0 0
OS/2

>
			 1 1 0 0 0 0 0 1 0 0 0 0
x

>
			 1 2 0 0 0 0 0 1 0 0 0 0
x

>
			 1 3 0 0 0 0 0 1 0 0 0 0
x

>
			 1 4 0 0 0 0 0 1 0 0 0 0
x

>
			 2 0 0 0 0 0 0 1 0 0 0 0
Windows 3.1 and Windows for Workgroups

>
			 2 1 0 0 0 0 0 1 0 0 0 0
x

>
			 2 3 0 0 0 0 0 1 0 0 0 0
x

>
			 2 4 0 0 0 0 0 1 0 0 0 0
x

>
			 3 0 0 0 0 0 0 1 0 0 0 0
Windows NT (server only)

>
			 3 1 0 0 0 0 0 1 0 0 0 0
x

>
			 3 3 0 0 0 0 0 1 0 0 0 0
x

>
			 3 4 0 0 0 0 0 1 0 0 0 0
x

>
			 4 0 0 0 0 0 0 1 0 0 0 0
Windows 95 (client only)

>
			 4 1 0 0 0 0 0 1 0 0 0 0
x

>
			 4 3 0 0 0 0 0 1 0 0 0 0
x

>
			 4 4 0 0 0 0 0 1 0 0 0 0
x

>
		[e]
	[tble]
[lay]
	Standard
	1031
	[rght]
		12960
		10166
		1
		900
		1200
		3
		960
		780
		0
		1
		0
		1
		0
		2
		1
		900
		9386
		1
		1
		3120
	[lft]
		12960
		10166
		1
		780
		1200
		3
		960
		900
		0
		1
		0
		1
		0
		2
		1
		780
		9266
		1
		1
		3120
	[hlft]
	[lyfrm]
		1
		3008
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		3
	[frmlay]
		960
		10166
		1
		720
		180
		3
		0
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		2
		4674
	[txt]
 

>
	[hrght]
	[lyfrm]
		1
		11200
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		1
	[frmlay]
		960
		10166
		1
		960
		180
		3
		0
		720
		0
		1
		0
		1
		1
		0
		1
		960
		9446
		1
		2
		4674
	[txt]

>
	[flft]
	[lyfrm]
		1
		5056
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		4
	[frmlay]
		12960
		10166
		1
		720
		480
		3
		11940
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		3
		9900
	[txt]
@Left pg foot@<+@><:R1,1,3,8486,><:P19999,0,4->  Network Configuration Guide	Lotus Confidential

>
	[frght]
	[lyfrm]
		1
		13248
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		2
	[frmlay]
		12960
		10166
		1
		900
		480
		3
		11940
		780
		0
		1
		0
		1
		1
		0
		1
		900
		9386
		1
		3
		9900
	[txt]
@Right pg foot@<+@><:R1,1,3,8486,>Lotus Confidential	Running Lotus Notes on NetBIOS  <:P19999,0,4->

>
[elay]
[l1]
	0
[pg]
	28
	23 0 80 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	47 99 99 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	75 0 0 0 0 0 0 40 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	101 98 12 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	111 805 11 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	117 68 60 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	123 447 19 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	133 57 7 0 0 1 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	134 0 5 512 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	158 102 92 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	179 95 68 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	187 1176 28 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	190 75 12 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	196 406 21 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	204 240 32 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	206 79 16 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	209 1271 20 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	212 187 18 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	214 116 16 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	229 0 10 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	254 94 10 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	284 97 44 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	307 95 71 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	333 103 75 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	358 0 0 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	388 198 76 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	422 0 89 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	425 0 0 1025 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
[edoc]
@Chapter title@<:s><:#300,8486>Chapter 4 Running Lotus Notes on NetBIOS

@See also prnt@<:s><:R1,0,><:#200,8486>This chapter provides information on installing and using Lotus Notes on a NetBIOS network.

@See also prnt@<:R><:#200,8486>

@Ahead@<:s><:#240,8486><:f220,BArial,0,0,0>About Notes and NetBIOS

<:s><:R1,1,1,1224,><:#200,8486>Lotus Notes is compatible with these NetBIOS network operating systems:

@Bullet@<:R><:#200,8486>DEC PATHWORKS

@Bullet@<:s><:#200,8486>IBM LAN Server

@Bullet@<:s><:#200,8486>Novell NetBIOS

@Bullet@<:#200,8486>Microsoft NetBEUI

<:s><:R1,1,1,1224,><:#200,8486><:>These are the Notes platforms that support the different versions of NetBIOS:

<:s><:R1,1,1,1224,><:t0>

<:s><:R1,1,1,1224,><:#200,8486>

<:R1,1,1,1224,><:#200,8486>

@Ahead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#240,8486><:>About NetBIOS port configuration options

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>The Notes port dialog configuration box contains additional options for configuring a Notes NetBIOS port. You get to this configuration dialog box by selecting File - Tools - Notes Preferences - Ports - NetBIOS Options.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>There are two fields in this box which can be set:

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#1200,8486>Unit number <:f180,BArial,>is an ordinal number assigned to the card to which the protocol driver is binding. The unit number assignments on a computer should start at 0. For example, if you have two network cards in a computer and have three protocols runn
ing on that computer such as NetBIOS, SPX and AppleTalk, with NetBIOS and SPX binding to the first card and AppleTalk binding to the second card, the NetBIOS and SPX ports will have a unit number of 0 and the AppleTalk port will have a unit number of 1. 
<:f>For NetBIOS, the unit number indicates which of multiple NetBIOS networks to use.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:#400,8486>Buffer size indicates the size of the network buffer. yy NEED MORE DETAIL The default is 2000bytes. yy WHEN WOULD YOU WANT TO CHANGE THIS?

@Ahead@<:s><:R1,1,1,1224,><:#240,8486>About Notes NetBIOS network drivers

<:s><:R1,1,1,1224,><:#200,8486>Notes includes two NetBIOS network drivers:

@Bullet@<:R1,1,1,1224,><:#400,8486>$NETBIOS.DLL uses the Submit interface and makes calls to NETAPI.DLL. To use this driver, you must install the IBM LAN Requester and start the LAN Requester before running Notes.

@Bullet@<:R1,1,1,1224,><:#200,8486>$IBMEENB.DLL uses the NB30 interface and makes calls to ACSNETB.DLL

<:R><:#200,8486>In most cases, you use $NETBIOS.DLL. Use $IBMEENB.DLL with these configurations:

@Bullet@<:R1,1,1,1224,><:#600,8486>IBM LAN Server 2.0 (or 3.0) LAN Requester is not installed, thus requiring the use of IBM NetBIOS. Without IBM LAN Server 2.0 (or 3.0) to provide the Submit interface API for IBM NetBIOS, the only API available to route NetBIOS calls over NetBEUI is the NB3
0 interface. 

@Bullet@<:R1,1,1,1224,><:#800,8486>IBM LAN Server 2.0 (or 3.0) or IBM Extended Services 1.0 and Novell NetWare Requestor for OS/2 2.0 are installed. The end-user who is running an application that only supports the NB30 interface, and wants to use Novell NetWare IPX-based NetBIOS, and, on th
e same system, IBM NetBIOS must be used for another application (also via the NB30 interface).

<:s><:R><:#200,8486>

<:#200,8486>

@Ahead@<:#240,8486><-!><:f220,BArial,0,0,0>About running<:f><:f220,BArial,0,0,0> Notes on 
<:f><:f220,BArial,0,0,0>PATHWORKS<:f>

<:#800,8486>DEC PATHWORKS is the Digital Equipment Corporation (DEC) networking software that connects workstations to servers across a DECnet</Y> network. You can connect Notes servers and workstations on DECnet networks across various hardware and software platforms.
 The Notes servers and workstations that support PATHWORKS are:

@Bullet@<:s><:#200,8486>OS/2 server and workstation

@Bullet@<:#200,8486>Windows 3.1 and Windows for Workgroups server and workstation

@Bullet@<:s><:#200,8486>Windows NT server

@Bullet@<:s><:#200,8486>Windows 95 workstation

@Bhead@<:#220,8486>Advantages of running Notes on PATHWORKS

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Provides Notes with access to the DECnet/OSI protocol on a wide area network (WAN).

@Bullet@<:s><:R1,1,1,1224,><:#400,8486>Provides a method of storing Notes server and workstation files on a VAX, which saves disk space on Notes servers and workstations.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Allows Notes users to use VAX/VMS print resources on a VAX/VMS

@Bullet@<:R1,1,1,1224,><:#600,8486>Allows Notes users to configure remote Notes workstations and servers for remote communications on PATHWORKS. This allows Notes users to dial into a DECnet routing node for access to any Notes server on the DECnet network.

@Bhead@<:R1,1,1,1224,><:#220,8486>System requirements for Notes and PATHWORKS

<:s><:R><:#400,8486>Consult the Lotus Notes Installation Guide for details about Notes server and workstation hardware and software requirements.

@Bhead@<:#220,8486>Recommendations when running Notes on PATHWORKS

@Bullet@<:R1,1,1,1224,><:#400,8486>Notes does not support combining PATHWORKS with other network operating systems, such as Novell, Banyan, or those based on LAN Manager.

@Bullet@<:R1,1,1,1224,><:#400,8486>A PATHWORKS DOS workstation with "NetWare Coexistence for PATHWORKS for DOS" , which is a companion product to PATHWORKS for DOS, cannot access NetWare Notes servers.

@Bullet@<:R1,1,1,1224,><:#400,8486>Do not make partial upgrades from one version of PATHWORKS to another. All OS/2 workstations on a DEC PATHWORKS network must have the same version level.<:>

@Bhead@<:R1,1,1,1224,><:#220,8486>About data security with PATHWORKS

<:s><:R1,1,1,720,><:#600,8486><:><:>If you store Notes databases on a VAX logical drive, limit access to this shared drive to one Notes server. If you store data from multiple Notes servers on the same VAX, create a secure logical drive for each server.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>When Notes server files are on a VMS system, the Notes and VMS system administrators must maintain optimum security. The VMS administrator must create a file service on the VAX, providing access to Notes databases stored on a VMS system only to the Notes se
rver that owns it. The PATHWORKS USE command makes the files inaccessible to other systems on the network, including other Notes servers, workstations, and non-Notes systems.

<:R1,1,1,1224,><:#400,8486>If you do not secure the VMS system, you could lose or corrupt your data and possibly cause the Notes server to crash.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,1,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Storing files on a VAX/VMS

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,2,1
@@EndSection

>

@Bhead title@<:s><:R1,1,1,1224,><:#220,8486><:><:>About storing Notes files on a VAX/VMS system

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>To save disk space on Notes servers and workstations, store Notes files on VAX/VMS systems.

@Chead@<:s><:R><:#200,8486>Notes server files

<:R1,1,1,1224,><:#600,8486>Store Notes databases on a PATHWORKS for VAX/VMS system. Use PATHWORKS for VAX/VMS file services to create a logical disk drive for the Notes server. This allows you to store Notes server files on a VAX/VMS system.

@Chead@<:s><:R><:#200,8486>Notes workstation files

<:R1,1,1,1224,><:#600,8486>Store Notes executables and personal database and workspace files, such as user ID files and the DESKTOP.DSK file, on the VAX drive. If you save Notes user IDs on the VAX drive, remember to password-protect them.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,3,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: About data security and PATHWORKS

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,4,1
@@EndSection

>

<:R1,1,1,1224,><:#200,8486>

@Ahead@<:R><:#240,8486><:><:><:><:>About running Notes and PATHWORKS on OS/2

@Ahead@<:#240,8486>Setting up Notes and PATHWORKS on OS/2

@Ahead@<:#480,8486>About running Notes and PATHWORKS on Windows 3.1 and Windows for Workgroups

@Ahead@<:#480,8486>Setting up Notes and PATHWORKS on Windows 3.1 and Windows for Workgroups

@Ahead@<:#240,8486>About running Notes and PATHWORKS on Windows NT

<:#600,8486>The Windows NT server provides built-in network support that makes it compatible with the DEC PATHWORKS network. You can run the Notes server for Windows NT on DEC PATHWORKS without any additional PATHWORKS or NT configuration, you just need to enable the N
otes NetBIOS port.

@Ahead@<:#240,8486>Setting up Notes and PATHWORKS on Windows NT

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><-!><-!>Launch the Notes workstation program on your NT server.

@Numbered list@<:s><:R><:#200,8486>Enable the network port for NetBIOS.

@Numbered list@<:s><:#200,8486>Restart the NT server.

<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>This port may have already been enabled when you installed Notes on the NT server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,5,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG)

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,6,1
@Build tag@@EndSection

>

<:R><:#200,8486>Print refs: Install Guide for setting up first port, Admin Guide port setup info in Ch.3?

@Ahead@<:#240,8486>About running Notes and PATHWORKS on Windows 95

@Ahead@<:#240,8486>Setting up Notes and PATHWORKS on Windows 95

@Ahead@<:#240,8486>

@Ahead@<:#240,8486>Setting up PATHWORKS on an Ethernet LAN

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>You can install the Notes server or workstation software on PATHWORKS for OS/2 systems, or a Notes workstation (only) on systems with PATHWORKS for DOS running Windows 3.0. When running Windows, you must run the PATHWORKS Windows setup utility, WIN3SETU, to
 configure PATHWORKS for DOS to use with Windows. For more information, see the PATHWORKS for DOS: Microsoft Windows Support Guide from DEC. For Windows 3.1, there is no need to run WIN3SETU.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>When using NETSETUP to install PATHWORKS for DOS on the workstation, load the Redirector in low memory by selecting the REDIR setting RAM. Do not select XMS. PATHWORKS does not support XMS. 

@Ahead@<:R><:#240,8486>Setting up PATHWORKS using NetBIOS Applications and LANSESS

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>It's best not to load LANSESS, but if you must, here are the switches you must set during NETSETUP:

<:R1,3,1,360,1,720,1,3600,><:#200,8486>Controller/Client 	Recommended LANSESS Switch Setting

<:R1,3,1,360,1,720,1,3600,><:#800,8486>3C523		/R:4 /W:4<**>3C503		/R:1 /W:4<**>NDIS		/R:4 /W:4<**>DEPCA, DE100, DE200	/R:4 /W:4

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>Setting these switches eliminates read/write errors and improves performance by fine-tuning read/write transaction sizes. 

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,7,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Troubleshooting: You get a random share errors message when you load LANSESS<-!>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,8,1
@@EndSection

>

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>

@Ahead@<:R><:#240,8486>Setting up PATHWORKS on a DECnet WAN

<:#800,8486>On an existing DECnet WAN, if your Notes server names are different from DECnet node names, you need to use the PATHWORKS Network Control Program (NCP) to define the Notes server remote-adapter-name parameter tells DECnet on which DECnet node the Notes serv
er resides, as in the following example.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>DEFINE REMOTE-ADAPTER-NAME "server_name    +" NODE node_name

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>where server_name is the name of the Lotus Notes server, and node_name is the name of the network node.

@Bullet@<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>In some versions of PATHWORKS, the remote-adapter-name must be exactly 16 characters. For server names that have fewer than 16 characters, use spaces to fill in the name to 15 characters and use a plus (+) sign as the sixteenth and final character such as, 
STAR_ZONE+.

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>If you're unsure of the Notes server name, use the Notes SHOW TASKS server command to display the server name.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>yy WHICH FILE DOES THIS SETTING GO INTO?

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>yy WHAT ABOUT WHEN YOU SET UP PATHWORKS ON A REMOTE LAN?

@Ahead@<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#240,8486>Setting up PATHWORKS to run on DOS 5.0

<:R><:#600,8486>PATHWORKS for DOS 4.0 does not officially support DOS 5.0. However, you can use the DOS SETVER utility to enable PATHWORKS for DOS 4.0 to run on DOS 5.0. Edit your CONFIG.SYS file to include this line: 

@Mono@<:#200,8486>device=C:\<<rDOSdirectory<;>\setver.exe

<:#200,8486>Then restart your system so these commands will take effect:

@Mono@<:#2200,8486>setver redir.exe 4.00<**>setver use.exe 4.00<**>setver emsload.exe 4.00<**>setver sch.exe 4.00<**>setver netsetup.exe 4.00<**>setver ncp.exe 4.00<**>setver dnnethat.exe 4.00<**>setver lad.exe 4.00<**>setver dll.exe 4.00<**>setver memman.exe 4.00<**>setver s
how.exe 4.00

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>For information on the SETVER command, see the DOS 5.0 User's Guide and Reference manual.

@Chead title@<:R1,1,1,1224,><:#200,8486>Example:  CONFIG.SYS file for PATHWORKS yy find release of PW

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#9200,8486>PROTSHELL=C:\OS2\PMSHELL.EXE C:\OS2\OS2.INI C:\OS2\OS2SYS.INI <**>    C:\OS2\CMD.EXE<**>SET COMSPEC=C:\OS2\CMD.EXE<**>LIBPATH=C:\PCSAOS2\DLL;C:\LANMAN\NETLIB;C:\OS2\DLL;C:\;D:\Notes;<**>SET PATH=C:\PCSAOS2\PBIN;C:\LANMAN\NETPROG;C:\OS2;<**>    C:\OS2\SYSTEM
;C:\OS2\INSTALL;C:\;D:\Notes;<**>SET DPATH=C:\PCSAOS2\DECNET;C:\PCSAOS2\PBIN;C:\PCSAOS2\CS;<**>   C:\LANMAN\NETPROG;C:\LANMAN\NETLIB;C:\OS2;C:\OS2\SYSTEM;<**>   C:\OS2\INSTALL;C:\;<**>SET PROMPT=$i<[>$p]<**>SET HELP=C:\OS2\HELP<**>BUFFERS=30<**>DISKCACHE=64
<**>MAXWAIT=3<**>MEMMAN=SWAP,MOVE,SWAPDOS<**>PROTECTONLY=NO<**>SWAPPATH=C:\OS2\SYSTEM 512<**>THREADS=128<**>COUNTRY=001,C:\OS2\SYSTEM\COUNTRY.SYS<**>DEVINFO=SCR,VGA,C:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_IBMVGA<**>SET VIO_IBMVGA=DEVICE(BVHVGA)<**>DEVICE
=C:\OS2\PMDD.SYS<**>SET KEYS=ON<**>SET BOOKSHELF=C:\OS2\BOOK<**>SHELL=C:\OS2\COMMAND.COM /P<**>BREAK=OFF<**>FCBS=16,8<**>RMSIZE=640<**>DEVICE=C:\OS2\EGA.SYS 
<**>DEVICE=C:\OS2\DOS.SYS <**>IOPL=YES<**>REM *************** PATHWORKS for OS/2 2.0 *****************<**>REM *************** Do not modify this block *****************<**>SET DECNET=C:\PCSAOS2\DECNET<**>SET DNETPATH=C:\PCSAOS2\DECNET<**>SET DNETMAIL=C:\PCS
AOS2\MAIL<**>DEVICE=C:\PCSAOS2\DEV\PROTMAN.OS2 /I:C:\PCSAOS2\DEV<**>DEVICE=C:\PCSAOS2\DEV\ELNKII.OS2<**>DEVICE=C:\PCSAOS2\DEV\DLLMAC.SYS<**>DEVICE=C:\PCSAOS2\DEV\DNP.SYS<**>DEVICE=C:\PCSAOS2\DEV\IOCBDRV.SYS<**>DEVICE=C:\LANMAN\DRIVERS\PROTOCOL\NETBEUI\NETBE
UI.OS2<**>DEVICE=C:\LANMAN\NETPROG\RDRHELP.SYS<**>IFS=C:\LANMAN\NETPROG\NETWKSTA.SYS /I:C:\LANMAN<**>REM *************** PATHWORKS for OS/2 2.0 *****************

@Chead title@<:R><:#200,8486>Example:  LANMAN.INI file for PATHWORKS yy find release of PW

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>;LAN Manager initialization file, for server configuration.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><[>networks]<**>This info is read by redir at device init time.  It is available to apps via NetBiosEnum.<**>  net1 = dec$nbe, 0<**>  net2 = netbeui$, 0

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486><[>workstation]<**>  ComputerName = PATWRK

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#4600,8486>;The following parameters generally do not need to be changed by the user. 
<**>  charcount = 16<**>  chartime = 250<**>  charwait = 3600<**>  domain = LANGROUP<**>  keepconn = 600<**>  keepsearch = 600<**>  mailslots = yes<**>  maxcmds = 16<**>  maxerrorlog = 100<**>  maxthreads = 10<**>  maxwrkcache = 64<**>  numalerts = 12<**>  
numcharbuf = 10<**>  numdgrambuf = 14<**>  numservices = 8<**>  numworkbuf = 15<**>  othdomains = 
<**>  printbuftime = 90<**>  sesstimeout = 45<**>  sizcharbuf  = 512<**>  sizerror = 1024<**>  sizworkbuf = 4096

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>; The next lines help you to locate bits in the wrkheuristics entry.<**>;                           1         2         3         4<**>                  01234567890123456789012345678901234567890<**>  wrkheuristics = 11111111213111111100010111200112210000000

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>  wrknets = net1, net2<**>  wrkservices = netpopup

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486><[>messenger]<**>  logfile = messages.log<**>  sizmessbuf = 4096

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><[>netshell]<**>  refresh = 15<**>  remote =<**>  username = AVALON

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#2000,8486><[>server]<**>  alertnames = AVALON<**>  auditing = no<**>  autodisconnect = -1<**>  autopath = srvauto.pro<**>  autoprofile = load<**>  maxusers = 10<**>  noauditing =<**>  security = share<**>  srvcomment = PATHWORKS for OS/2 2.0

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>; The following parameters generally do not need to be<**>; changed by the user.  NOTE:  srvnets= is represented in<**>; the server info struct as a 16-bit lan mask.  Srvnet names<**>; are converted to indexes within <[>networks] for the named nets.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#5200,8486>  accessalert = 5<**>  alertsched = 5<**>  diskalert = 300<**>  erroralert = 5<**>  guestacct = GUEST<**>  logonalert = 5<**>  maxauditlog = 100<**>  maxchdevjob = 6<**>  maxchdevq = 2<**>  maxchdevs = 2<**>  maxconnections = 128<**>  maxlocks = 64<**>  max
opens = 64<**>  maxsearches = 50<**>  maxsessopens = 50<**>  maxsessreqs = 50<**>  maxsessvcs = 1<**>  maxshares = 16<**>  netioalert = 5<**>  numadmin = 2<**>  numbigbuf = 3<**>  numfiletasks = 1<**>  numreqbuf = 50<**>  sizreqbuf = 1024<**>  srvanndelta =
 3000<**>  srvannounce = 60

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><**>; The next lines help you to locate bits in the srvheuristics entry.<**>;                           1<**>;                 01234567890123456789<**>  srvheuristics = 11110151111211001331

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>  srvhidden = NO<**>  srvnets = net1, net2<**>  srvservices = alerter<**>  userpath = accounts\userdirs

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486><[>alerter]<**>  sizalertbuf = 3072

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486><[>netrun]<**>  maxruns = 3<**>  runpath =

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#2600,8486><[>replicator]<**>  exportlist =<**>  exportpath = repl\export<**>  guardtime = 2<**>  importlist =<**>  importpath = repl\import<**>  interval = 5<**>  logon = user<**>  password =<**>  pulse = 3<**>  random = 60<**>  replicate = IMPORT<**>  tryuser = yes

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>ups]<**>  batterytime = 60<**>  messdelay = 5<**>  messtime = 120<**>  recharge = 100<**>  signals = 100<**>  voltlevels = 100

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486><[>netlogon]<**>  pulse = 300<**>  randomize = 30<**>  scripts = repl\import\scripts<**>  update = yes

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>remoteboot]<**>  configfile = dxmbb.cnf<**>  maxthreads = 10<**>  rpldir = rpl<**>  rpl1 = rplnet1.dll rplnet2.dll rploem.dll 0<**>  ;rpl2 = rplnet1.dll rplnet2.dll rploem.dll 1<**>  ;rpl2 = ethnet1.dll ethnet2.dll ethoem.dll 1

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486><[>services]<**>; Correlates name of service to pathname of service program.<**>; The pathname must be either

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#3000,8486>;	1) an absolute path (including the drive specification)<**>;			OR<**>;       
	2) a path relative to the LanMan root<**>  workstation = services\wksta.exe<**>  server = services\netsvini.exe<**>  messenger = services\msrvinit.exe<**>  netpopup = services\netpopup.exe<**>  alerter = services\alerter.exe<**>  netrun = services\runservr
.exe<**>  replicator = services\replicat.exe<**>  ups = services\ups.exe<**>  netlogon = services\netlogon.exe<**>  remoteboot = services\rplservr.exe<**>  timesource = services\timesrc.exe<**>  recvr = services\recvr.exe<:>

@Ahead@<:R><:p<* >><:><:>About running Notes on IBM LAN Server<-!> (OS/2 only)

<:#1000,8486>The Notes IBM OS/2 Extended Edition NetBIOS network driver, $IBMEENB.DLL, is an alternate NetBIOS driver for IBM OS/2 LAN Server systems. Lotus Notes is certified for the IBM OS/2 LAN Server network software, allowing you to connect Notes servers and workst
ations on IBM OS/2 LAN Server networks across various hardware and software platforms. The IBMEENB driver runs on OS/2 Notes servers and workstations with Presentation Manager.

<:#400,8486>The Lotus Notes IBMEENB network driver uses the NB30 interface. Applications using this interface make their NetBIOS calls to ACSNETB.DLL.

<:R1,13,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,1,5040,1,5760,1,6480,1,7200,1,7920,1,8640,1,9360,><:#200,8486>Running Lotus Notes with $IBMEENB.DLL provides the following features:

@Bullet@<:R1,1,1,1224,><:#600,8486>Supports communications between an OS/2 Notes server or workstation running IBMEENB and any Notes server or workstation running the standard Notes $NETBIOS.DLL network driver on an IBM/Microsoft compatible NetBIOS (NetBEUI) network, including the IBM LAN Su
pport program.

@Bullet@<:R1,1,1,1224,><:#200,8486>Allows IBMEENB users the option of not running IBM OS/2 LAN Server/LAN Requester.

@Note@<:R1,1,1,360,><:#400,8486>IBM Network Transport Services/2 (NTS/2) LAN Adapter and Protocol Support (LAPS) 1.0 is all that is required to run in this environment.

@Bhead@<:s><:R1,1,1,360,><:#220,8486>System requirements for Notes and IBM LAN Server

<:s><:R1,1,1,5760,><:#600,8486>Your Notes and IBM OS/2 LAN Server environment must meet the hardware and software requirements that are outlined in the Lotus Notes Server for OS/2 Installation Guide. In addition, you must have these operating system requirements:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>OS/2 Release 3 or 2.11

@Note@<:R1,1,1,360,><:#400,8486>Lotus Notes operation under IBM OS/2 2.0 with LAN Server has been certified with Service Pack XR06055. To get the service pack, contact IBM at 1-800-992-4777. 

<:s><:R1,1,1,360,><:#200,8486>You must have one of the following network software packages:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>IBM OS/2 LAN Server 3.0 (shipped with IBM Network Transport Services/2)

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>IBM OS/2 LAN Server 2.0 (includes LAN Adapter and Protocol Support)

@Bullet@<:s><:R1,1,1,360,><:#200,8486>IBM Network Transport Services/2 (NTS/2) LAN Adapter and Protocol Support (LAPS) 1.0<:>

<:R1,1,1,360,><:#200,8486>

@Ahead@<:s><:R><:#240,8486>Setting up Notes on IBM LAN Server (OS/2 only)

<:s><:#800,8486>This section provides installation and configuration guidelines for setting up Notes in typical IBM OS/2 LAN Server environments. In this environment, you can use an IBM OS/2 LAN Server as a server (such as a file, printer, or plotter server) or as a reques
ter (a client or workstation). In this documentation, IBM OS/2 LAN Server applies to either configuration.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>IBM NTS/2 is all that is required for Notes if you use the IBMEENB network driver and do not need the other services that LAN Server provides. IBM NTS/2 LAPS 1.0 is available as a separate package, or comes with IBM OS/2 LAN Server 3.0. An earlier version o
f LAPS comes with IBM OS/2 LAN Server 2.0. Refer to the documentation shipped with all three products for more information and guidelines.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>yy REVIEWERS CHECK THESE LAN SERVER REVISION NUMBERS

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>Notes supports the following:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>IBM OS/2 LAN Server 3.0 runs on IBM OS/2 Release 3 and 2.11.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>IBM OS/2 LAN Server 2.0 runs on IBM OS/2 Release 3 and 2.11

<:R1,1,1,1224,><:#200,8486>yy REVIEWERS, IS THIS STILL A NECESSARY WORKAROUND?

<:R1,1,1,1224,><:#800,8486>To run Notes with IBM OS/2 LAN Server 2.0, you must obtain and install the corrective service for IBM APAR IC04628. The APAR correction fixes a TRAP or HANG condition that occurs when a NetBIOS session closes. These replacement files are included with NTS/2
 and IBM OS/2 LAN Server 3.0, or available by calling 1-800-992-4777.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>IBM NTS/2 will run on both IBM OS/2 extended edition for Release 3 or 2.11.

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>IBMEENB supports NetBIOS sessions over IBM OS/2 LAN Server. The default maximum sessions, commands, and names values for NetBIOS are provided in the configuration files with LAN Server 3.0, LAN Server 2.0, or NTS/2. However, these resources are insufficient
 for Notes users and result in the Notes system message:

@Mono@<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>Insufficient network or adapter resources.

<:R1,1,1,1224,><:#400,8486>To change the allocated resources, you must edit the PROTOCOL.INI file or the IBMLAN.INI file, depending on your system configuration.

@Bullet@<:R1,1,1,1224,><:#600,8486>To change the maximum sessions, commands, and names values for Global Resources (PROTOCOL.INI), see the IBM book, Network Transport Services/2 LAN Adapter and Protocol Support Configuration Guide (S96F-8489). 

@Bullet@<:R1,1,1,1224,><:#600,8486>To change the maximum sessions, commands, and names values for  LAN Server Resources (IBMLAN.INI), see the IBM OS/2 LAN Server Network Administrator Reference Volume 2: Performance Tuning, Version 3.0 (S96F-8429).

@Ahead@<:s><:R><:#240,8486>About configuring network resources for the OS/2 Notes server and workstation

@Bhead@<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#220,8486>Notes server

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>The following LAN0 statement in NOTES.INI is the default port definition for the IBMEENB Notes server. 

@Indnt mono@<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>LAN0=$IBMEENB, 0, 50, 2000

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>The third argument (50) results in 50 sessions, 54 commands, 9 names. This argument configures the number of sessions and, indirectly, configures the commands that the Notes server might require. The maximum depends on your system limitations. The minimum i
s 25, resulting in 25 sessions, 29 commands and 9 names. If you specify a number less than 25, Notes allocates 25.

@Bullet@<:R1,1,1,1224,><:#800,8486>For each Notes server task that performs network input/output (I/O), add 16 sessions, 16 commands, and 8 names. Server tasks that require NetBIOS resources are REPLICATOR, ROUTER, and the Notes workstation, if it is being run on the Notes server. Other task
s that might be performing network I/O are CHRONOS and BACKGROUND EXCHANGE.

@Bullet@<:R1,1,1,1224,><:#400,8486>The following recommended  values are set for the Notes server LAN0 default (50) plus the REPLICATOR, ROUTER, and Notes workstation.

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486>Maximum sessions - minimum of 98

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486>Maximum commands - minimum of 102

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486><**>Maximum names - minimum of 33

@Note@<:R1,1,1,360,><:#800,8486>The recommended values above apply only to Notes operation. These values are in addition to those required by or already allocated for LAN Server (IBMLAN.INI) or other NetBIOS applications in the system. The sum of all these NetBIOS resources must not be gr
eater than the global settings in PROTOCOL.INI.

@Bhead@<:s><:R><:#220,8486>Notes workstation

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>The following LAN0 statement in NOTES.INI is the default port definition for an IBMEENB Notes workstation.

@Indnt mono@<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#200,8486>LAN0=$IBMEENB, 0, 50, 2000

<:s><:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>The third argument (50) does not apply to workstations and has no affect on performance. Notes requires 16 sessions, 16  commands, and 9 names for the workstation.

@Bullet@<:R1,1,1,1224,><:#600,8486>For each Notes workstation task that performs network I/O, add 16 sessions, 16 commands, and 8 names. Workstation tasks that  might be performing network I/O are CHRONOS and BACKGROUND EXCHANGE.

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>The following recommended values are set for the OS/2 Notes workstation only:

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486>Maximum sessions - minimum of 16

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486>Maximum commands - minimum of 16

@Indnt bullet@<:s><:R1,1,1,1224,><:#200,8486>Maximum names - minimum of 9

@Note@<:R1,1,1,360,><:#800,8486>The recommended values above apply only to Notes operation. These values are in addition to those required by or already allocated for IBM OS/2 LAN Server (IBMLAN.INI) or other NetBIOS applications in the system. The sum of all these NetBIOS resources must 
not be greater than the global settings in PROTOCOL.INI.

@Chead title@<:R><:#200,8486><:>Example:  CONFIG.SYS file for a Notes Server with IBM OS/2 LAN Server yy add release

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#16800,8486>IFS=D:\OS2\HPFS.IFS  /CACHE:64 /CRECL:4<**>PROTSHELL=D:\OS2\PMSHELL.EXE<**>SET USER_INI=D:\OS2\OS2.INI<**>SET SYSTEM_INI=D:\OS2\OS2SYS.INI<**>SET OS2_SHELL=D:\OS2\CMD.EXE<**>SET AUTOSTART=PROGRAMS,TASKLIST,FOLDERS<**>SET RUNWORKPLACE=D:\OS2\PMSHELL.EXE<**>S
ET COMSPEC=D:\OS2\CMD.EXE<**>LIBPATH=D:\IBMLAN\NETLIB;D:\MUGLIB\DLL;D:\IBMCOM\DLL;.;D:\OS2\DLL;<**>D:\OS2\MDOS;D:\;D:\OS2\APPS\DLL;E:\NOTES<**>SET PATH=D:\IBMLAN\NETPROG;D:\MUGLIB;D:\OS2;D:\OS2\SYSTEM;D:\OS2\MDOS\<**>	WINOS2;<**>D:\OS2\INSTALL;D:\;D:\OS2\MD
OS;D:\OS2\APPS;E:\NOTES;E:\DATA<**>SET DPATH=D:\IBMLAN\NETPROG;D:\IBMLAN;D:\MUGLIB;D:\IBMCOM;D:\OS2;D:\OS2\<**>	SYSTEM;<**>D:\OS2\MDOS\WINOS2;D:\OS2\INSTALL;D:\;D:\OS2\BITMAP;D:\OS2\MDOS;D:\<**>OS2\APPS;<**>SET PROMPT=$i<[>$p]<**>SET HELP=D:\OS2\HELP;D:\OS2
\HELP\TUTORIAL;<**>SET GLOSSARY=D:\OS2\HELP\GLOSS;<**>PRIORITY_DISK_IO=YES<**>FILES=20<**>DEVICE=D:\IBMCOM\PROTOCOL\LANPDD.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANVDD.OS2<**>DEVICE=D:\IBMCOM\LANMSGDD.OS2 /I:D:\IBMCOM 
<**>DEVICE=D:\IBMCOM\PROTMAN.OS2 /I:D:\IBMCOM<**>DEVICE=D:\OS2\TESTCFG.SYS<**>DEVICE=D:\OS2\DOS.SYS<**>DEVICE=D:\OS2\PMDD.SYS<**>BUFFERS=30<**>IOPL=YES<**>DISKCACHE=512,LW<**>MAXWAIT=1<**>MEMMAN=SWAP,PROTECT<**>REM SWAPPATH=D:\OS2\SYSTEM 2048 2048<**>SWAPPA
TH=E:\SWAP 2048 2048<**>BREAK=OFF<**>THREADS=255<**>PRINTMONBUFSIZE=134,134,134<**>COUNTRY=001,D:\OS2\SYSTEM\COUNTRY.SYS<**>SET KEYS=ON<**>REM SET DELDIR=C:\DELETE,512;D:\DELETE,512;E:\DELETE,512;<**>BASEDEV=PRINT01.SYS<**>BASEDEV=IBM1FLPY.ADD<**>BASEDEV=IB
M1S506.ADD<**>BASEDEV=OS2DASD.DMD<**>SET BOOKSHELF=D:\IBMLAN\BOOK;D:\OS2\BOOK<**>SET EPATH=D:\OS2\APPS<**>REM DEVICE=D:\OS2\APPS\SASYNCDA.SYS 
<**>PROTECTONLY=NO<**>SHELL=D:\OS2\MDOS\COMMAND.COM D:\OS2\MDOS /P<**>FCBS=16,8<**>RMSIZE=640<**>DEVICE=D:\OS2\MDOS\VEMM.SYS 
<**>DEVICE=D:\OS2\MDOS\VMOUSE.SYS <**>DOS=LOW,NOUMB<**>DEVICE=D:\OS2\MDOS\VDPX.SYS 
<**>DEVICE=D:\OS2\MDOS\VXMS.SYS /UMB<**>DEVICE=D:\OS2\MDOS\VDPMI.SYS 
<**>DEVICE=D:\OS2\MDOS\VWIN.SYS    <**>DEVICE=D:\OS2\MDOS\VCDROM.SYS 
<**>DEVINFO=SCR,VGA,D:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_VGA<**>SET VIO_VGA=DEVICE(BVHVGA)<**>DEVICE=D:\OS2\MDOS\VVGA.SYS  
<**>DEVICE=D:\OS2\POINTDD.SYS <**>DEVICE=D:\OS2\MOUSE.SYS <**>DEVICE=D:\OS2\COM.SYS<**>DEVICE=D:\OS2\MDOS\VCOM.SYS 
<**>CODEPAGE=437,850<**>DEVINFO=KBD,US,D:\OS2\KEYBOARD.DCP<**>TIMESLICE=33,59<**>RUN=D:\IBMCOM\PROTOCOL\NETBIND.EXE<**>RUN=D:\IBMCOM\LANMSGEX.EXE<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBEUI.OS2<**>DEVICE=D:\IBMLAN\NETPROG\RDRHELP.200<**>IFS=D:\IBMLAN\NETPROG\NETWK
STA.200 /I:D:\IBMLAN/N<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBIOS.OS2<**>DEVICE=D:\IBMCOM\MACS\IBMTOK.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANDD.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANDLLDD.OS2<**>DEVICE=D:\IBMCOM\MACS\ELNKII.OS2<**>RUN=D:\IBMCOM\PROTOCOL\LANDLL.EXE<**>
RUN=D:\IBMLAN\NETPROG\LSDAEMON.EXE

@Chead title@<:R><:#200,8486>Example:  IBMLAN.INI file for a Notes Server with IBM OS/2 LAN Server  yy add release

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>; OS/2 LAN Requester initialization file<**><[>networks]<**>  net1 = NETBEUI$,0,LM10,32,50,14<**>  net2 = NETBEUI$,1,LM10,32,50,14

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>; This information is read by the redirector at device initialization time.<**><[>requester]<**>  COMPUTERNAME = MISO<**>  DOMAIN = MISODOM

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#4400,8486>; The following parameters generally do not need to be<**>; changed by the user.<**>  charcount = 16<**>  chartime = 250<**>  charwait = 3600<**>  keepconn = 600<**>  keepsearch = 600<**>  maxcmds = 16<**>  maxerrorlog = 100<**>  maxthreads = 10<**>  maxwrk
cache = 64<**>  numalerts = 12<**>  numcharbuf = 10<**>  numservices = 7<**>  numworkbuf = 15<**>  numdgrambuf = 14<**>  othdomains = 
<**>  printbuftime = 90<**>  sesstimeout = 45<**>  sizcharbuf = 512<**>  sizerror = 1024<**>  sizworkbuf = 4096

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>; The next lines help you to locate bits in the wrkheuristics entry.<**>;                           1         2         3<**>;                 0123456789012345678901234567890123

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>  wrkheuristics = 1111111121311111110001011120111221<**>  wrkservices = LSCLIENT,MESSENGER,NETPOPUP,PEER<**>  wrknets = NET1,NET2

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486><[>messenger]<**>  logfile = messages.log<**>  sizmessbuf = 4096

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><[>peer]<**>  security = User<**>  username = KDOMO<**>  auditing = no

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#4400,8486>; The following parameters generally do not need to be<**>; changed by the user. NOTE : srvnets= is represented in<**>; the server info struct as a 16-bit lan mask. Srvnet names<**>; are converted to indexes within <[>networks] for the named nets.<**>  gues
tacct = guest<**>  autodisconnect = -1<**>  maxauditlog = 100<**>  maxchdevjob = 2<**>  maxchdevs = 1<**>  maxconnections = 26<**>  maxlocks = 64<**>  maxopens = 128<**>  maxsearches = 50<**>  maxsessopens = 120<**>  maxsessreqs = 25<**>  maxsessvcs = 1<**>
  maxshares = 16<**>  maxusers = 5<**>  numbigbuf = 4<**>  numfiletasks = 1<**>  numreqbuf = 10<**>  sizreqbuf = 4096

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>; The next lines help you to locate bits in the srvheuristics entry.<**>;                           1<**>;                 0123456789012345678

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>  srvheuristics = 1111014111131100133<**>  SRVSERVICES = <**>  srvnets = NET1,NET2

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486><[>lsclient]<**>  multilogon = no<**>  timesync = yes<**>  logonverification = local<**>  logonwarningmsgs = all

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486><[>replicator]<**>  replicate = IMPORT<**>  importpath = D:\ibmlan\repl\import<**>  tryuser = yes<**>  password = 

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#2400,8486><[>services]<**>; Correlates name of service to pathname of service program.<**>; The pathname must be either<**>;       1) an absolute path (including the drive specification)<**>;                       OR<**>;       2) a path relative to the IBMLAN root<**>
  lsclient = services\lsclient.exe<**>  messenger = services\msrvinit.exe<**>  netpopup = services\netpopup.exe<**>  peer = services\netpsini.exe<**>  replicator = services\replicat.exe<**>  requester = services\wksta.exe

@Chead title@<:R><:#200,8486>Example:  PROTOCOL.INI file for a Notes Server with IBM LAN Server yy add release

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486><[>PROT_MAN]<**>   DRIVERNAME = PROTMAN$

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#5800,8486><[>IBMLXCFG]<**>   IBMTOK_nif = IBMTOK.nif<**>   NETBEUI_nif = NETBEUI.nif<**>   LANDD_nif = LANDD.nif<**>   ELNKII_nif = ELNKII.nif<**><[>LANDD_nif]<**>   DriverName = LANDD$<**>   Bindings = IBMTOK_nif,ELNKII_nif<**>   ETHERAND_TYPE = "I","I"<**>   SYSTEM
_KEY = 0x0,0x0<**>   OPEN_OPTIONS = 0x2000,0x2000<**>   TRACE = 0x0,0x0<**>   LINKS = 8,8<**>   MAX_SAPS = 3,3<**>   MAX_G_SAPS = 0,0<**>   USERS = 3,3<**>   TI_TICK_G1 = 255,255<**>   T1_TICK_G1 = 15,15<**>   T2_TICK_G1 = 3,3<**>   TI_TICK_G2 = 255,255<**>
   T1_TICK_G2 = 25,25<**>   T2_TICK_G2 = 10,10<**>   IPACKETS = 250,250<**>   UIPACKETS = 100,100<**>   MAXTRANSMITS = 6,6<**>   MINTRANSMITS = 2,2<**>   TCBS = 64,64<**>   GDTS = 30,30<**>   ELEMENTS = 800,800

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#6000,8486><[>NETBEUI_nif]<**>   DriverName = netbeui$<**>   Bindings = IBMTOK_nif,ELNKII_nif<**>   ETHERAND_TYPE = "I"<**>   USEADDRREV = "YES"<**>   OS2TRACEMASK = 0x0<**>   SESSIONS = 130<**>   NCBS = 152<**>   NAMES = 47<**>   SELECTORS = 5<**>   USEMAXDATAGRAM = 
"NO"<**>   ADAPTRATE = 1000<**>   WINDOWERRORS = 0<**>   MAXDATARCV = 4168<**>   TI = 30000<**>   T1 = 500<**>   T2 = 200<**>   MAXIN = 1<**>   MAXOUT = 1<**>   NETBIOSTIMEOUT = 500<**>   NETBIOSRETRIES = 8<**>   NAMECACHE = 0<**>   PIGGYBACKACKS = 1<**>   
DATAGRAMPACKETS = 2<**>   PACKETS = 350<**>   LOOPPACKETS = 1<**>   PIPELINE = 5<**>   MAXTRANSMITS = 6<**>   MINTRANSMITS = 2<**>   DLCRETRIES = 5

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>IBMTOK_nif]<**>   DriverName = IBMTOK$<**>   ADAPTER = "PRIMARY"<**>   MAXTRANSMITS = 6<**>   RECVBUFS = 2<**>   RECVBUFSIZE = 256<**>   XMITBUFS = 1

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>ELNKII_nif]<**>   DriverName = ELNKII$<**>   interrupt = 3<**>   ioaddress = 0x300<**>   transceiver = "EXTERNAL"<**>   maxtransmits = 8<**>   xmitbufs = 2

@Chead title@<:R><:#200,8486>Example:  CONFIG.SYS file for a Notes Server with NTS/2 LAPS  yy add release

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#15400,8486>IFS=D:\OS2\HPFS.IFS  /CACHE:64 /CRECL:4<**>PROTSHELL=D:\OS2\PMSHELL.EXE<**>SET USER_INI=D:\OS2\OS2.INI<**>SET SYSTEM_INI=D:\OS2\OS2SYS.INI<**>SET OS2_SHELL=D:\OS2\CMD.EXE<**>SET AUTOSTART=PROGRAMS,TASKLIST,FOLDERS<**>SET RUNWORKPLACE=D:\OS2\PMSHELL.EXE<**>S
ET COMSPEC=D:\OS2\CMD.EXE<**>LIBPATH=D:\IBMCOM\DLL;.;D:\OS2\DLL;D:\OS2\MDOS;D:\;D:\OS2\APPS\DLL;E:\NOTES<**>SET PATH=D:\OS2;D:\OS2\SYSTEM;D:\OS2\MDOS\WINOS2;<**>D:\OS2\INSTALL;D:\;D:\OS2\MDOS;D:\OS2\APPS;E:\NOTES;E:\DATA<**>SET DPATH=D:\IBMCOM;D:\OS2;D:\OS2
\SYSTEM;D:\OS2\MDOS\WINOS2;<**>D:\OS2\INSTALL;D:\;D:\OS2\BITMAP;D:\OS2\MDOS;D:\OS2\APPS;<**>SET PROMPT=$i<[>$p]<**>SET HELP=D:\OS2\HELP;D:\OS2\HELP\TUTORIAL;<**>SET GLOSSARY=D:\OS2\HELP\GLOSS;<**>PRIORITY_DISK_IO=YES<**>FILES=20<**>DEVICE=D:\IBMCOM\PROTOCOL
\LANPDD.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANVDD.OS2<**>DEVICE=D:\IBMCOM\LANMSGDD.OS2 /I:D:\IBMCOM 
<**>DEVICE=D:\IBMCOM\PROTMAN.OS2 /I:D:\IBMCOM<**>DEVICE=D:\OS2\TESTCFG.SYS<**>DEVICE=D:\OS2\DOS.SYS<**>DEVICE=D:\OS2\PMDD.SYS<**>BUFFERS=30<**>IOPL=YES<**>DISKCACHE=512,LW<**>MAXWAIT=1<**>MEMMAN=SWAP,PROTECT<**>REM SWAPPATH=D:\OS2\SYSTEM 2048 2048<**>SWAPPA
TH=E:\SWAP 2048 2048<**>BREAK=OFF<**>THREADS=255<**>PRINTMONBUFSIZE=134,134,134<**>COUNTRY=001,D:\OS2\SYSTEM\COUNTRY.SYS<**>SET KEYS=ON<**>REM SET DELDIR=C:\DELETE,512;D:\DELETE,512;E:\DELETE,512;<**>BASEDEV=PRINT01.SYS<**>BASEDEV=IBM1FLPY.ADD<**>BASEDEV=IB
M1S506.ADD<**>BASEDEV=OS2DASD.DMD<**>SET BOOKSHELF=D:\OS2\BOOK<**>SET EPATH=D:\OS2\APPS<**>REM DEVICE=D:\OS2\APPS\SASYNCDA.SYS 
<**>PROTECTONLY=NO<**>SHELL=D:\OS2\MDOS\COMMAND.COM D:\OS2\MDOS /P<**>FCBS=16,8<**>RMSIZE=640<**>DEVICE=D:\OS2\MDOS\VEMM.SYS 
<**>DEVICE=D:\OS2\MDOS\VMOUSE.SYS <**>DOS=LOW,NOUMB<**>DEVICE=D:\OS2\MDOS\VDPX.SYS 
<**>DEVICE=D:\OS2\MDOS\VXMS.SYS /UMB<**>DEVICE=D:\OS2\MDOS\VDPMI.SYS 
<**>DEVICE=D:\OS2\MDOS\VWIN.SYS    <**>DEVICE=D:\OS2\MDOS\VCDROM.SYS 
<**>DEVINFO=SCR,VGA,D:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_VGA<**>SET VIO_VGA=DEVICE(BVHVGA)<**>DEVICE=D:\OS2\MDOS\VVGA.SYS  
<**>DEVICE=D:\OS2\POINTDD.SYS <**>DEVICE=D:\OS2\MOUSE.SYS <**>DEVICE=D:\OS2\COM.SYS 
<**>DEVICE=D:\OS2\MDOS\VCOM.SYS <**>CODEPAGE=437,850<**>DEVINFO=KBD,US,D:\OS2\KEYBOARD.DCP<**>TIMESLICE=33,59<**>RUN=D:\IBMCOM\PROTOCOL\NETBIND.EXE<**>RUN=D:\IBMCOM\LANMSGEX.EXE<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBEUI.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBIOS.O
S2<**>DEVICE=D:\IBMCOM\MACS\IBMTOK.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANDD.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANDLLDD.OS2<**>DEVICE=D:\IBMCOM\MACS\ELNKII.OS2<**>RUN=D:\IBMCOM\PROTOCOL\LANDLL.EXE

@Chead title@<:R><:#200,8486>Example:  PROTOCOL.INI for a Notes Server running IBM NTS/2 LAPS  yy add release

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>PROT_MAN]<**>   DRIVERNAME = PROTMAN$<**><[>IBMLXCFG]<**>   IBMTOK_nif = IBMTOK.nif<**>   NETBEUI_nif = NETBEUI.nif<**>   LANDD_nif = LANDD.nif<**>   ELNKII_nif = ELNKII.nif

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#4800,8486><[>LANDD_nif]<**>   DriverName = LANDD$<**>   Bindings = IBMTOK_nif,ELNKII_nif<**>   ETHERAND_TYPE = "I","I"<**>   SYSTEM_KEY = 0x0,0x0<**>   OPEN_OPTIONS = 0x2000,0x2000<**>   TRACE = 0x0,0x0<**>   LINKS = 8,8<**>   MAX_SAPS = 3,3<**>   MAX_G_SAPS = 0,0<**>
   USERS = 3,3<**>   TI_TICK_G1 = 255,255<**>   T1_TICK_G1 = 15,15<**>   T2_TICK_G1 = 3,3<**>   TI_TICK_G2 = 255,255<**>   T1_TICK_G2 = 25,25<**>   T2_TICK_G2 = 10,10<**>   IPACKETS = 250,250<**>   UIPACKETS = 100,100<**>   MAXTRANSMITS = 6,6<**>   MINTRANS
MITS = 2,2<**>   TCBS = 64,64<**>   GDTS = 30,30<**>   ELEMENTS = 800,800

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#6000,8486><[>NETBEUI_nif]<**>   DriverName = netbeui$<**>   Bindings = IBMTOK_nif,ELNKII_nif<**>   ETHERAND_TYPE = "I"<**>   USEADDRREV = "YES"<**>   OS2TRACEMASK = 0x0<**>   SESSIONS = 98<**>   NCBS = 102<**>   NAMES = 33<**>   SELECTORS = 5<**>   USEMAXDATAGRAM = "
NO"<**>   ADAPTRATE = 1000<**>   WINDOWERRORS = 0<**>   MAXDATARCV = 4168<**>   TI = 30000<**>   T1 = 500<**>   T2 = 200<**>   MAXIN = 1<**>   MAXOUT = 1<**>   NETBIOSTIMEOUT = 500<**>   NETBIOSRETRIES = 8<**>   NAMECACHE = 0<**>   PIGGYBACKACKS = 1<**>   D
ATAGRAMPACKETS = 2<**>   PACKETS = 350<**>   LOOPPACKETS = 1<**>   PIPELINE = 5<**>   MAXTRANSMITS = 6<**>   MINTRANSMITS = 2<**>   DLCRETRIES = 5

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486><[>IBMTOK_nif]<**>   DriverName = IBMTOK$<**>   ADAPTER = "PRIMARY"<**>   MAXTRANSMITS = 6<**>   RECVBUFS = 2<**>   RECVBUFSIZE = 256<**>   XMITBUFS = 1

<:R><:#1400,8486><[>ELNKII_nif]<**>   DriverName = ELNKII$<**>   interrupt = 3<**>   ioaddress = 0x300<**>   transceiver = "EXTERNAL"<**>   maxtransmits = 8<**>   xmitbufs = 2

<:R1,1,1,360,><:#200,8486>

@Chead title@<:R><:#200,8486>Example: LAN server port status

<:#200,8486>The port status information for a NetBIOS port resembles the following:

@Mono@<:#200,8486>Netbios unit 0 status (LANA Version 2.0)

@Mono@<:R1,5,1,2390,1,2629,1,3830,1,5499,1,6709,><:#2000,8486>Traffic and Error Statistics:	<**>   Reporting period (minutes):	290<**>   Packets transmitted:	0	<**>   Packets received:	0	<**>   CRC errors:	0	<**>   Alignment errors:	0<**>   Collisions:	0<**>   Aborted transmissions:	0<**>   Retransmissions:	0	<**>   R
eceiver exhausted resources:0

@Mono@<:R1,5,1,2390,1,2629,1,3830,1,5499,1,6709,><:#1200,8486>Adapter Resources:<**>   Total command blocks:	12<**>   Available command blocks:	3<**>   Maximum sessions:	6	<**>   Sessions in use:	6	<**>   Session data packet size:	1486

@Mono@<:R1,4,1,2390,1,4901,1,5068,1,6503,><:#1800,8486>Adapter name table (7 names):<**>Name 0: MKTG	Name number: 2	Status: 4 registered<**>Name 1: MKTG	Name number: 3	Status: 4 registered<**>Name 2: SMITH	Name number: 4	Status: 84 grp registered<**>Name 3: JBROWN	Name number: 5	Status: 4 registered<**>Name 4: 
IRISNAMESERVER	3Name number: 6	Status: 84 grp registered<**>Name 5: MARKETING	+Name number: 7	Status: 4 registered<**>Name 6: IRISMULTICAST	/Name number: 8	Status: 84 grp registered

@Mono@<:R1,6,1,2629,1,2917,1,4350,1,6072,1,7459,1,8320,><:#400,8486>Adapter session table (5 sessions):<**>LSN  State  Local Name     Remote Name   Receives      Sends

@Mono@<:R1,6,1,2629,1,2917,1,4350,1,6216,1,7459,1,8320,><:#1000,8486>2  Listen pending	MKTG	*	 0	 0	<**>3  Session created	GFY	R&D SERVER	 0	 0	<**>4  Listen pending	MKTG	*	 0	 0	<**>5  Listen pending	IRISNAMESERVER 3*	 0	 0	6  Listen pending	JANE BROWN +	*	 0	 0

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:R><:#200,8486><:N795478803,JY,65535,9,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Checking the status of a Notes network port

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,10,1
@@EndSection

>

<:R><:#200,8486>print ref:

<:#200,8486>For information on these fields, see Chapter 1.

@Bhead@<:#220,8486>

@Ahead@<:s><:#240,8486>About running Notes on Novell NetBIOS<-!><-!>

<:#600,8486><:>Novell NetBIOS offers a way for Notes users to connect servers and workstations with the NetBIOS protocol, while using Novell NetWare. NetWare Windows .DLL files are not required when using Notes with Novell NetBIOS. Novell NetBIOS is the only type of Ne
tBIOS that can use the Novell IPX protocol.

<:s><:#200,8486>The Notes servers and workstations that support Novell NetBIOS are:

@Bullet@<:s><:#200,8486>OS/2 server and workstation

@Bullet@<:#200,8486>Windows 3.1 and Windows for Workgroups server and workstation

@Bullet@<:s><:#200,8486>Windows NT server

@Bullet@<:s><:#200,8486>Windows 95 workstation

<:#200,8486>

@Ahead@<:#240,8486>About the Novell configuration file (NET.CFG)

<:#800,8486>To run the OS/2 Notes server, you must use a Novell configuration file called NET.CFG to properly allocate resources. NET.CFG sets the network packet frame types and increases default values required by a Notes server. If NET.CFG does not exist on your Note
s server, create it in the root directory of the server.

<:#200,8486>yy add info here on creating NET.CFG and what has to be there for Notes

@Ahead@<:s><:#240,8486>About NetBIOS configurable parameters

<:#400,8486>If you use the Notes NetBIOS network driver, you must configure NetBIOS to provide enough resources to run the OS/2 Notes server. Add the lines below to the NET.CFG file. Press Enter after each line.

@Mono@<:s><:#600,8486>NetWare NetBIOS<**>  sessions 64<**>  commands 96

<:s><:#600,8486>The sessions parameter sets the maximum number of NetBIOS sessions the OS/2 Requester will support. You must increase this parameter to allow multiple user access to the Notes server. The default is 32.

<:s><:#600,8486>The commands parameter sets the number of NetBIOS commands the OS/2 Requester will store while waiting for previous commands to execute. This must also be increased to handle heavy Notes traffic. The default is 12.

<:s><:#600,8486>Without these changes to the parameters, the Notes server will hang when the default settings are exceeded, and existing sessions will be frozen until the system is restarted. For more information on the OS/2 Requester and NetBIOS, see the Novell manual Net
Ware Requester for OS/2 .<-!>

<:R1,1,1,5760,><:#200,8486>

@Ahead@<:R1,1,1,0,><:#240,8486><:><:><-!><-!><:><:><:><-!><-!><:>About running Notes and NETBIOS on OS/2

<:s><:R1,1,1,360,><:#200,8486>The following system requirements to run Notes on OS/2:

<:R1,1,1,360,><:#400,8486>LAN connection - <:f180,,0,0,0>Ethernet, Arcnet, or Token Ring network interface card and device driver software compliant with Novell open datalink (ODI) specifications and the Novell NetWare 
<:f><:f180,,0,0,0>Requester<+&><:f200,,0,0,0>TM<-&><:f180,,0,0,0> for OS/2<:f>

<:s><:R><:#400,8486>Operating system - <:f180,,0,0,0>OS/2 Release 3 or 2.11<:f><:f180,,0,0,0>. 
<-!><:f><:f180,,0,0,0>Use respective vendor-supplied OS/2. If you use IBM hardware, use OS/2 Standard Edition<:f>.

<:R1,1,1,360,><:#400,8486>The Notes NetWare NETBIOS network driver requires the correct NetWare Requester for your OS/2 platform. 

<:s><:R1,1,1,1224,><:#200,8486>For Notes servers or workstations running OS/2 Release 3 you need:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Novell NetWare Requester for OS/2 Release 3

<:s><:R1,1,1,1224,><:#200,8486>For Notes servers or workstations running OS/2 2.01 you need:

@Bullet@<:s><:R1,1,1,1224,><:#200,8486>Novell NetWare Requester for OS/2 2.01

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,11,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: <:f180,,0,0,0>Obtaining Netware software for OS/2<:f>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,12,1
@@EndSection

>

<:R1,1,1,0,><:#200,8486>

@Ahead@<:R1,1,1,0,><:#240,8486>Setting up Notes and NETBIOS on OS/2

<:R1,1,1,360,><:#600,8486><-!><-!><:><-!>The Notes NetWare NETBIOS network driver requires the correct NetWare Requester for your OS/2 platform. Before you install Notes on your server or workstation, follow the instructions in this section in conjunction with the Lotus Notes Instal
lation Guide.<-!>

@Numbered list@<:R1,1,1,1080,><:#400,8486>Edit the CONFIG.SYS file to enable the NETBIOS.SYS and NBDAEMON.EXE files for the NetWare NETBIOS driver.

@Numbered list@<:R><:#400,8486>Check the sample CONFIG.SYS file and Novell configuration files for additional changes you might want to make.<-">

@Numbered list@<:s><:#200,8486>Restart the Notes server and workstations for the changes to take effect.

<:R1,1,1,360,><:#800,8486>Novell NetWare Requester for OS/2 2.01<+!> <-!>is required for Notes servers or workstations running OS/2 2.0 or 2.1. You must use this software with Notes under NETBIOS. 
<-!>In the United States, you can order the software by calling 1-800-UPDATE1. Outside the United States, contact your local Novell office. You can also download the software from CompuServe.

@Bhead@<:s><:R1,1,1,0,><:#220,8486>

<:R1,1,1,0,><:#200,8486>

@Bhead title@<:s><:R1,1,1,360,><:#220,8486><-!><-!><:><-!>Getting the OS/2 2.01 NetWare Requester

<:R1,1,1,1080,><:#400,8486>More complete instructions for installing the update are in the NOVFILES forum under Client Kits, OS/2 Client Kit, NetWare Client Kit - OS/2 Documentation.

<:R1,3,1,1080,1,2160,1,5040,><:#200,8486>Do not use the files from NSD202.EXE with NetWare Requester for OS/2 2.01.

@Numbered list@<:s><:R1,3,1,1080,1,2160,1,5040,><:#200,8486>Dial and log in to CompuServe.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Type GO NOVFILES.

@Numbered list@<:s><:R1,1,1,1080,><:#200,8486>Choose Client Kits.

@Numbered list@<:s><:R1,1,1,1080,><:#200,8486>Choose OS/2 Client Kit.

@Numbered list@<:s><:R1,1,1,1080,><:#200,8486>Choose NetWare Client Kit - OS/2 Files.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Download the files WSOS21.EXE, WSOS22.EXE, and lWSOS2D.EXE.

@Numbered list@<:R1,1,1,1080,><:#200,8486>See the file README.1ST, which is in the file WSOS21.EXE, for information on installing the update.

@Ahead@<:R1,1,1,0,><:#480,8486>About running Notes and Novell NetBIOS on Windows 3.1 and Windows for Workgroups

@Bhead@<:s><:R1,1,1,0,><:#220,8486>About Notes and NetWare Windows .DLL files

<:s><:R><:#400,8486>NetWare Windows .DLL files must be present on Notes systems using Novell NetBIOS. Make sure that you have the correct version of these files.

<:s><:#1000,8486>There are three generations of NetWare Windows .DLL files: those from "NetWare C Interface for Windows" (before version 1.3); those from "NetWare C Interface for Windows" Version 1.3 or higher; and those from the "NetWare Client SDK" Version 1.0 or higher. 
(The NetWare Client SDK replaces the "NetWare C Interface for Windows") Notes Release 4 works with all generations of NetWare Windows .DLL files.

<:s><:#600,8486>The Notes installation program (optionally) copies the necessary third generation .DLL files to the Notes system, checking file versions so only the latest versions are installed. The Notes NetBIOS network driver detects which .DLL files are present, and lo
ads the appropriate ones.

<:#200,8486>If NWCALLS.DLL is present, Notes loads and uses these third generation .DLL files:

<:R1,1,1,3420,><:#400,8486>NWCALLS.DLL<**>NWIPXSPX.DLL

<:R><:#200,8486>If NWNETAPI.DLL is present, Notes loads and uses these second generation .DLL files:

<:#400,8486>NWIPXSPX.DLL<**>NWNETAPI.DLL

<:#200,8486>If NWWRKSTN.DLL is present, Notes loads and uses these first generation .DLL files:

<:#1000,8486>NWIPXSPX.DLL<**>NWWRKSTN.DLL<**>NWBIND.DLL<**>NWCONN.DLL<**>NWSAP.DLL

@Bhead@<:#220,8486>About requirements for Notes and Novell NetBIOS on Windows

<:#400,8486>LAN connection - <:f180,,0,0,0>Ethernet, Arcnet, or Token Ring network interface card and device driver software compliant with Novell open datalink (ODI) specifications<:f>

<:#400,8486>Operating system <:f180,,0,0,0>(server) - <:f180,,0,0,0>MS-DOS<:f200,,0,0,0></n> 
<:f180,,0,0,0>or PC-DOS 5.0 with Windows 3.1 installed and SMARTDrive or another compatible disk cache

@Table Text@<+@><:s><:I0,0,0,0><:S+-1><:#422,8486><:f180,,0,0,0>Operating system (workstation) - <:f180,,0,0,0>MS-DOS or PC-DOS 3.1 or higher version with Windows 3.0 or higher versions (3.1 recommended)<:f>

@Table Text@<+@><:s><:I0,0,0,0><:S+-1><:#211,8486><:f180,,0,0,0>Network software <:f>(server) - Novell NetWare workstation software using the NetBIOS protocol

@Table Text@<+@><:I0,0,0,0><:S+-1><:#633,8486>Network software (workstation) - Novell NetWare workstation software using NetBIOS protocols for connecting to a Windows Notes server; NetBIOS or NETBIOS protocol for connecting to an OS/2 Notes server; and NETBIOS protocol for connecting to a Notes Server 
for NetWare.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,13,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Obtaining NetWare software for Windows

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,14,1
@@EndSection

>

<:R1,1,1,0,><:#200,8486>

@Ahead@<:R1,1,1,0,><:#480,8486>Setting up Notes and Novell NETBIOS on Windows 3.1 and Windows for Workgroups

<:R1,1,1,0,><:#200,8486>To set up Notes to run on NOVELL NETBIOS and the Windows platform, you need to:

@Numbered list@<:R><:#400,8486>Edit the SYSTEM.INI file on the Notes Windows servers and workstations. 
<+!><+">??Jump to steps topic "Editing the SYSTEM.INI file on a Notes Windows server or workstation"<-"><-!>

@Numbered list@<:#400,8486>Edit the NET.CFG file on the Notes Windows servers and workstations. 
<+!><+">??Jump to steps topic "Editing the NET.CFG file on a Notes Windows server or workstation"<-"><-!>

@Numbered list@<:s><:#200,8486>Restart the Notes server and workstation for the changes to take effect.

<:R1,1,1,0,><:#200,8486>

@Bhead title@<:R1,1,1,1224,><:#220,8486><-!><-!><:><-!>Editing the SYSTEM.INI file on a Notes Windows server or workstation

<:R><:#400,8486>The SYSTEM.INI file is configured during Notes for Windows setup when you select NetWare as your network operating system.

@Numbered list@<:#400,8486>For a Notes Windows server or workstation, make sure that the SYSTEM.INI file contains the following lines: 

@Indnt mono@<:#400,8486><[>boot]<**>network.drv=NETWARE.DRV

@Numbered list@<:#200,8486>For Windows enhanced mode, make sure that the <[>386Enh] section contains the following line: 

@Indnt mono@<:#400,8486><[>386Enh]<**>network=vnetware.386, vipx.386

@Numbered list@<:R1,1,1,360,><:#800,8486>If you are running Windows in Standard mode, you must run the NetWare Task Switched Buffer Manager program. For Windows 3.0 the program is TBMI.COM, for Windows 3.1 it is TBMI2.COM. This program manages the use of network buffers and is not necessary in Win
dows enhanced mode: NetWare allocates buffers as needed. <+!><+">??what is the buffer program?<-"><-!>

@Bhead title@<:R1,1,1,1224,><:#220,8486><-!><-!><:><-!>Editing the NET.CFG file on a Notes server or workstation for Windows

<:R><:#600,8486>When you run a Notes server or workstation for Windows on Novell NETBIOS, you can use a Novell configuration file called NET.CFG to allocate system resources. NET.CFG sets the network packet frame types and increases the default values required by a Notes s
erver. 

@Bhead@<:#220,8486>For Notes servers

<:#200,8486>If NET.CFG does not exist on your Notes server, create it in the root directory of the server.

<:#200,8486>For a Notes server, add the following lines to the NET.CFG file. Press ENTER after each line.'

<:#200,8486>yy get updated lines to add here

@Bhead@<:#220,8486>For Notes workstations

<:#200,8486>If NET.CFG does not exist on your Notes workstation, create it in the root directory of the workstation.

<:#200,8486>For a Notes workstation, add the following lines to the NET.CFG file. Press ENTER after each line.'

<:#200,8486>yy get updated lines to add here

<:#200,8486>

<:R1,1,1,1224,><:#200,8486>

@Ahead@<:R1,1,1,1224,><:#480,8486>Ways to set up network drivers for Notes workstations for Windows and NOVELL NETBIOS

<:s><:R><:#600,8486>Notes currently supports Notes workstations running in Windows Enhanced mode using the Notes NetBIOS driver. (The Notes NetBIOS driver does not support Windows Standard mode.) Before you set up your Notes servers or workstations, you should set up network d
rivers for NetBIOS.

<:s><:#400,8486>On Windows workstations in the Novell NetBIOS environment, you can set up network drivers using one of two methods:

@Bullet@<:#400,8486>Using the older, dedicated IPX shell created with the WSGEN utility.<+!><+">??Jump to steps topic "Using the IPX approach to set up Windows workstations with NetBIOS"<-"><-!>

@Bullet@<:#400,8486>Using ODI drivers, which support multiple protocols on a single workstation. 
<+!><+">??Jump to steps topic "Using the IPXODI approach to set up Windows workstations with NetBIOS"<-"><-!>

<:R1,1,1,360,><:#200,8486>

@Ahead@<:R1,1,1,360,><:#240,8486>Using the IPX approach to set up Windows workstations with Novell NetBIOS

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#800,8486>If you use this approach, you need the IPX.COM file created with WSGEN. The drivers to the network card are linked into IPX.COM rather than a separate ODI driver. 
<+!><+">??find out what WSGEN is  <-"><-!>If you are using the Novell dedicated IPX approach, these files are required when running Notes with the Notes NetBIOS port driver:

<:R1,1,1,1224,><:#600,8486>IPX.COM<**>NETX.COM<**>WINUP9.EXE or a set of updated SPX files for Windows

@Bhead@<:R1,1,1,1224,><:#220,8486>IPX.COM

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#400,8486>To find out what version of IPX.COM you are currently using, change to the directory containing IPX.COM, type 

@Indnt mono@<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#200,8486>ipx i

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#200,8486>and press ENTER.

<:R1,1,1,1224,><:#600,8486>To use Notes with Novell NetBIOS, you must have IPX.COM Version 3.10, which is the latest version of IPX.COM and the only one that works with the Notes NetBIOS driver. (Novell no longer officially supports the original IPX.COM method and, instead, is promot
ing the IPXODI approach.)

<:R1,1,1,1224,><:#600,8486>Use the Novell WSGEN utility and the file IPX.OBJ to generate the appropriate IPX.COM version. You can find the IPX.OBJ file on older NetWare driver disks or in a file called DOSUP9.EXE, which is available exclusively on CompuServe.

@Bhead@<:R1,1,1,1224,><:#220,8486>NETX.COM

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#400,8486>Lotus recommends that you use NETX.COM (Version 3.22 or higher) with either the Notes workstation or server for Windows. You can find the latest version of NETX.COM in the file DOSUP9.EXE.

<:R1,1,1,1224,><:#400,8486>To determine the version of NETX.COM you are currently using, change to the directory containing the file NETX.COM, type 

@Indnt mono@<:R1,1,1,1224,><:#200,8486>netx i

<:R1,1,1,1224,><:#200,8486>and press ENTER.

@Bhead@<:R1,1,1,1224,><:#220,8486>WINUP9.EXE

<:R1,1,1,1224,><:#400,8486>Novell sometimes updates the files available on CompuServe. If WINUP9.EXE is not available, look for a newer file, such as WINUP10.EXE or WINUP11.EXE, and so on. 

<:R1,1,1,1224,><:#600,8486>WINUP9.EXE is available from CompuServe. The files included in WINUP9.EXE are also available (at this printing) with the latest version of the Novell NetWare Client Kit for DOS that accompanies NetWare 4.x.

<:R1,1,1,1224,><:#400,8486>You can order the NetWare Client Kit for DOS/Windows from Novell in the United States by calling 1-800-UPDATE1. To order this software outside of the U.S., contact your local Novell office.

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:R><:#200,8486><:N795478803,JY,65535,15,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: <:f180,,0,0,0>Getting<:f><:f180,,0,0,0> DOSUP9.EXE, 
<:f><:f180,,0,0,0>Getting<:f><:f180,,0,0,0> WINUP9.EXE<:f>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,16,1
@@EndSection

>

<:R><:#200,8486>

<:R1,1,1,1224,><:#200,8486>

@Bhead title@<:R1,1,1,1224,><:#220,8486>Getting WINUP9.EXE

@Numbered list@<:R1,1,1,1080,><:#200,8486>Dial and log in to CompuServe.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Type 

@Indnt mono@<:R1,1,1,1080,><:#200,8486>GO NOVFILES

@Numbered list@<:R1,1,1,1080,><:#200,8486>Choose Download WINUP9.EXE from the menu.

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#400,8486>To install the files included in WINUP9.EXE, replace the existing versions of the files typically located in the WINDOWS\SYSTEM subdirectory with the newer versions in WINUP9.EXE.

@Ahead@<:R1,1,1,360,><:#240,8486>Using the IPXODI approach to set up Windows workstations with Novell NetBIOS

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>ODI card drivers are specific to each network card. ODI drivers for most cards are supplied on a disk that accompanies the card. Drivers for the most popular cards can also be found on the original NetWare Requester for DOS disks that are supplied with NetW
are. Additional drivers and updates to previously released drivers can also be found in subsequently released NetWare for DOS updates such as DOSUP9.EXE.

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#400,8486>When using the Novell IPXODI approach, you need these files to use your DOS/Windows workstations with Notes:

<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#200,8486>yy include where to get each file after each number

@Numbered list@<:R1,1,1,1224,><:#200,8486>LSL.COM (available as part of the DOSUP9.EXE file)

@Numbered list@<:R1,1,1,1224,><:#200,8486>The ODI network card driver for your card

@Numbered list@<:R1,1,1,1224,><:#200,8486><**>IPXODI.COM (available as part of the DOSUP9.EXE file)

@Numbered list@<:R1,1,1,1224,><:#200,8486><**>NETX.COM

@Numbered list@<:R1,1,1,1224,><:#200,8486><**>WINUP9.EXE (a set of updated NetWare files for Windows)

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,17,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: <:f180,,0,0,0>Getting DOSUP9.EXE<:f>

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,18,1
@@EndSection

>

<:s><:R><:#200,8486>

@Chead title@<:R1,5,1,720,1,2160,1,2880,1,3600,1,4320,><:#200,8486>

@Bhead title@<:R1,1,1,360,><:#220,8486>Getting DOSUP9.EXE

<:R1,1,1,360,><:#600,8486>Novell sometimes updates the DOSUP files on CompuServe. If DOSUP9.EXE is not available, look for a newer file, such as DOSUP10.EXE or DOSUP11.EXE, and so on. Before installing DOSUP files, make sure you have the latest versions of these files.

@Numbered list@<:s><:R1,1,1,1080,><:#200,8486>Dial and log in to CompuServe.

@Numbered list@<:s><:R1,1,1,1080,><:#200,8486>Type 

@Indnt mono@<:R1,1,1,1080,><:#200,8486>GO NOVFILES

@Numbered list@<:R1,1,1,1080,><:#200,8486>Choose Download DOSUP9.EXE from the menu. 

<:R1,1,1,360,><:#200,8486>

@Ahead@<:s><:R><:#240,8486><:><:><:><:>About running Notes and Novell NetBIOS on Windows NT

<:#600,8486>The Windows NT server provides built-in network support that makes it compatible with Novell NetWare. You can run the Notes server for Windows NT on Novell and Novell NetBIOS without any additional NetWare or NT configuration, you just need to enable the No
tes NetBIOS port.

@Ahead@<:s><:#240,8486>Setting up Notes and Novell NetBIOS on Windows NT

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><-!><-!>Launch the Notes workstation program on your NT server.

@Numbered list@<:s><:R><:#200,8486>Enable the network port for NetBIOS.

@Numbered list@<:s><:#200,8486>Restart the NT server.

<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>This port may have already been enabled when you installed Notes on the NT server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,19,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,20,1
@Build tag@@EndSection

>

<:R><:#200,8486>Print refs: Install Guide for setting up first port, Admin Guide port setup info in Ch.3?

@Ahead@<:#240,8486>About running Notes and Novell NetBIOS on Windows 95

@Ahead@<:#240,8486>Setting up Notes and Novell NetBIOS on Windows 95

@Ahead@<:R1,1,1,0,><:#240,8486>About running Notes on Microsoft NetBEUI<-!><-!>

<:R><:#200,8486><:>The Notes servers and workstations that support Microsoft NetBEUI are:

@Bullet@<:s><:#200,8486>OS/2 server and workstation

@Bullet@<:#200,8486>Windows 3.1 and Windows for Workgroups server and workstation

@Bullet@<:s><:#200,8486>Windows NT server

@Bullet@<:#200,8486>Windows 95 workstation

@Ahead@<:#240,8486>About running Notes and NetBEUI on OS/2

@Ahead@<:#240,8486>Setting up Notes and NetBEUI on OS/2

@Ahead@<:#240,8486>About running Notes and NetBEUI on Windows 3.1 and Windows for Workgroups

@Ahead@<:#240,8486>Setting up Notes and NetBEUI on Windows 3.1 and Windows for Workgroups

@Ahead@<:#240,8486>About running Notes and NetBEUI on Windows NT

<:#600,8486>The Windows NT server provides built-in network support that makes it compatible with Novell NetWare. You can run the Notes server for Windows NT on Novell and Novell NetBIOS without any additional NetWare or NT configuration, you just need to enable the No
tes NetBIOS port.

@Ahead@<:#240,8486>Setting up Notes and NetBEUI on Windows NT

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><-!><-!>Launch the Notes workstation program on your NT server.

@Numbered list@<:s><:R><:#200,8486>Enable the network port for NetBIOS.

@Numbered list@<:s><:#200,8486>Restart the NT server.

<:s><:R1,20,1,0,1,360,1,360,1,720,1,1080,1,1080,1,1440,1,1800,1,2160,1,2520,1,2880,1,3240,1,3600,1,3960,1,4320,1,4680,1,5040,1,5400,1,5760,1,6120,><:#200,8486>This port may have already been enabled when you installed Notes on the NT server.

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:s><:R><:#200,8486><:N795478803,JY,65535,21,1
@Build tag@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Enabling a network port (AG)

@See also btn@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,22,1
@Build tag@@EndSection

>

<:R><:#200,8486>Print refs: Install Guide for setting up first port, Admin Guide port setup info in Ch.3?

@Ahead@<:#240,8486>About running Notes and NetBEUI on Windows 95

@Ahead@<:#240,8486>Setting up Notes and NetBEUI on Windows 95

@Ahead@<:R1,1,1,0,><:#240,8486>

>

[Embedded]
00096879
