[ver]
	4
[sty]
	
[files]
[charset]
	82
	ANSI (Windows, IBM CP 1252)
[revisions]
	0
[prn]
	HP LaserJet 4P/4MP
[port]
	LPT1:
[lang]
	1
[fldnames]
	Field1
	Field2
	Field3
	Field4
	Field5
	Field6
	Field7
	Field8
[desc]
	modems/scripts
	
	
	
	
	801524439
	34
	780276418
	5062
	18
	0
	0
	0
	0
	
	
	
	
	
	
	1
[fopts]
	0
	1
	0
	0
	
	
[lnopts]
	2
	Body Text
	1
[docopts]
	5
	2
[GramStyle]
	
[ParaNum]
	1
[tag]
	Body Text
	2
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Ahead
	3
	[fnt]
		Arial
		220
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		240
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		2160
		3
		0
		1
		1
		1
		65
		10
		1
	[spec]
		0
		1
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead title
	4
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		79
		0
		3
		100
	[brk]
		80
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Chead title
	5
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead
	6
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		180
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Chead
	7
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Numbered list
	8
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		300
		300
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		5
		<*:>.
		0
		3
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Numbered list
	0
	0
[tag]
	1st lev para
	9
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		68
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	1st lev para
	0
	0
[tag]
	Bullet
	11
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		120
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Bullet
	2
	1
	160
	1
	400
	0
[tag]
	Indnt bullet
	12
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		420
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		16
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Indnt bullet
	0
	0
[tag]
	2nd lev para
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		600
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	2nd lev para
	0
	0
[tag]
	See also prnt
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also prnt
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Book art
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Book art
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Callout text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Callout text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Figure title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		40
		60
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Figure title
	0
	0
[tag]
	Chapter title
	0
	[fnt]
		Arial
		280
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		300
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Chapter title
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	1st pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	1st pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Right pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Right pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Left pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Left pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Table title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		60
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		7
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Table title
	0
	0
[tag]
	Table col hd
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		4
	[line]
		10
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		6
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table col hd
	0
	0
[tag]
	Table Text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table Text
	0
	0
[tag]
	See also hlp
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		40
		4
		180
		0
		3
		100
	[brk]
		96
	[line]
		9
		0
		3
		0
		1
		1
		1
		70
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	0
	120
[tag]
	See also btn
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		240
	[spc]
		24
		200
		4
		0
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Crossref
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		513
		3
		0
		300
		600
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Crossref
	0
	0
[tag]
	Indnt caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt caution
	0
	0
[tag]
	Indnt tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		324
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt tip
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Indnt note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt note
	0
	0
[tag]
	Caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Caution
	0
	0
[tag]
	Tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		324
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Tip
	0
	0
[tag]
	Note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Note
	0
	0
[tag]
	Mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Indnt mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		300
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Dhead
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		4
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Parameter
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Parameter
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Formula
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Formula
	0
	0
[tag]
	Browse
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		+
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Browse
	0
	0
[tag]
	Keyword
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		K
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Keyword
	0
	0
[tag]
	Context
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		#
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Context
	0
	0
[tag]
	Title
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		$
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Title
	0
	0
[tag]
	Macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		!
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Macros
	0
	0
[tag]
	Footnote
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		244
		0
	[spc]
		40
		2400
		3
		0
		0
		1
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		256
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Footnote
	0
	0
[tag]
	Alink
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		A
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Alink
	0
	0
[tag]
	Butnbar
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		0
		0
		3
		100
	[brk]
		48
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Butnbar
	0
	0
[tag]
	Window
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		>
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Window
	0
	0
[tag]
	Win95 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		W
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win95 macros
	0
	0
[tag]
	Win31 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		X
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win31 macros
	0
	0
[tag]
	Build tag
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		*
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Build tag
	0
	0
[frm]
	15
	1572932
	960
	960
	9440
	11128
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	20
	0
	0
	0 18432
	[frmlay]
		4076
		8480
		3
		0
		0
		3
		960
		0
		0
		2
		0
		1
		1
		0
		1
		1500
		9626
		0
	[tbl]
		 12 4 200 86 4132 86 1 43 43
		[h]
			 0 410 86 2 0 1 0
			 1 1000 86 2 0 1 0
			 2 400 86 2 0 1 0
			 3 400 86 2 0 1 0
			 4 1200 86 2 0 1 0
			 5 800 86 2 0 1 0
			 6 1200 86 2 0 1 0
			 7 1000 86 2 0 1 0
			 8 1000 86 2 0 1 0
			 9 1000 86 2 0 1 0
			 10 1758 86 2 0 1 0
			 11 1479 86 2 0 1 0
		[e]
		[w]
			 0 1038 86 2 0
			 1 2538 86 2 0
			 2 1863 86 2 0
			 3 2654 86 2 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Script command

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@Description 

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@Syntax

>
			 0 3 0 0 0 0 0 1 0 0 0 0
@Table col hd@Examples

>
			 1 0 0 0 0 0 0 1 0 0 0 0
<:R1,4,1,0,1,720,1,1440,1,2160,>BREAK 

>
			 1 1 0 0 0 0 0 1 0 0 0 0
<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Break" # "command in script file"><:X8,-32768;Index "Script files" # "break command">Sends a communications break. Time is specified in 100ms intervals. Default is 500ms. Maximum is 2000ms. Timing of breaks is not exact.

>
			 1 2 0 0 0 0 0 1 0 0 0 0
BREAK <[>time]

>
			 1 3 0 0 0 0 0 1 0 0 0 0
BREAK 1  Sends a 100ms break

<:R1,5,1,2390,1,2869,1,3347,1,3826,1,4303,>BREAK  Sends a 500ms break

>
			 2 0 0 0 0 0 0 1 0 0 0 0
DTR_HIGH

>
			 2 1 0 0 0 0 0 1 0 0 0 0
<:X8,-32768;Index "DTR_HIGH" # "command in script file"><:X8,-32768;Index "Script files" # "dtr_high command">Raises the DTR signal on the selected port.

>
			 2 2 0 0 0 0 0 1 0 0 0 0
DTR_HIGH

>
			 3 0 0 0 0 0 0 1 0 0 0 0
DTR_LOW <:X8,-32768;Index "DTR_LOW" # "command in script file"><:X8,-32768;Index "Script files" # "dtr_low command">  

>
			 3 1 0 0 0 0 0 1 0 0 0 0
Lowers the DTR signal on the selected port.

>
			 3 2 0 0 0 0 0 1 0 0 0 0
DTR_LOW

>
			 4 0 0 0 0 0 0 1 0 0 0 0
ERROR <:X8,-32768;Index "Error" # "command in script file"><:X8,-32768;Index "Script files" # "error command">  

>
			 4 1 0 0 0 0 0 1 0 0 0 0
Tells the script file to branch to the specified label if an error previously occurred. If no label is specified, the ERROR condition is cleared but no branch occurs.

>
			 4 2 0 0 0 0 0 1 0 0 0 0
ERROR  label

>
			 5 0 0 0 0 0 0 1 0 0 0 0
FAIL   

>
			 5 1 0 0 0 0 0 1 0 0 0 0
Terminates the execution of the current script. The optional text string is logged in the standard Notes log file LOG.NSF.

>
			 5 2 0 0 0 0 0 1 0 0 0 0
FAIL <[>text string]


>
			 6 0 0 0 0 0 0 1 0 0 0 0
GOTO     <:X8,-32768;Index "GOTO" # "command in script file"><:X8,-32768;Index "Script files" # "goto command">

>
			 6 1 0 0 0 0 0 1 0 0 0 0
Branches unconditionally to the specified label. If the label does not exist, the script file terminates, and the error is logged in the standard Notes log file, LOG.NSF.

>
			 6 2 0 0 0 0 0 1 0 0 0 0
 GOTO label


>
			 7 0 0 0 0 0 0 1 0 0 0 0
LOG OFF

>
			 7 1 0 0 0 0 0 1 0 0 0 0
 <:X8,-32768;Index "LOG OFF" # "command in script file"><:X8,-32768;Index "Script files" # "log off command">Turns off informational logging and overrides the port setup parameter (for execution of this script only). Uses the standard Notes log file, LOG.NS
F.

>
			 7 2 0 0 0 0 0 1 0 0 0 0
LOG OFF

>
			 8 0 0 0 0 0 0 1 0 0 0 0
LOG ON   

>
			 8 1 0 0 0 0 0 1 0 0 0 0
 <:X8,-32768;Index "LOG ON" # "command in script file"><:X8,-32768;Index "Script files" # "log on command">Turns on informational logging and overrides the port setup parameter (for execution of this script only). Uses the standard Notes log file, LOG.NSF.

>
			 8 2 0 0 0 0 0 1 0 0 0 0
LOG ON   

>
			 9 0 0 0 0 0 0 1 0 0 0 0
REPLY  <:X8,-32768;Index "REPLY" # "command in script file"><:X8,-32768;Index "Script files" # "reply command">

>
			 9 1 0 0 0 0 0 1 0 0 0 0
Sends a string to the serial port.  CR/LF (carriage return/line feed) is sent at the end of the string unless the semicolon (;) is specified after the end quote.

>
			 9 2 0 0 0 0 0 1 0 0 0 0
  REPLY "string" <[>;]

>
			 9 3 0 0 0 0 0 1 0 0 0 0
<:R1,5,1,2390,1,2869,1,3347,1,3826,1,4781,>REPLY "OK"  Send OK

<:R1,5,1,2390,1,2869,1,3347,1,3826,1,4781,>REPLY "^1"  Send first input parameter

>
			 10 0 0 0 0 0 0 1 0 0 0 0
WAIT    <:X8,-32768;Index "WAIT" # "command in script file"><:X8,-32768;Index "Script files" # "wait command">

>
			 10 1 0 0 0 0 0 1 0 0 0 0
Waits a given amount of time for the specified string, which must be enclosed in quotes. Any data other than a matched string is passed along (case sensitive). If a time is not specified, the maximum time of 60 seconds is used.   

>
			 10 2 0 0 0 0 0 1 0 0 0 0
WAIT <[>time] <[>FOR "string"]


>
			 10 3 0 0 0 0 0 1 0 0 0 0
WAIT 10 for "hello"   Waits 10 seconds for the string to be received

WAIT 5  Waits 5 seconds, then continues

WAIT for "hello"  Waits 60 seconds for string to be received.

>
			 11 0 0 0 0 0 0 1 0 0 0 0
WATCH   

>
			 11 1 0 0 0 0 0 1 0 0 0 0
<:X8,-32768;Index "WATCH" # "command in script file"><:X8,-32768;Index "Script files" # "watch command">Same as WAIT, but with multiple responses and actions.  The WATCH command  terminates (continues to next instruction) when any of the strings are matched
, or upon timeout.


>
			 11 2 0 0 0 0 0 1 0 0 0 0
 WATCH <[>time] <[>FOR]

 "string1" statement

 "string2" statement

ENDW


>
			 11 3 0 0 0 0 0 1 0 0 0 0
WATCH 10 for  Waits 10 seconds for the following conditions

"User:" REPLY "^1"

"Password:" REPLY "^2"

ENDW

>
		[e]
	[tble]
[frm]
	9
	1572932
	960
	4690
	9438
	7145
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	15
	1
	0
	768 65389
	[frmlay]
		9318
		8478
		3
		0
		0
		3
		4690
		0
		0
		2
		0
		1
		1
		0
		1
		1320
		9446
		0
	[tbl]
		 7 4 200 86 2023 86 1 43 43
		[h]
			 0 210 86 2 0 4 0
			 1 200 86 2 0 3 0
			 2 600 86 2 0 1 0
			 3 200 86 2 0 4 0
			 4 200 86 2 0 4 0
			 5 200 86 2 0 4 0
			 6 200 86 2 0 4 0
		[e]
		[w]
			 0 1746 86 2 0
			 1 923 86 2 0
			 2 890 86 2 0
			 3 4532 86 2 0
		[e]
		[data]
			 0 0 0 0 0 0 0 1 0 0 0 0
@Table col hd@Port

>
			 0 1 0 0 0 0 0 1 0 0 0 0
@Table col hd@Name

>
			 0 2 0 0 0 0 0 1 0 0 0 0
@Table col hd@Driver

>
			 0 3 0 0 0 0 0 1 0 0 0 0
@Table col hd@More Setup options

>
			 1 0 0 0 0 0 0 1 0 0 0 0
??

>
			 1 1 0 0 0 0 0 1 0 0 0 0
AppleTalk

>
			 1 2 0 0 0 0 0 1 0 0 0 0
ATALK

>
			 2 0 0 0 0 0 0 1 0 0 0 0
COM1-5

>
			 2 1 0 0 0 0 0 1 0 0 0 0
COM1-5

>
			 2 2 0 0 0 0 0 1 0 0 0 0
XPC

>
			 2 3 0 0 0 0 0 1 0 0 0 0
Modem type, port speed, Volume, Dial Mode, Dial Timeout, Log modem and log, Hardware control as well as editing modem files or selecting acquire scripts

>
			 3 0 0 0 0 0 0 1 0 0 0 0
LAN0

>
			 3 1 0 0 0 0 0 1 0 0 0 0
LAN0

>
			 3 2 0 0 0 0 0 1 0 0 0 0
NETBIOS

>
			 3 3 0 0 0 0 0 1 0 0 0 0
Unit Number, Buffer Size

>
			 4 0 0 0 0 0 0 1 0 0 0 0
SPX

>
			 4 1 0 0 0 0 0 1 0 0 0 0
SPX

>
			 4 2 0 0 0 0 0 1 0 0 0 0
NWSPX

>
			 4 3 0 0 0 0 0 1 0 0 0 0
Receive and Send Buffers per session, SPX sessions

>
			 5 0 0 0 0 0 0 1 0 0 0 0
TCP

>
			 5 1 0 0 0 0 0 1 0 0 0 0
TCP

>
			 5 2 0 0 0 0 0 1 0 0 0 0
TCP

>
			 5 3 0 0 0 0 0 1 0 0 0 0
Secondary Name server, Host name or address

>
			 6 0 0 0 0 0 0 1 0 0 0 0
Vines

>
			 6 1 0 0 0 0 0 1 0 0 0 0
Vines

>
			 6 2 0 0 0 0 0 1 0 0 0 0
Vines

>
			 6 3 0 0 0 0 0 1 0 0 0 0
None

>
		[e]
	[tble]
[frm]
	24
	1572868
	720
	3995
	9206
	10984
	0
	3
	1
	1 0 0 0 0 0 0
	0
	16777215
	21
	2
	0
	0 0
	[frmlay]
		3300
		8486
		3
		0
		0
		3
		3995
		0
		0
		2
		0
		9
		0
		9
		1
		1560
		9806
		0
	[tbl]
		 8 3 200 86 2731 86 1 43 43
		[h]
			 0 210 0 2 0 3 0
			 1 600 0 2 0 2 0
			 2 600 0 2 0 2 0
			 3 400 0 2 0 1 0
			 4 400 0 2 0 1 0
			 5 1200 0 2 0 1 0
			 6 1800 0 6 0 1 0
			 7 1200 20 6 0 1 0
		[e]
		[w]
			 0 1858 0 6 0
			 1 2576 0 6 0
			 2 4011 0 6 0
		[e]
		[data]
			 0 0 0 0 0 0 512 1 0 0 0 0
@Table col hd@<:I0,0,0,0>Statistic Name

>
			 0 1 0 0 0 0 512 1 0 0 0 0
@Table col hd@Description

>
			 0 2 0 0 0 0 512 1 0 0 0 0
@Table col hd@Comments

>
			 1 0 0 0 0 0 0 1 0 0 0 0
User messages sent

>
			 1 1 0 0 0 0 0 1 0 0 0 0
Number of transmit requests issued by the user for one or more packets

>
			 1 2 0 0 0 0 0 1 0 0 0 0
The number should keep increasing, meaning transmission is occurring normally. If the number stops increasing, there is a problem with the port.

>
			 2 0 0 0 0 0 0 1 0 0 0 0
User messages received

>
			 2 1 0 0 0 0 0 1 0 0 0 0
Number of transmit requests issued by the sender for one or more packets

>
			 2 2 0 0 0 0 0 1 0 0 0 0
The number should keep increasing, meaning transmission is occurring normally. If the number stops increasing, there is a problem with the port.

>
			 3 0 0 0 0 0 0 1 0 0 0 0
User bytes sent

>
			 3 1 0 0 0 0 0 1 0 0 0 0
Number of bytes sent from this port

>
			 4 0 0 0 0 0 0 1 0 0 0 0
User bytes received

>
			 4 1 0 0 0 0 0 1 0 0 0 0
Number of bytes received on this port

>
			 5 0 0 0 0 0 0 1 0 0 0 0
Retransmitted packets

>
			 5 1 0 0 0 0 0 1 0 0 0 0
The number of packets transmitted again, due to errors

>
			 5 2 0 0 0 0 0 1 0 0 0 0
Useful in checking remote transmissions; a high number (over one or so per minute) indicates a problem and will noticeably slow performance. The server's modem needs to have RTS/CTS Flow Control enabled, or if RTS/CTS is unsupported, the port speed needs to
 be lowered.

>
			 6 0 0 0 0 0 0 1 0 0 0 0
CRC errors

>
			 6 1 0 0 0 0 0 1 0 0 0 0
The number of Cyclic Redundancy Check (CRC) errors reported on this port

>
			 6 2 0 0 0 0 0 1 0 0 0 0
Cyclic Redundancy Checks are used to verify that messages are transmitted and received accurately. CRC errors mean that the CRC included in the frame is not consistent with the actual number of bits in the frame. Such errors slow transmission speed. The ser
ver's modem needs to have RTS/CTS Flow Control enabled, or if RTS/CTS is unsupported, the port speed needs to be lowered.

>
			 7 0 0 0 0 0 0 1 0 0 0 0
Port errors detected

>
			 7 1 0 0 0 0 0 1 0 0 0 0
Port errors on this port

>
			 7 2 0 0 0 0 0 1 0 0 0 0
Indicates port driver buffer overflow or possible parity errors. More than 10 or so per phone call indicates a problem. Could happen intermittently if occasionally noisy lines cause data to back up. If the problem persists, you may need to reconfigure the d
river or upgrade the RS</m>232 port.

>
		[e]
	[tble]
[lay]
	Standard
	1031
	[rght]
		12960
		10166
		1
		960
		1200
		3
		960
		720
		0
		1
		0
		1
		0
		2
		1
		960
		9446
		1
		1
		3120
	[lft]
		12960
		10166
		1
		720
		1200
		3
		960
		960
		0
		1
		0
		1
		0
		2
		1
		720
		9206
		1
		1
		3120
	[hlft]
	[lyfrm]
		1
		3008
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		17
	[frmlay]
		960
		10166
		1
		720
		180
		3
		0
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		2
		4674
	[txt]
@Header@
>
	[hrght]
	[lyfrm]
		1
		11200
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		1
	[frmlay]
		960
		10166
		1
		960
		180
		3
		0
		720
		0
		1
		0
		1
		1
		0
		1
		960
		9446
		1
		2
		4674
	[txt]

>
	[flft]
	[lyfrm]
		1
		5056
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		18
	[frmlay]
		12960
		10166
		1
		720
		480
		3
		11940
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		3
		9900
	[txt]
@Left pg foot@<+@><:R1,1,3,8190,><:P19999,0,8->  Adminstrator's Guide	Lotus Confidential

>
	[frght]
	[lyfrm]
		1
		13248
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		2
	[frmlay]
		12960
		10166
		1
		900
		480
		3
		11940
		780
		0
		1
		0
		1
		1
		0
		1
		900
		9386
		1
		3
		9900
	[txt]
@Right pg foot@<+@><:R1,1,3,8486,>Lotus Confidential	Administrator's Guide  <:P19999,0,8->

>
[elay]
[l1]
	0
[pg]
	17
	11 0 5 580 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	32 121 98 36 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	49 188 31 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	79 103 103 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	104 0 0 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	131 203 17 68 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	160 0 75 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	184 1 5 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 4 0 0
	185 0 0 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	218 0 53 36 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	253 0 67 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	286 0 45 36 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	303 0 5 580 1 0 0 240 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	309 0 0 36 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	333 199 78 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	360 0 82 4 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	384 0 0 1029 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
[edoc]
@Chapter title@<:s>Chapter 8 Using Notes with Modems

<:s>This chapter provides information and instructions on setting up modems on your Notes servers. Information on creating and using asynchronous communications scripts with your modems is also provided. 


@Ahead@<:s>About Notes and modems

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Notes can use both networks and modems to communicate with other servers and workstations. Configuring and enabling COM ports on Notes servers lets servers connect to other servers and workstations via a modem. Modems provide a way for servers and workstati
ons to communicate when they are not directly connected via a local network (LAN). Connected ports and modems on servers can route mail or replicate to other Notes servers or workstations. 

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>After you install additional modems on the server, you must add and enable the server port. The number of modems that you can use on a server is dependent on the operating system and the number of available COM ports. You may want to add, change, or delete 
COM port information when a modem is installed or removed from a server port. 

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Although this section describes configuration of both server and workstation, the emphasis is on the server. See the 
<+">Notes Mobile User's Guide<-"> for more information on configuring modems and ports on your workstation.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>INDEX - network protocols, network ports, modems, Notes network names, secondary,

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:s><:R1,0,><:p<* >>About Notes and the X.PC protocol

<:s><:R><:>The X.PC driver is installed as a standard Notes driver when you install with either the Notes server and workstation software. You use this protocol when you install a modem on your workstation or server. X.PC is the protocol that allows Notes servers a
nd workstations to communicate over asynchronous communication ports, using modems. Asynchronous communications ports are also called COM ports. The X.PC protocol is provided with all Notes workstation and server software, and is automatically installed wit
h the Notes software. 

@Bhead@<:s>Enabling ports

<:s>When you want to set up remote communication from or to a Notes server or workstation, you must enable a COM port and select XPC as the driver. On Notes servers, you must enable a COM port for each modem on the server. If you call a Notes server from a mobi
le workstation, you usually enable one COM port. 

@Bhead@<:s>Configuring modem files

The way that your modems work with Notes are determined in the modem command files, which are also installed with the Notes software. These data files use the extension .MDM, and are typically installed in the Notes directory during Notes software installat
ion. For more information on these files, read the file TEMPLATE.MDM.

@Bhead@<:s>Configuring X.PC driver

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>The X.PC driver is also installed automatically with the Notes software. You may customize the driver for remote communications between Notes servers and workstations by using asynchronous communication scripts. 

@See also btn@<:s><:R>

<:R1,4,1,0,1,720,1,1440,1,2160,>See also Customizing the X.PC protocol driver, Enabling workstation and server ports; About asynchronous communication scripts; About selecting scripts

@Ahead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About modem command files

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>A modem command file provides the software that allows servers and workstations to communicate via their modems. You can customize the modem command file to perform additional actions immediately before or after the modem connection. 

<:R1,4,1,0,1,720,1,1440,1,2160,>Modem files use the .MDM extension and are usually located in the Notes directory. These modem files cover a wide variety of modems as well as generic AUTO.CONFIGURE files and the modem template file. Usually, you customize the generic modem file. You could
 also rename a specific modem file as long as you documented it. 

@Chead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@Chead@<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Specifying a modem command file for your modem<:X8,-32768;Index "Configuring" # "modem"><:X8,-32768;Index "Modem" # "configuring">

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Before you begin, install the modem on the server's COM port. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon on the Notes desktop. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select File - Tools - Notes Preferences and then select Ports. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select the <:X8,-32768;Index "Port" # "additional setup for modem"><:X8,-32768;Index "Additional setup" # "for modem">COM1 (serial) port. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select Additional Setup. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Modem" # "command file"><:X8,-32768;Index "Command file for modem" #><:X8,-32768;Index ".MDM file" #><:X8,-32768;Index "Modem" # ".MDM file">Select your modem's command file from the Modem Type list box or type the file name for the selec
ted command file is displayed in the Command File field. Modem command files are located in the Notes data directory with the file extension .MDM. 
<:X8,-32768;Index "Modem" # "autoconfigure"><:X8,-32768;Index "Autoconfigure modem command file" #>If you don't know your modem type, try one of the two Auto Configure files at the end of the list:

@Indnt bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Auto Configure (Hayes</n> compatible non</m>V.42 modems)

@Indnt bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Auto Configure (Hayes compatible V.42 modems)

@2nd lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>An Auto Configure file checks the modem's speed and then selects a Hayes</m>compatible modem command file accordingly. Most modems are not truly Hayes</m>compatible (especially 9600 bps modems), so an Auto Configure file may not work. 

@2nd lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>If you're using a null modem to set up a direct serial connection to another machine, choose a Null Modem file from the end of the list. 
<:X8,-32768;Index "Null modem" #><:X8,-32768;Index "Modem" # "null">(A null modem is a direct connection between the serial ports of two computers using a null modem cable in place of modems.)

@2nd lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>If your modem command file isn't listed and the Auto Configure files don't work, edit an existing command file or create a new one.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Specify the <:X8,-32768;Index "Modem" # "options">Speaker Volume to Low, Medium, or High to hear the modem dialing and establishing carrier. 
<:X8,-32768;Index "Modem" # "speaker volume">The default is Off,which means you cannot hear the modem. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Be sure Tone is selected for the Dial Mode <:X8,-32768;Index "Modem" # "dial mode">unless your modem requires pulse dialing.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Specify the modem speed in the Maximum Speed field. <:X8,-32768;Index "Modem" # "speed"><:X8,-32768;Index "Speed" # "modem">Notes uses the 
<+">lesser<-"> of the speed you select here and the maximum speed specified in the .MDM file. For example, select 19,200 bps and if the .MDM file specifies 9600 bps as the maximum, Notes uses 9600 bps as the maximum speed.

@Indnt note@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Use a lower speed if you are having trouble with a noisy phone line or can't establish the carrier with a remote modem.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Specify the amount of time in the Dial Timeout field. <:X8,-32768;Index "Modem" # "dial timeout">If the server cannot connect to another, it times out after a number of seconds. Increase when using pulse dialing or when calling overseas. Decrease if your mo
dem doesn't detect busy signals.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Specify the amount of time in the Hangup if idle field. <:X8,-32768;Index "Modem" # "hangup if idle">When there is a modem connection but no user data is passing through, it forces a hangup. Usually, when a Notes server finishes a call, it hangs up. If a re
mote user forgets to hang up or a remote server crashes, the line may remain open. 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>On a port where workstation users call in, you may want the server to wait longer before hanging up; users may need time to read or compose long documents. You may want the server to hang up sooner on a server</m>only port; data flow between servers is rela
tively constant (so a relatively short idle time probably means the servers are finished with their session).

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>The hangup time is determined by the calling and answering computers. For example, if hangup time is 15 minutes on one machine and 10 minutes on the other, the call hangs up after 10 minutes of idle time.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select Log Modem I/O if you suspect a problem with the modem and deselect the option when the problem is fixed. T<:X8,-32768;Index "Modem" # "logging modem I/O"><:X8,-32768;Index "Log" # "logging modem I/O to">he Log Modem I/O option records modem control s
trings and responses in the Miscellaneous Events view in the server's Notes Log and adds a lot of extra information to the Notes Log. For more information about troubleshooting modems, see 
<+">Troubleshooting or Mobile Notes<-">.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select the RTS/CTS Flow Control <:X8,-32768;Index "Flow Control" #><:X8,-32768;Index "RTS/CTS Flow Control" #><:X8,-32768;Index "Modem" # "RTS/CTS flow control">option to control data flow between the computer and the modem. The default is selected. Deselec
t it only if the modem doesn't support flow control, or if using certain null modem connections or some add</m>in equipment (for example, older versions of DigiBoard]).

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>RTS/CTS stands for Request to Send/Clear to Send. RTS is a signal from the computer or terminal to the modem, announcing its readiness to send data. CTS is the modem's "go</m>ahead" response. When used for flow control, the RTS signal also tells the modem t
hat the computer is prepared to accept data.

@Indnt note@<:R1,4,1,0,1,720,1,1440,1,2160,>When using a null modem, the Maximum Speed selected on both computers must be identical (but no greater than 19,200). Deselect RTS/CTS Flow Control if the null modem cable doesn't support RTS/CTS modem control signals. 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Turning Flow Control off, especially with a fast modem (9600 bps or faster), may cause many CRC errors and retransmissions. These appear in the Notes Log Phone Calls view. If you see errors on connections from one server to 
<+">all<-"> other servers, data is probably being lost between this server and its modem; Flow Control on this server is probably off. If errors are only on connections with certain other servers, Flow Control on 
<+">those<-"> servers is probably off. Turning Flow Control on will solve the problem.

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>On null modems that don't support RTS/CTS modem control signals, lowering the Maximum Speed should reduce CRC errors and retransmissions. Remember to set both ends to the same maximum speed.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select Log Script I/O to record asynchronous script file responses in the Miscellaneous Events view in the server's Notes Log and if you suspect a problem with a script file. Deelect the option when the problem is fixed, since it adds a lot of extra informa
tion to the Notes Log. For more information about asynchronous communications scripts, see Appendix E.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select Scripts to bring up the Specify Acquire Script Information dialog box where you can select or edit an asynchronous communications script. XREF NCG

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>When you have completed modem setup, select OK twice to return to the Notes workspace.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Press ESC to exit the Notes workstation. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon on the Notes desktop.

@Bhead title@<+@><:s><:R1,1,1,2520,>Editing modem command files

<+@><:s><:R1,5,1,1920,1,2400,1,2880,1,3360,1,3840,>To select and edit modem files, you must determine which additional setup options you want to use. 

@Numbered list@<+@><:s><:R1,5,1,1920,1,2400,1,2880,1,3360,1,3840,>Double-click the Notes workstation icon on the Notes desktop.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Choose File - Tools - Notes Preferences and then select Ports. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select a COM port in the Communication Ports list. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select More Setup to determine the options for the specified communication port.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Specify the modem type.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select Edit.

@Numbered list@<+@><:s><:R1,1,1,2520,>Scroll horizontally and vertically to view the entire file. 

@Numbered list@<+@><:s><:R1,1,1,2520,>Make your changes to the contents of the specified modem file.   

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>After you view or modify the modem file, select one of the following to exit: 

@Indnt bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Save to save the changes to the same modem file.

@Indnt bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Save As to save the changes to a new modem file.

@Indnt bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Done to exit without saving your changes. 

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Click OK.

@Numbered list@<+@><:s><:R1,1,1,2520,>Shut down the server and double-click the Notes server icon. 

@Bhead title@<+@><:s><:R1,1,1,2520,>

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Setting additional port information on workstations or servers

<+@><:R1,1,1,2520,>

@Ahead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About customizing the X.PC protocol driver

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>You can customize the Notes X.PC driver for your system by using asynchronous communication scripts.

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Asynchronous scripts" #><:X8,-32768;Index "Script files" #>Notes supports the use of asynchronous scripts for X.25 and other applications beyond simple modem</m>to</m>modem connections. The asynchronous scripting feature is fully integrat
ed into the Notes X.PC driver and extends the capabilities of the Notes serial port to support the use of X.25 PADs, modem pools, and security devices, in addition to regular modem connections.

@Bhead@<:s><:R>Script files

Script files are similar to modem command files in that they both set up communications equipment to work in a given environment. Modem command files (.MDM files) set up the serial port for Notes to talk to a modem, usually in situations where 1) the Notes 
workstation or server making the call is connected directly to a modem, and 2) the Notes server answering the call is also connected directly to a modem. Scripts (.SCR files) set up communications equipment other than modems, for example, when connectivity 
involves the use of an asynchronous Packet Assembler/Disassembler (PAD) on an X.25 network.

@Bhead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Script file format

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "defined">A script is an ASCII text file containing keywords, commands, and arguments that comprise a set of instructions. These instructions tell Notes what to do to make the connection between one piece of hardware and a
nother.

@Bhead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Script types

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Scripts are either acquire or connect scripts, depending on whether the script is executed before or after the modem commands are executed. See Selecting an Acquire script; Selecting a Connect script.

@Bhead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Script commands

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Network administrators write scripts using the Script Language Definition. The commands included in the script file depend entirely on the device the file is setting up.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About Notes and X.PC; examples 

<:R>

@Chead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Examples: Script for mobile X.25

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "PAD" # "connecting to with a script file"><:X8,-32768;Index "X.25" # "connecting to a PAD with a script file"><:X8,-32768;Index "Script files" # "using to connect to a PAD">For X.25 applications, a Notes workstation is connected to a mode
m, and a call is made to an asynchronous PAD on an X.25 network. After connecting to the PAD, a Notes connect script issues a login sequence with the PAD.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,><[>insert conceptual art of a mobile X.25 script - prev from Admin Guide Appx E]

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@Chead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Examples: Script for asynchronous switches

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Modem pool" # "connecting to with a script file"><:X8,-32768;Index "Script files" # "using to connect to a pooled modem"><:X8,-32768;Index "Pool" #>In a modem pool application, a Notes workstation is connected to an asynchronous switch. T
he acquire script issues commands to this switch that allow a Notes workstation to connect to the correct modem. Note that for servers, this setup is not recommended for receiving calls. 

<:s><:R>

<[>insert conceptual art of an asynchronous switch example - prev from Admin Guide Appx E]

<:s>

@See also hlp@<:s>

<:s>Customizing the X.PC protocol driver


@Ahead@<:s>About writing a script

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:>Scripts contain additional commands that the server or workstation must perform each time you connect. There are two types of scripts:

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Acquire script

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Executed before the modem commands are issued. Use Acquire scripts to access or "acquire" the modem. For example, use an acquire script to access the appropriate modem in a modem pool before the modem call is made. Acquire scripts are used on a per port bas
is.

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Connect script

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Executed after the modem commands are issued. Use connect scripts to issue commands to an answering device, such as a PAD or a security device. Connect scripts can use up to four optional arguments, and are used on a per call basis. 

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:>Network administrators and <:X8,-32768;Index "Script files" # "writing">others who are familiar with the data communications equipment may write scripts.  

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>About script file format; About script commands; Selecting an Acquire script; Selecting a Connect script; 

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About script file format

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "format">A script file contains keywords and script command lines. The keywords identify and classify the script file, and are described below. The command lines are executed sequentially and are described in "About Script
 Language Definition." 

@Chead@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Script file keywords

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "keywords">The following keywords are used when writing script files:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "description"><:X8,-32768;Index "Description" # "DESC line of script file">DESC 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>A one</m>line description of the script file's purpose. This description also appears in the appropriate dialog box where you select that type of script (see "Selecting Script Files"). You must always include a DESC line in a script file so a description ap
pears in the dialog box.

@Indnt mono@<:R1,4,1,0,1,720,1,1440,1,2160,>DESC This script logs in via Telenet<[> X.25

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "type"><:X8,-32768;Index "Type" # "of script file">TYPE

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Tells whether the script is an ACQUIRE or CONNECT script. For example:

@Indnt mono@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>TYPE CONNECT or TYPE ACQUIRE 

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "arguments"><:X8,-32768;Index "Arguments" # "in script file">ARG1...ARG4

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>For Connect scripts only, these optional keywords precede a description of each of the four script arguments. If you do not enter a description here, nothing appears in the Connect script dialog box under the heading, "Connect script arguments." For example
, use the following script arguments in a Connect script file :

@Indnt mono@<:R1,4,1,0,1,720,1,1440,1,2160,>ARG1 1. REMOTE DTE ADDRESS:

@Indnt mono@<:R1,4,1,0,1,720,1,1440,1,2160,>ARG2 2. None entered:

@Indnt mono@<:R1,4,1,0,1,720,1,1440,1,2160,>ARG3 3. None entered:

@Indnt mono@<:R1,4,1,0,1,720,1,1440,1,2160,>ARG4 4. None entered:

@Note@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>The default script parameters are defined in the Remote Connection document for the remote server as Script Arguments. See "Selecting Script Files" for information about overriding script arguments when the call is made.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About example script files

<:R1,4,1,0,1,720,1,1440,1,2160,>Two example script files are copied to your Notes data directory when you install Notes. They are commented, fully</m>functional script file examples provided to explain the contents and uses of a Notes script file.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>SPRNTPAD.SCR

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>This script file was created for dialing in to a Sprint</n><:f,BArial,> 
<:f>PAD, but can also be used as a starting point for creating new script files for other PADs.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>COMSERV.SCR

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>This script file is an example of how an administrator might create a virtual circuit between a PC and a modem, which are connected by communications servers. It was created for acquiring a pooled modem via a bridge, but can also be used as a starting point
 for creating new script files for other communications servers.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>These sample files are fully commented (The semicolons in the ASCII file are removed for easier reading. All comment lines must begin with a semicolon to prevent errors.) For the most current files, check the samples provided with Notes.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@See also hlp@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>See also Creating or editing script files

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>About script language definition

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>General rules for writing script files are:

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>LABELS 

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Lines starting with a colon indicate a label

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>COMMENT LINES

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Lines starting with a semi</m>colon indicate a comment line

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>MAXIMUM LINE LENGTH

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>80 characters

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>MAXIMUM LABEL LENGTH

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Up to 8 significant characters

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>CONTROL CHARACTERS

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Control characters 0 - 20H can be embedded in strings (e.g. ^M is CTRL+M). Use double carets for literal caret (e.g., ^^M is CARET+M).

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>CONNECT SCRIPT ARGUMENTS

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Connect scripts can have up to 4 optional arguments: ^1, ^2, ^3, ^4. (See REPLY command for an example.) These correspond to the argument descriptions entered in the Call Setup dialog box, and the Script Arguments entered in the Remote Connection document f
or the remote server. The values entered replace the ^1, ^2, ^3, or ^4 in the script when the file is executed.

@Bullet@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>DTR

@1st lev para@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Data Terminal Ready (DTR) is raised at the start of script file processing.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Creating or editing a script file

<:R1,4,1,0,1,720,1,1440,1,2160,>Script files contain <:X8,-32768;Index "Script files" # "script language definition">ASCII text and use the .SCR extension. To review or edit the contents of these files, you can use Notes.

@Numbered list@<+@><:s><:R1,5,1,1920,1,2400,1,2880,1,3360,1,3840,>Double-click the Notes workstation icon on the Notes desktop.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose File - Tools - Notes Preferences.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Click Ports.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select one of the COM1-5 ports.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select More Setup.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select Acquire.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Select Edit in the Acquire Script dialog box. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make your changes to the Acquire script and click OK. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>?CAN"T FIND??  Specify Connect Script Information dialog boxes.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Click OK twice to exit the dialog boxes.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>???Do you NEEDED??Press ESC to save and exit Notes server.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,>See also 

<:R>

@Chead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Details: Creating or editing a script file

<:R1,4,1,0,1,720,1,1440,1,2160,>Since asynchronous scripts are ASCII files, you do not need a special editor to create or edit script files. To review or edit the contents of these files, use an ASCII editor. Save the file with the .SCR extension and copy it to the Notes data directory.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,>Table of script commands

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Script files" # "commands"><:X8,-32768;Index "Commands" # "in script files">The available script commands are described in this table.

<:R1,4,1,0,1,720,1,1440,1,2160,> <:t0>

<:R>

@Ahead@
@Ahead@
@Ahead@About cc:Mail address script format

<:><:X8,-32768;Index "cc:Mail" # "and script files"><:X8,-32768;Index "Script files" # "and cc:Mail">The asynchronous scripting feature provides limited support for the cc:Mail address script format. This support is described below:

In cc:Mail format, each line may consist of three components separated by one or more spaces. These components appear in the command line in the following order from left to right:

@Bullet@First component: 

@1st lev para@The prompt time</m>out interval (number of seconds to wait before completing the step without a prompt)

@Bullet@Second component:

@1st lev para@The prompt character(s) to wait for before inputting data

@Bullet@Third component: 

@1st lev para@The text data to send to the network

In addition to command lines conforming to the format described above, the following two command lines are also supported:

@Bullet@PROMPT OFF

@1st lev para@No prompt (default). Lines in the command file are allowed to time out if the exact prompt is not matched.

@Bullet@PROMPT ON

@1st lev para@Forces an exact match of the prompt string (including case). If there is no match, the call is aborted.


@Chead title@
@Chead title@Example: cc:Mail address script format

In this example, the commented text describes what happens in the script. 

@Mono@1 zzz ^M	

@Mono@Wait up to 1 second for "zzz," then send carriage return ^M

@Mono@10 NUMBER 2513042351

@Mono@Wait up to 10 seconds for "NUMBER," then send 2513042351 

@Mono@PROMPT ON

@Mono@5 B2400 HELLO	

@Mono@Wait up to 5 seconds for "B2400," and when received, send "HELLO," otherwise, timeout



@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,>About making a call using the script file

@1st Paragraph@<:R1,4,1,0,1,720,1,1440,1,2160,>You may want to select a script to perform specific tasks before or after you connect to the server, such as providing additional security or specifying a specific modem on a server. 

@1st Paragraph@<:R1,4,1,0,1,720,1,1440,1,2160,>  You must perform the following tasks before you can complete the call.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Check script file location and contents, and log file

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Make sure the script file resides in the same directory as the modem command files (usually the Notes data directory).

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Check that the script file contains a DESC and a TYPE keywords. A script file without the proper TYPE doesn't display in the appropriate dialog box and cannot be selected.

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>If necessary, enable Log Script I/O to capture scripting events in the Notes Log. This option appears in the More Setup dialog box.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Create or edit the remote connection document

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>When you are using scripts, you can enter values in the Remote Connection document that tell Notes which script file to use as a default and what arguments it needs to make the connection

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Select and edit Connect or Acquire scripts

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>XREFSee the steps topic

<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Selecting an Acquire script

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon on the Notes desktop.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select File - Mobile - Call Server.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose More Options.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select the port you want to use. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select Setup.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select the script you want to use in the Connect Script list.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose Edit to view or edit the script file.

<:R1,4,1,0,1,720,1,1440,1,2160,>	<[>insert screenshot of Edit script file dialog box]

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Save your changes and choose Done.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make your changes in the More Options dialog box and click OK. XREF

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make your changes in the Call Server dialog box and click OK. XREF 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select Auto Dial to make the call to the server.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Chead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Details: Selecting an Acquire script

<:R1,4,1,0,1,720,1,1440,1,2160,>You can also edit Acquire scripts with an ASCII editor. 

<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Selecting a Connect script

<:R1,4,1,0,1,720,1,1440,1,2160,>When you want to select or edit an existing connect script, you must call the server.<:X8,-32768;Index "Script files" # "selecting connect script"><:X8,-32768;Index "Connect script" # "selecting">

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Be sure to call the server before you select or edit an existing connect script.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select File - Mobile - Call Server.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose More Options, and then choose Call Setup.

<:R1,4,1,0,1,720,1,1440,1,2160,>	<[>insert screenshot of Connect script dialog box]

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select the script file you want to use in the Connect Script list. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose Edit to view or edit the script file.

<:R1,4,1,0,1,720,1,1440,1,2160,>	<[>insert screenshot of Edit script file dialog box]

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Enter up to four arguments to add or change the default value of the arguments. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Click Edit to change the descriptions next to the ARG1...4 keywords and their values in the script.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Save your changes and choose Done.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make your changes to the More Options dialog box and click OK. XREF

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Save your changes and choose Done.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make your changes to the Call Server dialog box and click OK. XREF

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,> Select Auto Dial to make the call to the server.

<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Chead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Details: Selecting a Connect script

<:R1,4,1,0,1,720,1,1440,1,2160,>You can also edit Connect scripts with an ASCII editor. 

<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Completing the call to the server using a script file

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Be sure that you performed these tasks before you complete the call.

@Indnt bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Checked the location and contents of the script file.

@Indnt bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Edited remote connection documents in the Name & Address book.

@Indnt bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Selected and edited either Connect or an Acquire script file.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon on the Notes desktop<:X8,-32768;Index "Script files" # "making a call with">.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose File - Mobile - Call Server.

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>The defaults from the Remote Connection document are displayed.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Make any necessary changes to the default settings. 

@Indnt note@<:R1,4,1,0,1,720,1,1440,1,2160,>Your changes are not saved to the Remote Connection document in the Name & Address Book.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose More Options to access the appropriate dialog box for the type of script you are selecting.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select the script to use for this call. For a Connect script, specify values for the arguments to be passed to the script, if different from those displayed.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose Edit to view or change the script file. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Save your changes and choose Done.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Click OK to return to the Call Server dialog box. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose Auto Dial to start the call. Messages appear on the status line to keep you informed of the call's progress.<:X8,-32768;Index "Acquire script" #><:X8,-32768;Index "Connect script" #>

<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>See also Checking the status of the X.PC port

@Bhead title@<:R>

@Ahead@
@Ahead@About troubleshooting Notes and X.PC

<:R1,4,1,0,1,720,1,1440,1,2160,><-!>When you cannot connect remotely via a modem to a server from another server or workstation, check the following items before you continue:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>The type of modem you're using

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Make sure that the modem is the correct type and model for your server or workstation. Check for any damages. Check the modem settings and make the needed changes to speed, switch settings, firmware version, and ROM version. Make the changes one at a time t
o see the effect of each change.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>The modem file you're using

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Make sure that the modem file uses the correct syntax for description, type, doesn't contain any bugs, spelling errors, missing command parameters, or incorrect settings or responses. Check the DOS time stamp and last revision date of the file. Make sure yo
u specified the correct directory for the file,

@Bullet@<:R>The Miscellaneous Events view in Notes log file

@1st lev para@Check the view for any information on the attempted connections. 

<:R1,4,1,0,1,720,1,1440,1,2160,>If you do find something that doesn't seem correct, swap the offending hardware or software with working hardware or software. 

<:R1,4,1,0,1,720,1,1440,1,2160,>If you are still having problems, there are additional items you can check, some of which are time-consuming to test but will usually resolve your modem problem.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Check if the modems on both servers or the remote server and the mobile workstation are compatible.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Recheck the configuration of the modem to make sure the selected ports, options, parameters, or settings are complete and correct; that you have a completed Connection document; and you are using the correct connectors and appropriate dip switches.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Check if the line is analog or digital; you made a manual or automatic call; the length of timeout and hangup settings; and whether you selected RTS/CTS flow control.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:R><:p<* >><:><+->About <--><+,>CH<-,><+->ECKING <--><+,>THE STATUS OF THE 
<-,><++>X.PC <-+><+,>PORT<-,>

<:X8,-32768;Index "Showing port status" # "XPC"><:X8,-32768;Index "XPC" # "showing port status"><:X8,-32768;Index "Showing port status" # "X.25"><:X8,-32768;Index "X.25" # "showing port status">The port status information for an XPC or X.25 communications p
ort sends messages to the Notes log (LOG.NSF) file that are similar to the following messages. The following table explains these entries to the LOG.NSF file.

@Mono@Waiting for incoming phone call

@Mono@Counts since the beginning of the last connection:

@Mono@<:R1,5,1,2390,1,2629,1,3107,1,5499,1,6709,>16 user messages sent<**>16 user messages received<**>1495 user bytes sent<**>1365 user bytes received<**>0 retransmitted packets<**>0 CRC errors detected<**>0 port errors detected

@Ahead@<:R><:t2>


@Bhead title@<-!>Checking the status of the X.PC port

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double-click the Notes workstation icon on the Notes desktop. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Double- click the Notes log (LOG.NSF) icon on the Notes desktop. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select View - Miscellaneous Events to view the contents of the log file. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select File - Close to exit the log file.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:R>

@Ahead@<+@><:R1,4,1,0,1,720,1,1440,1,2160,>EXTRA?? Done in NCG already?? Do not edit this section

@Dhead@<+@><:R1,4,1,0,1,720,1,1440,1,2160,>Available ports and drivers

<:R1,4,1,0,1,720,1,1440,1,2160,>The Notes X.PC driver is always installed with Notes. Use the XPC driver when you add a COM port (COM1-5) for remote ports. Use LAN0-4 for local area network ports using a local network driver. 

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>The list of available drivers is dependent on which Notes network drivers are installed. Other drivers may be installed but are not useable until the corresponding local area network software is installed. Then you can add LAN ports. The following network p
orts may be available after you install Notes: 

<:s><:R1,4,1,0,1,720,1,1440,1,2160,><:t1>

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,><-#><+)>Adding or updating workstation and server ports<-)><+*>H_ADDING_OR_UPDATING_WORKSTATION_AND_SERVER_PORTS<-*>

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Setting additional port information on workstations or servers

<+@><:R1,5,1,1920,1,2400,1,2880,1,3360,1,3840,>To select asynchronous scripts, select a modem file, determine the number of send/receive buffers, you must determine which additional setup options you use. Each network protocol requires different information. 

@Numbered list@<+@><:R1,5,1,1920,1,2400,1,2880,1,3360,1,3840,>Double-click the Notes workstation icon on the Note desktop.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Choose File - Tools - Notes Preferences.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Click Ports. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select a network port in the Communication Ports list. 

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>If you selected LAN0-LAN4 and NetBIOS, you must indicate the Unit Number and Buffer Size. The Unit Number is incremented by 1, as you define additional LAN ports. 

@Bullet@<+@><:R1,1,1,2520,>If you selected LAN0-LAN4 and AppleTalk, you need ??????.

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>If you selected COM1-COM5, indicate the modem type, maximum port speed, speaker volume, and dial tone. You can also request Log modem I/O, log script I/O, Hardware Flow Control, Dial timeout, Hangup if idle, and the port number. You can also select the Edit
 or Acquire option. 

@Bullet@<+@><:R1,1,1,2520,>If you selected SPX, indicate the number of SPX sessions as well as Send and Receive Packet Buffers per session.

@Bullet@<+@><:R1,1,1,2520,>If you selected TCP/IP, indicate the Secondary Notes Name Server and the TCP/IP Host Name or Address.

@Bullet@<+@><:R1,1,1,2520,>You cannot select Vines since it is not available.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select More Setup to determine the options for the specified communication port.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Specify the information in the Additional Setup dialog boxes.

@Numbered list@<:s><:R1,4,1,0,1,720,1,1440,1,2160,>Click OK.

@Numbered list@<+@><:s><:R1,1,1,2520,>Reboot or launch the Notes server.

<:s><:R1,4,1,0,1,720,1,1440,1,2160,>

@Bhead@<:R1,4,1,0,1,720,1,1440,1,2160,><:f240,,><:><-!>MOVE TO Chapter 5 System Growth ...<:f>..

@Bhead@<:R1,4,1,0,1,720,1,1440,1,2160,>Configuring Multiple Network Ports or Drivers

<:R1,4,1,0,1,720,1,1440,1,2160,>If a server is connected to multiple networks, edit its Server document to include the names of all the networks. You may also need to change the settings in the Port Setup dialog box to enable the appropriate ports. For complete instructions, see "Configur
ing Network Ports" in Appendix B.

@Bhead@<:R1,4,1,0,1,720,1,1440,1,2160,>Details: Configuring Multiple Network Ports or Drivers

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Server" # "setting up modem"><:X8,-32768;Index "Modem" # "setting up for the server">Notes servers on different networks can communicate over a telephone line, null modem, or other medium. In addition, users can dial up the server to acce
ss databases and send and receive mail remotely. 

<:R1,4,1,0,1,720,1,1440,1,2160,>If you didn't select a serial port during Server Setup<+">, <-">read the next few sections to set up the server for remote communication. The tasks include:

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Adding and enabling the serial port

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Setting up the modem in Notes

@Chead@<:R1,4,1,0,1,720,1,1440,1,2160,>Adding and Enabling the Port

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Configuring" # "serial port"><:X8,-32768;Index "Serial port" # "configuring"><:X8,-32768;Index "Port" # "serial"><:X8,-32768;Index "Remote" # "communication between servers"><:X8,-32768;Index "WAN communication between servers" #>For the 
additional Notes server to communicate with a remote Notes system, you must first attach an analog telephone line and a modem to the server. (Alternately, attach a null modem cable to two Notes servers.)<+!> 
<-!>Then configure the serial port and modem, from the workstation/administration program of the server. You can enable up to 16 ports.

<:R1,4,1,0,1,720,1,1440,1,2160,>{bmc pfnlm.bmp} To use a modem, the Notes for NetWare Server needs the asynchronous I/O driver files AIO.NLM and AIOCOMX.NLM. These are shipped with NetWare 3.12 and later, but if you are running NetWare 3.11, contact Novell to acquire these files. Then be 
sure that AIOCOMX.NLM is loaded.

@Tip@<:R1,4,1,0,1,720,1,1440,1,2160,>It's best to have your telephone company disable Call Waiting, Phone Mail, Call Park, and so on. These features affect the dial tone, or interrupt the carrier signal. (To temporarily disable Call Waiting in some locations, you can use *70, as the dialing pr
efix on a tone dial phone or 11</m>70 on a rotary dial phone. Check with your telephone company for more information.)

<:R1,4,1,0,1,720,1,1440,1,2160,>To add, redefine, or enable the port: 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Shut down the Notes server if it's running.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>From the Notes workstation program, choose File - Tools </m> Notes Setup, Ports. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>For details about this dialog box, see Appendix B, "Configuring Network Ports."

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Port" # "enabling a"><:X8,-32768;Index "Enabling a port" #>To enable a disabled port, highlight the port and select Enable Port.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Port" # "redefining a"><:X8,-32768;Index "Redefining a port" #>To change a port's settings, highlight the port and select Redefine Port.

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Port" # "adding a"><:X8,-32768;Index "Adding a port" #>To add a port, select Add Port to specify settings and then Enable port.

@Indnt note@<:R1,4,1,0,1,720,1,1440,1,2160,>If you enable a COM port, make sure the LAN adapter card does not use an Interrupt Request (IRQ) that conflicts with the COM port. COM1 uses IRQ4; COM2 uses IRQ3.<:X8,-32768;Index "Conflict" # "between network and serial port"><:X8,-32768;Index "IRQ conflict" # "between network and serial port">

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Select Encrypt Network Data <:X8,-32768;Index "Encryption" # "encrypting network data"><:X8,-32768;Index "Encrypt Network Data option" #>to encrypt data on the channel. This reduces data throughput slightly.

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>You can encrypt serial and network ports, and you can enable it at either end. If the option is selected on one end, it forces encryption upon the other end.

<:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,>About setting up dial</m>in servers

<:R1,4,1,0,1,720,1,1440,1,2160,><:X8,-32768;Index "Dial</m>in server" #><:X8,-32768;Index "Server" # "dial</m>in">Users may dial in to the Notes server from their homes, from other offices, or while they're travelling. Other servers may use the dial-in process if the network is not availa
ble. Before you begin to install and setup the modems, consider the number of modems you may need. :

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>How many busy signals are acceptable to your users? 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>It's unrealistic to expect that remote users never get a busy signal when trying to dial the server. However, you may want them to reach the server successfully nine times out of ten. Weigh the expense of purchasing more modems against what is acceptable to
 users when dial</m>in access to the server starts becoming difficult. 

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>Do users take advantage of workstation replication when accessing the<+"> server? 
<-">

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>Encourage users to use replication, instead of working interactively, to reduce server demand. With replication, remote users keep replicas of databases on their workstations, work on them without a dial</m>up connection, then connect to the server to excha
nge new and updated documents with the server's database. 

@Bullet@<:R1,4,1,0,1,720,1,1440,1,2160,>What types of users dial in to this server? 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>If users trying to access this server never work on a network and use the dial</m>up method exclusively (for example, sales representatives who are on the road), demand for the server will be higher than if they are occasional dial</m>up users.

<:R1,4,1,0,1,720,1,1440,1,2160,>{bmc pfos2.bmp}You may also want to consider installing a DigiBoard if you have an OS/2 Server. This card allows several ports on a single board so that you can connect multiple modems to a single serial port. 

@Bhead title@<:R1,4,1,0,1,720,1,1440,1,2160,>Setting up modems on a server<:X8,-32768;Index "Dial</m>in server" # "equipment needed">

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Install and set up the Notes server. Be sure the COM (serial) ports are enabled and the modems are properly set up

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Install at least one modem (9600 bps recommended) on the server. 

@Numbered list@<:R1,4,1,0,1,720,1,1440,1,2160,>Install two to four additional modems if you expect heavy dial</m>up use. Figure up to 16 ports or modems on a Notes server. 

<:R1,4,1,0,1,720,1,1440,1,2160,> 

@1st lev para@<:R1,4,1,0,1,720,1,1440,1,2160,>

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,>About setting up dial</m>up users<:X8,-32768;Index "Dial</m>in server" # "setting up users"><:X8,-32768;Index "Server" # "setting up dial</m>up users">

@hd:D@<:R1,4,1,0,1,720,1,1440,1,2160,>Before users can access a dial-in server, administrators must purchase a workstation license for each user, register new users, provide ID files and initial user passwords, specify the home server name and telephone number, give access to the server and its
 COM ports.

@hd:D@<:R1,4,1,0,1,720,1,1440,1,2160,>Check the <+">Mobile User's Guide<-"> for the list of tasks that users must perform before they can access databases on servers via modems. 

@Ahead@<:R1,4,1,0,1,720,1,1440,1,2160,>

<:R1,4,1,0,1,720,1,1440,1,2160,>

>

[Embedded]
00084150
