[ver]
	4
[sty]
	
[files]
[charset]
	82
	ANSI (Windows, IBM CP 1252)
[revisions]
	0
[sequence]
	9
	0
	0
	0
	23
	3
	Numbered list
	0
	Bullet
	0
	Indnt bullet
	0
	Indnt caution
	0
	Indnt tip
	0
	Indnt note
	0
	Caution
	0
	Tip
	0
	Note
	0
	Browse
	0
	Keyword
	0
	Context
	0
	Title
	0
	Macros
	0
	Alink
	0
	Butnbar
	0
	Window
	0
	Win95 macros
	0
	Win31 macros
	0
	Build tag
	0
	_COND_IF
	0
	_COND_ELSE
	0
	_COND_ENDIF
[prn]
	HP LaserJet III PostScript
[port]
	LPT2:
[lang]
	1
[fldnames]
	Field1
	Field2
	Field3
	Field4
	Field5
	Field6
	Field7
	Field8
[desc]
	
	
	
	
	
	801506576
	46
	780275445
	2402
	20
	0
	0
	0
	0
	
	
	
	
	
	
	1
[fopts]
	0
	1
	0
	0
	
	
[lnopts]
	2
	Body Text
	1
[docopts]
	5
	2
[GramStyle]
	
[ParaNum]
	1
[tag]
	Body Text
	2
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Ahead
	3
	[fnt]
		Arial
		220
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		240
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		2160
		3
		0
		1
		1
		1
		65
		10
		1
	[spec]
		0
		1
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead title
	4
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		79
		0
		3
		100
	[brk]
		80
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Chead title
	5
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		112
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Body Text
	0
	0
[tag]
	Bhead
	6
	[fnt]
		Arial
		200
		0
		16385
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		220
		4
		180
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		2
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Chead
	7
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		3
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Numbered list
	8
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		300
		300
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		5
		<*:>.
		0
		3
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Numbered list
	0
	0
[tag]
	1st lev para
	9
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		68
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	1st lev para
	0
	0
[tag]
	Bullet
	11
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		120
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Bullet
	2
	1
	160
	1
	400
	0
[tag]
	Indnt bullet
	12
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		420
		180
		180
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		16
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		</U>
		0
		3
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Indnt bullet
	0
	0
[tag]
	2nd lev para
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		600
		0
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	2nd lev para
	0
	0
[tag]
	See also prnt
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also prnt
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Book art
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Book art
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Callout text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Callout text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Figure title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		40
		60
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Figure title
	0
	0
[tag]
	Chapter title
	0
	[fnt]
		Arial
		280
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		300
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Chapter title
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	1st pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	1st pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Right pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Right pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Left pg foot
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Left pg foot
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Table title
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		60
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		7
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Table title
	0
	0
[tag]
	Table col hd
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		4
	[line]
		10
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		6
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table col hd
	0
	0
[tag]
	Table Text
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		1
		0
		0
		0
	[spc]
		40
		200
		4
		79
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		256
		1
		0
		
		
		
	Table Text
	0
	0
[tag]
	See also hlp
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		40
		4
		180
		0
		3
		100
	[brk]
		96
	[line]
		9
		0
		3
		0
		1
		1
		1
		70
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	0
	120
[tag]
	See also btn
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		240
	[spc]
		24
		200
		4
		0
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	See also btn
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Crossref
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		513
		3
		0
		300
		600
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Crossref
	0
	0
[tag]
	Indnt caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt caution
	0
	0
[tag]
	Indnt tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		324
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt tip
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Indnt note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		300
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Indnt note
	0
	0
[tag]
	Caution
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		720
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Caution
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Caution
	0
	0
[tag]
	Tip
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		324
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Tip
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Tip
	0
	0
[tag]
	Note
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		468
		0
	[spc]
		40
		200
		4
		19
		60
		3
		100
	[brk]
		4
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		Note
		0
		3
		1
		1
		0
		0
		0
	[nfmt]
		256
		1
		2
		.
		,
		$
	Note
	0
	0
[tag]
	Mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		48
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Indnt mono
	0
	[fnt]
		Courier New
		180
		0
		32768
	[algn]
		1
		3
		300
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		32
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Indnt mono
	15
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	1
	2880
	1
	3360
	1
	3840
	1
	4320
	1
	4800
	1
	5280
	1
	5760
	1
	6240
	1
	6720
	1
	7200
	0
[tag]
	Dhead
	0
	[fnt]
		Arial
		180
		0
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		100
		0
		3
		100
	[brk]
		68
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		4
		
		0
		1
		1
		0
		2
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		$
	Body Text
	0
	0
[tag]
	Parameter
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		0
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Parameter
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	Formula
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		19
		60
		3
		100
	[brk]
		36
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Formula
	0
	0
[tag]
	Browse
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		+
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Browse
	0
	0
[tag]
	Keyword
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		K
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Keyword
	0
	0
[tag]
	Context
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		#
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Context
	0
	0
[tag]
	Title
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		$
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Title
	0
	0
[tag]
	Macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		!
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Macros
	0
	0
[tag]
	Footnote
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		244
		0
	[spc]
		40
		2400
		3
		0
		0
		1
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		
		0
		1
		1
		256
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Footnote
	0
	0
[tag]
	Alink
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		A
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Alink
	0
	0
[tag]
	Butnbar
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		0
		0
	[spc]
		40
		200
		4
		0
		0
		3
		100
	[brk]
		48
	[line]
		16
		0
		3
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		\li-140 
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		272
		1
		2
		.
		,
		wr
	Butnbar
	0
	0
[tag]
	Window
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		>
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Window
	0
	0
[tag]
	Win95 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		W
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win95 macros
	0
	0
[tag]
	Win31 macros
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		X
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Win31 macros
	0
	0
[tag]
	Build tag
	0
	[fnt]
		Arial
		180
		0
		16384
	[algn]
		1
		3
		0
		139
		139
	[spc]
		24
		200
		4
		0
		0
		3
		100
	[brk]
		4
	[line]
		16
		0
		3
		0
		1
		2
		2
		20
		20
		1
	[spec]
		0
		0
		*
		0
		3
		1
		256
		1
		0
		0
	[nfmt]
		280
		1
		3
		.
		,
		$
	Build tag
	0
	0
[tag]
	_COND_IF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		IF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ELSE
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ELSE
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[tag]
	_COND_ENDIF
	0
	[fnt]
		Arial
		240
		255
		16385
	[algn]
		1
		3
		0
		0
		0
	[spc]
		24
		200
		4
		100
		0
		3
		100
	[brk]
		100
	[line]
		8
		0
		1
		0
		1
		1
		1
		10
		10
		1
	[spec]
		0
		0
		ENDIF
		0
		1
		1
		0
		0
		0
		0
	[nfmt]
		280
		1
		2
		.
		,
		$
	Body Text
	5
	1
	480
	1
	960
	1
	1440
	1
	1920
	1
	2400
	0
[lay]
	Standard
	1031
	[rght]
		12960
		10166
		1
		960
		1200
		3
		960
		720
		0
		1
		0
		1
		0
		2
		1
		960
		9446
		1
		1
		3120
	[lft]
		12960
		10166
		1
		720
		1200
		3
		960
		960
		0
		1
		0
		1
		0
		2
		1
		720
		9206
		1
		1
		3120
	[hlft]
	[lyfrm]
		1
		3008
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		3
	[frmlay]
		960
		10166
		1
		720
		180
		3
		0
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		2
		4674
	[txt]
>
	[hrght]
	[lyfrm]
		1
		11200
		0
		0
		10166
		960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		1
	[frmlay]
		960
		10166
		1
		960
		180
		3
		0
		720
		0
		1
		0
		1
		1
		0
		1
		960
		9446
		1
		2
		4674
	[txt]

>
	[flft]
	[lyfrm]
		1
		5056
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		4
	[frmlay]
		12960
		10166
		1
		720
		480
		3
		11940
		960
		0
		1
		0
		1
		1
		0
		1
		720
		9206
		1
		3
		9900
	[txt]
@Left pg foot@<+@><:R1,1,3,8486,><:P19999,0,7->  Network Configuration Guide	Lotus Confidential

>
	[frght]
	[lyfrm]
		1
		13248
		0
		11760
		10166
		12960
		0
		1
		3
		1 0 0 0 0 0 0
		0
		0
		2
	[frmlay]
		12960
		10166
		1
		900
		480
		3
		11940
		780
		0
		1
		0
		1
		1
		0
		1
		900
		9386
		1
		3
		9900
	[txt]
@Right pg foot@<+@><:R1,1,3,8486,>Lotus Confidential	Running Lotus Notes on Multiple Protocols  <:P19999,0,7->

>
[elay]
[l1]
	0
[pg]
	20
	23 108 21 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	46 84 91 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	78 102 27 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	102 110 33 32 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	132 0 0 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	147 435 51 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	167 17 19 0 0 1 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	173 1204 27 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	179 34 27 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	184 637 27 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	188 91 96 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	191 1349 47 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	201 111 66 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	212 173 7 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	229 0 47 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	233 1621 25 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	233 3396 50 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	235 695 18 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	237 671 18 0 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
	239 0 0 1025 0 0 0 200 65535 Standard	65535 0 0	0 0 0 0 0 0 0 65535 0 0 65535 0 0 0 0 0
[edoc]
@Chapter title@<:#300,8486><-!>Chapter 7 Running Lotus Notes Using Multiple Protocols<-!>

<:#200,8486><-!>This chapter describes how to set up Notes servers and workstations to run multiple network protocols.<-!>

@Ahead@<:#240,8486>About concepts for running Notes on multiple protocols

<:#1000,8486>Installing more than one network protocol on a Notes server or workstation, allows that machine to be compatible with a wider variety of other Notes servers and workstations. This chapter provides installation and configuration information about running Not
es servers and workstations on multiple protocols. To prepare to run your Notes servers and workstations on more than one network protocol, you should be familiar with the following concepts:

@Bullet@<:#400,8486>Which network protocols you can use with Notes servers and workstations 
<+"><+!>yy jump to Chapter 1 "About Notes and networks"<-!><-">

@Bullet@<:#400,8486>Which network standards your network protocols are compliant with, NDIS or ODI 
<+!><+">yy jump to Chapter 1 "About protocol standards supported by Notes-compliant network protocols"<-"><-!>

@Bullet@<:#600,8486>The procedures required to set up each single protocol on your Notes server or workstation 
<+!><+">yy jump to Chapter 1 "About which protocols run on Notes" which describes the individual protocol chapters and has jumps to them<-"><-!>

@Bullet@<:#200,8486>ODI and NDIS protocol standards <+!><+">yy <-!><-"><+!><+">jump to Chapter 1 "About network interface standards"<-"><-!>

@Bullet@<:#200,8486>Network interface cards <-!><-"><+!><+">yy <-!><-"><+!><+">jump to Chapter 1 "About network interface cards"<-"><-!><-!><-">

@Bullet@<:R1,1,1,1224,><:#400,8486>If multiple protocols can be loaded on the same network interface card (using one unit number). This depends on which standard is used<+!><+"> 
<-!><-"><+!><+">yy <-!><-"><+!><+">jump to "About Notes and network interface cards"<-"><-!>

@Bullet@<:R1,1,1,1224,><:#600,8486>The sequence in which the network protocol drivers have been loaded. In Notes, you determine this by examining the unit number, assuming the correct port driver has been assigned to the correct network card driver. 
<+!><+">yy <-!><-"><+!><+">jump to Chapter 1 "About the network unit number"<-"><-!>

@Bullet@<:R><:#400,8486>Your multiple protocol configuration/common Notes multiple protocol configurations<+!><+"> 
<-!><-"><+!><+">yy <-!><-"><+!><+">jump to this chapter, "About common Notes multiple protocol configurations"<-"><-!>

@Note@<:#600,8486><:>You cannot run Notes in an environment where NetBIOS protocols operate over TCP/IP. An example of one of these environments is the TCP/IP NetBIOS that is included with IBM LAN Manager 2.1.

<:#200,8486>

@Ahead@<:#240,8486>About network protocol compatibilty with network interface cards

<:#400,8486>To install network protocols on Notes servers and workstations, you must first install at least one network interface card. 
<+!><+">yy jump to Chapter 1 "About network interface cards"<-"><-!>

<:#600,8486>Normally, you install one protocol on each network interface card. You can install more than one protocol on a card, depending on the network standard with which it is compliant; ODI or NDIS. These are general rules for determining protocol compliance and c
ompatibility with network interface cards:

@Bullet@<:#200,8486>You can install up to four NDIS-compliant protocols on one network interface card.

@Bullet@<:R1,1,1,1224,><:#200,8486>You can install up to <+!><+">yy how many<-"><-!> ODI-compliant protocols on one network interface card.

@Bullet@<:R1,1,1,1224,><:#400,8486>You must purchase a dedicated network interface card for each proprietary protocol such as Banyan VINES.

@Bhead@<:R1,1,1,1080,><:#220,8486>Adding an ODI-compliant network protocol on a Notes server or workstation

<:R><:#400,8486>The following sections outline the procedures for adding an ODI-compliant network protocol on a separate network interface card on a Notes server. 

<:#400,8486>Install additional network protocols on a separate network interface card if that protocol meets any of the following conditions:

@Bullet@<:R1,1,1,1224,><:#400,8486>The additional protocol runs with a proprietary driver, such as Banyan VINES or IBM OS/2 EE for Token Ring.

@Bullet@<:R1,1,1,1224,><:#400,8486>The additional protocol runs with drivers that do not comply with the same protocol standard as your existing protocols.

@Bullet@<:R1,1,1,1224,><:#200,8486>You want to dedicate a separate card to an additional NDIS protocol.

<:R><:#800,8486>If you are trying to install an additional ODI-compliant protocol on a Notes OS/2 server already running another ODI-compliant protocol, the protocols can share a single network interface card. The procedure is similar to that described for installing multi
ple NDIS protocols earlier in this chapter. <+!><+">yy jump to NDIS procedure<-"><-!>

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:R><:#200,8486><:N795478803,JY,65535,1,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#600,8486>See related topics: Table of LAN protocols supported by Notes servers by platform, Table of LAN protocols supported by Notes workstations by platform, About protocol standards, Table of protocol standards supported by Notes network protocols

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,2,1
@@EndSection

>

<:R><:#200,8486>

@Ahead@<:#240,8486>About adding a network protocol to a Notes OS/2 server or workstation

<:#200,8486>Notes supports these protocols on the OS/2 platform:

@Bullet@<:#200,8486>AppleTalk

@Bullet@<:#200,8486>Banyan VINES

@Bullet@<:#200,8486>NetBIOS

@Bullet@<:#200,8486>NetWare SPX

@Bullet@<:#200,8486>TCP/IP

<:#400,8486>These are requirements for adding a network protocol to a Notes server or workstation when network protocols already exist on the machine: 

@Bullet@<:R1,1,1,1224,><:#800,8486>If you are using NDIS drivers, or the VINES proprietary network driver, and the Notes server or workstation is configured with NDIS drivers you can add an additional NDIS-compliant protocol on the existing network interface card. Otherwise, you must install
 a separate card for additional protocols.

@Bullet@<:R1,1,1,1224,><:#600,8486>If you are using Digital Equipment Corporation (DEC) PATHWORKS, you can install additional NDIS-compliant protocols on the existing network interface card because PATHWORKS uses NDIS-compliant protocol drivers.

@Bullet@<:R1,1,1,1224,><:#600,8486>If you are using IBM TCP/IP or FTP Software, Inc. PC/TCP, you can install additional NDIS-compliant protocols on the existing netowrk interface card because PATHWORKS uses NDIS-compliant protocol drivers.

@Bullet@<:R1,1,1,1224,><:#1000,8486>If you are using IBM OS/2 Extended Edition (EE) LAN Requester, you can install additional NDIS-compliant protocol drivers on an existing Ethernet card, but not to an existing Token Ring card because IBM OS/2 Extended Edition uses its own proprietary driver 
for Token Ring cards. When using IBM OS/2 Extended Edition Token Ring support on a Notes OS/2 server or workstation, you must install an additional network interface card for additional protocols.

@Bullet@<:R1,1,1,1224,><:#400,8486>If you are using Microsoft LAN Manager, you can install additional NDIS-compliant protocol on an existing network interface card.

@Indnt note@<:R1,1,1,360,><:#800,8486>LAN Manager NetWare Connectivity (provided with LAN Manager version 2.1 and higher) provides NDIS-based NetWare drivers so that NetWare and other NDIS protocols (for example, NetBIOS) can share the same adapter card. Since this is a DOS-based product, the f
unctionality applies only to Windows (DOS) workstations and is included in Windows for Workgroups software. 

@Bullet@<:R1,1,1,1224,><:#600,8486>If you are using Novell NetWare Requester with SPX you must install additional protocols on separate network interface cards, unless the additional protocols are ODI-compliant because NetWare Requester uses ODI network drivers rather than NDIS drivers.

@Ahead@<:R><:#240,8486>About adding a network protocol to a Notes Windows 3.X server or workstation

<:#200,8486>Notes supports these protocols on the Windows 3.x platform:

@Bullet@<:#200,8486>Banyan VINES

@Bullet@<:#200,8486>NetBIOS

@Bullet@<:#200,8486>NetWare SPX

@Bullet@<:#200,8486>TCP/IP

@Ahead@<:#240,8486>

@Ahead@<:#240,8486>About adding a network protocol to a Notes Windows NT server or workstation

<:#200,8486>Notes supports these protocols on the Windows NT platform:

@Bullet@<:#200,8486>AppleTalk

@Bullet@<:#200,8486>Banyan VINES

@Bullet@<:#200,8486>NetBIOS

@Bullet@<:#200,8486>NetWare SPX

@Bullet@<:#200,8486>TCP/IP

@Ahead@<:#240,8486>

@Ahead@<:#240,8486>About adding a network protocol to a Notes Macintosh workstation

<:#200,8486>Notes supports these protocols on the Macintosh platform:

@Bullet@<:#200,8486>AppleTalk

@Bullet@<:#200,8486>MacTCP

<:#200,8486>

@Ahead@<:#240,8486>About adding a network protocol to a Notes UNIX server or workstation

<:#200,8486>Notes supports these protocols on the UNIX platform:

@Bullet@<:#200,8486>NetWare SPX

@Bullet@<:#200,8486>TCP/IP

@Bhead@<:#220,8486>

@Ahead@<:#240,8486><-!>Installing multiple protocols on a Notes server or workstation

<:#200,8486>When you install multiple protocols on a Notes server or workstation, you either install them:

@Bullet@<:#200,8486>On one network interface card

@Bullet@<:#200,8486>On more than one network interface card (one protocol per card)

@Bhead@<:R1,1,1,1080,><:#220,8486>Installing multiple protocols on one network card

<:R><:#400,8486>print only: Use the guidelines in Chapter 1 to determine whether or not you can install more than one protocol on a network card.

<:#400,8486>Determine whether or not you can install more than one protocol on a network card. 
<+!><+">yy jump to About network protocol compatibilty with network interface cards<-"><-!>

<:#800,8486>You can put both ODI-based and NDIS-based protocols on one network interface card.  The most common tools you can use to do this are Novell's ODINSUP and IBM's ODI2NDI. 
<+!><+">yy researching<-!><-"><+!><+"> whether Lotus will officially support these for v4.  They have not been officially supported in past Notes releases.<-"><-!>

<:R1,1,1,1224,><:#200,8486>A typical scenario through which you would install multiple protocols on one network interface cards is:

@Numbered list@<:R><:#200,8486>Install one network interface card and one network protocol and make sure they work.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Save the configuration files.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Remove the first protocol, and install the second protocol on the card and make sure that it works.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Reinstall the first protocol.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Make sure that both protocols work together.

<:R1,1,1,1080,><:#400,8486>For more than two protocols, repeat step 3 for each protocol, then reinstall the other protocols one at a time, testing the configuration after each installation.

@Bhead@<:R><:#220,8486>Installing multiple protocols on two network cards<-!>

<:R1,1,1,1224,><:#600,8486>Sometimes you must install more than one network card for your protocols because of compatibility issues. A typical scenario through which you would install multiple protocols on two network interface cards is:

@Numbered list@<:R><:#200,8486>Install one network interface card and one network protocol and make sure they work.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Save the configuration files.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Remove the first protocol, and install the second protocol on the card and make sure that it works.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Add the second card, keeping only one protocol active.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Make sure the protocol works after the hardware change.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Install the second protocol on the second card and make sure it works.

@Ahead@<:R><:#240,8486>

@Ahead@<:#480,8486>Adding an ODI or NDIS-compliant network protocol to a Notes server or workstation

<:#200,8486>This is the general procedure to add a network protocol to a Notes server or workstation:

@Numbered list@<:R1,1,1,1080,><:#600,8486>Install an additional network interface card if necessary. Generally, you will need to install one for ODI-compliant protocols, while NDIS-compliant protocols can share a card and do not require that you install a new card. 

@Numbered list@<:R1,1,1,1080,><:#1400,8486>Copy all the network files, including the protocol driver and Protocol Manager files, for the new protocol into a directory on the Notes server or workstation. You may need to create a directory for these files, depending on the requirements for a given pro
tocol. <**><**>For example, to install the Notes AppleTalk protocol, you would create an AppleTalk files directory (C:\ATALK), then copy all the AppleTalk files from the Notes AppleTalk for OS/2 disk to this directory.

@Numbered list@<:R1,1,1,1080,><:#400,8486>Install the protocol manager software on the Notes server or workstation, if necessary. 
<+!><+">yy <-!><-"><+!><+">jump to "Installing p<-!><-"><+!><+">rotocol manager software"<-"><-!>

@Numbered list@<:R1,1,1,1080,><:#400,8486>Install the protocol driver software on the Notes server or workstation, if necessary. 
<+!><+">yy <-!><-"><+!><+">jump to "Installing Protocol Manager"<-"><-!>

@Numbered list@<:R1,1,1,1080,><:#400,8486>Edit the error log for the new network protocol, if necessary (as in the case of Notes AppleTalk). 
<+!><+">yy <-!><-"><+!><+">jump to "Editing the error log for a network protocol"<-"><-!>

@Numbered list@<:R1,1,1,1080,><:#200,8486>Restart the Notes server or workstation to load the new protocol files.

@Numbered list@<:R1,1,1,1080,><:#800,8486>If you are installing protocols on a Notes server, launch the server with the Notes workstation icon and enable the network port for the new protocol using File - Tools - Notes Preferences - Ports. If you are installing protocols on a Notes workstation, use
 the File - Tools - Notes Preferences - Ports to enable the network port for the new protocol.

@Numbered list@<:R1,1,1,1080,><:#400,8486>Add the new network name to the Server document on the Notes Name & Address Book (the NAMES.NSF file).

@Numbered list@<:R1,1,1,1080,><:#200,8486>Restart the Notes server.

@See also hlp@<:R1,4,1,0,1,720,1,1440,1,2160,><:#110,8486>

@See also btn@<:R><:#200,8486><:N795478803,JY,65535,3,1
@@Section("See related topics",9, SWISS, 0, 2313, 64, 1, 360, "")

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>See related topics: Adding or enabling a port (AG), Installing protocol manager software

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486><:N795732042,JY,65535,4,1
@@EndSection

>

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>print ref: Administrator's Guide, Chapter 3

@See also btn@<:R1,4,1,0,1,720,1,1440,1,2160,><:#200,8486>Chapter 1, Notes and networks, Installing protocol manager software

<:R1,1,1,1080,><:#200,8486>

@Ahead@<:R1,1,1,1080,><:#240,8486>About common multiple protocol configurations for Notes

<:R1,1,1,1080,><:#200,8486>There are many possible multiple protocol configurations. These are some of the most common:

@Bullet@<:R1,1,1,1080,><:#200,8486>NetWare NetBIOS with IBM LAN Server 3.0 NetBIOS <+!><+">yy <-!><-"><+!><+">insert jump to topic of same name<-"><-!>

@Bullet@<:R1,1,1,1080,><:#200,8486>AppleTalk with Novell/Token Ring (SPX) <+!><+">yy <-!><-"><+!><+">i<-!><-"><+!><+">nsert jump to topic of same name<-"><-!>

@Bullet@<:R1,1,1,1080,><:#200,8486>DEC PATHWORKS with AppleTalk <+!><+">yy <-!><-"><+!><+">insert jump to topic of same name<-"><-!>

@Bullet@<:R1,1,1,1080,><:#400,8486>AppleTalk, FTP TCP/IP, and SPX on two network interface cards <+!><+">yy 
<-!><-"><+!><+">insert jump to topic of same name<-"><-!>

@Bullet@<:R1,1,1,1080,><:#400,8486>AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS on Ethernet <+!><+">yy 
<-!><-"><+!><+">insert jump to topic of same name<-"><-!>

<:R1,1,1,1080,><:#200,8486>print only: Need a topic that points out what's available online and in help.

<:R1,1,1,1080,><:#200,8486>

@Ahead@<:R1,1,1,1080,><:#240,8486>Running NetWare NetBIOS with IBM LAN Server 3.0 NetBIOS

<:R1,1,1,1080,><:#400,8486>To run Notes on Novell NetWare NetBIOS with IBM LAN Server 3.0 NetBIOS under OS/2 2.1, you must complete each of the following tasks on the Notes server and/or workstation:

<:R1,1,1,1080,><:#400,8486>Task 1: Install Novell NetWare Requester for OS/2 (Version 2.01).<+!><+"> yy jump to Installing Novell NetWare Requester for OS/2 (Chapter 4, SPX) 
<-"><-!>

<:R1,1,1,1080,><:#200,8486>Task 2: Copy the file NETBIOS.SYS from OS2V2A.EXE to your NetWare directory.

<:R1,1,1,1080,><:#400,8486>Task 3: Install the IBM NTS/2 LAPS utility, which is shipped with IBM OS/2 LAN Server 3.0. 
<+!><+">yy jump to Installing and configuring the LAPS utility (IBM)<-"><-!>

<:R1,1,1,1080,><:#400,8486>Task 4: Configure Notes for IBM LAN Server 2.0 NetBIOS.  <+!><+">yy 
<-!><-"><+!><+">jump to Configuring Lotus Notes for IBM LAN Server 2.0 NetBIOS<-"><-!>

<:R1,1,1,1080,><:#400,8486>Task 5: Configure the Notes port driver for IBM LAN Server 2.0 NetBIOS. 
<+!><+">yy <-!><-"><+!><+">jump to Configuring the Notes Port Driver for IBM LAN Server 2.0 NetBIOS<-"><-!>

@Bhead title@<:R1,1,1,1080,><:#220,8486>

<:R1,1,1,1080,><:#200,8486>

@Bhead title@<:R><:#220,8486>Installing and configuring the LAPS utility (IBM)

<:#800,8486>IBM NTS/2 LAPS is a utility that provides protocol drivers for IBM OS/2 NetBIOS, IBM IEEE 802.2, and IBM NetWare Requester. The IBM NetWare Requester driver enables an NDIS-compliant protocol driver to communicate with an ODI-compliant protocol driver. When
 you install LAPS it automatically sets up the CONFIG.SYS and PROTOCOL.INI for use with the network.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Insert the IBM NTS/2 Disk 1 in Drive A: (or B:), type LAPS and press ENTER.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Select Install, select the local target drive, then select Configure.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Select Configure LAN Transports to display the Configure Workstation window. 

@Numbered list@<:R1,1,1,1080,><:#400,8486>From the Network Adapters box, add a network adapter, such as 3Com 3C503 Etherlink Adapter. You can select more than one adapter, if necessary.

@Numbered list@<:R1,1,1,1080,><:#400,8486>In the Protocols box, add these protocols: IBM OS/2 NetBIOS, IBM NetWare Requester, IBM IEEE 802.2

@Note@<:R1,1,1,1080,><:#200,8486>IBM IEEE 802.2 is required for IBM NetWare Requester.

@Numbered list@<:R1,1,1,1080,><:#3400,8486>To edit one or more of the drivers selected in the Network Adapters and Protocols boxes above, highlight the driver in the Current Configuration box, select Edit, and follow the steps below:<**><**>a. If you are installing LAPS on a Notes server, edit the I
BM OS/2 NetBIOS protocol to increase the values for Maximum Sessions, Maximum Commands, and Maximum Names, which correspond to the values for Sessions, NCBS, and Names, respectively, in the PROTOCOL.INI file documented in "Sample Configuration Files" later.
 <**><**>b.To edit the IBM NetWare Requester (ODI2NDI) protocol, edit the fields as follows:  
<**>Network adapter address: You must specify a value for this parameter, even if you use a universally administered address.<**>Ethernet address format, using the IEEE standard notation. The address begins with the letter i, for example, i02608c4e0652.<**>
IBM Token-Ring Network format, the address begins with the letter t, for example, t10005af00043.<**>Frame Header Support: 
<**>For Token Ring, select Yes for all frame header support fields associated with Token Ring.<**>For Ethernet, select Yes or all frame header support fields associated with Ethernet. 

@Indnt note@<:R1,1,1,360,><:#600,8486>The IBM NTS/2 LAPS configuration above adds the word REM to the beginning of the NetWare device statement that loads the protocol driver and replaces this statement with the IBM NetWare Requester driver.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Click OK and then exit the LAPS application.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Restart your system.

@Numbered list@<:R1,1,1,1080,><:#400,8486>Obtain the fix file ODI2NDI.OS2 dated 5/5/93 or later and copy it to the IBMCOM\PROTOCOL directory.

@Numbered list@<:R1,1,1,1080,><:#200,8486>Install IBM LAN Requester.

@Numbered list@<:R1,1,1,1080,><:#2000,8486>After Installation, edit IBMLAN.INI (located in IBMLAN directory) as follows:<**>Under <[>networks] heading, locate the following line: 
<**>net1 = NETBEUI$,0,LM10,72,96,32<**>Under this line, type the line below:<**><**>net2 = IPXNB$,0,LM10,64,96,14<**><**>The net1 and net2 lines in the <[>networks] section define which transport protocol is assigned to each virtual adapter number. In the e
xample above, the "net1" line assigns NETBEUI as the protocol when calls are made to NETAPI.DLL specifying adapter 0. 

@Bhead title@<:R1,1,1,1080,><:#220,8486>Configuring Lotus Notes for IBM LAN Server 2.0 NetBIOS

<:R><:#200,8486>Lotus provides the following two NetBIOS port drivers:

<:R1,1,1,1224,><:#400,8486>NETBIOS is implemented by $NETBIOS.DLL, uses the Submit interface, and makes calls to NETAPI.DLL

<:R1,1,1,1224,><:#400,8486>IBMEENB is implemented by $IBMEENB.DLL, uses the NB30 interface, and makes calls to ACSNETB.DLL.

<:R><:#200,8486>The only configurations that require using IBMEENB under OS/2 2.x are as follows:

<:R1,1,1,1224,><:#600,8486>IBM LAN Server 2.0 (or 3.0) LAN Requester is not installed, thus requiring the use of IBM NetBIOS. Without IBM LAN Server 2.0 (or 3.0) to provide the Submit interface API for IBM NetBIOS, the only API available to route NetBIOS calls over NETBEUI is the NB3
0 interface.

<:R1,1,1,1224,><:#800,8486>IBM LAN Server 2.0 (or 3.0) or IBM Extended Services 1.0 and Novell NetWare Requester for OS/2 2.0 are installed. The end-user is running an application that only supports the NB30 interface and he or she wants to use Novell NetWare IPX-based NetBIOS, and, 
on the same system, IBM NetBIOS must be used for another application (also via the NB30 interface).

@Note@<:R><:#600,8486>If you don't have to use IBMEENB, you will use the NetBIOS port driver, which uses the Submit interface. This implies that you installed the IBM LAN Requester, and therefore, must start the LAN Requester before running Notes.

@Bhead title@<:#220,8486>Configuring the Notes Port Driver for IBM LAN Server 2.0 NetBIOS

<:#1000,8486>A Notes server can support a network protocol on each port. To set up a second network protocol, you must add a second network name to the Notes Network field of the Server document in the Domain Name & Address Book. When both names are listed in the same o
rder that they are assigned to the LAN ports, Notes can function properly on both networks and provide access for both types of network clients simultaneously.

<:#400,8486>When a Notes server or workstation is properly configured for IBM LAN Server 2.0 NetBIOS, its NOTES.INI file includes the following lines:

<:R1,1,1,1080,><:#600,8486>Ports=LAN0,LAN1<**>LAN0=NETBIOS,0,15,2000<**>LAN1=NETBIOS,1,15,2000

@Ahead@<:R1,1,1,1080,><:#240,8486>Running AppleTalk with Novell/Token Ring

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>To run both AppleTalk and Novell NetBIOS or SPX on a Notes server, you must install AppleTalk on one network card and NetBIOS/SPX on a separate card. These working sample files appear below: PROTOCOL.INI, NET.CFG, and CONFIG.SYS.

@Chead@<:R><:#200,8486>Sample PROTOCOL.INI file for AppleTalk and Token Ring

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486><[>PROTMAN]<**>    DriverName = PROTMAN$

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><[>ATALK_XIF]<**>    DriverName = ATALK$<**>    Bindings = IBMTOK_NIF<**>    PortType = TokenTalk

<:R><:#600,8486><[>IBMTOK_NIF]<**>    DriverName = IBMTOK$ <**>    Alternate

@Chead@<:#200,8486>Sample NET.CFG File for AppleTalk and Token Ring

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>NetWare Requester<**>	preferred sprod_1

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>NetWare NetBIOS<**>	sessions 64<**>	commands 96

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>Protocol Stack IPX<**>	sockets 128

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>Protocol Stack SPX<**>	sessions 60

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>Link Driver Token<**>	Primary

@Chead@<:R><:#200,8486>Sample CONFIG.SYS File for AppleTalk and Token Ring

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#15400,8486>REM	CONFIG.SYS for dual Token Ring adapters running NetWare + AppleTalk<**>REM<**>REM	IBM OS/2 EE V1.3.01 CSD 5050 (now 5200)<**>REM<**>REM	Machine configuration:<**>REM	ZEOS 386/25, ISA only, 8Mb RAM, 200Mb disk<**>REM	(2) IBM 16/4 Token Ring Adapters<**>R
EM	Alternate: IRQ 2, D8000, 16K RAM, 16Mbps<**>REM	Primary: IRQ 3, D4000, 16K RAM, 16Mbps<**>REM<**>REM	ATALK must run on Alternate adapter (see PROTOCOL.INI; 
<**>REM	IPX/SPX on Primary (see NET.CFG)<**>REM<**>PROTSHELL=C:\OS2\PMSHELL.EXE C:\OS2\OS2.INI C:\OS2\OS2SYS.INI C:\OS2\CMD.EXE<**>SET COMSPEC=C:\OS2\CMD.EXE<**>LIBPATH=C:\OS2\DLL;C:\;C:\NETWARE;C:\NOTES;C:\ATALK<**>SET PATH=C:\OS2;C:\MUGLIB;C:\OS2\SYSTEM;C
:\OS2\INSTALL;C:\;L:\OS2;C:\NOTES;<**>	C:\NOTES\DATA;<**>SET DPATH=C:\OS2;C:\MUGLIB\DLL;C:\OS2\SYSTEM;C:\OS2\INSTALL;C:\;C:\NETWARE;<**>	C:\ATALK<**>SET PROMPT=$i<[>$p]<**>SET HELP=C:\OS2\HELP;<**>BUFFERS=60<**>IOPL=YES<**>DISKCACHE=1024<**>MAXWAIT=3<**>MEM
MAN=SWAP,MOVE,SWAPDOS<**>PROTECTONLY=YES<**>SWAPPATH=C:\OS2\SYSTEM 512<**>THREADS=255<**>COUNTRY=001,C:\OS2\SYSTEM\COUNTRY.SYS<**>DEVINFO=SCR,VGA,C:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_IBMVGA<**>SET VIO_IBMVGA=DEVICE(BVHVGA)<**>DEVICE=C:\OS2\COM01.SYS<**>
DEVICE=C:\OS2\POINTDD.SYS<**>DEVICE=C:\OS2\MSINP01.SYS<**>DEVICE=C:\OS2\MOUSE.SYS TYPE=MSINP$<**>DEVICE=C:\OS2\PMDD.SYS<**>SET KEYS=ON<**>SET BOOKSHELF=C:\OS2\BOOK;<**>SHELL=C:\OS2\COMMAND.COM /P<**>BREAK=OFF<**>FCBS=16,8<**>RMSIZE=640<**>REM DEVICE=C:\OS2\
EGA.SYS<**>DEVICE=C:\OS2\DOS.SYS<**>DEVINFO=KBD,US,C:\OS2\KEYBOARD.DCP<**>CODEPAGE=437,850<**>REM --- NetWare Requester statements BEGIN ---<**>DEVICE=C:\NETWARE\LSL.SYS<**>RUN=C:\NETWARE\DDAEMON.EXE<**>DEVICE=C:\NETWARE\TOKEN.SYS<**>REM DEVICE=C:\NETWARE\R
OUTE.SYS<**>DEVICE=C:\NETWARE\IPX.SYS<**>DEVICE=C:\NETWARE\SPX.SYS<**>RUN=C:\NETWARE\SPDAEMON.EXE<**>REM DEVICE=C:\NETWARE\NMPIPE.SYS<**>REM DEVICE=C:\NETWARE\NPSERVER.SYS<**>REM RUN=C:\NETWARE\NPDAEMON.EXE NP_COMPUTERNAME<**>DEVICE=C:\NETWARE\NWREQ.SYS<**>
IFS=C:\NETWARE\NWIFS.IFS<**>RUN=C:\NETWARE\NWDAEMON.EXE<**>REM DEVICE=C:\NETWARE\NETBIOS.SYS<**>REM RUN=C:\NETWARE\NBDAEMON.EXE<**>REM RUN=C:\NETWARE\NWSPOOL.EXE<**>REM --- NetWare Requester statements END ---<**>REM 
	--  AppleTalk statements start ---<**>DEVICE=c:\atalk\protman.os2 /i:c:\atalk<**>DEVICE=c:\atalk\ibmtok.os2<**>DEVICE=c:\atalk\atalk2v2.os2<**>RUN=c:\atalk\atalkini.exe<**>REM 
	Set up Log file <**>SET AppleTalk_LogFile=c:\notes\atalk.log<**>SET AppleTalk_LogFileSize=100<**>SET AppleTalk_ErrorFreq=20<**>REM - End of AppleTalk statements --

@Ahead@<:R1,1,1,1080,><:#240,8486>Running DEC PATHWORKS with AppleTalk

<:R><:#600,8486>The following are sample PROTOCOL.INI, CONFIG.SYS, and STARTUP.CMD files for running both AppleTalk and PATHWORKS on a Notes server using two 3C523 3Com EtherLink /MC network cards for each protocol.

@Chead@<:#200,8486>Sample PROTOCOL.INI for DEC PATHWORKS with AppleTalk

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486><[>PROTMAN]<**>  DRIVERNAME = PROTMAN$

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>;<[>NETBEUI_XIF]<**>;  Drivername = netbeui$<**>;  SESSIONS = 40<**>;  NCBS = 85<**>;  BINDINGS = ELNKMC_NIF

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1200,8486><[>DATALINK]<**>   Drivername = DLL$DEC<**>   Bindings =  ELNKMC_NIF2<**>   RC_Buffers = 32<**>   RL_Buffers = 43<**>   Tx_Buffers = 16

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#3400,8486><[>ELNKMC_NIF]<**>;   3C523 3Com EtherLink /MC adapter<**>    DRIVERNAME = ELNKMC$<**>;       2nd driver name = ELNKMC2$<**>    MAXTRANSMITS = 40<**>;       number of transmit queue elements (optional, default = 12)<**>;       Min = 8, Max = 50<**>;       U
se the default for DOS and normal OS/2 clients<**>;       Set MAXTRANSMITS = 40 for OS/2 servers<**>;   NETADDRESS = "02608C123456"<**>;       network address (optional, default = network adapter PROM value)<**>;       the network address is 12 hex digits e
nclosed in quotes<**>   SLOTNUMBER = 3<**>;       Microchannel slot number (optional, default = scan for adapter)<**>;       Min = 1, Max = 8<**>;       This parameter is needed to install the 2nd adapter in a higher<**>;       slot number

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486><[>ELNKMC_NIF2]<**>    DRIVERNAME = ELNKMC2$<**>    MAXTRANSMITS = 40<**>    SLOTNUMBER = 4 

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1600,8486><[>ATALK2_XIF]<**>; PROTOCOL.INI section for AppleTalk Phase 2 Protocol Stack/Router<**>; Refer to the LAN Manager Services for Macintosh Administrator's Guide<**>  Bindings = ELNKMC_NIF<**>  DriverName = ATALK$<**>  EnableRouter = No<**>  Port = ELNKMC_NIF
<**>  PortType = EtherTalk

@Chead@<:R><:#200,8486>Sample CONFIG.SYS for DEC PATHWORKS with AppleTalk

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#12200,8486>IFS=C:\LANMAN21\NETPROG\HPFS386.IFS /I:C:\LANMAN21 <**>RUN=C:\LANMAN21\NETPROG\CACHE.EXE 
<**>PROTSHELL=C:\OS2\PMSHELL.EXE C:\OS2\OS2.INI C:\OS2\OS2SYS.INI 
<**>	C:\OS2\CMD.EXE<**>SET COMSPEC=C:\OS2\CMD.EXE<**>LIBPATH=C:\LANMAN21\NETLIB;C:\PCSAOS2\DLL;C:\OS2\DLL;C:\OS2\SUPPORT;<**>  C:\;C:\NOTES;C:\NOTESDAT;<**>SET PATH=C:\LANMAN21\NETPROG;C:\PCSAOS2\PBIN;C:\OS2;C:\OS2\SYSTEM;<**>  C:\OS2\INSTALL;C:\OS2\SUPPORT
;C:\;C:\NOTES;C:\NOTESDAT;<**>SET DPATH=C:\LANMAN21\NETPROG;C:\PCSAOS2\DECNET;C:\PCSAOS2\PBIN;<**>  C:\PCSAOS2\CS;C:\OS2;C:\OS2\SYSTEM;C:\OS2\INSTALL;C:\;<**>SET PROMPT=$i<[>$p]<**>SET HELP=C:\OS2\HELP<**>BUFFERS=12<**>MAXWAIT=1<**>MEMMAN=SWAP,MOVE,SWAPDOS<**>
PROTECTONLY=YES<**>SWAPPATH=C:\OS2\SYSTEM 512<**>THREADS=255<**>COUNTRY=001,C:\OS2\SYSTEM\COUNTRY.SYS<**>devinfo=kbd,us,c:\os2\keyboard.dcp<**>codepage=437,850<**>DEVINFO=SCR,VGA,C:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_IBMVGA<**>SET VIO_IBMVGA=DEVICE(BVH
VGA)<**>DEVICE=C:\OS2\POINTDD.SYS<**>DEVICE=C:\OS2\MSPS202.SYS <**>DEVICE=C:\OS2\MOUSE.SYS TYPE=MSPS2$<**>DEVICE=C:\OS2\PMDD.SYS<**>SET KEYS=ON<**>DEVICE=C:\OS2\SUPPORT\DENON.VSD 
<**>DEVICE=C:\OS2\SUPPORT\STDCDROM.VSD <**>DEVICE=C:\OS2\SUPPORT\CDROM.TSD 
<**>RUN=C:\OS2\SUPPORT\LOGWRITE.EXE <**>SET BOOKSHELF=C:\OS2\BOOK<**>SHELL=C:\OS2\COMMAND.COM /P<**>BREAK=OFF<**>FCBS=16,8<**>RMSIZE=640<**>REM DEVICE=C:\OS2\EGA.SYS<**>REM  DEVICE=C:\OS2\DOS.SYS<**>IOPL=YES<**>tracebuf=1<**>REM ====== LANMAN 2.1 === DO NOT
 MODIFY BETWEEN THESE LINES === LANMAN 2.1 <**>SET DECNET=C:\PCSAOS2\DECNET<**>SET DNETPATH=C:\PCSAOS2\DECNET<**>SET DNETMAIL=C:\PCSAOS2\MAIL<**>DEVICE=C:\LANMAN21\DRIVERS\PROTMAN\PROTMAN.OS2 /i:C:\LANMAN21<**>DEVICE=C:\LANMAN21\DRIVERS\ETHERNET\ELNKMC\ELNK
MC.OS2<**>DEVICE=C:\LANMAN21\DRIVERS\ETHERNET\ELNKMC\ELNKMC.OS2<**>REM DEVICE=C:\LANMAN21\DRIVERS\PROTOCOL\NETBEUI\NETBEUI.OS2<**>DEVICE=C:\PCSAOS2\DEV\DLLMAC.SYS<**>DEVICE=C:\PCSAOS2\DEV\DNP.SYS<**>DEVICE=C:\PCSAOS2\DEV\IOCBDRV.SYS<**>DEVICE=C:\LANMAN21\NE
TPROG\RDRHELP.SYS<**>DEVICE=C:\LANMAN21\DRIVERS\PROTOCOL\APPLTALK\ATALK2\ATALK2V2.OS2<**>RUN=C:\LANMAN21\DRIVERS\PROTOCOL\APPLTALK\ATALKINI.EXE<**>IFS=C:\LANMAN21\NETPROG\NETWKSTA.SYS /i:C:\LANMAN21<**>REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE L
INES === LANMAN 2.1 <**>DISKCACHE=64<**>TIMESLICE=33,59

@Chead@<:R><:#200,8486>Sample STARTUP.CMD for DEC PATHWORKS with AppleTalk

<:#1000,8486>@@REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES === LANMAN 2.1<**>NET START WORKSTATION<**>@REM ====== LANMAN 2.1 === DO NOT MODIFY BETWEEN THESE LINES === LANMAN 2.1<**>start notes server<**>exit

@Ahead@<:R1,1,1,1080,><:#240,8486>Running AppleTalk, FTP TCP/IP, and SPX on two network cards

<:R><:#1000,8486><:>The four files below CONFIG.SYS, NET.CFG, STARTUP.CMD, and PROTOCOL.INI show how to use Notes AppleTalk, FTP Software PC/TCP, and Novell NetWare protocols on a single system using two network interface cards. In the sample setup, the two NDIS-compliant p
rotocols, Notes AppleTalk and PC/TCP are on the same card, Novell NetWare is on a separate card, and the Notes server uses four ports: NetBIOS (with NetWare's NetBIOS emulator), SPX, TCPFTP, and ATALK. 

<:#200,8486>The information in bold indicates AppleTalk and Notes information.

@Chead@<:#200,8486>Sample CONFIG.SYS for AppleTalk, FTP PCTCP, and Novell NetWare

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#13400,8486>PROTSHELL=C:\OS2\PMSHELL.EXE C:\OS2\OS2.INI C:\OS2\OS2SYS.INI <**>	C:\OS2\CMD.EXE<**>SET COMSPEC=C:\OS2\CMD.EXE<**>LIBPATH=c:\os2\dll;c:\;c:\netware;c:\pctcp\dll;c:\atalk;d:\notes;<**>SET PATH=c:\os2;\system;c:\os2\install;c:\;c:\netware;c:\pctcp\bin;c:\ata
lk;d:\notes;<**>	d:\brief<**>SET DPATH=c:\os2;c:\os2\system;c:\os2\install;c:\;c:\netware;c:\pctcp\etc;c:\atalk;<**>	d:\notes;<**>SET PROMPT=<[>$p]<**>SET HELP=C:\OS2\HELP;c:\pctcp\etc<**>BUFFERS=60<**>IOPL=YES<**>DISKCACHE=64<**>MAXWAIT=1<**>MEMMAN=SWAP,MO
VE,SWAPDOS,LP<**>PROTECTONLY=YES<**>SWAPPATH=C:\OS2\SYSTEM 512<**>THREADS=255<**>COUNTRY=001,C:\OS2\SYSTEM\COUNTRY.SYS<**>DEVINFO=SCR,VGA,C:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_IBMVGA<**>SET VIO_IBMVGA=DEVICE(BVHVGA)<**>DEVICE=C:\OS2\POINTDD.SYS<**>REM 
DEVICE=C:\OS2\MSPS201.SYS<**>REM DEVICE=C:\OS2\MOUSE.SYS TYPE=MSPS2$<**>DEVICE=C:\OS2\PMDD.SYS<**>DEVICE=C:\OS2\COM01.SYS<**>SET KEYS=ON<**>SET BOOKSHELF=C:\OS2\BOOK;<**>SHELL=C:\OS2\COMMAND.COM /P<**>BREAK=OFF<**>FCBS=16,8<**>RMSIZE=640<**>REM DEVICE=C:\OS
2\EGA.SYS<**>DEVICE=C:\OS2\DOS.SYS<**>DEVINFO=KBD,US,C:\OS2\KEYBOARD.DCP<**>CODEPAGE=437,850<**>REM *** ftp pc/tcp configuration statements &<**>REM *** Lotus Notes AppleTalk configuration statements<**>SET TZ=EST5EDT<**>REM * DEVICE=c:\pctcp\drv\protman.os
2 /i:c:\pctcp\drv<**>DEVICE=c:\atalk\protman.os2 /i:c:\pctcp\drv<**>device=c:\pctcp\drv\elnkii.os2<**>SET PCTCP=c:\pctcp\etc\pctcp.ini<**>DEVICE=c:\pctcp\drv\socket.os2<**>IFS = c:\pctcp\drv\nfsifs.sys<**>REM --- NetWare Requester statements BEGIN ---<**>DE
VICE=c:\netware\lsl.sys<**>RUN=c:\netware\ddaemon.exe<**>DEVICE=c:\netware\3c503.sys<**>DEVICE=c:\netware\Ipx.sys<**>DEVICE=c:\netware\spx.sys<**>RUN=c:\netware\spdaemon.exe<**>REM DEVICE=c:\netware\nmpipe.sys<**>REM DEVICE=c:\netware\npserver.sys<**>REM RU
N=c:\netware\npdaemon.exe NP_COMPUTERNAME<**>DEVICE=\NWREQ.SYS<**>IFS=c:\netware\nwifs.ifs<**>RUN=c:\netware\nwdaemon.exe<**>DEVICE=c:\netware\netbios.sys<**>RUN=c:\netware\nbdaemon.exe<**>REM RUN=c:\netware\nwspool.exe<**>REM --- NetWare Requester statemen
ts END ---<**>REM * DEVICE=c:\netware\odinsup.sys<**>device=c:\atalk\atalk2v2.os2<**>run=c:\atalk\atalkini.exe<**>TIMESLICE=33,59

@Chead@<:R><:#200,8486>Sample NET.CFG for AppleTalk, FTP PCTCP, and Novell NetWare

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>;link driver NE3200<**>;       frame ethernet_802.3<**>;       frame ethernet_ii<**>;       frame ethernet_802.2<**>;       frame ethernet_snap

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486>link driver 3c503<**>       frame ethernet_802.3<**>       frame ethernet_ii<**>       frame ethernet_802.2<**>       frame ethernet_snap

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>;link support<**>;       buffers 15 4210

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>;protocol ODINSUP<**>;       bind NE3200

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#400,8486>;protocol ODINSUP<**>;	bind 3c503

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>netware netbios<**>  sessions 64<**>  commands 96<**>  names  64

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#800,8486>netware requester<**>  sessions 20<**>  cache buffers 128<**>  request retries 40

@Chead@<:R><:#200,8486>Sample PROTOCOL.INI for AppleTalk, FTP PCTCP, and Novell NetWare

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1400,8486>;       FTP Software template for protocol.ini<**>;               this template should be merged with a MAC driver<**>;               protocol.ini. The resultant file should reside in<**>;               a directory pointed to by the /i: option of the<**>;  
             protman.os2 statement in config.sys<**>;                       Example:<**>;                       device=c:\pctcp\ndis\protman.os2 /i:c:\pctcp\ndis;

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1600,8486>;************************<**>;**     PROTOCOLS      **<**>;************************<**>;FTP PC/TCP for OS/2<**><[>SOCKET]<**>   drivername = $SOCKET<**>;  bindings =   x3c503<**>   bindings = ELNKII

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1000,8486><[>ATALK_XIF]<**>   drivername = ATALK$<**>;  Bindings =   x3c503<**>   Bindings = ELNKII<**>   PortType =   EtherTalk

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#600,8486>;************************<**>;**     ADAPTERS       **<**>;************************

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#1800,8486><[>ELNKII]<**>    DriverName = ELNKII$<**>    Interrupt = 5<**>    IOAddress = 0x310<**>    DMAChannel = 3<**>    MaxTransmits = 40<**>;   Transceiver = External<**>    Transceiver  = Onboard<**><[>x3c503]

@Chead@<:R><:#200,8486>Sample STARTUP.CMD for AppleTalk, FTP PCTCP, and Novell NetWare

<:#1000,8486>netbind<**>c:\atalk\tpause 45<**>tcpmgr start<**>cd \notes<**>notes server

<:R1,1,1,1080,><:#200,8486><:>

@Ahead@<:R1,1,1,1080,><:#240,8486>Running AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS on Ethernet

<:R1,1,1,1080,><:#800,8486><:>The four files below CONFIG.SYS, NET.CFG, STARTUP.CMD, and PROTOCOL.INI show how to use Notes AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS protocols on Ethernet. In this sample setup, the Notes server has five network ports, one for each network protoc
ol. Below are versions of the network protocols used to make the configuration files in this section.

@Bhead@<:R><:#220,8486>OS/2

<:#1600,8486>Build 6.514.  This is the GA release, without any patches.<**>SYSLEVEL shows:<**>D:\OS2\INSTALL\SYSLEVEL.OS2<**>IBM OS/2 Base Operating System<**>Version 2.10     Component ID 562107701<**>Type 0<**>Current CSD level: XR02010<**>Prior   CSD level: XR02010

@Bhead@<:#220,8486>IBM LAPS

<:#400,8486>This version of LAPS came with IBM TCP/IP v2.0, and is slightly newer than the version with LAN Server.

<:#1200,8486>SYSLEVEL shows:<**>D:\IBMCOM\SYSLEVEL.TRP<**>IBM OS/2 LAN Adapter and Protocol Support<**>Version 2.13     Component ID 562125303<**>Current CSD level: WR06000<**>Prior   CSD level: WR06000

@Bhead@<:#220,8486>IBM LAN Requester (NetBeui)

<:#400,8486>This is the requester which comes with IBM LAN Server v3.0.  We have other servers running IBM LAN Server with AppleTalk on the same card.

<:#2800,8486>SYSLEVEL shows:<**>D:\IBMLAN\SYSLEVEL.REQ<**>IBM OS/2 LAN Requester<**>Version 3.00     Component ID 562125301<**>Current CSD level: IP07000<**>Prior   CSD level: IP07000<**>D:\IBMLAN\SYSLEVEL.LSR<**>IBM OS/2 LAN Server/Requester Product<**>Version 3.00    
 Component ID 562125305<**>Current CSD level: IP07000<**>Prior   CSD level: IP07000<**>IBM TCP/IP<**>SYSLEVEL shows:<**>D:\TCPIP\SYSLEVEL.TCP

@Bhead@<:#220,8486>TCP/IP

<:#800,8486><**>BASE  for OS/2 2.0 and 2.1<**>Version 2.00     Component ID 562208600<**>Current CSD level: UN00000<**>Prior   CSD level: UN00000

@Bhead@<:#220,8486>NetWare NetBIOS

<:#200,8486>This driver is from NetWare for OS/2 CSD NSD201.

@Bhead@<:#220,8486>NetWare SPX

<:#200,8486>This driver is from NetWare for OS/2 CSD NSD201.

<:#200,8486>The Notes "show port" command shows:

<:#200,8486>NetWare OS/2 Requester version: v2.1a

<:#200,8486>NetWare SPX version: v3.0b

@Bhead@<:#220,8486>AppleTalk

<:#200,8486>This is the new AppleTalk software version 1.1b

<:#200,8486>When the driver loads, the following line is displayed:

<:#200,8486>Lotus Notes AppleTalk Phase II Protocol Stack for OS/2 2.1 Version 1.1b

@Chead@<:#200,8486>Sample CONFIG.SYS file for AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS on Ethernet

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#23600,8486>REM IFS=D:\OS2\HPFS.IFS  /CACHE:64 /CRECL:4<**>PROTSHELL=D:\OS2\PMSHELL.EXE<**>SET USER_INI=D:\OS2\OS2.INI<**>SET SYSTEM_INI=D:\OS2\OS2SYS.INI<**>SET OS2_SHELL=D:\OS2\CMD.EXE<**>SET AUTOSTART=PROGRAMS,TASKLIST,FOLDERS,CONNECTIONS<**>SET RUNWORKPLACE=D:\OS2\
PMSHELL.EXE<**>SET COMSPEC=D:\OS2\CMD.EXE<**>LIBPATH=D:\IBMCOM\DLL;D:\IBMLAN\NETLIB;D:\MUGLIB\DLL;.;D:\OS2\DLL;D:\OS2\MDOS;D:\;D:\OS2\APPS\DLL;D:\NET\PACER\v1.1b;D:\N\BIN\PBIN;C:\NET\NETWARE\NW312\OS2;D:\TCPIP\DLL;<**>SET PATH=D:\IBMLAN\NETPROG;D:\MUGLIB;D:
\OS2;D:\OS2\SYSTEM;D:\OS2\MDOS\WINOS2;D:\OS2\INSTALL;D:\;D:\OS2\MDOS;D:\OS2\APPS;D:\N\BIN\PBIN;C:\NET\NETWARE\NW312\OS2;L:\OS2;P:\OS2;L:\NLS;P:\NLS;D:\TCPIP\BIN;<**>SET DPATH=D:\IBMCOM;D:\IBMLAN\NETPROG;D:\IBMLAN;D:\MUGLIB;D:\OS2;D:\OS2\SYSTEM;D:\OS2\MDOS\W
INOS2;D:\OS2\INSTALL;D:\;D:\OS2\BITMAP;D:\OS2\MDOS;D:\OS2\APPS;D:\NET\PACER\v1.1b;C:\NET\NETWARE\NW312\OS2;<**>SET PROMPT=$i<[>$p]<**>SET HELP=D:\OS2\HELP;D:\OS2\HELP\TUTORIAL;D:\TCPIP\HELP;<**>SET GLOSSARY=D:\OS2\HELP\GLOSS;<**>SET IPF_KEYS=SBCS<**>PRIORIT
Y_DISK_IO=YES<**>FILES=20<**>DEVICE=D:\IBMCOM\PROTOCOL\LANPDD.OS2<**>DEVICE=D:\IBMCOM\PROTOCOL\LANVDD.OS2<**>DEVICE=D:\IBMCOM\LANMSGDD.OS2 /I:D:\IBMCOM 
<**>DEVICE=D:\IBMCOM\PROTMAN.OS2 /I:D:\IBMCOM<**>DEVICE=D:\OS2\TESTCFG.SYS<**>DEVICE=D:\OS2\DOS.SYS<**>DEVICE=D:\OS2\PMDD.SYS<**>BUFFERS=30<**>IOPL=YES<**>DISKCACHE=1024,LW,AC:D<**>MAXWAIT=3<**>MEMMAN=SWAP,PROTECT<**>SWAPPATH=D:\OS2\SYSTEM 2048 2048<**>BREA
K=OFF<**>THREADS=256<**>PRINTMONBUFSIZE=134,134,134<**>COUNTRY=001,D:\OS2\SYSTEM\COUNTRY.SYS<**>SET KEYS=ON<**>REM SET DELDIR=C:\DELETE,512;D:\DELETE,512;<**>BASEDEV=PRINT01.SYS<**>BASEDEV=IBM1FLPY.ADD<**>BASEDEV=IBM1S506.ADD<**>BASEDEV=OS2DASD.DMD<**>SET B
OOKSHELF=D:\IBMLAN\BOOK;D:\OS2\BOOK;D:\TCPIP\DOC;<**>SET EPMPATH=D:\OS2\APPS;<**>DEVICE=D:\OS2\APPS\SASYNCDA.SYS 
<**>PROTECTONLY=yes<**>SHELL=D:\OS2\MDOS\COMMAND.COM D:\OS2\MDOS<**>FBS=16,8<**>RMSIZE=640<**>DEVICE=D:\OS2\MDOS\VEMM.SYS 
<**>DOS=LOW,NOUMB<**>DEVICE=D:\OS2\MDOS\VDPX.SYS <**>DEVICE=D:\OS2\MDOS\VXMS.SYS /UMB<**>DEVICE=D:\OS2\MDOS\VDPMI.SYS 
<**>DEVICE=D:\OS2\MDOS\VCDROM.SYS <**>DEVICE=D:\OS2\MDOS\VWIN.SYS 
<**>DEVICE=D:\OS2\OS2CDROM.DMD /Q<**>IFS=D:\OS2\CDFS.IFS /Q <**>BASEDEV=OS2SCSI.DMD 
<**>BASEDEV=AHA154X.ADD <**>DEVICE=D:\OS2\MDOS\VMOUSE.SYS <**>DEVICE=D:\OS2\POINTDD.SYS 
<**>DEVICE=D:\OS2\MOUSE.SYS <**>DEVICE=D:\OS2\COM.SYS <**>DEVICE=D:\OS2\MDOS\VCOM.SYS 
<**>CODEPAGE=437,850<**>DEVINFO=KBD,US,D:\OS2\KEYBOARD.DCP<**>DEVINFO=SCR,VGA,D:\OS2\VIOTBL.DCP<**>SET VIDEO_DEVICES=VIO_SVGA<**>SET VIO_SVGA=DEVICE(BVHVGA,BVHSVGA)<**>DEVICE=D:\OS2\MDOS\VSVGA.SYS<**>device=d:\net\pacer\v1.1b\atalk2v2.os2<**>run=d:\net\pace
r\v1.1b\atalkini.exe<**>RUN=D:\IBMCOM\PROTOCOL\NETBIND.EXE<**>RUN=D:\IBMCOM\LANMSGEX.EXE<**>DEVICE=D:\IBMLAN\NETPROG\RDRHELP.200<**>REM --- NetWare Requester statements BEGIN ---<**>SET NWLANGUAGE=ENGLISH<**>DEVICE=C:\NET\NETWARE\NW312\OS2\LSL.SYS<**>RUN=C:
\NET\NETWARE\NW312\OS2\DDAEMON.EXE<**>device = D:\ibmcom\protocol\odi2ndi.os2<**>REM -- ODI-Driver Files BEGIN --<**>REM DEVICE=C:\NET\NETWARE\NW312\OS2\3C503.SYS<**>REM DEVICE=C:\NET\NETWARE\NW312\OS2\ROUTE.SYS<**>REM -- ODI-Driver Files END --<**>DEVICE=C
:\NET\NETWARE\NW312\OS2\IPX.SYS<**>DEVICE=C:\NET\NETWARE\NW312\OS2\SPX.SYS<**>RUN=C:\NET\NETWARE\NW312\OS2\SPDAEMON.EXE<**>REM DEVICE=C:\NET\NETWARE\NW312\OS2\NMPIPE.SYS<**>REM DEVICE=C:\NET\NETWARE\NW312\OS2\NPSERVER.SYS<**>REM RUN=C:\NET\NETWARE\NW312\OS2
\NPDAEMON.EXE<**>DEVICE=C:\NET\NETWARE\NW312\OS2\NWREQ.SYS<**>IFS=C:\NET\NETWARE\NW312\OS2\NWIFS.IFS<**>RUN=C:\NET\NETWARE\NW312\OS2\NWDAEMON.EXE<**>DEVICE=C:\NET\NETWARE\NW312\OS2\NETBIOS.SYS<**>RUN=C:\NET\NETWARE\NW312\OS2\NBDAEMON.EXE<**>DEVICE=C:\NET\NE
TWARE\NW312\OS2\VIPX.SYS<**>DEVICE=C:\NET\NETWARE\NW312\OS2\VSHELL.SYS GLOBAL<**>REM --- NetWare Requester statements END ---<**>DEVICE=D:\IBMCOM\MACS\EXP16.OS2<**>RUN=D:\IBMLAN\NETPROG\LSDAEMON.EXE<**>DEVICE=D:\IBMLAN\NETPROG\VNETAPI.OS2<**>RUN=D:\IBMLAN\N
ETPROG\VNRMINIT.EXE<**>DEVICE=D:\IBMCOM\PROTOCOL\INET.SYS<**>DEVICE=D:\IBMCOM\PROTOCOL\IFNDIS.SYS<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBEUI.OS2<**>IFS=D:\IBMLAN\NETPROG\NETWKSTA.200 /I:D:\IBMLAN/N<**>DEVICE=D:\IBMCOM\PROTOCOL\NETBIOS.OS2<**>SET ETC=D:\TCPIP\ETC<**>
SET TMP=D:\TCPIP\TMP<**>SET READIBM=D:\TCPIP\DOC<**>SET HOSTNAME=zeus<**>RUN=D:\TCPIP\BIN\CNTRL.EXE

@Chead@<:R1,1,1,1080,><:#200,8486>Sample PROTOCOL.INI file for AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS on Ethernet

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#12000,8486><[>PROT_MAN]<**>   DRIVERNAME = PROTMAN$<**><[>IBMLXCFG]<**>   NETBEUI_nif = NETBEUI.NIF<**>   ODI2NDI_nif = ODI2NDI.NIF<**>   TCPIP_nif = TCPIP.nif<**>   EXP16_nif = EXP16.nif<**><[>NETBEUI_nif]<**>   DriverName = netbeui$<**>   Bindings = EXP16_nif<**>   
ETHERAND_TYPE = "I"<**>   USEADDRREV = "YES"<**>   OS2TRACEMASK = 0x0<**>   SESSIONS = 40<**>   NCBS = 95<**>   NAMES = 21<**>   SELECTORS = 5<**>   USEMAXDATAGRAM = "NO"<**>   ADAPTRATE = 1000<**>   WINDOWERRORS = 0<**>   MAXDATARCV = 4168<**>   TI = 30000
<**>   T1 = 500<**>   T2 = 200<**>   MAXIN = 1<**>   MAXOUT = 1<**>   NETBIOSTIMEOUT = 500<**>   NETBIOSRETRIES = 8<**>   NAMECACHE = 0<**>   PIGGYBACKACKS = 1<**>   DATAGRAMPACKETS = 2<**>   PACKETS = 350<**>   LOOPPACKETS = 1<**>   PIPELINE = 5<**>   MAXT
RANSMITS = 6<**>   MINTRANSMITS = 2<**>   DLCRETRIES = 5<**><[>ATALK_XIF]<**>  DriverName = ATALK$<**>  Bindings = EXP16_nif<**>  PortType = EtherTalk<**><[>ODI2NDI_nif]<**>   DriverName = odi2ndi$<**>   Bindings = EXP16_nif<**>   NETADDRESS = "i00AA00242F4
C"<**>   TOKEN-RING = "no"<**>   TOKEN-RING_SNAP = "no"<**>   ETHERNET_802.3 = "yes"<**>   ETHERNET_802.2 = "no"<**>   ETHERNET_II = "no"<**>   ETHERNET_SNAP = "no"<**>   TRACE = 0x0<**><[>TCPIP_nif]<**>   DriverName = TCPIP$<**>   Bindings = EXP16_nif<**>;
 Intel EtherExpress(tm) 16 Ethernet Adapter<**><[>EXP16_nif]<**>  IOADDRESS = 0x300<**>  DRIVERNAME = EXP16$<**>; OS/2 LAN Requester initialization file

@Chead@<:R1,1,1,1080,><:#200,8486>Sample IBMLAN.INI file for AppleTalk, IBM TCP/IP, SPX, and Novell NetBIOS on Ethernet

<:R1,8,1,0,1,720,1,720,1,1440,1,2160,1,2880,1,3600,1,4320,><:#12000,8486><[>networks]<**>  net1 = NETBEUI$,0,LM10,32,50,14<**>; Added this line by hand, to make NetWare NetBIOS work with Notes.<**>  net2 = ipxnb$,0,LM10,32,50,14<**>; This information is read by the redirector at device initialization time.<**><[>requester]<**>  
COMPUTERNAME = ZEUS<**>  DOMAIN = IRI<**>; The following parameters generally do not need to be<**>; changed by the user.<**>  charcount = 16<**>  chartime = 250<**>  charwait = 3600<**>  keepconn = 600<**>  keepsearch = 600<**>  maxcmds = 16<**>  maxerrorl
og = 100<**>  maxthreads = 10<**>  maxwrkcache = 64<**>  numalerts = 12<**>  numcharbuf = 10<**>  numservices = 7<**>  numworkbuf = 15<**>  numdgrambuf = 14<**>  othdomains = 
<**>  printbuftime = 90<**>  sesstimeout = 45<**>  sizcharbuf = 512<**>  sizerror = 1024<**>  sizworkbuf = 4096<**>; The next lines help you to locate bits in the wrkheuristics entry.<**>;                           1         2         3<**>;                
 0123456789012345678901234567890123<**>  wrkheuristics = 1111111121311111110001011120111221<**>  wrkservices = LSCLIENT<**>  wrknets = NET1<**><[>messenger]<**>  logfile = messages.log<**>  sizmessbuf = 4096<**><[>lsclient]<**>  multilogon = no<**>  timesyn
c = yes<**>  logonverification = domain<**>  logonwarningmsgs = all<**><[>replicator]<**>  replicate = IMPORT<**>  importpath = D:\ibmlan\repl\import<**>  tryuser = yes<**>  password = 
<**><[>services]<**>; Correlates name of service to pathname of service program.<**>; The pathname must be either<**>;       1) an absolute path (including the drive specification)<**>;                       OR<**>;       2) a path relative to the IBMLAN ro
ot<**>  lsclient = services\lsclient.exe<**>  messenger = services\msrvinit.exe<**>  netpopup = services\netpopup.exe<**>  replicator = services\replicat.exe<**>  requester = services\wksta.exe

<:R1,1,1,1080,><:#200,8486>

<:R><:#200,8486>

>

[Embedded]
00072382
