                    /\_______  |\___________
                ;:::\        \/       /    /___:::;
                ;:::/  ^ ____/  .___ /.   ____/:::;
                ;::/     \::\___     \   \_/  \:::;
                ;:/       \::/        >        /::;
                ;<________/:<________/\_______/StE!

                          -*  Present *-


                         S C R L  *CRACKED*
             Semiconductor Cross Reference Library V5.9a


      GETTING STARTED

      Semiconductor Cross-Reference Library is very easy to use,
      and  understand.  It takes  longer to create  the  indexes
      than  it does to  learn how  to use  SCRL, On line help is
      provided if needed.

      You must have at least 15 Buffers and 15 files set in your
      CONFIG.SYS file: BUFFERS=15     FILES=15

      The first time SCRL is run, it will create indexes.
      Depending on the speed of your computer this can take
      a few minutes.

      SCRL needs 11 meg of hard drive space to operate and a EGA
      or VGA/SVGA monitor to be able to display the graphics.

      If at anytime you get Index(NTX) Error or any of the search
      functions are not  working properly.  Go to TECH HELP in the
      Main Menu and select REINDEX DATA FILES, this should correct
      any of these type of problems. **IMPORTANT**: This is a  DOS
      program, it will run  SLOWER  and on some computers it might
      not run at all under Windows!!

      INSTALLING SCRL
         1. Place distribution disk in A or B drive.

         2. Change to distribution drive.  A: <Enter>   or   B: <Enter>

         3. Type  INSTALL  followed by drive, directory you wish
            to install SCRL.


            EXAMPLE:    INSTALL c:\SCRL <ENTER>

         4. Change to installed drive.   C: <Enter>

         5. Change to the SCRL directory.  cd\SCRL <Enter>

         6. Execute SCRL and it will create the index files.
            SCRL <Enter>


      UPGRADING TO NEWER VERSION
         1. Change to drive SCRL is currently installed on.   C: <Enter>

         2. Change to directory SCRL is currently installed in.
            cd\scrl <Enter>

         3. Delete all files in directory SCRL is currently installed in.
            del *.*  <Enter>

            WARNING!!  WARNING!! Make Sure Your In The CORRECT Directory
            Before Performing Step 3!!!!!!

         4. Follow steps 1 through 6 above.


      PACKAGING
         You might wonder why  we use  manila  folders(new and recycled) to
         to ship our products in.  We know it  doesn't look very impressive
         but we want to impress our customers  with our products and prices
         and not with expensive  packaging that you will throw in the trash
         any way.  Keeping our over head down and passing the savings on to
         you is much more important to us.


                 W A R R A N T Y    D I S C L A I M E R
                ----------------------------------------

         THIS PRODUCT IS LICENSED  "AS IS" WITHOUT WARRANTY OF ANY
         KIND;  ALL WARRANTIES ARE DISCLAIMED.  BY USING THE SCRL.
         PRODUCT, YOU AGREE THAT CUSTOM SOFTWARE CREATORS WILL NOT
         BE LIABLE TO YOU OR  ANY THIRD  PARTY FOR  ANY USE OF (OR
         INABILITY TO USE)  THIS  SOFTWARE,  OR  FOR  ANY  DAMAGES
         WHATSOEVER (INCLUDING WITHOUT LIMITATION DAMAGES FOR LOSS
         OF  BUSINESS  PROFITS,  BUSINESS  INTERRUPTION,  LOSS  OF
         BUSINESS  INFORMATION,  AND THE LIKE).  EVEN  IF  WE  ARE
         APPRISED  OF  POSSIBILITY  OF  SUCH  DAMAGES  OCCURRING.
         BECAUSE  SOME  STATES  DO  NOT  ALLOW  THE  EXCLUSION  OR
         LIMITATION OF LIABILITY  FOR  CONSEQUENTIAL OR INCIDENTAL
         DAMAGES,  THE ABOVE LIMITATION MAY NOT APPLY TO YOU.



         CUSTOM SOFTWARE CREATORS
         P.O. BOX 1092
         ST. BETHLEHEM, TN. 37155
         (615)647-6120

         INTERNET:  DAVISM@APSU02.APSU.EDU

         COMPUSERVE:  73651,423

         CRACKED BY BLASTSOFT

         pARASiTe
