LN:DI Professional Edition Release Notes
--------------------------------------------

This document contains release information for the LN:DI Professional Edition
Release 2.6. Updates to the product will be available through the standard Lotus distribution mechanism, Knowledge Base.

After installing the LN:DI Professional Edition client you must modify your Autoexec.bat file. If you are running in a Lotus Notes environment, the Notes program directory must be in your path statement. If you are running in a cc:Mail environment the cc:Mail program directory must be in your path statement.

If you have both the Lotus Notes and cc:Mail program directories in your 
path statement, the LN:DI Professional Edition will use the mail system which is listed first in your path statement.

The LN:DI Professional Edition will not work with the Lotus Notes mail transport when the Notes user ID has a domain certificate about to expire. This problem will be resolved in a later release of Lotus 
Notes.

Users of Compaq Pentium systems with a QVision video controller card must 
add the following line in their SYSTEM.INI file in order for the LN:DI Professional Edition to function properly. Locate the following line in the WIN.INI file, [mga.drv], and under it place the line devbits=off. You will need to restart your system for these changes to take effect.

After installation of the LN:DI Professional Edition you must select File-Printer Setup and select a printer prior to printing a document.

 
Scanners Supported in this release
----------------------------------

The following scanners have been certified for use with LN:DI Professional Edition and have Isis drivers provided. For SCSI based scanners, only Adaptec SCSI controller cards, and vendor specific interface cards listed below are supported.


1. Canon IX-4015 Scanner


Tested with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.

Choose Canon IX-4015, IX-3010 w/ ASPI Isis Driver


2. Microtek Scanmaker II

Tested  with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.

Choose Microtek Scanmaker III w/ASPI Isis Driver

Color scanning is not supported with this scanner, nor is the use of a Sheetfeeder.


3. Fujitsu M3093E

Tested with Kofax 9250 card with Kofax KIPP v2.1.1 software installed.

Choose Kofax BIC Driver ( Simplex ) as the Isis Driver

4. Agfa StudioScan II with Sheetfeeder

Tested with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.

Choose Agfa Studio Series w/ASPI Isis Driver

Sheetfeeder option is not supported in this release.


5. Ricoh IS520 

Tested with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.

Using Ricoh IS-510 & IS-520 Isis Driver.

Duplex mode is not supported in this release.


6. TDC DS 2600

Tested with Kofax 9250 and 9275 card with Kofax KIPP v2.1.1 software installed.

Choose Kofax BIC Simplex Isis Driver

Duplex mode is not supported in this release.


7. Bell and Howell Copi Scan II ( 3338WT )

Tested with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.
 
Choose Bell & Howell RSC (SCSI) Isis Driver


Tested with Kofax 9250 card with Kofax KIPP v2.1.1 software installed.

Choose Kofax BIX Simplex Isis Driver

Border Detect must be disabled in the Isis driver configuration in order for LN:DI Professional to work with this scanner ( choose More in Scanner Setup and disable Border Detect checkbox.)  


8. Microtek Scanmaker II  

Tested with Microtek Scanmaker card ( PNR ) loading their SCSI Driver in CONFIG.SYS

Choose Microtek Scanmaker II Isis Driver

Color scanning and use of the Sheetfeeder option are not supported in this release.

9. Hewlett-Packard ScanJet, Plus, IIC, IIp, IIcx, IIIp, and 3C scanners.

Tested with Adaptec 1542CF SCSI Card with Adaptec  ASPI4DOS.SYS Driver loaded in CONFIG.SYS.

Choose HP ScanJet, Plus, IIc, IIp, IIcx, or IIIp

Tested with Hewlett-Packard SCSI card ( PNR ) loading their SCSI Drivers in CONFIG.SYS.

Choose HP ScanJet, Plus, IIc, IIp, IIcx, or IIIp


