Mwave Patch for Modem performance
=================================

Patch Highlights
----------------
The following patch is intended to improve modem though put performance. 

This patch is intended for limited distribution to IBM customers.
This patch has received limited testing before release by IBM,
therefore we strongly suggest you back up your hard drive before
applying it.  Upon the next release of Mwave code this patch will
be obsolete.


Patch Scope
-----------
This patch is for a DOS/Windows and OS/2 environments.


Patch Contents
--------------
  This patch contains the following Mwave files, which are replaced:
      MVP.DSP
      V42.DSP

  It also contains installation related files:
      FIX.BAT


Patch Prerequisites
-------------------
  1. Mwave Version 1.1 needs to be present on your computer. It is not
     recommended for pervious releases of Mwave.


Patch Instructions
------------------
  1. Install Mwave Version 1.1 code.

  2. Either in DOS or a DOS window

     A. execute this patch by following the following steps:

        change the default drive to the location of the patch disk by
               entering A: (enter)

               where "A:" is the location of the patch disk.

        enter  FIX C xxx       (enter)

               where  "C"  is the drive letter where Mwave code is
                      located (typically this is drive C).

                      "xxx" is the directory structure chosen when
                      Mwave code was installed

                      typically this is:

                          xxx = MWD      for DOS
                          xxx = MWW      for Windows
                          xxx = MWAVEOS2 for OS2

     B. You need to re-run this patch for each operating system that you
        have the Mwave Modem installed.
