Span-N Network Version - 25 Users

Serial Number: BH202c000353-0025-1B2B

Default User:     SPAN
Default Password: SPAN

Disk one is the Administrator and Client Software
Disk two is the Gateway

Quick setup: Get a workstation that you can dedicate as a gateway, install
a modem, set it for 300 baud (yes that's right, 300 baud!). Install Windows,
connect it to the network, keep it was simple as possible (no screen savers,
no E-mail, nothing extra, keep it as vanilla as you can) Be sure to use the
latest VLM's, you don't need WFW networking enabled.  Be sure to CASTOFF ALL
messages so a network broadcast doesn't pause the gateway.  

Now install the Admin software, specify the gateway name.  Enter names, pins,
and phone numbers of the paging services and users and you're ready to roll.
It works with just about and alpha/numeric paging service.



