#  These are sample settings that Enterprise Wide
#  needs in the net.cfg file

Link Support
   Buffers 8 1500
   MemPool 4096
   Max Stacks 8
   Max Boards 4

Link Driver EWPPP
   COMPORT_NUM 1
   X25 0                        ;Sends <cr> forwarding char to X.25 pad.
   Frame ETHERNET_II
   Protocol IPX         8137    ETHERNET_II
   Protocol IP          800     ETHERNET_II
   Protocol ARP         806     ETHERNET_II
   Protocol RARP        8035    ETHERNET_II
   Protocol TSC         7453    ETHERNET_II
   MRU 1500                     ;Maximum frame size
   R_CMAP 0x00002000            ;List of control characters used by link
   R_VJ_COMP 1                  ;Enables Van Jacobson header compression
   R_VJ_SLOTS 4                 ;Size of Van Jacobson compression table.
   R_IPX_HDR_COMP 4             ;Size of IPX header compression table.
   HDLC_T1 3                    ;Link timeout for reliable connections.
   IP_ADDR 0.0.0.0              ;Example.  You must tailor this.
   BITRATE 1152                  ;Example.  You must tailor this.
                                ;    96 for 9600 baud
                                ;   192 for 19200 baud
                                ;   384 for 38400 baud
                                ;   576 for 57600 baud


Protocol TSC
   Bind #1


Netware DOS Requester
   first network drive = F
   netware protocol    = BIND, NDS 
   auto retry          = 0
   vlm                 = AUTO.VLM
