-----------------------------------------------------------------------------
Delrina WinFax PRO             README (Networks) Notes           June 2, 1995
for Networks 4.1
=============================================================================

The following information reflects changes made since the Delrina WinFax PRO 
for Networks Setup Guide and User's Guide went to press, and should be 
reviewed prior to running WinFax PRO for Networks. 

Also review the README file for the main WinFax program for information that 
has changed since the Delrina WinFax PRO User's Guide went to press.

Where applicable, these notes refer to specific sections in the 
appropriate manual.

WinFax online help can provide you with detailed information when you need it 
most -- while you are using WinFax. To get help from any dialog or window in 
WinFax, press F1.


General
=======

Window for Workgroups 3.11 and Real Mode NetBEUI
----------------------------------------------------
If you are running WinFax PRO for Networks 4.0 (TSRs) under Windows for
Workgroups 3.11 in its native networking environment (Windows Network), 
real mode NetBEUI drivers must be loaded prior to loading the TSRs. 
With WinFax PRO for Networks 4.1, real mode NetBEUI drivers are not 
required if you are using DLLs, provided that there are no other 
applications that require these drivers.
 
To remove the real mode NetBEUI drivers,

1. In the Windows SYSTEM.INI file, remove the line ...

	 Autostart=NETBEUI 

   ... from the [network drivers] section.

			AND/OR

2. Edit the AUTOEXEC.BAT file so that the first line reads ...

	NET START

    ... instead of ...
 
	NET START NETBEUI

    ... as was the case with WinFax PRO for Networks 4.0.


Windows for Workgroups 3.11 Users
---------------------------------
If you have disk or printer sharing active in Windows for Workgroups, 
and your computer is configured for a Class 1 or Class 2 fax/modem, 
you may experience an occasional pause when sending or receiving faxes. 
The pause can impact faxing reliability. To ensure that WinFax PRO for 
Networks can fax reliably, either:

- Turn off your disk and printer sharing options in Windows for Workgroups. 
  Double click Network Setup in the Network Group. Click the Sharing button 
  and disable both of the sharing options in the dialog that appears.            

- Move the fax/modem(s) to another system that is not configured to share 
  disk or printer services in Windows for Workgroups.


Enabling NCSI Client Services with an Always IN2000 SCSI Adapter
-----------------------------------------------------------------
You may encounter problems if you are using an Always IN2000 SCSI adapter with 
the VCN:1-02 or VCN:1-03 revision of IN-2000 BIOS and you enable 
NCSI Client Services.

Later revisions of the IN2000 BIOS have been tested successfully with NCSI 
Client Services enabled.

      
Novell Users
------------
Ensure that you have the following driver versions:

 DRIVER        VERSION           HOW TO CHECK
 ======     ===============      ============
 IPX        3.10 or greater        ipx i
 IPXODI     2.12 or greater        ipxodi ?
 NETX       3.32 or greater        netx ?
 VLM        1.20 or greater        nver

Note:  If you have to upgrade any of these drivers, contact Novell.


Technical Support
-----------------
Refer to the Getting Help chapter of the Delrina WinFax PRO for Networks 
Setup Guide before calling Delrina technical support. To contact Delrina 
Technical Support, call:

(716) 853-3009  in the United States (716 is a Buffalo NY area code)
(416) 441-1928  in Canada (416 is a Toronto ON area code)


WinFax PRO for Networks and Win'95
----------------------------------
Since Win'95 is still in beta and has not been officially released,
the initial release of Delrina WinFax PRO for Networks 4.1 will not 
support Win'95, even though preliminary tests have been extremely successful.   


Delrina WinFax PRO for Networks Setup Guide
===========================================

Installing or Changing your WinFax PRO for Networks DOS Server Setup 
(pages 5-28 to 5-31 and 6-28 to 6-29)
--------------------------------------------------------
You cannot install or change the setup of a WinFax PRO for Networks 
DOS Server if CAS fax/modem TSRs are loaded and active.

The SETUPDOS program terminates when CAS fax/modems TSRs are active.
