LN:DI Image Processing Server 2.6 Release Notes
===============================================

Software Problem Report Fixes
-----------------------------

*       Import Multi-page tiff files:  Fixed problem with importing pages of 
        multi-page tiff files in the wrong order

*       Memory Problem:  Fixed memory problem where after the IPS processed a 
        number of requests, an error would appear stating the same memory
        block was deleted twice. 

*       Log Information:  Total Processing Time is now logged in the log
        database

*       IPS log database:  Fixed problem of continuously logging information.
        It no longer grows to an astronomical size

*       Fixed Interchange request failing when Administration database not
        on the IPS machine 

*       Fixed problem with Interchange not removing LN:DI icon

*       Fixed Interchange problem with not being able to process all types of
        DocLinks (e.g. those created with HiTest tools)


New Features
------------

*       Capability to OCR a LN:DI Document

*       Mail-in Database Option for OCR:  Added capability to send OCR
        results to a mail-in database and to specify the destination field
        for the OCR text.

*       Automatic Compaction:   Added feature to have the IPS automatically
        compact local databases.

*       IPS Forms:  Added new and improved forms 

*       Better handling of Delivery Errors



Upgrading from a previous release of the IPS
--------------------------------------------

When upgrading the IPS from 2.5 to 2.6, the associated IPS databases need to
be manually updated by replacing the design of each of these databases with
the new IPS templates.  You will need to highlight the following databases
and select Design...Replace Design (Note: You should make a backup of these
databases before proceeding with this update since this will overwrite any
custom designing you have done).


IPS Administration Database
IPS Log Database
IPS Mail Database
IPS Forms Database

 
MSS Configuration Instructions
------------------------------

MSS 2.5

IPS 2.6 installs the MSS 2.6 client dlls during the installation process. 
If you are using the IPS with MSS 2.5, you must install the MSS 2.5 client
update after you install the IPS.  The MSS 2.5 client update diskette is 
included with MSS Release 2.5.

If you are installing the IPS 2.6 Upgrade, the existing MSS client dlls and
configuration will not be changed.

The following DLL's must be located in the IPS directory.

IMNET_WC.DLL    20,231  10-5-94
MSSAPI_W.DLL    36,079  10-5-94

The following parameters must be included in the MSSCLINT.INI file:

[SERVER]
CONNECT_NAME= <path of shared directory (e.g. M:\SHAREDIR)>

[GENERAL PURPOSE]
CONNECT_NAME=

Refer to page 6 of the MSS Release 2.5 Update Sheet for details on
configuring the MSS.


MSS 2.6

The following DLL's must be located in the IPS directory:

MSSAPI_W.DLL       54,643       06-06-95
MSSRES.DLL         52,224       06-06-95
NLDAPI.DLL          5,264       06-06-95
NETCP_W.DLL        43,232       06-06-95
NETFP_W.DLL        22,279       06-06-95
NETIPX_W.DLL       20,794       06-06-95
NETNP_W.DLL        13,102       06-06-95

The following parameters must be included in the MSSCLINT.INI file.  The
values entered in this file depend on what MSS network driver you are using.

[SERVER]

CONNECT_NAME=
DLL_NAME =


Network Driver          DLL_NAME        CONNECT_NAME
--------------          ------------    ------------
NetWare SPX             NETIPX_W        Server Name defined in NetWare
                                        SPX driver configuration on
                                        MSS server
                                    
TCP/IP                  NETCP_W         Host name of MSS server

Named Pipes             NETNP_W         \\<server_name>\PIPE\MSSPIPE where
                                        <server_name> is the name of the MSS
                                        server
                                        - From LAN Requester if using
                                          LAN Server
                                        - From MSS_VINES_HANDLE environment
                                          variable if using Banyan VINES
                                        - From NPDAEMON statement in
                                          CONFIG.SYS if using NetWare
                                                                                          
MSS File Pipes          NETFP_W         Fully qualified path to shared
                                        directory from the IPS 
                                                                                                
Refer to the LN:DI MSS 2.6 Administrator's Guide for more information on
MSS network communications.                                                                                                                                                                                                                                      
