        #
        | README file for
        |
        | Telix for DOS, version 3.51
        |
        | Copyright (c) 1994-96 ELSA GmbH, Aachen (Germany)
        |
        |                                     Subsidary:
        | ELSA GmbH                           ELSA Inc.
        | Sonnenweg 11                        2150 Trade Zone Blvd.
        | D-52070 Aachen                      Suite 101
        | Germany                             San Jose, CA 95131
        |                                     USA
        |
        | Phone      : +49-241-9177-0         Phone: +1-408-935-0350
        | Support Fax: +49-241-9177-113       Phone:  1-800-272-ELSA
        | BBS (modem): +49-241-9177-981       Fax  : +1-408-935-0370
        | BBS (ISDN) : +49-241-9177-7800      BBS  : +1-408-935-0380
        | CompuServe : GO ELSA                CIS  : GO ELSA
        | WWW        : http://www.elsa.de     WWW  : http://www.elsa.com
        |
        | 04/19/96, bg


        Table of Contents

        1.      Overview
        2.      Contents
        3.      Installation
        4.      Notes


------------------------------------------------------------------------

1.      Overview

        This directory contains the installation files of Telix
        for DOS v3.51.


------------------------------------------------------------------------

2.      Contents

        INSTALL.BAT          Installation batch file
        INSTALL.DAT          Ressource file for INST.EXE
        INST.EXE             Installation program
        README.TXT           This file
        SETUP.PIF            PIF file for installing under Windows
        TELIX351.DAT         Compressed data file


------------------------------------------------------------------------

3.      Installation

        Before you can run Telix for DOS, you must install it first.
        To start the installation please type INSTALL at the DOS prompt
        and press the <Enter> key. If you want to start the
        installation of Telix for DOS under Windows, please launch
        the SETUP.PIF file (e.g. in the Windows file manager) instead
        of.  Then follow the instructions on the screen. After the
        installation has been finished succesfully, type TELIX at the
        DOS prompt and press the <Enter> key.  However, if you decided
        to modify your AUTOEXEC.BAT file during the installation
        process, you should reboot your PC before to let the changes
        take effect.


------------------------------------------------------------------------

4.      Notes

        Please do NOT start the installation by only running the
        INST.EXE file. In that case Telix will not work properly!

        If your modem brand cannot be found in the modem list, which is
        displayed during the modem configuration process, please select
        an appropriate one of the 'Generic' models!


------------------------------------------------------------------------
